<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Wire-to-Board Connectors - WR-BHD &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-11-27&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="62701421621">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1.27mm Male THT Box Header Straight, 14Pins</description>
</package>
<package name="62501421621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Box Headerr, 14 pins</description>
</package>
<package name="62531420621">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male SMT Box Header,14 pins</description>
</package>
<package name="61200622323">
<description>&lt;B&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Board to Cable Transition Connector, 6 Pins</description>
</package>
<package name="61202421721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54 mm Male Angled Box Header,24 Pins</description>
</package>
<package name="61203421721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54 mm Male Angled Box Header,34 Pins</description>
</package>
<package name="61201020621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt;&lt;BR&gt;2.54 mm Male SMT Box Header,10 pins</description>
</package>
<package name="62704421721">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1,27mm Male THT Box Header Right angle, 44Pins</description>
</package>
<package name="61203422323">
<description>&lt;B&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54mm Board to Cable Transition Connector, 34 Pins</description>
</package>
<package name="61201621621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header,16 Pins</description>
</package>
<package name="62505022323">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;-2.00 mm Board to Cable Transition Connector,50 pins</description>
</package>
<package name="612006235121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header High Temperature, 6 Pins</description>
</package>
<package name="612008235121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header High Temperature, 8 Pins</description>
</package>
<package name="62505021621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Box Headerr, 50 pins</description>
</package>
<package name="61202022821">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header with long lever,20 Pins</description>
</package>
<package name="62501422323">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Board to Cable Transition Connector, 14 pins</description>
</package>
<package name="61202622323">
<description>&lt;B&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54mm Board to Cable Transition Connector, 26 Pins</description>
</package>
<package name="612034235121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header High Temperature, 34 Pins</description>
</package>
<package name="61205021721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54 mm Male Angled Box Header,50 Pins</description>
</package>
<package name="62701021721">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1,27mm Male THT Box Header Right angle, 10Pins</description>
</package>
<package name="62703021721">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1,27mm Male THT Box Header Right angle, 30Pins</description>
</package>
<package name="61201422921">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Angled Box Header with long lever, 14 Pins</description>
</package>
<package name="62504022121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Angled Box Header w. Lever,40 Pins</description>
</package>
<package name="61204022121">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;  2.54 mm Male Angled Box Header with short lever,40 Pins</description>
</package>
<package name="61201422021">
<description>&lt;b&gt;WR-BHD &lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header with short lever,14 Pins</description>
</package>
<package name="62701221621">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1.27mm Male THT Box Header Straight, 12Pins</description>
</package>
<package name="61203422921">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Angled Box Header with long lever, 34 Pins</description>
</package>
<package name="62701221721">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1,27mm Male THT Box Header Right angle, 12Pins</description>
</package>
<package name="612016235221">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Angled Box Header High Temperature, 16 Pins</description>
</package>
<package name="612020235221">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Angled Box Header High Temperature, 20 Pins</description>
</package>
<package name="61202422121">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;  2.54 mm Male Angled Box Header with short lever,24 Pins</description>
</package>
<package name="62531620621">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male SMT Box Header,16 pins</description>
</package>
<package name="61205022323">
<description>&lt;B&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54mm Board to Cable Transition Connector, 50 Pins</description>
</package>
<package name="62701621621">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1.27mm Male THT Box Header Straight, 16Pins</description>
</package>
<package name="612040235121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header High Temperature, 40 Pins</description>
</package>
<package name="62503422323">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Board to Cable Transition Connector,34 pins</description>
</package>
<package name="62531020621">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male SMT Box Header,10 pins</description>
</package>
<package name="61200621721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54 mm Male Angled Box Header, 6 Pins</description>
</package>
<package name="61202622021">
<description>&lt;b&gt;WR-BHD &lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header with short lever, 26 Pins</description>
</package>
<package name="61203420621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt;&lt;BR&gt;2.54 mm Male SMT Box Header, 34 pins</description>
</package>
<package name="62706021721">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1,27mm Male THT Box Header Right angle, 60Pins</description>
</package>
<package name="62501022121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Angled Box Header w. Lever, 10 pins</description>
</package>
<package name="61231020621">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header

&lt;/B&gt;&lt;BR&gt; &lt;BR&gt;2.54 mm, SMT, 10Pins</description>
</package>
<package name="612020235121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header High Temperature, 20 Pins</description>
</package>
<package name="61200621621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header, 6 Pins</description>
</package>
<package name="61206021621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header,60Pins</description>
</package>
<package name="62504021621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Box Headerr, 40 pins</description>
</package>
<package name="612006235221">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Angled Box Header High Temperature, 6 Pins</description>
</package>
<package name="61201421721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54 mm Male Angled Box Header,14 Pins</description>
</package>
<package name="61201022323">
<description>&lt;B&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54mm Board to Cable Transition Connector, 10 Pins</description>
</package>
<package name="62732020621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 20pins, SMT</description>
</package>
<package name="61202020621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt;&lt;BR&gt;2.54 mm Male SMT Box Header,20 pins</description>
</package>
<package name="61203422821">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header with long lever,34 Pins</description>
</package>
<package name="62705021721">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1,27mm Male THT Box Header Right angle, 50Pins</description>
</package>
<package name="62504422021">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Box Header with Lever,44 pins</description>
</package>
<package name="612010235121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header High Temperature, 10 Pins</description>
</package>
<package name="62534420621">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male SMT Box Header,44 pins</description>
</package>
<package name="61201422323">
<description>&lt;B&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54mm Board to Cable Transition Connector, 14 Pins</description>
</package>
<package name="62533020621">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male SMT Box Header,30 pins</description>
</package>
<package name="62702420621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 24pins, SMT</description>
</package>
<package name="62503021621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Box Headerr, 30 pins</description>
</package>
<package name="61206421621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header,64Pins</description>
</package>
<package name="61204020621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt;&lt;BR&gt;2.54 mm Male SMT Box Header, 40 pins</description>
</package>
<package name="61201622121">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;  2.54 mm Male Angled Box Header with short lever,16 Pins</description>
</package>
<package name="61202422021">
<description>&lt;b&gt;WR-BHD &lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header with short lever, 24 Pins</description>
</package>
<package name="62701020621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 10pins, SMT</description>
</package>
<package name="61205022921">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Angled Box Header with long lever, 50 Pins</description>
</package>
<package name="62703020621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 30pins, SMT</description>
</package>
<package name="61231420621">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header

&lt;/B&gt;&lt;BR&gt; &lt;BR&gt;2.54 mm, SMT, 14Pins</description>
</package>
<package name="61202422821">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header with long lever,24 Pins</description>
</package>
<package name="61205022821">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header with long lever,50 Pins</description>
</package>
<package name="62702021721">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1,27mm Male THT Box Header Right angle, 20Pins</description>
</package>
<package name="62502022323">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Board to Cable Transition Connector,20 pins</description>
</package>
<package name="61202621721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54 mm Male Angled Box Header,26 Pins</description>
</package>
<package name="612026235121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header High Temperature, 26 Pins</description>
</package>
<package name="612026235221">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Angled Box Header High Temperature,26 Pins</description>
</package>
<package name="61200821621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header, 8 Pins</description>
</package>
<package name="62502621621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Box Headerr,26 pins</description>
</package>
<package name="612010235221">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Angled Box Header High Temperature,10 Pins</description>
</package>
<package name="62735020621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 50pins, SMT</description>
</package>
<package name="62503421721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Angled Box Header,34 pins</description>
</package>
<package name="61204021721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54 mm Male Angled Box Header, 40 Pins</description>
</package>
<package name="62535020621">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male SMT Box Header,50 pins</description>
</package>
<package name="62502622121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Angled Box Header w. Lever,26 pins</description>
</package>
<package name="61201621721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54 mm Male Angled Box Header, 16 Pins</description>
</package>
<package name="61232020621">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header

&lt;/B&gt;&lt;BR&gt; &lt;BR&gt;2.54 mm, SMT, 20Pins</description>
</package>
<package name="62702621721">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1,27mm Male THT Box Header Right angle, 26Pins</description>
</package>
<package name="61201021621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header, 10 Pins</description>
</package>
<package name="62702421721">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1,27mm Male THT Box Header Right angle, 24Pins</description>
</package>
<package name="62704021621">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1.27mm Male THT Box Header Straight, 40Pins</description>
</package>
<package name="62705020621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 50pins, SMT</description>
</package>
<package name="62701220621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 12pins, SMT</description>
</package>
<package name="61202421621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header, 24 Pins</description>
</package>
<package name="62503422121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Angled Box Header w. Lever,34 Pins</description>
</package>
<package name="62502022121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Angled Box Header w. Lever,20 pins</description>
</package>
<package name="62704420621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 44pins, SMT</description>
</package>
<package name="62533420621">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male SMT Box Header,34 pins</description>
</package>
<package name="62501621721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Angled Box Header,16 pins</description>
</package>
<package name="62505021721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Angled Box Header,50 pins</description>
</package>
<package name="62501422121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Angled Box Header w. Lever, 14 pins</description>
</package>
<package name="62731020621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 10pins, SMT</description>
</package>
<package name="62702621621">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1.27mm Male THT Box Header Straight, 26Pins</description>
</package>
<package name="62504421621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Box Headerr, 44 pins</description>
</package>
<package name="61200821721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54 mm Male Angled Box Header, 8 Pins</description>
</package>
<package name="612014235221">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Angled Box Header High Temperature,14 Pins</description>
</package>
<package name="62703421621">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1.27mm Male THT Box Header Straight, 34Pins</description>
</package>
<package name="62702021621">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1.27mm Male THT Box Header Straight, 20Pins</description>
</package>
<package name="61203921621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header,39 Pins</description>
</package>
<package name="61202622821">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header with long lever, 26 Pins</description>
</package>
<package name="61203422021">
<description>&lt;b&gt;WR-BHD &lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header with short lever,34 Pins</description>
</package>
<package name="61200820621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt;&lt;BR&gt;2.54 mm Male SMT Box Header,,8 pins</description>
</package>
<package name="61201622821">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header with long lever,16 Pins</description>
</package>
<package name="62504021721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Angled Box Header,40 pins</description>
</package>
<package name="62704421621">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1.27mm Male THT Box Header Straight, 44Pins</description>
</package>
<package name="62703021621">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1.27mm Male THT Box Header Straight, 30Pins</description>
</package>
<package name="61201022821">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header with long lever, 10 Pins</description>
</package>
<package name="61205021621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header,50 Pins</description>
</package>
<package name="61204021621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header, 40 Pins</description>
</package>
<package name="62701420621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 14pins, SMT</description>
</package>
<package name="62501421721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Angled Box Header,14 pins</description>
</package>
<package name="62503421621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Box Headerr, 34 pins</description>
</package>
<package name="62702020621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 20pins, SMT</description>
</package>
<package name="61204022021">
<description>&lt;b&gt;WR-BHD &lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header with short lever, 40 Pins</description>
</package>
<package name="61201422121">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;  2.54 mm Male Angled Box Header with short lever,14 Pins</description>
</package>
<package name="61201422821">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header with long lever, 14 Pins</description>
</package>
<package name="62504421721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Angled Box Header,44 pins</description>
</package>
<package name="62501022021">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Box Header with Lever, 10 pins</description>
</package>
<package name="61202022121">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;  2.54 mm Male Angled Box Header with short lever,, 20 Pins</description>
</package>
<package name="62501621621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Box Headerr,  16 pins</description>
</package>
<package name="61206022921">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Angled Box Header with long lever,60 Pins</description>
</package>
<package name="62505022021">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Box Header with Lever,50 pins</description>
</package>
<package name="612034235221">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Angled Box Header High Temperature,34 Pins</description>
</package>
<package name="61206422821">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header with long lever, 64 Pins</description>
</package>
<package name="62534020621">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male SMT Box Header,40 pins</description>
</package>
<package name="61201622921">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Angled Box Header with long lever,  16 Pins</description>
</package>
<package name="62701421721">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1,27mm Male THT Box Header Right angle, 14Pins</description>
</package>
<package name="62502622021">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Box Header with Lever,26 pins</description>
</package>
<package name="61206022021">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever 
&lt;br&gt;&lt;/b&gt;60 Pins</description>
</package>
<package name="612050235221">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Angled Box Header High Temperature,50 Pins</description>
</package>
<package name="62701021621">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1.27mm Male THT Box Header Straight, 10Pins</description>
</package>
<package name="612008235221">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Angled Box Header High Temperature,8 Pins</description>
</package>
<package name="61202620621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt;&lt;BR&gt;2.54 mm Male SMT Box Header, 26 pins</description>
</package>
<package name="61233420621">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header

&lt;/B&gt;&lt;BR&gt; &lt;BR&gt;2.54 mm, SMT, 34Pins</description>
</package>
<package name="62502421621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Box Headerr, 24Pins;</description>
</package>
<package name="62701621721">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1,27mm Male THT Box Header Right angle, 16Pins</description>
</package>
<package name="61204022821">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header with long lever,40 Pins</description>
</package>
<package name="62502021621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Box Headerr, 20 pins</description>
</package>
<package name="61201022021">
<description>&lt;b&gt;WR-BHD &lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header with short lever,10 Pins</description>
</package>
<package name="61202022921">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Angled Box Header with long lever, 20 Pins</description>
</package>
<package name="61232620621">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header

&lt;/B&gt;&lt;BR&gt; &lt;BR&gt;2.54 mm, SMT, 26Pins</description>
</package>
<package name="61202422921">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Angled Box Header with long lever,  24 Pins</description>
</package>
<package name="62501022323">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Board to Cable Transition Connector, 10 pins</description>
</package>
<package name="62705021621">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1.27mm Male THT Box Header Straight, 50Pins</description>
</package>
<package name="62733020621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 30pins, SMT</description>
</package>
<package name="61231620621">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header

&lt;/B&gt;&lt;BR&gt; &lt;BR&gt;2.54 mm, SMT, 16Pins</description>
</package>
<package name="61201022921">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Angled Box Header with long lever, 10 Pins</description>
</package>
<package name="62502621721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Angled Box Header,26 pins</description>
</package>
<package name="62702620621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 26pins, SMT</description>
</package>
<package name="62706021621">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1.27mm Male THT Box Header Straight, 60Pins</description>
</package>
<package name="612050235121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header High Temperature, 50 Pins</description>
</package>
<package name="612016235121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header High Temperature, 16 Pins</description>
</package>
<package name="62501021621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Box Headerr, 10 pins</description>
</package>
<package name="62502022021">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Box Header with Lever,20 pins</description>
</package>
<package name="62532020621">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male SMT Box Header,20 pins</description>
</package>
<package name="61201622021">
<description>&lt;b&gt;WR-BHD &lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header with short lever,16 Pins</description>
</package>
<package name="61202021721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54 mm Male Angled Box Header, 20 Pins</description>
</package>
<package name="62501021721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Angled Box Header,10 pins</description>
</package>
<package name="612040235221">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Angled Box Header High Temperature,40 Pins</description>
</package>
<package name="62504022021">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Box Header with Lever,40 pins</description>
</package>
<package name="62532620621">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male SMT Box Header,26 pins</description>
</package>
<package name="62501422021">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Box Header with Lever,14 Pins</description>
</package>
<package name="61201420621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt;&lt;BR&gt;2.54 mm Male SMT Box Header,14 pins</description>
</package>
<package name="62503422021">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Box Header with Lever,34 pins</description>
</package>
<package name="61201022121">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;  2.54 mm Male Angled Box Header with short lever,10 Pins</description>
</package>
<package name="61202420621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt;&lt;BR&gt;2.54 mm Male SMT Box Header, 24 pins</description>
</package>
<package name="62502622323">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Board to Cable Transition Connector,26 pins</description>
</package>
<package name="61203422121">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;  2.54 mm Male Angled Box Header with short lever,34 Pins</description>
</package>
<package name="61203421621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header,34 Pins</description>
</package>
<package name="62734020621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 40pins, SMT</description>
</package>
<package name="62703421721">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1,27mm Male THT Box Header Right angle, 34Pins</description>
</package>
<package name="61202021621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header, 20 Pins</description>
</package>
<package name="62731620621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 16pins, SMT</description>
</package>
<package name="62704020621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 40pins, SMT</description>
</package>
<package name="61204022323">
<description>&lt;B&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54mm Board to Cable Transition Connector, 40 Pins</description>
</package>
<package name="62704021721">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1,27mm Male THT Box Header Right angle, 40Pins</description>
</package>
<package name="61202622121">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;  2.54 mm Male Angled Box Header with short lever, 26 Pins</description>
</package>
<package name="62731220621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 12pins, SMT</description>
</package>
<package name="61234020621">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header

&lt;/B&gt;&lt;BR&gt; &lt;BR&gt;2.54 mm, SMT, 40Pins</description>
</package>
<package name="62703420621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 34pins, SMT</description>
</package>
<package name="62734420621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 44pins, SMT</description>
</package>
<package name="61205022021">
<description>&lt;b&gt;WR-BHD &lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header with short lever, 50 Pins</description>
</package>
<package name="61200822323">
<description>&lt;B&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54mm Board to Cable Transition Connector, 8 Pins</description>
</package>
<package name="61206022821">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header with long lever,60 Pins</description>
</package>
<package name="62733420621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 34pins, SMT</description>
</package>
<package name="61201620621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt;&lt;BR&gt;2.54 mm Male SMT Box Header,16 pins</description>
</package>
<package name="62731420621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 14pins, SMT</description>
</package>
<package name="62732420621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 24pins, SMT</description>
</package>
<package name="61202622921">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Angled Box Header with long lever,  26 Pins</description>
</package>
<package name="62502021721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.00 mm Male Angled Box Header,20 pins</description>
</package>
<package name="62503022323">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Board to Cable Transition Connector,30 pins</description>
</package>
<package name="62732620621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 26pins, SMT</description>
</package>
<package name="61205022121">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;  2.54 mm Male Angled Box Header with short lever, 50 Pins</description>
</package>
<package name="62504422121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Angled Box Header w. Lever,44 pins</description>
</package>
<package name="61204022921">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Angled Box Header with long lever, 40 Pins</description>
</package>
<package name="612014235121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header High Temperature,14 Pins</description>
</package>
<package name="61232420621">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header

&lt;/B&gt;&lt;BR&gt; &lt;BR&gt;2.54 mm, SMT, 24Pins</description>
</package>
<package name="62505022121">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Male Angled Box Header w. Lever,50 pins</description>
</package>
<package name="62702421621">
<description>&lt;B&gt;WR-BHD 
&lt;/B&gt;&lt;BR&gt;1.27mm Male THT Box Header Straight, 24Pins</description>
</package>
<package name="61202621621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header, 26 Pins</description>
</package>
<package name="61201421621">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;2.54 mm Male Box Header, 14 Pins</description>
</package>
<package name="62504022323">
<description>&lt;b&gt;WR-BHD&lt;/b&gt;&lt;br&gt;2.00 mm Board to Cable Transition Connector,40 pins</description>
</package>
<package name="62701620621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch: 1.27mm, 16pins, SMT</description>
</package>
<package name="61202022323">
<description>&lt;B&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54mm Board to Cable Transition Connector, 20 Pins</description>
</package>
<package name="61201622323">
<description>&lt;B&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;.54mm Board to Cable Transition Connector, 16 Pins</description>
</package>
<package name="61201021721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54 mm Male Angled Box Header, 10 Pins</description>
</package>
<package name="61206021721">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt; 2.54 mm Male Angled Box Header, 60 Pins</description>
</package>
<package name="61206022121">
<description>&lt;b&gt;WR-BHD&lt;/B&gt; &lt;BR&gt;  2.54 mm Male Angled Box Header with short lever, 60 Pins</description>
</package>
<package name="61202022021">
<description>&lt;b&gt;WR-BHD &lt;/b&gt;&lt;br&gt;2.54 mm Male Box Header with short lever,20 Pins</description>
</package>
</packages>
<symbols>
<symbol name="7X2MT-1">
<description>7x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="7X2MS">
<description>7x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="7X2MT">
<description>7x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="17X2MT_1">
<description>17x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="5X2MS">
<description>5x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="3X2FT">
<description>3X2Rows Female THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="22X2MT_1">
<description>22x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
</symbol>
<symbol name="12X2MT_1">
<description>12x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="8X2MT">
<description>8x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="3X2MT">
<description>3x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="17X2FT">
<description>17X2Rows Female THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="4X2MT">
<description>4x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="10X2MT">
<description>10x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="7X2FT">
<description>7X2Rows Female THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="20X2MT_1">
<description>20x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="25X2MT">
<description>25x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
</symbol>
<symbol name="25X2FT">
<description>25X2Rows Female THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
</symbol>
<symbol name="17X2MT">
<description>17x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="15X2MT_1">
<description>15x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="13X2FT">
<description>13X2Rows Female THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="25X2MT_1">
<description>25x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
</symbol>
<symbol name="6X2MT">
<description>6x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="7X2MT_1">
<description>7x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="5X2MT_1">
<description>5x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="6X2MT_1">
<description>6x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="10X2MT_1">
<description>10x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="8X2MS">
<description>8x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="8X2MT_1">
<description>8x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="8X2MT-1">
<description>8x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="17X2MS">
<description>17x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="20X2MT">
<description>20x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="3X2MT_1">
<description>3x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="13X2MT">
<description>13x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="30X2MT_1">
<description>30x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="53" direction="pas"/>
<pin name="54" direction="pas"/>
<pin name="55" direction="pas"/>
<pin name="56" direction="pas"/>
<pin name="57" direction="pas"/>
<pin name="58" direction="pas"/>
<pin name="59" direction="pas"/>
<pin name="60" direction="pas"/>
</symbol>
<symbol name="5X2FT">
<description>5X2Rows Female THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="30X2MT">
<description>30x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="53" direction="pas"/>
<pin name="54" direction="pas"/>
<pin name="55" direction="pas"/>
<pin name="56" direction="pas"/>
<pin name="57" direction="pas"/>
<pin name="58" direction="pas"/>
<pin name="59" direction="pas"/>
<pin name="60" direction="pas"/>
</symbol>
<symbol name="12X2MS-1">
<description>12x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="10X2MS">
<description>10x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="10X2MS-2">
<description>10x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="5X2MT">
<description>5x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="15X2MT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="22X2MT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
</symbol>
<symbol name="32X2MT">
<description>32x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="53" direction="pas"/>
<pin name="54" direction="pas"/>
<pin name="55" direction="pas"/>
<pin name="56" direction="pas"/>
<pin name="57" direction="pas"/>
<pin name="58" direction="pas"/>
<pin name="59" direction="pas"/>
<pin name="60" direction="pas"/>
<pin name="61" direction="pas"/>
<pin name="62" direction="pas"/>
<pin name="63" direction="pas"/>
<pin name="64" direction="pas"/>
</symbol>
<symbol name="22X2MS">
<description>22x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
</symbol>
<symbol name="20X2MS">
<description>20x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="15X2MS">
<description>15x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="12X2MT">
<description>12x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="5X2MS-1">
<description>5x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="13X2MT_1">
<description>13x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="15X2MS-1">
<description>15x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="10X2FT">
<description>10X2Rows Female THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="25X2MS-2">
<description>25x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
</symbol>
<symbol name="25X2MS">
<description>25x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
</symbol>
<symbol name="20X2MT-1">
<description>20x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="25X2MS-1">
<description>25x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
</symbol>
<symbol name="6X2MS">
<description>5x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="22X2MS-1">
<description>22x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
</symbol>
<symbol name="13X2MT-1">
<description>13x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="5X2MS-2">
<description>5x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="10X2MT-1">
<description>10x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="4X2MT_1">
<description>4x2Row Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="17X2MT-1">
<description>17x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="19X2+1MT">
<description>19x2Rows +1, Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
</symbol>
<symbol name="4X2MS">
<description>4x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="22X2MT-1">
<description>22x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
</symbol>
<symbol name="7X2MS-1">
<description>7x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="10X2MS-1">
<description>10x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="15X2MT-1">
<description>15x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="13X2MS">
<description>13x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="5X2MT-1">
<description>5x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="25X2MT-1">
<description>25x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
</symbol>
<symbol name="15X2MS-2">
<description>15x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="30X2MT-1">
<description>30x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="53" direction="pas"/>
<pin name="54" direction="pas"/>
<pin name="55" direction="pas"/>
<pin name="56" direction="pas"/>
<pin name="57" direction="pas"/>
<pin name="58" direction="pas"/>
<pin name="59" direction="pas"/>
<pin name="60" direction="pas"/>
</symbol>
<symbol name="13X2MS-1">
<description>13x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="12X2MS">
<description>12x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="20X2MS-2">
<description>20x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="20X2MS-1">
<description>20x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="8X2MS-2">
<description>8x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="20X2FT">
<description>20X2Rows Female THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="6X2MS-1">
<description>5x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="17X2MS-1">
<description>17x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="22X2MS-2">
<description>22x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
</symbol>
<symbol name="4X2FT">
<description>4X2Rows Female THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="17X2MS-2">
<description>17x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="7X2MS-2">
<description>7x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="15X2FT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="12X2MS-2">
<description>12x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="13X2MS-2">
<description>13x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="12X2MT-1">
<description>12x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="8X2MS-1">
<description>8x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="8X2FT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="6253XX20621_62531420621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA9T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel with Cap
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS"/>
</gates>
<devices>
<device name="" package="62531420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62531420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="21.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 62531420621 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62531420621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21621_62501421621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT"/>
</gates>
<devices>
<device name="" package="62501421621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62501421621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="21.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62501421621 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62501421621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21621_62701421621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION:
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT-1"/>
</gates>
<devices>
<device name="" package="62701421621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62701421621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="15.24mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62701421621 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62701421621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21721_61202421721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-29&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT_1"/>
</gates>
<devices>
<device name="" package="61202421721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202421721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="40.68mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202421721 "/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61202421721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22323_61200622323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2FT"/>
</gates>
<devices>
<device name="" package="61200622323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61200622323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="13.07mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61200622323"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61200622323"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21721_62704421721" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-03-02&lt;BR&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2MT_1"/>
</gates>
<devices>
<device name="" package="62704421721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62704421721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="34.29mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62704421721 "/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62704421721 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21721_61203421721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-29&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT_1"/>
</gates>
<devices>
<device name="" package="61203421721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61203421721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="58.46mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61203421721 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61203421721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX20621_61201020621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS"/>
</gates>
<devices>
<device name="" package="61201020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="20.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value=" 61201020621 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61201020621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61201621621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="61201621621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201621621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="27.98mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201621621 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61201621621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22323_61203422323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2FT"/>
</gates>
<devices>
<device name="" package="61203422323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61203422323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="48.63mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61203422323 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61203422323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22323_62505022323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval：E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2FT"/>
</gates>
<devices>
<device name="" package="62505022323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62505022323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="54.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62505022323 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62505022323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235121_612008235121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="612008235121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612008235121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="17.78mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612008235121"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="612008235121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235121_612006235121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="612006235121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612006235121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="15.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612006235121"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="612006235121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22821_61202022821" prefix="J">
<description>&lt;b&gt;2.54 mm Male Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT"/>
</gates>
<devices>
<device name="" package="61202022821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202022821?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="44.9mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202022821 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202022821 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21621_62505021621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT"/>
</gates>
<devices>
<device name="" package="62505021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62505021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="57.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62505021621 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62505021621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22323_62501422323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval：E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2FT"/>
</gates>
<devices>
<device name="" package="62501422323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62501422323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="18.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62501422323 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62501422323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21721_61205021721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-29&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT_1"/>
</gates>
<devices>
<device name="" package="61205021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61205021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="71.16mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61205021721 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61205021721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235121_612034235121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT"/>
</gates>
<devices>
<device name="" package="612034235121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612034235121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="50.8mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612034235121"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="612034235121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22323_61202622323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2FT"/>
</gates>
<devices>
<device name="" package="61202622323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202622323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="38.47mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202622323 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202622323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21721_62703021721" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15X2MT_1"/>
</gates>
<devices>
<device name="" package="62703021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62703021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="25.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62703021721 "/>
<attribute name="PINS" value=" 30 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62703021721 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21721_62701021721" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="62701021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62701021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="12.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62701021721 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62701021721 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22121_62504022121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header w. Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121"&gt;
https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT_1"/>
</gates>
<devices>
<device name="" package="62504022121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62504022121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="55.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62504022121 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62504022121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22921_61201422921" prefix="J">
<description>&lt;b&gt;2.54 mm Male Angled Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_1"/>
</gates>
<devices>
<device name="" package="61201422921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201422921?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="37.28mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201422921 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61201422921 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22921_61203422921" prefix="J">
<description>&lt;b&gt;2.54 mm Male Angled Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT_1"/>
</gates>
<devices>
<device name="" package="61203422921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61203422921?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="62.68mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61203422921 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61203422921 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22121_61204022121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT_1"/>
</gates>
<devices>
<device name="" package="61204022121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61204022121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="70.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61204022121 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61204022121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21621_62701221621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION:
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="62701221621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62701221621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="13.97mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62701221621 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62701221621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21721_62701221721" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_1"/>
</gates>
<devices>
<device name="" package="62701221721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62701221721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="13.97mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62701221721 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62701221721 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235221_612020235221" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_1"/>
</gates>
<devices>
<device name="" package="612020235221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612020235221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="33mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612020235221"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="612020235221"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22021_61201422021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT"/>
</gates>
<devices>
<device name="" package="61201422021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201422021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="37.28mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61201422021"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61201422021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235221_612016235221" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_1"/>
</gates>
<devices>
<device name="" package="612016235221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612016235221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="27.92mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612016235221"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="612016235221"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22323_61205022323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2FT"/>
</gates>
<devices>
<device name="" package="61205022323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61205022323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="68.95mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61205022323 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61205022323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22121_61202422121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT_1"/>
</gates>
<devices>
<device name="" package="61202422121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202422121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="49.98mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202422121 "/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61202422121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6253XX20621_62531620621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA9T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel with Cap
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS"/>
</gates>
<devices>
<device name="" package="62531620621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62531620621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="23.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 62531620621 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62531620621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21621_62701621621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION:
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT-1"/>
</gates>
<devices>
<device name="" package="62701621621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62701621621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="16.51mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62701621621 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62701621621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22323_62503422323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval：E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2FT"/>
</gates>
<devices>
<device name="" package="62503422323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62503422323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="38.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62503422323 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62503422323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6253XX20621_62531020621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA9T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel with Cap
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS"/>
</gates>
<devices>
<device name="" package="62531020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62531020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="17.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62531020621"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62531020621"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235121_612040235121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT"/>
</gates>
<devices>
<device name="" package="612040235121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612040235121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="58.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612040235121"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="612040235121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21721_61200621721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-29&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_1"/>
</gates>
<devices>
<device name="" package="61200621721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61200621721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="15.28mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61200621721"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61200621721"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22021_61202622021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT"/>
</gates>
<devices>
<device name="" package="61202622021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202622021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="52.52mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202622021 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202622021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX20621_61203420621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MS"/>
</gates>
<devices>
<device name="" package="61203420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61203420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="50.98mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value=" 61203420621 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61203420621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21721_62706021721" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="30X2MT_1"/>
</gates>
<devices>
<device name="" package="62706021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62706021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="44.45mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62706021721 "/>
<attribute name="PINS" value=" 60 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62706021721 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6123XX20621_61231020621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;
Material Properties&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-09-06&lt;BR&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS"/>
</gates>
<devices>
<device name="" package="61231020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61231020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="20.32mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 61231020621 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61231020621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235121_612020235121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT"/>
</gates>
<devices>
<device name="" package="612020235121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612020235121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="33mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612020235121"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="612020235121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22121_62501022121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header w. Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121"&gt;
https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="62501022121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62501022121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="25.7 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62501022121 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62501022121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61200621621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="61200621621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61200621621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="15.28mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61200621621"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61200621621"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61206021621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="30X2MT"/>
</gates>
<devices>
<device name="" package="61206021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61206021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="83.86mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61206021621 "/>
<attribute name="PINS" value=" 60 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61206021621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235221_612006235221" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_1"/>
</gates>
<devices>
<device name="" package="612006235221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612006235221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="15.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612006235221"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="612006235221"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21621_62504021621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT"/>
</gates>
<devices>
<device name="" package="62504021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62504021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="47.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62504021621 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62504021621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21721_61201421721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-29&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_1"/>
</gates>
<devices>
<device name="" package="61201421721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201421721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="27.98mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201421721 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61201421721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22323_61201022323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2FT"/>
</gates>
<devices>
<device name="" package="61201022323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201022323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="18.15mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201022323 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61201022323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX20621_61202020621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MS"/>
</gates>
<devices>
<device name="" package="61202020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="33.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value=" 61202020621 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202020621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22821_61203422821" prefix="J">
<description>&lt;b&gt;2.54 mm Male Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT"/>
</gates>
<devices>
<device name="" package="61203422821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61203422821?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="62.68mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61203422821 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61203422821 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22021_62504422021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header with Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2MT"/>
</gates>
<devices>
<device name="" package="62504422021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62504422021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="59.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62504422021 "/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62504422021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6273XX20621_62732020621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MS-2"/>
</gates>
<devices>
<device name="" package="62732020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62732020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="19.05mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62732020621 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62732020621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21721_62705021721" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT_1"/>
</gates>
<devices>
<device name="" package="62705021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62705021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="38.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62705021721 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62705021721 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235121_612010235121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="612010235121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612010235121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="20.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612010235121"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="612010235121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6253XX20621_62533020621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA9T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel with Cap
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15X2MS"/>
</gates>
<devices>
<device name="" package="62533020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62533020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="37.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 62533020621 "/>
<attribute name="PINS" value=" 30 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62533020621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6253XX20621_62534420621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA9T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel with Cap
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2MS"/>
</gates>
<devices>
<device name="" package="62534420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62534420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="51.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 62534420621 "/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62534420621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61206421621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32X2MT"/>
</gates>
<devices>
<device name="" package="61206421621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61206421621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="88.94mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61206421621 "/>
<attribute name="PINS" value=" 64 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61206421621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX20621_62702420621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MS-1"/>
</gates>
<devices>
<device name="" package="62702420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62702420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="21.59mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62702420621 "/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62702420621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX20621_61204020621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MS"/>
</gates>
<devices>
<device name="" package="61204020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61204020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="58.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value=" 61204020621 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61204020621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX20621_62701020621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS-1"/>
</gates>
<devices>
<device name="" package="62701020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62701020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="12.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62701020621 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62701020621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21621_62503021621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15X2MT"/>
</gates>
<devices>
<device name="" package="62503021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62503021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="37.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62503021621 "/>
<attribute name="PINS" value=" 30 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62503021621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22323_61201422323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2FT"/>
</gates>
<devices>
<device name="" package="61201422323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201422323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="23.23mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201422323 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61201422323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22121_61201622121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_1"/>
</gates>
<devices>
<device name="" package="61201622121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201622121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="39.82mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201622121 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61201622121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6123XX20621_61231420621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;
Material Properties&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-09-06&lt;BR&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS"/>
</gates>
<devices>
<device name="" package="61231420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61231420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="25.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 61231420621 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61231420621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22021_61202422021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT"/>
</gates>
<devices>
<device name="" package="61202422021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202422021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="49.98mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202422021 "/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202422021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22921_61205022921" prefix="J">
<description>&lt;b&gt;2.54 mm Male Angled Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT_1"/>
</gates>
<devices>
<device name="" package="61205022921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61205022921?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="83mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61205022921 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61205022921 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX20621_62703020621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15X2MS-1"/>
</gates>
<devices>
<device name="" package="62703020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62703020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="25.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62703020621 "/>
<attribute name="PINS" value=" 30 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62703020621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22821_61205022821" prefix="J">
<description>&lt;b&gt;2.54 mm Male Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT"/>
</gates>
<devices>
<device name="" package="61205022821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61205022821?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="83mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61205022821 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61205022821 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21721_62702021721" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_1"/>
</gates>
<devices>
<device name="" package="62702021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62702021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="19.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62702021721 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62702021721 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21721_61202621721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-29&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT_1"/>
</gates>
<devices>
<device name="" package="61202621721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202621721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="50.84mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202621721 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61202621721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235121_612026235121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT"/>
</gates>
<devices>
<device name="" package="612026235121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612026235121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="40.62mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612026235121"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="612026235121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22821_61202422821" prefix="J">
<description>&lt;b&gt;2.54 mm Male Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT"/>
</gates>
<devices>
<device name="" package="61202422821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202422821?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="49.98mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202422821 "/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202422821 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22323_62502022323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval：E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2FT"/>
</gates>
<devices>
<device name="" package="62502022323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62502022323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="24.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62502022323 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62502022323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235221_612026235221" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT_1"/>
</gates>
<devices>
<device name="" package="612026235221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612026235221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="40.62mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612026235221"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="612026235221"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235221_612010235221" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="612010235221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612010235221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="20.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612010235221"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="612010235221"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21621_62502621621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT"/>
</gates>
<devices>
<device name="" package="62502621621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62502621621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="33.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62502621621 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62502621621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61200821621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="61200821621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61200821621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="17.82mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61200821621 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61200821621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6273XX20621_62735020621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MS-2"/>
</gates>
<devices>
<device name="" package="62735020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62735020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="38.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62735020621 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62735020621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22121_62502622121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header w. Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121"&gt;
https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT_1"/>
</gates>
<devices>
<device name="" package="62502622121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62502622121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="41.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62502622121 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62502622121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6123XX20621_61232020621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;
Material Properties&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-09-06&lt;BR&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MS"/>
</gates>
<devices>
<device name="" package="61232020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61232020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="33.05mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 61232020621 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61232020621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21721_61204021721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-29&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT_1"/>
</gates>
<devices>
<device name="" package="61204021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61204021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="58.46mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61204021721 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61204021721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21721_62503421721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT_1"/>
</gates>
<devices>
<device name="" package="62503421721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62503421721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="41.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62503421721 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62503421721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6253XX20621_62535020621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA9T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel with Cap
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MS"/>
</gates>
<devices>
<device name="" package="62535020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62535020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="57.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 62535020621 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62535020621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21721_61201621721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-29&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_1"/>
</gates>
<devices>
<device name="" package="61201621721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201621721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="33.06mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201621721 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61201621721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21721_62702621721" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT_1"/>
</gates>
<devices>
<device name="" package="62702621721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62702621721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="22.86mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62702621721 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62702621721 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61201021621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="61201021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="20.36mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201021621 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61201021621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21721_62702421721" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT_1"/>
</gates>
<devices>
<device name="" package="62702421721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62702421721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="21.59mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62702421721 "/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62702421721 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21621_62704021621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION:
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT-1"/>
</gates>
<devices>
<device name="" package="62704021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62704021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="31.75mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62704021621 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62704021621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX20621_62705020621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MS-1"/>
</gates>
<devices>
<device name="" package="62705020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62705020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="38.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62705020621 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62705020621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX20621_62701220621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MS"/>
</gates>
<devices>
<device name="" package="62701220621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62701220621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="13.97mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62701220621 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62701220621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22121_62502022121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header w. Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121"&gt;
https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_1"/>
</gates>
<devices>
<device name="" package="62502022121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62502022121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="35.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62502022121 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62502022121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22121_62503422121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header w. Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121"&gt;
https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT_1"/>
</gates>
<devices>
<device name="" package="62503422121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62503422121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="49.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62503422121 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62503422121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61202421621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT"/>
</gates>
<devices>
<device name="" package="61202421621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202421621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="38.14mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202421621 "/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202421621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX20621_62704420621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2MS-1"/>
</gates>
<devices>
<device name="" package="62704420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62704420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="34.29mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62704420621 "/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62704420621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6253XX20621_62533420621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA9T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel with Cap
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MS"/>
</gates>
<devices>
<device name="" package="62533420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62533420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="41.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 62533420621 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62533420621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21721_62501621721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_1"/>
</gates>
<devices>
<device name="" package="62501621721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62501621721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="23.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62501621721 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62501621721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21721_62505021721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT_1"/>
</gates>
<devices>
<device name="" package="62505021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62505021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="57.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62505021721 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62505021721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22121_62501422121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header w. Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121"&gt;
https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_1"/>
</gates>
<devices>
<device name="" package="62501422121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62501422121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="29.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62501422121 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62501422121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21621_62702621621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION:
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT-1"/>
</gates>
<devices>
<device name="" package="62702621621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62702621621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="22.86mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62702621621 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62702621621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6273XX20621_62731020621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS-2"/>
</gates>
<devices>
<device name="" package="62731020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62731020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="12.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62731020621 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62731020621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21621_62504421621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
</gates>
<devices>
<device name="" package="62504421621">
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62504421621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="51.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62504421621 "/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62504421621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21721_61200821721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-29&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_1"/>
</gates>
<devices>
<device name="" package="61200821721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61200821721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="17.82mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61200821721 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61200821721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235221_612014235221" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_1"/>
</gates>
<devices>
<device name="" package="612014235221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612014235221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="25.38mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612014235221"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="612014235221"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21621_62703421621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION:
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT-1"/>
</gates>
<devices>
<device name="" package="62703421621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62703421621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="27.94mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62703421621 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62703421621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61203921621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="19X2+1MT"/>
</gates>
<devices>
<device name="" package="61203921621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61203921621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="58.46mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61203921621 "/>
<attribute name="PINS" value=" 39 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61203921621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21621_62702021621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION:
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT-1"/>
</gates>
<devices>
<device name="" package="62702021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62702021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="19.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62702021621 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62702021621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22821_61202622821" prefix="J">
<description>&lt;b&gt;2.54 mm Male Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT"/>
</gates>
<devices>
<device name="" package="61202622821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202622821?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="52.52mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202622821 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202622821 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX20621_61200820621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS"/>
</gates>
<devices>
<device name="" package="61200820621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61200820621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="17.96mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value=" 61200820621 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61200820621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22021_61203422021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT"/>
</gates>
<devices>
<device name="" package="61203422021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61203422021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="62.68mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61203422021 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61203422021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22821_61201622821" prefix="J">
<description>&lt;b&gt;2.54 mm Male Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="61201622821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201622821?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="39.82mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201622821 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61201622821 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21721_62504021721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT_1"/>
</gates>
<devices>
<device name="" package="62504021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62504021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="47.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62504021721 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62504021721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22821_61201022821" prefix="J">
<description>&lt;b&gt;2.54 mm Male Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="61201022821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201022821?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="32.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61201022821"/>
<attribute name="PINS" value="10"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61201022821"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61205021621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT"/>
</gates>
<devices>
<device name="" package="61205021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61205021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="71.16mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61205021621 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61205021621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21621_62704421621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION:
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2MT-1"/>
</gates>
<devices>
<device name="" package="62704421621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62704421621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="34.29mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62704421621 "/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62704421621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21721_62501421721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_1"/>
</gates>
<devices>
<device name="" package="62501421721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62501421721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="21.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62501421721 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62501421721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21621_62703021621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION:
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15X2MT-1"/>
</gates>
<devices>
<device name="" package="62703021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62703021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="25.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62703021621 "/>
<attribute name="PINS" value=" 30 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62703021621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21621_62503421621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT"/>
</gates>
<devices>
<device name="" package="62503421621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62503421621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="41.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62503421621 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62503421621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX20621_62701420621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS-1"/>
</gates>
<devices>
<device name="" package="62701420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62701420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="15.24mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62701420621 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62701420621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61204021621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT"/>
</gates>
<devices>
<device name="" package="61204021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61204021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="58.46mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61204021621 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61204021621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX20621_62702020621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MS-1"/>
</gates>
<devices>
<device name="" package="62702020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62702020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="19.05mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62702020621 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62702020621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22021_61204022021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT"/>
</gates>
<devices>
<device name="" package="61204022021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61204022021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="70.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61204022021 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61204022021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22121_61201422121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_1"/>
</gates>
<devices>
<device name="" package="61201422121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201422121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="37.28mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201422121 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61201422121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21721_62504421721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2MT_1"/>
</gates>
<devices>
<device name="" package="62504421721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62504421721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="51.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62504421721 "/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62504421721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22821_61201422821" prefix="J">
<description>&lt;b&gt;2.54 mm Male Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT"/>
</gates>
<devices>
<device name="" package="61201422821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201422821?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="37.28mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201422821 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61201422821 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22021_62501022021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header with Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="62501022021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62501022021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="25.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62501022021 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62501022021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22121_61202022121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_1"/>
</gates>
<devices>
<device name="" package="61202022121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202022121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="44.9mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202022121 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61202022121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21621_62501621621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="62501621621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62501621621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="23.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62501621621 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62501621621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22921_61206022921" prefix="J">
<description>&lt;b&gt;2.54 mm Male Angled Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="30X2MT_1"/>
</gates>
<devices>
<device name="" package="61206022921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61206022921?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="95.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61206022921 "/>
<attribute name="PINS" value=" 60 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61206022921 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22021_62505022021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header with Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT"/>
</gates>
<devices>
<device name="" package="62505022021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62505022021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="65.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62505022021 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62505022021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22821_61206422821" prefix="J">
<description>&lt;b&gt;2.54 mm Male Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32X2MT"/>
</gates>
<devices>
<device name="" package="61206422821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61206422821?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="100.78mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61206422821 "/>
<attribute name="PINS" value=" 64 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61206422821 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235221_612034235221" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT_1"/>
</gates>
<devices>
<device name="" package="612034235221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612034235221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="50.8mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612034235221"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="612034235221"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6253XX20621_62534020621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA9T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel with Cap
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MS"/>
</gates>
<devices>
<device name="" package="62534020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62534020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="47.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 62534020621 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62534020621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22921_61201622921" prefix="J">
<description>&lt;b&gt;2.54 mm Male Angled Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_1"/>
</gates>
<devices>
<device name="" package="61201622921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201622921?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="39.82mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201622921 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61201622921 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21721_62701421721" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-03-02&lt;BR&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_1"/>
</gates>
<devices>
<device name="" package="62701421721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62701421721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="15.24mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62701421721 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62701421721 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22021_62502622021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header with Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT"/>
</gates>
<devices>
<device name="" package="62502622021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62502622021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="41.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62502622021 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62502622021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235221_612050235221" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT_1"/>
</gates>
<devices>
<device name="" package="612050235221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612050235221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="71.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612050235221"/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="612050235221"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21621_62701021621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION:
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT-1"/>
</gates>
<devices>
<device name="" package="62701021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62701021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="12.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62701021621 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62701021621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235221_612008235221" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_1"/>
</gates>
<devices>
<device name="" package="612008235221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612008235221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="17.78mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612008235221"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="612008235221"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22021_61206022021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="30X2MT"/>
</gates>
<devices>
<device name="" package="61206022021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61206022021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="95.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61206022021 "/>
<attribute name="PINS" value=" 60 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61206022021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX20621_61202620621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MS"/>
</gates>
<devices>
<device name="" package="61202620621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202620621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="40.82mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value=" 61202620621 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202620621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6123XX20621_61233420621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;
Material Properties&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-09-06&lt;BR&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MS"/>
</gates>
<devices>
<device name="" package="61233420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61233420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="50.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 61233420621 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61233420621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21721_62701621721" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_1"/>
</gates>
<devices>
<device name="" package="62701621721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62701621721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="16.51mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62701621721 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62701621721 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21621_62502421621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT"/>
</gates>
<devices>
<device name="" package="62502421621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62502421621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="32.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62502421621 "/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62502421621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22821_61204022821" prefix="J">
<description>&lt;b&gt;2.54 mm Male Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT"/>
</gates>
<devices>
<device name="" package="61204022821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61204022821?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="70.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61204022821 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61204022821 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21621_62502021621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT"/>
</gates>
<devices>
<device name="" package="62502021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62502021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="27.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62502021621 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62502021621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6123XX20621_61232620621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;
Material Properties&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-09-06&lt;BR&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MS"/>
</gates>
<devices>
<device name="" package="61232620621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61232620621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="40.64mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 61232620621 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61232620621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22921_61202022921" prefix="J">
<description>&lt;b&gt;2.54 mm Male Angled Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_1"/>
</gates>
<devices>
<device name="" package="61202022921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202022921?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="44.9mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202022921 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61202022921 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22021_61201022021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="61201022021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201022021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="32.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61201022021"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61201022021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22921_61202422921" prefix="J">
<description>&lt;b&gt;2.54 mm Male Angled Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT_1"/>
</gates>
<devices>
<device name="" package="61202422921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202422921?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="49.98mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202422921 "/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61202422921 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6123XX20621_61231620621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;
Material Properties&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-09-06&lt;BR&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS"/>
</gates>
<devices>
<device name="" package="61231620621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61231620621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="27.94mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 61231620621 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61231620621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22323_62501022323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval：E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2FT"/>
</gates>
<devices>
<device name="" package="62501022323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62501022323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="14.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62501022323 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62501022323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6273XX20621_62733020621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15X2MS-2"/>
</gates>
<devices>
<device name="" package="62733020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62733020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="25.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62733020621 "/>
<attribute name="PINS" value=" 30 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62733020621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21621_62705021621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION:
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT-1"/>
</gates>
<devices>
<device name="" package="62705021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62705021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="38.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62705021621 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62705021621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22921_61201022921" prefix="J">
<description>&lt;b&gt;2.54 mm Male Angled Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="61201022921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201022921?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="32.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61201022921"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61201022921"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX20621_62702620621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MS-1"/>
</gates>
<devices>
<device name="" package="62702620621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62702620621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="22.86mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62702620621 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62702620621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21721_62502621721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT_1"/>
</gates>
<devices>
<device name="" package="62502621721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62502621721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="33.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62502621721 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62502621721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235121_612016235121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="612016235121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612016235121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="27.92mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612016235121"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="612016235121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21621_62706021621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION:
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-02-09&lt;BR&gt;
20212 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="30X2MT-1"/>
</gates>
<devices>
<device name="" package="62706021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62706021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="44.45mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62706021621 "/>
<attribute name="PINS" value=" 60 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62706021621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21621_62501021621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32924v209%20Family_WR-BHD_6250xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_6250XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="62501021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62501021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="17.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62501021621 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62501021621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235121_612050235121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT"/>
</gates>
<devices>
<device name="" package="612050235121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612050235121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="71.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612050235121"/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="612050235121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6253XX20621_62532020621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA9T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel with Cap
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MS"/>
</gates>
<devices>
<device name="" package="62532020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62532020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="27.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 62532020621 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62532020621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22021_62502022021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header with Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT"/>
</gates>
<devices>
<device name="" package="62502022021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62502022021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="35.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62502022021 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62502022021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21721_61202021721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-29&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_1"/>
</gates>
<devices>
<device name="" package="61202021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="38.14mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202021721 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61202021721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22021_61201622021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT"/>
</gates>
<devices>
<device name="" package="61201622021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201622021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="39.82mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201622021 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61201622021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21721_62501021721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="62501021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62501021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="17.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62501021721 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62501021721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6253XX20621_62532620621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA9T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel with Cap
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/catalog/media/o32950v209%20Family_WR-BHD_6253xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_SMT_MALE_BOX_HEADER_6253XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MS"/>
</gates>
<devices>
<device name="" package="62532620621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62532620621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="33.25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 62532620621 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62532620621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235221_612040235221" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32907v209%20Family_WR-BHD_6120xx235221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_HIGH_TEMPERATURE_6120XX235221&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT_1"/>
</gates>
<devices>
<device name="" package="612040235221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612040235221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="58.4mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612040235221"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="612040235221"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22021_62504022021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header with Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT"/>
</gates>
<devices>
<device name="" package="62504022021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62504022021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="55.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62504022021 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62504022021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22021_62501422021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header with Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT"/>
</gates>
<devices>
<device name="" package="62501422021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62501422021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="29.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62501422021 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62501422021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX20621_61201420621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS"/>
</gates>
<devices>
<device name="" package="61201420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="25.58mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value=" 61201420621 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61201420621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22021_62503422021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Box Header with Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32934v209%20Family_WR-BHD_6250xx22021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_BOX_HEADER_WITH_LEVER_6250XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT"/>
</gates>
<devices>
<device name="" package="62503422021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62503422021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="49.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62503422021 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62503422021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX20621_61202420621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MS"/>
</gates>
<devices>
<device name="" package="61202420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="38.28mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value=" 61202420621 "/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202420621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22121_61201022121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="61201022121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201022121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="32.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61201022121"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61201022121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22323_62502622323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval：E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2FT"/>
</gates>
<devices>
<device name="" package="62502622323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62502622323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="30.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62502622323 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62502622323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22121_61203422121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT_1"/>
</gates>
<devices>
<device name="" package="61203422121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61203422121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="62.68mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61203422121 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61203422121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61203421621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT"/>
</gates>
<devices>
<device name="" package="61203421621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61203421621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="50.84mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61203421621 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61203421621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6273XX20621_62734020621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MS-2"/>
</gates>
<devices>
<device name="" package="62734020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62734020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="31.75mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62734020621 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62734020621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21721_62703421721" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-03-02&lt;BR&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MT_1"/>
</gates>
<devices>
<device name="" package="62703421721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62703421721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="27.94mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62703421721 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62703421721 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61202021621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT"/>
</gates>
<devices>
<device name="" package="61202021621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202021621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="33.06mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202021621 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202021621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX20621_62704020621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MS-1"/>
</gates>
<devices>
<device name="" package="62704020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62704020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="31.75mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62704020621 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62704020621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6273XX20621_62731620621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS-2"/>
</gates>
<devices>
<device name="" package="62731620621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62731620621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="16.51mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62731620621 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62731620621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21721_62704021721" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375402v209%20Family_WR-BHD_6270xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_ANGLED_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT_1"/>
</gates>
<devices>
<device name="" package="62704021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62704021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="31.75mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62704021721 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62704021721 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22121_61202622121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT_1"/>
</gates>
<devices>
<device name="" package="61202622121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202622121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="52.52mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202622121 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61202622121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22323_61204022323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2FT"/>
</gates>
<devices>
<device name="" package="61204022323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61204022323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="56.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61204022323 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61204022323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6273XX20621_62731220621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MS-1"/>
</gates>
<devices>
<device name="" package="62731220621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62731220621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="13.97mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62731220621 "/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62731220621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6123XX20621_61234020621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;
Material Properties&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-09-06&lt;BR&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MS"/>
</gates>
<devices>
<device name="" package="61234020621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61234020621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="58.42mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 61234020621 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61234020621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX20621_62703420621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MS-1"/>
</gates>
<devices>
<device name="" package="62703420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62703420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="27.94mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62703420621 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62703420621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6273XX20621_62734420621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2MS-2"/>
</gates>
<devices>
<device name="" package="62734420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62734420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="34.29mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62734420621 "/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62734420621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22323_61200822323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2FT"/>
</gates>
<devices>
<device name="" package="61200822323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61200822323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="15.61mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61200822323 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61200822323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22021_61205022021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT"/>
</gates>
<devices>
<device name="" package="61205022021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61205022021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="83mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61205022021 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61205022021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22821_61206022821" prefix="J">
<description>&lt;b&gt;2.54 mm Male Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58844v209%20Family_2.54mm_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_LONG_LEVER_6120XX22821&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="30X2MT"/>
</gates>
<devices>
<device name="" package="61206022821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61206022821?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="95.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61206022821 "/>
<attribute name="PINS" value=" 60 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61206022821 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6273XX20621_62733420621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2MS-2"/>
</gates>
<devices>
<device name="" package="62733420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62733420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="27.94mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62733420621 "/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62733420621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6273XX20621_62731420621">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS-2"/>
</gates>
<devices>
<device name="" package="62731420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62731420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="15.24mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62731420621 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62731420621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22323_62503022323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval：E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15X2FT"/>
</gates>
<devices>
<device name="" package="62503022323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62503022323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="34.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62503022323 "/>
<attribute name="PINS" value=" 30 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62503022323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX21721_62502021721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32929v209%20Family_WR-BHD_6250xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_6250XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_1"/>
</gates>
<devices>
<device name="" package="62502021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62502021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="27.25mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62502021721 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62502021721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX20621_61201620621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS"/>
</gates>
<devices>
<device name="" package="61201620621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201620621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="28.12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value=" 61201620621 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61201620621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6273XX20621_62732420621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MS-2"/>
</gates>
<devices>
<device name="" package="62732420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62732420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="21.59mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62732420621 "/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62732420621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22121_61205022121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT_1"/>
</gates>
<devices>
<device name="" package="61205022121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61205022121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="83mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61205022121 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61205022121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6273XX20621_62732620621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MS-2"/>
</gates>
<devices>
<device name="" package="62732620621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62732620621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="22.86mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62732620621 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62732620621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22921_61204022921" prefix="J">
<description>&lt;b&gt;2.54 mm Male Angled Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2MT_1"/>
</gates>
<devices>
<device name="" package="61204022921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61204022921?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="70.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61204022921 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61204022921 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22921_61202622921" prefix="J">
<description>&lt;b&gt;2.54 mm Male Angled Box Header with long lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o58851v209%20Family_long_lever_WR-BHD_6120xx22x21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_WITH_LONG_LEVER_6120XX22921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT_1"/>
</gates>
<devices>
<device name="" package="61202622921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202622921?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="52.52mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202622921 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61202622921 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6123XX20621_61232420621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male SMT Box Header&lt;/b&gt;
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;
Material Properties&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 up to +125 °C
&lt;BR&gt;Compliance	RoHS
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Gender	Male
&lt;BR&gt;

&lt;BR&gt;&lt;B&gt;Certification&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32919v209%20Family_WR-BHD_612xxx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/BHD_2_54_SMT_MALE_BOX_HEADER_6120XX20621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-27&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MS"/>
</gates>
<devices>
<device name="" package="61232420621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61232420621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="38.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61232420621 "/>
<attribute name="PINS" value=" 24"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="612324620621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22121_62504422121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header w. Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121"&gt;
https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2MT_1"/>
</gates>
<devices>
<device name="" package="62504422121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62504422121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="59.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62504422121 "/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62504422121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX235121_612014235121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header High Temperature&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32904v209%20Family_WR-BHD_6120xx235121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_HIGH_TEMPERATURE_6120XX235121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-03-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT"/>
</gates>
<devices>
<device name="" package="612014235121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/612014235121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="25.38mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="612014235121"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="612014235121"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX21621_62702421621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION:
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375404v209%20Family_WR-BHD_6270xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT-1"/>
</gates>
<devices>
<device name="" package="62702421621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62702421621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="21.59mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 62702421621 "/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62702421621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61202621621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2MT"/>
</gates>
<devices>
<device name="" package="61202621621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202621621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="40.68mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202621621 "/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202621621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22121_62505022121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Male Angled Box Header w. Lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32938v209%20Family_WR-BHD_6250xx22121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121"&gt;
https://www.we-online.de/katalog/en/em/BHD_2_00_MALE_ANGLED_BOX_HEADER_WITH_LEVER_6250XX22121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2MT_1"/>
</gates>
<devices>
<device name="" package="62505022121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62505022121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="65.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62505022121 "/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 62505022121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22323_61202022323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2FT"/>
</gates>
<devices>
<device name="" package="61202022323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202022323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="30.85mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202022323 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202022323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6270XX20621_62701620621" prefix="J">
<description>&lt;b&gt;WR-BHD 1.27 mm Male SMT Box Header &lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 1.27 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material Nylon 9T 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Contact Material Brass 
&lt;BR&gt;Contact Plating Gold over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Working Voltage 50 V (AC) 
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval E323964 
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o375406v209%20Family_WR-BHD_6270xx20621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER"&gt;https://www.we-online.com/catalog/en/WR_BHD_1_27_MM_MALE_SMT_BOX_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-08-24&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS-1"/>
</gates>
<devices>
<device name="" package="62701620621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62701620621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="16.51mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 62701620621 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="1.27mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62701620621 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21721_61201021721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-29&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_1"/>
</gates>
<devices>
<device name="" package="61201021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="25.44mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201021721 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61201021721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21621_61201421621" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32884v209%20Family_WR-BHD_6120xx21621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621"&gt;https://www.we-online.com/catalog/en/BHD_2_54_MALE_BOX_HEADER_6120XX21621&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-3-12&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT"/>
</gates>
<devices>
<device name="" package="61201421621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201421621?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="25.44mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201421621 "/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61201421621 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6250XX22323_62504022323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.00 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2 mm
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval：E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32943v209%20Family_WR-BHD_6250xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_00_BOARD_TO_CAB_TRANSITION_CONNECTOR_6250XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-11-04&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2FT"/>
</gates>
<devices>
<device name="" package="62504022323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62504022323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="44.1mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 62504022323 "/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 62504022323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22323_61201622323" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Board to Cable Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32892v209%20Family_WR-BHD_6120xx22323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_BOARD_TO_CAB_TRANSITION_CONNECTOR_6120XX22323&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-31&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2FT"/>
</gates>
<devices>
<device name="" package="61201622323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61201622323?ae"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="25.77mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61201622323 "/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61201622323 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22021_61202022021" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT"/>
</gates>
<devices>
<device name="" package="61202022021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61202022021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="44.9mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61202022021 "/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value=" 61202022021 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX21721_61206021721" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Angled Box Header&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
CERTIFICATION:
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o32888v209%20Family_WR-BHD_6120xx21721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_ANGLED_BOX_HEADER_6120XX21721&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-29&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="30X2MT_1"/>
</gates>
<devices>
<device name="" package="61206021721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61206021721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="83.86mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61206021721 "/>
<attribute name="PINS" value=" 60 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61206021721 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6120XX22121_61206022121" prefix="J">
<description>&lt;b&gt;WR-BHD 2.54 mm Male Box Header with short lever&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material :Copper Alloy
&lt;BR&gt;Contact Plating :Gold
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +125 °C 
&lt;BR&gt;Compliance:RoHS 
&lt;BR&gt;Working Voltage: 250 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 20 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging :Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o77864v209%20Family_61201022821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021"&gt;https://www.we-online.de/katalog/en/em/BHD_2_54_MALE_BOX_HEADER_WITH_SHORT_LEVER_6120XX22021&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-30&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="30X2MT_1"/>
</gates>
<devices>
<device name="" package="61206022121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61206022121?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="95.7mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61206022121 "/>
<attribute name="PINS" value=" 60 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value=" 61206022121 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
