<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Board to Board Connectors &amp;Wire to  Board Connector - WR-MM &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020b, 2020-07-27&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="690368171472">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w. Polarization and w/o Latch, 14 Pins</description>
</package>
<package name="690368172072">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w. Polarization and w/o Latch, 20 Pins</description>
</package>
<package name="690368171272">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w. Polarization and w/o Latch, 12 Pins</description>
</package>
<package name="690368172272">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w. Polarization and w/o Latch, 22 Pins</description>
</package>
<package name="690368171872">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w. Polarization and w/o Latch, 18 Pins</description>
</package>
<package name="690368171072">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w. Polarization and w/o Latch,  10 Pins</description>
</package>
<package name="690368180472">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w/o Latch &amp; w/o Polarization, 4 Pins</description>
</package>
<package name="690368171672">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w. Polarization and w/o Latch, 16 Pins</description>
</package>
<package name="690367191672">
<description>&lt;b&gt;WR-MM&lt;/B&gt;&lt;bR&gt;Female Connector with Latch &amp; w/o Polarization, 16 Pins</description>
</package>
<package name="690367280876">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female SMT Connector with Polarization, 8 pins</description>
</package>
<package name="690368181272">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w/o Latch &amp; w/o Polarization, 12 Pins</description>
</package>
<package name="690207102672">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Transition Connector,26 Pins</description>
</package>
<package name="690367282476">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female SMT Connector with Polarization, 24 pins</description>
</package>
<package name="690367181472">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female Connector w/o Latch &amp; w/o Polarization, 14 Pins</description>
</package>
<package name="690367192272">
<description>&lt;b&gt;WR-MM&lt;/B&gt;&lt;bR&gt;Female Connector with Latch &amp; w/o Polarization,22 Pins</description>
</package>
<package name="690368181072">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w/o Latch &amp; w/o Polarization, 10 Pins</description>
</package>
<package name="690367282076">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female SMT Connector with Polarization, 20 pins</description>
</package>
<package name="690367182072">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female Connector w/o Latch &amp; w/o Polarization, 20 Pins</description>
</package>
<package name="690367191072">
<description>&lt;b&gt;WR-MM&lt;/B&gt;&lt;bR&gt;Female Connector with Latch &amp; w/o Polarization,10 Pins</description>
</package>
<package name="690368182072">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w/o Latch &amp; w/o Polarization, 20 Pins</description>
</package>
<package name="690367180872">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female Connector w/o Latch &amp; w/o Polarization, 8 Pins</description>
</package>
<package name="690367281676">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female SMT Connector with Polarization,16 pins</description>
</package>
<package name="690367181272">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female Connector w/o Latch &amp; w/o Polarization, 12 Pins</description>
</package>
<package name="690367182472">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female Connector w/o Latch &amp; w/o Polarization,24 Pins</description>
</package>
<package name="690367290476">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female SMT Connector with Latch &amp; Polarization, 4 pins</description>
</package>
<package name="690357281876">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt; Male SMT Connector w/o Latch &amp; w/o Polarization, 18 pins</description>
</package>
<package name="690357281676">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt; Male SMT Connector w/o Latch &amp; w/o Polarization, 16 pins</description>
</package>
<package name="690357101472">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Male Connector w/o Latch &amp; w. Polarization, 14 Pins</description>
</package>
<package name="690367292476">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female SMT Connector with Latch &amp; Polarization, 24 pins</description>
</package>
<package name="690367290676">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female SMT Connector with Latch &amp; Polarization, 6 pins</description>
</package>
<package name="690368181672">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w/o Latch &amp; w/o Polarization, 16 Pins</description>
</package>
<package name="690368192672">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female Angled Connector with Latch &amp; w. Polarization, 26 Pins</description>
</package>
<package name="690367291476">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female SMT Connector with Latch &amp; Polarization,14 pins</description>
</package>
<package name="690368191672">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female Angled Connector with Latch &amp; w. Polarization,  16 Pins</description>
</package>
<package name="690357102672">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Male Connector w/o Latch &amp; w. Polarization, 26 Pins</description>
</package>
<package name="690367281276">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female SMT Connector with Polarization, 12 pins</description>
</package>
<package name="690357101272">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Male Connector w/o Latch &amp; w. Polarization, 12 Pins</description>
</package>
<package name="690367292276">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female SMT Connector with Latch &amp; Polarization, 22 pins</description>
</package>
<package name="690367292676">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female SMT Connector with Latch &amp; Polarization, 26 pins</description>
</package>
<package name="690368182672">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w/o Latch &amp; w/o Polarization, 26 Pins</description>
</package>
<package name="690357280476">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt; Male SMT Connector w/o Latch &amp; w/o Polarization, 4pins</description>
</package>
<package name="690367182672">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female Connector w/o Latch &amp; w/o Polarization, 26 Pins</description>
</package>
<package name="690357281076">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt; Male SMT Connector w/o Latch &amp; w/o Polarization, 10 pins</description>
</package>
<package name="690207100872">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Transition Connector,8 Pins</description>
</package>
<package name="690207100472">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Transition Connector, 4 Pins</description>
</package>
<package name="690357101072">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Male Connector w/o Latch &amp; w. Polarization,  10 Pins</description>
</package>
<package name="690368190872">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female Angled Connector with Latch &amp; w. Polarization,  8 Pins</description>
</package>
<package name="690368192472">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female Angled Connector with Latch &amp; w. Polarization,  24 Pins</description>
</package>
<package name="690357101872">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Male Connector w/o Latch &amp; w. Polarization, 18 Pins</description>
</package>
<package name="690367281876">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female SMT Connector with Polarization,18 pins</description>
</package>
<package name="690367181872">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female Connector w/o Latch &amp; w/o Polarization, 18 Pins</description>
</package>
<package name="690368191472">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female Angled Connector with Latch &amp; w. Polarization, 14 Pins</description>
</package>
<package name="690357280676">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt; Male SMT Connector w/o Latch &amp; w/o Polarization,  6 pins</description>
</package>
<package name="690367180672">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female Connector w/o Latch &amp; w/o Polarization,6 Pins</description>
</package>
<package name="690357282676">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt; Male SMT Connector w/o Latch &amp; w/o Polarization,  26 pins</description>
</package>
<package name="690357101672">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Male Connector w/o Latch &amp; w. Polarization,  16 Pins</description>
</package>
<package name="690357102072">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Male Connector w/o Latch &amp; w. Polarization,  20 Pins</description>
</package>
<package name="690357102272">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Male Connector w/o Latch &amp; w. Polarization,  22 Pins</description>
</package>
<package name="690368170472">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w. Polarization and w/o Latch, 4 Pins</description>
</package>
<package name="690368180672">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w/o Latch &amp; w/o Polarization, 6 Pins</description>
</package>
<package name="690367291676">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female SMT Connector with Latch &amp; Polarization,16 pins</description>
</package>
<package name="690367291276">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female SMT Connector with Latch &amp; Polarization,12 pins</description>
</package>
<package name="690207101872">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Transition Connector,18Pins</description>
</package>
<package name="690367190472">
<description>&lt;b&gt;WR-MM&lt;/B&gt;&lt;bR&gt;Female Connector with Latch &amp; w/o Polarization,4 Pins</description>
</package>
<package name="690367280676">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female SMT Connector with Polarization, 6Pins</description>
</package>
<package name="690207101472">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Transition Connector,14 Pins</description>
</package>
<package name="690357100672">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Male Connector w/o Latch &amp; w. Polarization,  6 Pins</description>
</package>
<package name="690368182472">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w/o Latch &amp; w/o Polarization, 24 Pins</description>
</package>
<package name="690367180472">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female Connector w/o Latch &amp; w/o Polarization, 4 Pins</description>
</package>
<package name="690207102472">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Transition Connector, 24 Pins</description>
</package>
<package name="690368181872">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w/o Latch &amp; w/o Polarization, 18 Pins</description>
</package>
<package name="690368192072">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female Angled Connector with Latch &amp; w. Polarization, 20 Pins</description>
</package>
<package name="690357100472">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Male Connector w/o Latch &amp; w. Polarization, 4 Pins</description>
</package>
<package name="690367281476">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female SMT Connector with Polarization, 14 pins</description>
</package>
<package name="690368170872">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w. Polarization and w/o Latch,  8 Pins</description>
</package>
<package name="690367181672">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female Connector w/o Latch &amp; w/o Polarization,16 Pins</description>
</package>
<package name="690207101672">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Transition Connector,16 Pins</description>
</package>
<package name="690368191072">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female Angled Connector with Latch &amp; w. Polarization, 10 Pins</description>
</package>
<package name="690367182272">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female Connector w/o Latch &amp; w/o Polarization,22 Pins</description>
</package>
<package name="690207101272">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Transition Connector,12 Pins</description>
</package>
<package name="690368182272">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w/o Latch &amp; w/o Polarization,  22 Pins</description>
</package>
<package name="690368191272">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female Angled Connector with Latch &amp; w. Polarization,12 Pins</description>
</package>
<package name="690367191472">
<description>&lt;b&gt;WR-MM&lt;/B&gt;&lt;bR&gt;Female Connector with Latch &amp; w/o Polarization, 14 Pins</description>
</package>
<package name="690207102272">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Transition Connector, 22 Pins</description>
</package>
<package name="690367191272">
<description>&lt;b&gt;WR-MM&lt;/B&gt;&lt;bR&gt;Female Connector with Latch &amp; w/o Polarization,12 Pins</description>
</package>
<package name="690367190872">
<description>&lt;b&gt;WR-MM&lt;/B&gt;&lt;bR&gt;Female Connector with Latch &amp; w/o Polarization,8 Pins</description>
</package>
<package name="690357282476">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt; Male SMT Connector w/o Latch &amp; w/o Polarization,  24 pins</description>
</package>
<package name="690367292076">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female SMT Connector with Latch &amp; Polarization,20 pins</description>
</package>
<package name="690357281276">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt; Male SMT Connector w/o Latch &amp; w/o Polarization, 12 pins</description>
</package>
<package name="690367190672">
<description>&lt;b&gt;WR-MM&lt;/B&gt;&lt;bR&gt;Female Connector with Latch &amp; w/o Polarization, 6 Pins</description>
</package>
<package name="690367291076">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female SMT Connector with Latch &amp; Polarization, 10 pins</description>
</package>
<package name="690367192072">
<description>&lt;b&gt;WR-MM&lt;/B&gt;&lt;bR&gt;Female Connector with Latch &amp; w/o Polarization, 20 Pins</description>
</package>
<package name="690207100672">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Transition Connector, 6 Pins</description>
</package>
<package name="690367192472">
<description>&lt;b&gt;WR-MM&lt;/B&gt;&lt;bR&gt;Female Connector with Latch &amp; w/o Polarization, 24 Pins</description>
</package>
<package name="690368181472">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w/o Latch &amp; w/o Polarization, 14 Pins</description>
</package>
<package name="690357280876">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt; Male SMT Connector w/o Latch &amp; w/o Polarization,  8 pins</description>
</package>
<package name="690357102472">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Male Connector w/o Latch &amp; w. Polarization,  24 Pins</description>
</package>
<package name="690357282276">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt; Male SMT Connector w/o Latch &amp; w/o Polarization, 22 pins</description>
</package>
<package name="690368172672">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w. Polarization and w/o Latch,  26 Pins</description>
</package>
<package name="690368190472">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female Angled Connector with Latch &amp; w. Polarization, 4 Pins</description>
</package>
<package name="690367282676">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female SMT Connector with Polarization,26 pins</description>
</package>
<package name="690207102072">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Transition Connector,20 Pins</description>
</package>
<package name="690368170672">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w. Polarization and w/o Latch, 6 Pins</description>
</package>
<package name="690367282276">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female SMT Connector with Polarization,22 pins</description>
</package>
<package name="690357282076">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt; Male SMT Connector w/o Latch &amp; w/o Polarization,  20 pins</description>
</package>
<package name="690367192672">
<description>&lt;b&gt;WR-MM&lt;/B&gt;&lt;bR&gt;Female Connector with Latch &amp; w/o Polarization, 26 Pins</description>
</package>
<package name="690357100872">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Male Connector w/o Latch &amp; w. Polarization,  8 Pins</description>
</package>
<package name="690207101072">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt;  Transition Connector,10 Pins</description>
</package>
<package name="690368191872">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female Angled Connector with Latch &amp; w. Polarization, 18 Pins</description>
</package>
<package name="690367291876">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female SMT Connector with Latch &amp; Polarization, 18 pins</description>
</package>
<package name="690368180872">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w/o Latch &amp; w/o Polarization,8 Pins</description>
</package>
<package name="690368172472">
<description>&lt;b&gt;WR-MM &lt;/b&gt;&lt;br&gt;Female Angled Connector w. Polarization and w/o Latch, 24 Pins</description>
</package>
<package name="690368190672">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female Angled Connector with Latch &amp; w. Polarization, 6 Pins</description>
</package>
<package name="690357281476">
<description>&lt;B&gt;WR-MM&lt;/B&gt;&lt;BR&gt; Male SMT Connector w/o Latch &amp; w/o Polarization,  14 pins</description>
</package>
<package name="690367191872">
<description>&lt;b&gt;WR-MM&lt;/B&gt;&lt;bR&gt;Female Connector with Latch &amp; w/o Polarization, 18 Pins</description>
</package>
<package name="690367290876">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female SMT Connector with Latch &amp; Polarization, 8 pins</description>
</package>
<package name="690367181072">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female Connector w/o Latch &amp; w/o Polarization,10 Pins</description>
</package>
<package name="690368192272">
<description>&lt;B&gt;WR-MM&lt;/B&gt; &lt;BR&gt;Female Angled Connector with Latch &amp; w. Polarization, 22 Pins</description>
</package>
<package name="690367281076">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female SMT Connector with Polarization, 10 pins</description>
</package>
<package name="690367280476">
<description>&lt;b&gt;WR-MM&lt;/b&gt;&lt;br&gt; Female SMT Connector with Polarization, 4 pins</description>
</package>
</packages>
<symbols>
<symbol name="16FT">
<description>16Pins Female THT</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="8FS_1">
<description>8 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="22FT">
<description>22Pins Female THT</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="14FT">
<description>14Pins Female THT</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="26MT_1">
<description>26Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="24FS_1">
<description>24 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="10FT">
<description>10Pins Female THT</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="20FS_1">
<description>20 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="12FT">
<description>12Pins Female THT</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="16FS_1">
<description>16 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="24FT">
<description>24Pins Female THT</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="4FS">
<description>4Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="8FT">
<description>8Pins Female THT</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="14MT">
<description>14Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="16MS">
<description>16Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="6FS">
<description>6Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="24FS">
<description>24Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="26FT">
<description>26Pins Female THT</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="22FS">
<description>22Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="12FS_1">
<description>12 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="26MT">
<description>26Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="18MS">
<description>18Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="26FS">
<description>26Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="4MS">
<description>4Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="8MT_1">
<description>8Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="4MT_1">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="18FS_1">
<description>18 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="10MS">
<description>10Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="18MT">
<description>18Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="6MS">
<description>6Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="16MT">
<description>16Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="6FT">
<description>6Pins Female THT</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="16FS">
<description>16Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="4FT">
<description>4Pins Female THT</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="12FS">
<description>12Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="18MT_1">
<description>18Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="6FS_1">
<description>6 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="6MT">
<description>6Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="14MT_1">
<description>14Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="14FS_1">
<description>14 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="12MT_1">
<description>12Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="4MT">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="16MT_1">
<description>16Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="14FS">
<description>14Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="22MT_1">
<description>22Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="20FS">
<description>20Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="24MS">
<description>24Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="6MT_1">
<description>6Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="8MS">
<description>8Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="10FS">
<description>10Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="18FT">
<description>18Pins Female THT</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="24MT_1">
<description>24Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="12MS">
<description>12Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="12MT">
<description>12Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="26FS_1">
<description>26 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="22MS">
<description>22Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="20MT_1">
<description>20Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="24MT">
<description>24Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="20FT">
<description>20Pins Female THT</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="22FS_1">
<description>22 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="20MS">
<description>20Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="26MS">
<description>26Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="10MT">
<description>10Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="8MT">
<description>8Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="22MT">
<description>22Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="10MT_1">
<description>10Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="4FS_1">
<description>4 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="18FS">
<description>18Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="20MT">
<description>20Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="14MS">
<description>14Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="10FS_1">
<description>10 Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="8FS">
<description>8Pins Female SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="690367191672" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector with Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16FT"/>
</gates>
<devices>
<device name="" package="690367191672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367191672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367191672"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367191672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367280876" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8FS_1"/>
</gates>
<devices>
<device name="" package="690367280876">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367280876.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367280876"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367280876"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368181272" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12FT"/>
</gates>
<devices>
<device name="" package="690368181272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368181272.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368181272"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368181272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690207102672" prefix="J">
<description>&lt;b&gt;WR-MM Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72"&gt;https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26MT_1"/>
</gates>
<devices>
<device name="" package="690207102672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690207102672.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="36.45mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690207102672"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690207102672"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367282476" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24FS_1"/>
</gates>
<devices>
<device name="" package="690367282476">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367282476.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367282476"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367282476"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367181472" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14FT"/>
</gates>
<devices>
<device name="" package="690367181472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367181472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367181472"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367181472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368181072" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10FT"/>
</gates>
<devices>
<device name="" package="690368181072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368181072.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368181072"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368181072"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367282076" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20FS_1"/>
</gates>
<devices>
<device name="" package="690367282076">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367282076.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367282076"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367282076"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367192272" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector with Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22FT"/>
</gates>
<devices>
<device name="" package="690367192272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367192272.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367192272"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367192272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367182072" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20FT"/>
</gates>
<devices>
<device name="" package="690367182072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367182072.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367182072"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367182072"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367191072" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector with Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10FT"/>
</gates>
<devices>
<device name="" package="690367191072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367191072.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367191072"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367191072"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368182072" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20FT"/>
</gates>
<devices>
<device name="" package="690368182072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368182072.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368182072"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368182072"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367180872" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8FT"/>
</gates>
<devices>
<device name="" package="690367180872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367180872.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367180872"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367180872"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367281676" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16FS_1"/>
</gates>
<devices>
<device name="" package="690367281676">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367281676.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367281676"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367281676"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367181272" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12FT"/>
</gates>
<devices>
<device name="" package="690367181272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367181272.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367181272"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367181272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367182472" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24FT"/>
</gates>
<devices>
<device name="" package="690367182472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367182472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367182472"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367182472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367290476" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Latch &amp; Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web 1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;

Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4FS"/>
</gates>
<devices>
<device name="" package="690367290476">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367290476.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367290476"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367290476"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357281676" prefix="J">
<description>&lt;b&gt;WR-MM Male SMT Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16MS"/>
</gates>
<devices>
<device name="" package="690357281676">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357281676.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690357281676"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357281676"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368171472" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w. Polarization and w/o Latch&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14FT"/>
</gates>
<devices>
<device name="" package="690357101472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368171472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368171472"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368171472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357281876" prefix="J">
<description>&lt;b&gt;WR-MM Male SMT Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18MS"/>
</gates>
<devices>
<device name="" package="690357281876">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357281876.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690357281876"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357281876"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368192672" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector with Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2020-07-06
&lt;BR&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26FT"/>
</gates>
<devices>
<device name="" package="690368192672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368192672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368192672"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368192672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357101472" prefix="J">
<description>&lt;b&gt;WR-MM Male Connector w/o Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14MT"/>
</gates>
<devices>
<device name="" package="690357101472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357101472.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690357101472"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357101472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368181672" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16FT"/>
</gates>
<devices>
<device name="" package="690368181672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368181672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368181672"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368181672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367290676" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Latch &amp; Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web 1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;

Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6FS"/>
</gates>
<devices>
<device name="" package="690367290676">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367290676.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367290676"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367290676"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367292476" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Latch &amp; Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web 1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;

Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24FS"/>
</gates>
<devices>
<device name="" package="690367292476">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367292476.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367292476"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367292476"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367291476" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Latch &amp; Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web 1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;

Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14FS"/>
</gates>
<devices>
<device name="" package="690367291476">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367291476.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367291476"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367291476"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368191672" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector with Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2020-07-06
&lt;BR&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16FT"/>
</gates>
<devices>
<device name="" package="690368191672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368191672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368191672"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368191672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357102672" prefix="J">
<description>&lt;b&gt;WR-MM Male Connector w/o Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26MT"/>
</gates>
<devices>
<device name="" package="690357102672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357102672.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690357102672"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357102672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367281276" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12FS_1"/>
</gates>
<devices>
<device name="" package="690367281276">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367281276.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367281276"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367281276"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357101272" prefix="J">
<description>&lt;b&gt;WR-MM Male Connector w/o Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12MT"/>
</gates>
<devices>
<device name="" package="690357101272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357101272.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690357101272"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357101272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368171272" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w. Polarization and w/o Latch&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12FT"/>
</gates>
<devices>
<device name="" package="690357101272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368171272.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368171272"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368171272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368182672" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26FT"/>
</gates>
<devices>
<device name="" package="690368182672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368182672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368182672"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368182672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367292676" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Latch &amp; Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web 1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;

Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26FS"/>
</gates>
<devices>
<device name="" package="690367292676">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367292676.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367292676"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367292676"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357280476" prefix="J">
<description>&lt;b&gt;WR-MM Male SMT Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS"/>
</gates>
<devices>
<device name="" package="690357280476">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357280476.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690357280476"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357280476"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367292276" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Latch &amp; Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web 1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;

Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22FS"/>
</gates>
<devices>
<device name="" package="690367292276">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367292276.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367292276"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367292276"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690207100472" prefix="J">
<description>&lt;b&gt;WR-MM Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72"&gt;https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT_1"/>
</gates>
<devices>
<device name="" package="690207100472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690207100472.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="8.51mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690207100472"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690207100472"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357281076" prefix="J">
<description>&lt;b&gt;WR-MM Male SMT Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS"/>
</gates>
<devices>
<device name="" package="690357281076">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357281076.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690357281076"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357281076"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357101072" prefix="J">
<description>&lt;b&gt;WR-MM Male Connector w/o Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT"/>
</gates>
<devices>
<device name="" package="690357101072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357101072.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690357101072"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357101072"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368190872" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector with Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2020-07-06
&lt;BR&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8FT"/>
</gates>
<devices>
<device name="" package="690368190872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368190872.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368190872"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368190872"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368171072" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w. Polarization and w/o Latch&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10FT"/>
</gates>
<devices>
<device name="" package="690357101072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368171072.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368171072"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368171072"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368192472" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector with Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2020-07-06
&lt;BR&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24FT"/>
</gates>
<devices>
<device name="" package="690368192472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368192472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368192472"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368192472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690207100872" prefix="J">
<description>&lt;b&gt;WR-MM Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72"&gt;https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT_1"/>
</gates>
<devices>
<device name="" package="690207100872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690207100872.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="13.59mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690207100872"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690207100872"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367182672" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26FT"/>
</gates>
<devices>
<device name="" package="690367182672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367182672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367182672"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367182672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367281876" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18FS_1"/>
</gates>
<devices>
<device name="" package="690367281876">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367281876.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367281876"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367281876"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367181872" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18FT"/>
</gates>
<devices>
<device name="" package="690367181872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367181872.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367181872"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367181872"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368171872" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w. Polarization and w/o Latch&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18FT"/>
</gates>
<devices>
<device name="" package="690357101872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368171872.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368171872"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368171872"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368191472" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector with Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2020-07-06
&lt;BR&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14FT"/>
</gates>
<devices>
<device name="" package="690368191472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368191472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368191472"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368191472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357101872" prefix="J">
<description>&lt;b&gt;WR-MM Male Connector w/o Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18MT"/>
</gates>
<devices>
<device name="" package="690357101872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357101872.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690357101872"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357101872"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357280676" prefix="J">
<description>&lt;b&gt;WR-MM Male SMT Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS"/>
</gates>
<devices>
<device name="" package="690357280676">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357280676.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690357280676"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357280676"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357282676" prefix="J">
<description>&lt;b&gt;WR-MM Male SMT Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26MS"/>
</gates>
<devices>
<device name="" package="690357282676">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357282676.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690357282676"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357282676"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368172072" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w. Polarization and w/o Latch&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20FT"/>
</gates>
<devices>
<device name="" package="690357102072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368172072.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368172072"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368172072"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367180672" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6FT"/>
</gates>
<devices>
<device name="" package="690367180672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367180672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367180672"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367180672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357102072" prefix="J">
<description>&lt;b&gt;WR-MM Male Connector w/o Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20MT"/>
</gates>
<devices>
<device name="" package="690357102072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357102072.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690357102072"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357102072"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368171672" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w. Polarization and w/o Latch&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16FT"/>
</gates>
<devices>
<device name="" package="690357101672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368171672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368171672"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368171672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357102272" prefix="J">
<description>&lt;b&gt;WR-MM Male Connector w/o Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22MT"/>
</gates>
<devices>
<device name="" package="690357102272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357102272.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690357102272"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357102272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357101672" prefix="J">
<description>&lt;b&gt;WR-MM Male Connector w/o Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16MT"/>
</gates>
<devices>
<device name="" package="690357101672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357101672.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690357101672"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357101672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368172272" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w. Polarization and w/o Latch&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22FT"/>
</gates>
<devices>
<device name="" package="690357102272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368172272.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368172272"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368172272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368170472" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w. Polarization and w/o Latch&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4FT"/>
</gates>
<devices>
<device name="" package="690368170472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368170472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368170472"/>
<attribute name="PINS" value="4"/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368170472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367291676" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Latch &amp; Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web 1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;

Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16FS"/>
</gates>
<devices>
<device name="" package="690367291676">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367291676.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367291676"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367291676"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690207101872" prefix="J">
<description>&lt;b&gt;WR-MM Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72"&gt;https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18MT_1"/>
</gates>
<devices>
<device name="" package="690207101872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690207101872.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="26.29mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690207101872"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690207101872"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368180672" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6FT"/>
</gates>
<devices>
<device name="" package="690368180672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368180672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368180672"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368180672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367291276" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Latch &amp; Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web 1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;

Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12FS"/>
</gates>
<devices>
<device name="" package="690367291276">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367291276.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367291276"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367291276"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368180472" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4FT"/>
</gates>
<devices>
<device name="" package="690368170472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368180472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368180472"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368180472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367190472" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector with Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4FT"/>
</gates>
<devices>
<device name="" package="690367190472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367190472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367190472"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367190472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690207101472" prefix="J">
<description>&lt;b&gt;WR-MM Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72"&gt;https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14MT_1"/>
</gates>
<devices>
<device name="" package="690207101472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690207101472.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="21.21mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690207101472"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690207101472"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367280676" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6FS_1"/>
</gates>
<devices>
<device name="" package="690367280676">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367280676.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367280676"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367280676"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357100672" prefix="J">
<description>&lt;b&gt;WR-MM Male Connector w/o Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="690357100672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357100672.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690357100672"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357100672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367180472" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4FT"/>
</gates>
<devices>
<device name="" package="690367180472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367180472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367180472"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367180472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368182472" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24FT"/>
</gates>
<devices>
<device name="" package="690368182472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368182472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368182472"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368182472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368181872" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18FT"/>
</gates>
<devices>
<device name="" package="690368181872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368181872.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368181872"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368181872"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690207102472" prefix="J">
<description>&lt;b&gt;WR-MM Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72"&gt;https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24MT_1"/>
</gates>
<devices>
<device name="" package="690207102472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690207102472.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="33.91mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690207102472"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690207102472"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368192072" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector with Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2020-07-06
&lt;BR&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20FT"/>
</gates>
<devices>
<device name="" package="690368192072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368192072.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368192072"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368192072"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357100472" prefix="J">
<description>&lt;b&gt;WR-MM Male Connector w/o Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="690357100472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357100472.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690357100472"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357100472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367181672" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16FT"/>
</gates>
<devices>
<device name="" package="690367181672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367181672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367181672"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367181672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367281476" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14FS_1"/>
</gates>
<devices>
<device name="" package="690367281476">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367281476.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367281476"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367281476"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690207101672" prefix="J">
<description>&lt;b&gt;WR-MM Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72"&gt;https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16MT_1"/>
</gates>
<devices>
<device name="" package="690207101672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690207101672.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="23.75mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690207101672"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690207101672"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368170872" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w. Polarization and w/o Latch&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8FT"/>
</gates>
<devices>
<device name="" package="690368170872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368170872.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368170872"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368170872"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368191072" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector with Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2020-07-06
&lt;BR&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10FT"/>
</gates>
<devices>
<device name="" package="690368191072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368191072.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368191072"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368191072"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690207101272" prefix="J">
<description>&lt;b&gt;WR-MM Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72"&gt;https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12MT_1"/>
</gates>
<devices>
<device name="" package="690207101272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690207101272.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="18.67mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690207101272"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690207101272"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367182272" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22FT"/>
</gates>
<devices>
<device name="" package="690367182272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367182272.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367182272"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367182272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368182272" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22FT"/>
</gates>
<devices>
<device name="" package="690368182272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368182272.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368182272"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368182272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368191272" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector with Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2020-07-06
&lt;BR&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12FT"/>
</gates>
<devices>
<device name="" package="690368191272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368191272.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368191272"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368191272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367191472" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector with Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14FT"/>
</gates>
<devices>
<device name="" package="690367191472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367191472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367191472"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367191472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367191272" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector with Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12FT"/>
</gates>
<devices>
<device name="" package="690367191272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367191272.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367191272"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367191272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690207102272" prefix="J">
<description>&lt;b&gt;WR-MM Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72"&gt;https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22MT_1"/>
</gates>
<devices>
<device name="" package="690207102272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690207102272.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="31.37mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690207102272"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690207102272"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367190872" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector with Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8FT"/>
</gates>
<devices>
<device name="" package="690367190872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367190872.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367190872"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367190872"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357282476" prefix="J">
<description>&lt;b&gt;WR-MM Male SMT Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24MS"/>
</gates>
<devices>
<device name="" package="690357282476">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357282476.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690357282476"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357282476"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357281276" prefix="J">
<description>&lt;b&gt;WR-MM Male SMT Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12MS"/>
</gates>
<devices>
<device name="" package="690357281276">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357281276.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690357281276"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357281276"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367190672" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector with Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6FT"/>
</gates>
<devices>
<device name="" package="690367190672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367190672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367190672"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367190672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367292076" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Latch &amp; Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web 1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;

Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20FS"/>
</gates>
<devices>
<device name="" package="690367292076">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367292076.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367292076"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367292076"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367192072" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector with Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20FT"/>
</gates>
<devices>
<device name="" package="690367192072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367192072.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367192072"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367192072"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367291076" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Latch &amp; Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web 1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;

Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10FS"/>
</gates>
<devices>
<device name="" package="690367291076">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367291076.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367291076"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367291076"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690207100672" prefix="J">
<description>&lt;b&gt;WR-MM Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72"&gt;https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT_1"/>
</gates>
<devices>
<device name="" package="690207100672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690207100672.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="11.05mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690207100672"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690207100672"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367192472" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector with Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24FT"/>
</gates>
<devices>
<device name="" package="690367192472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367192472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367192472"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367192472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368181472" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14FT"/>
</gates>
<devices>
<device name="" package="690368181472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368181472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368181472"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368181472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357282276" prefix="J">
<description>&lt;b&gt;WR-MM Male SMT Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22MS"/>
</gates>
<devices>
<device name="" package="690357282276">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357282276.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690357282276"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357282276"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368172672" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w. Polarization and w/o Latch&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26FT"/>
</gates>
<devices>
<device name="" package="690368172672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368172672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368172672"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368172672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357280876" prefix="J">
<description>&lt;b&gt;WR-MM Male SMT Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS"/>
</gates>
<devices>
<device name="" package="690357280876">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357280876.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690357280876"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357280876"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357102472" prefix="J">
<description>&lt;b&gt;WR-MM Male Connector w/o Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24MT"/>
</gates>
<devices>
<device name="" package="690357102472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357102472.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690357102472"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357102472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690207102072" prefix="J">
<description>&lt;b&gt;WR-MM Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72"&gt;https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20MT_1"/>
</gates>
<devices>
<device name="" package="690207102072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690207102072.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="28.83mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690207102072"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690207102072"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367282676" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26FS_1"/>
</gates>
<devices>
<device name="" package="690367282676">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367282676.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367282676"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367282676"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368170672" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w. Polarization and w/o Latch&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6FT"/>
</gates>
<devices>
<device name="" package="690368170672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368170672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368170672"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368170672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357282076" prefix="J">
<description>&lt;b&gt;WR-MM Male SMT Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20MS"/>
</gates>
<devices>
<device name="" package="690357282076">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357282076.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690357282076"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357282076"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368190472" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector with Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2020-07-06
&lt;BR&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4FT"/>
</gates>
<devices>
<device name="" package="690368190472">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368190472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368190472"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368190472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367192672" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector with Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26FT"/>
</gates>
<devices>
<device name="" package="690367192672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367192672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367192672"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367192672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367282276" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22FS_1"/>
</gates>
<devices>
<device name="" package="690367282276">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367282276.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367282276"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367282276"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690207101072" prefix="J">
<description>&lt;b&gt;WR-MM Transition Connector&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Transition
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33156v209%20Family_WR-MM_69020710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72"&gt;https://katalog.we-online.com/en/em/MM_TRANSITION_CONNECTOR_69020710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT_1"/>
</gates>
<devices>
<device name="" package="690207101072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690207101072.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="16.13mm"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690207101072"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690207101072"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357100872" prefix="J">
<description>&lt;b&gt;WR-MM Male Connector w/o Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33157v209%20Family_WR-MM_69035710xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_MALE_CONNECTOR_W_O_LATCH_AND_WITH_POLARIZATION_69035710XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="690357100872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357100872.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690357100872"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357100872"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368191872" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector with Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2020-07-06
&lt;BR&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18FT"/>
</gates>
<devices>
<device name="" package="690368191872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368191872.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368191872"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368191872"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367291876" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Latch &amp; Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web 1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;

Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18FS"/>
</gates>
<devices>
<device name="" package="690367291876">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367291876.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367291876"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367291876"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368180872" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33163v209%20Family_WR-MM_69036818xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036818XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8FT"/>
</gates>
<devices>
<device name="" package="690368180872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368180872.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368180872"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368180872"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368172472" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector w. Polarization and w/o Latch&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class:25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;IR 1:1.5A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33162v209%20Family_WR-MM_69036817xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_W_O_LATCH_WITH_POLARIZATION_69036817XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-29
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24FT"/>
</gates>
<devices>
<device name="" package="690368172472">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368172472.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368172472"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368172472"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367191872" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector with Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33160v209%20Family_WR-MM_69036719xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72_2_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_WITH_LATCH_W_O_POLARIZATION_69036719XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18FT"/>
</gates>
<devices>
<device name="" package="690367191872">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367191872.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367191872"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367191872"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690357281476" prefix="J">
<description>&lt;b&gt;WR-MM Male SMT Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33158v209%20Family_WR-MM_69035728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_MALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69035728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14MS"/>
</gates>
<devices>
<device name="" package="690357281476">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690357281476.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690357281476"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690357281476"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367181072" prefix="J">
<description>&lt;b&gt;WR-MM Female Connector w/o Latch &amp; w/o Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class :25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33159v209%20Family_Wr-MM_69036718xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_CONNECTOR_W_O_LATCH_AND_POLARIZATION_69036718XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10FT"/>
</gates>
<devices>
<device name="" package="690367181072">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367181072.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690367181072"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367181072"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367290876" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Latch &amp; Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33161v209%20WR-MiMo_69036729xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: Web 1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036729XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;

Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8FS"/>
</gates>
<devices>
<device name="" package="690367290876">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367290876.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367290876"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367290876"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368190672" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector with Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2020-07-06
&lt;BR&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6FT"/>
</gates>
<devices>
<device name="" package="690368190672">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368190672.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368190672"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368190672"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690368192272" prefix="J">
<description>&lt;b&gt;WR-MM Female Angled Connector with Latch &amp; w. Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33164v209%20Family_WR-MM_69036819xx72.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: web1:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
web2:&lt;a href="https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72"&gt;https://katalog.we-online.com/en/em/MM_1_27_FEMALE_ANGLED_CONNECTOR_WITH_LATCH_AND_POLARIZATION_69036819XX72&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2020-07-06
&lt;BR&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22FT"/>
</gates>
<devices>
<device name="" package="690368192272">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690368192272.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="690368192272"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="690368192272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367281076" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10FS_1"/>
</gates>
<devices>
<device name="" package="690367281076">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367281076.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367281076"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367281076"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="690367280476" prefix="J">
<description>&lt;b&gt;WR-MM Female SMT Connector with Polarization&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 2.54 mm 
&lt;BR&gt;Quality Class25 Mating cycles
&lt;BR&gt;Gender:Female
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Insulator Material:PA6T
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color:Red
&lt;BR&gt;Contact Material :Phosphor Bronze
&lt;BR&gt;Contact Plating :Mat Tin over Nickel
&lt;BR&gt;Contact Type: Stamped 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 °C up to +105 °C 
&lt;BR&gt;Compliance Lead free / RoHS 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 1:1.5 A
&lt;BR&gt;Working Voltage 100 V (AC) 
&lt;BR&gt;Withstanding Voltage:500 V (AC) 
&lt;BR&gt;Contact Resistance: 10 mΩ 
&lt;BR&gt;Insulation Resistance:1000 MΩ 
&lt;BR&gt;
PACKAGING PROPERTIES:
&lt;BR&gt;cULus Approval:E323964
&lt;BR&gt;
&lt;BR&gt;Packaging :Tape and Reel
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58636v209%20Family_Female_SMT_ConnectorWPolarzation_WR-MM_69036728xx76.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see:Web1: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76_2&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Web2: &lt;a href="https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76"&gt;https://katalog.we-online.com/en/em/MM_1_27_SMT_FEMALE_CONNECTOR_WITH_POLARIZATION_69036728XX76&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-28
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4FS_1"/>
</gates>
<devices>
<device name="" package="690367280476">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/690367280476.pdf"/>
<attribute name="GENDER" value="Female"/>
<attribute name="IR" value="1.5A"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="690367280476"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value=" 2.54 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="690367280476"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
