<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Single Coil Power Inductors - WE-HCM&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-09-10&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-HCM_4035_74434035007">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;4035,SMT,2Pins</description>
</package>
<package name="WE-HCM_1323">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1323,SMT,2Pins</description>
</package>
<package name="WE-HCM_4035_74434035010">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;4035,SMT,2Pins</description>
</package>
<package name="WE-HCM_1050">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1050,SMT,2Pins</description>
</package>
<package name="WE-HCM_4030">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;4030,SMT,2Pins</description>
</package>
<package name="WE-HCM_1190">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1190,SMT,2Pins</description>
</package>
<package name="WE-HCM_1435">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1435,SMT,3Pins</description>
</package>
<package name="WE-HCM_1088">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1088,SMT,2Pins</description>
</package>
<package name="WE-HCM_1390">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1390,SMT,2Pins</description>
</package>
<package name="WE-HCM_1820">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1820,SMT,6Pins,One turn</description>
</package>
<package name="WE-HCM_1070">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1070,SMT,2Pins</description>
</package>
<package name="WE-HCM_1820_THREE-TURNS">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1820,SMT,6Pins,Three turns</description>
</package>
<package name="WE-HCM_1078">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1078,SMT,2Pins</description>
</package>
<package name="WE-HCM_1350">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1350,SMT,2Pins</description>
</package>
<package name="WE-HCM_1088B">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1088,SMT,2Pins</description>
</package>
<package name="WE-HCM_1012">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1012,SMT,2Pins</description>
</package>
<package name="WE-HCM_7070">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;7070,SMT,2Pins</description>
</package>
<package name="WE-HCM_1820_PARALLEL">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1820,SMT,6Pins,Parallel</description>
</package>
<package name="WE-HCM_1411">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1411,SMT,2Pins</description>
</package>
<package name="WE-HCM_1820_TWO-TURNS">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1820,SMT,2Pins,Two turns</description>
</package>
<package name="WE-HCM_1088A">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1088,SMT,2Pins</description>
</package>
<package name="WE-HCM_5030">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;5030,SMT,2Pins</description>
</package>
<package name="WE-HCM_9065">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;9065,SMT,2Pins</description>
</package>
<package name="WE-HCM_7050">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;7050,SMT,2Pins</description>
</package>
<package name="WE-HCM_1240">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1240,SMT,2Pins</description>
</package>
<package name="WE-HCM_1052">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1052,SMT,2Pins</description>
</package>
</packages>
<symbols>
<symbol name="WE-HCM_1820_THREE-TURNS">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="L_POINT_GAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WE-HCM_1820">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WE-HCM_1820_TWO-TURNS">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-HCM_1820_PARALLEL">
<pin name="IN" direction="pas"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-HCM_1323" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun,Shan 2019-08-08&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74431323012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431323012.pdf"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="45A"/>
<attribute name="LR" value="0.117uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74431323012"/>
<attribute name="RDC" value="0.7mOhm"/>
<attribute name="VALUE" value="0.12uH"/>
</technology>
<technology name="_74431323016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431323016.pdf"/>
<attribute name="FRES" value="113MHz"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="33A"/>
<attribute name="LR" value="0.149uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74431323016"/>
<attribute name="RDC" value="0.7mOhm"/>
<attribute name="VALUE" value="0.16uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_4035" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;


Created by Ella Wu  2020-5-13&lt;br&gt;
2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="_74434035007" package="WE-HCM_4035_74434035007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74434035007.pdf"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="29A"/>
<attribute name="ISAT" value="17A"/>
<attribute name="LR" value="0.01uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74434035007"/>
<attribute name="RDC" value="0.37mOhm"/>
<attribute name="VALUE" value="0.07uH"/>
</technology>
</technologies>
</device>
<device name="_74434035010" package="WE-HCM_4035_74434035010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74434035010.pdf"/>
<attribute name="FRES" value="69MHz"/>
<attribute name="IR" value="29A"/>
<attribute name="ISAT" value="16A"/>
<attribute name="LR" value="0.016uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74434035010"/>
<attribute name="RDC" value="0.37mOhm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1050" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;



Updated by  Yingchun,Shan 2019-08-08&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744303012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744303012.pdf"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="55A"/>
<attribute name="LR" value="0.118uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744303012"/>
<attribute name="RDC" value="0.325mOhm"/>
<attribute name="VALUE" value="0.12uH"/>
</technology>
<technology name="_744303015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744303015.pdf"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="42A"/>
<attribute name="LR" value="0.15uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744303015"/>
<attribute name="RDC" value="0.325mOhm"/>
<attribute name="VALUE" value="0.155uH"/>
</technology>
<technology name="_744303022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744303022.pdf"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="30A"/>
<attribute name="LR" value="0.18uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744303022"/>
<attribute name="RDC" value="0.325mOhm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1190" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu. 2021-09-10&lt;br&gt;
2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1190">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744301025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744301025.pdf"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="65A"/>
<attribute name="LR" value="0.25uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744301025"/>
<attribute name="RDC" value="0.32mOhm"/>
<attribute name="VALUE" value="0.25uH"/>
</technology>
<technology name="_744301033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744301033.pdf"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="46A"/>
<attribute name="LR" value="0.325uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744301033"/>
<attribute name="RDC" value="0.32mOhm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744301047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744301047.pdf"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="35A"/>
<attribute name="LR" value="0.24uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744301047"/>
<attribute name="RDC" value="0.32mOhm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_4030" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;


Created by Ella Wu  2020-5-13&lt;br&gt;
2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_4030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744340300025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744340300025.pdf"/>
<attribute name="FRES" value="180MHz"/>
<attribute name="IR" value="27A"/>
<attribute name="ISAT" value="45A"/>
<attribute name="LR" value="0.025uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744340300025"/>
<attribute name="RDC" value="0.27mOhm"/>
<attribute name="VALUE" value="0.025uH"/>
</technology>
<technology name="_744340300030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744340300030.pdf"/>
<attribute name="FRES" value="170MHz"/>
<attribute name="IR" value="27A"/>
<attribute name="ISAT" value="44A"/>
<attribute name="LR" value="0.029uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744340300030"/>
<attribute name="RDC" value="0.27mOhm"/>
<attribute name="VALUE" value="0.03uH"/>
</technology>
<technology name="_744340300055">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744340300055.pdf"/>
<attribute name="FRES" value="123MHz"/>
<attribute name="IR" value="27A"/>
<attribute name="ISAT" value="24A"/>
<attribute name="LR" value="0.055uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744340300055"/>
<attribute name="RDC" value="0.27mOhm"/>
<attribute name="VALUE" value="0.055uH"/>
</technology>
<technology name="_744340300075">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744340300075.pdf"/>
<attribute name="FRES" value="106MHz"/>
<attribute name="IR" value="27A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="LR" value="0.075uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744340300075"/>
<attribute name="RDC" value="0.27mOhm"/>
<attribute name="VALUE" value="0.075uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1435" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2019-01-14&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1435">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74431435010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431435010.pdf"/>
<attribute name="FRES" value="87MHz"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="80A"/>
<attribute name="LR" value="0.099uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74431435010"/>
<attribute name="RDC" value="0.28mOhm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_74431435012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431435012.pdf"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="69A"/>
<attribute name="LR" value="0.119uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74431435012"/>
<attribute name="RDC" value="0.28mOhm"/>
<attribute name="VALUE" value="0.12uH"/>
</technology>
<technology name="_74431435015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431435015.pdf"/>
<attribute name="FRES" value="84MHz"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="61A"/>
<attribute name="LR" value="0.147uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74431435015"/>
<attribute name="RDC" value="0.28mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
<technology name="_74431435018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431435018.pdf"/>
<attribute name="FRES" value="63MHz"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="55A"/>
<attribute name="LR" value="0.175uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74431435018"/>
<attribute name="RDC" value="0.28mOhm"/>
<attribute name="VALUE" value="0.18uH"/>
</technology>
<technology name="_74431435022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431435022.pdf"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="41A"/>
<attribute name="LR" value="0.211uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74431435022"/>
<attribute name="RDC" value="0.28mOhm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1088" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2019-01-14&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1088">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443082010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443082010.pdf"/>
<attribute name="FRES" value="94MHz"/>
<attribute name="IR" value="60A"/>
<attribute name="ISAT" value="113A"/>
<attribute name="LR" value="0.099uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443082010"/>
<attribute name="RDC" value="0.18mOhm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_7443082012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443082012.pdf"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="60A"/>
<attribute name="ISAT" value="92A"/>
<attribute name="LR" value="0.118uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443082012"/>
<attribute name="RDC" value="0.18mOhm"/>
<attribute name="VALUE" value="0.12uH"/>
</technology>
<technology name="_7443082015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443082015.pdf"/>
<attribute name="FRES" value="63MHz"/>
<attribute name="IR" value="60A"/>
<attribute name="ISAT" value="85A"/>
<attribute name="LR" value="0.147uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443082015"/>
<attribute name="RDC" value="0.18mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
<technology name="_7443082017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443082017.pdf"/>
<attribute name="FRES" value="56MHz"/>
<attribute name="IR" value="60A"/>
<attribute name="ISAT" value="64A"/>
<attribute name="LR" value="0.15uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443082017"/>
<attribute name="RDC" value="0.18mOhm"/>
<attribute name="VALUE" value="0.17uH"/>
</technology>
<technology name="_7443082018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443082018.pdf"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IR" value="60A"/>
<attribute name="ISAT" value="63A"/>
<attribute name="LR" value="0.165uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443082018"/>
<attribute name="RDC" value="0.18mOhm"/>
<attribute name="VALUE" value="0.18uH"/>
</technology>
<technology name="_7443082022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443082022.pdf"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="IR" value="60A"/>
<attribute name="ISAT" value="56A"/>
<attribute name="LR" value="0.154uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443082022"/>
<attribute name="RDC" value="0.18mOhm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1820" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;



Updated by Ella Wu 2019-06-22&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HCM_1820"/>
</gates>
<devices>
<device name="" package="WE-HCM_1820">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="_74431821100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431821100.pdf"/>
<attribute name="FRES" value="47MHz"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="LR" value="0.03uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74431821100"/>
<attribute name="RDC" value="0.33mOhm"/>
<attribute name="VALUE" value="0.13uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1390" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;


Updated by  Yingchun,Shan 2019-08-08&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1390">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744309012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744309012.pdf"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="47.5A"/>
<attribute name="ISAT" value="125A"/>
<attribute name="LR" value="0.12uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744309012"/>
<attribute name="RDC" value="0.165mOhm"/>
<attribute name="VALUE" value="0.12uH"/>
</technology>
<technology name="_744309025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744309025.pdf"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="47.5A"/>
<attribute name="ISAT" value="81A"/>
<attribute name="LR" value="0.245uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744309025"/>
<attribute name="RDC" value="0.165mOhm"/>
<attribute name="VALUE" value="0.25uH"/>
</technology>
<technology name="_744309033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744309033.pdf"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="47.5A"/>
<attribute name="ISAT" value="62.5A"/>
<attribute name="LR" value="0.31uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744309033"/>
<attribute name="RDC" value="0.165mOhm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744309047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744309047.pdf"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="47.5A"/>
<attribute name="ISAT" value="40.5A"/>
<attribute name="LR" value="0.2uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744309047"/>
<attribute name="RDC" value="0.165mOhm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1070" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;


Updated by  Yingchun,Shan 2019-08-08&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744308015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744308015.pdf"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="58A"/>
<attribute name="LR" value="0.15uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744308015"/>
<attribute name="RDC" value="0.37mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
<technology name="_744308020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744308020.pdf"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="48A"/>
<attribute name="LR" value="0.198uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744308020"/>
<attribute name="RDC" value="0.37mOhm"/>
<attribute name="VALUE" value="0.2uH"/>
</technology>
<technology name="_744308025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744308025.pdf"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="44A"/>
<attribute name="LR" value="0.246uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744308025"/>
<attribute name="RDC" value="0.37mOhm"/>
<attribute name="VALUE" value="0.25uH"/>
</technology>
<technology name="_744308033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744308033.pdf"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="30A"/>
<attribute name="LR" value="0.305uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744308033"/>
<attribute name="RDC" value="0.37mOhm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744308040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744308040.pdf"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="26A"/>
<attribute name="LR" value="0.345uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744308040"/>
<attribute name="RDC" value="0.37mOhm"/>
<attribute name="VALUE" value="0.4uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1350" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun,Shan 2019-08-08&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1350">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744305022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744305022.pdf"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="42A"/>
<attribute name="LR" value="0.215uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744305022"/>
<attribute name="RDC" value="0.155mOhm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744305033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744305033.pdf"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="26A"/>
<attribute name="LR" value="0.27uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744305033"/>
<attribute name="RDC" value="0.155mOhm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744305040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744305040.pdf"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="LR" value="0.1uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744305040"/>
<attribute name="RDC" value="0.155mOhm"/>
<attribute name="VALUE" value="0.4uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1820_THREE-TURNS" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-22&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HCM_1820_THREE-TURNS"/>
</gates>
<devices>
<device name="" package="WE-HCM_1820_THREE-TURNS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="_74431821100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431821100.pdf"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="23A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="LR" value="0.1uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74431821100"/>
<attribute name="RDC" value="0.33mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1078" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;



Updated by  Yingchun,Shan 2019-08-08&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1078">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443081010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443081010.pdf"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="100A"/>
<attribute name="LR" value="0.1uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443081010"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_7443081012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443081012.pdf"/>
<attribute name="FRES" value="74MHz"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="85A"/>
<attribute name="LR" value="0.12uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443081012"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="VALUE" value="0.12uH"/>
</technology>
<technology name="_7443081015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443081015.pdf"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="67A"/>
<attribute name="LR" value="0.15uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443081015"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
<technology name="_7443081018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443081018.pdf"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="60A"/>
<attribute name="LR" value="0.176uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443081018"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="VALUE" value="0.18uH"/>
</technology>
<technology name="_7443081022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443081022.pdf"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="45A"/>
<attribute name="LR" value="0.2uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443081022"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_7443081030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443081030.pdf"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="32A"/>
<attribute name="LR" value="0.14uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443081030"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="VALUE" value="0.3uH"/>
</technology>
<technology name="_7443081040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443081040.pdf"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="21A"/>
<attribute name="LR" value="0.05uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443081040"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="VALUE" value="0.4uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1012" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2020-5-13&lt;br&gt;
2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74431012007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431012007.pdf"/>
<attribute name="FRES" value="149MHz"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="125A"/>
<attribute name="LR" value="0.069uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74431012007 "/>
<attribute name="RDC" value="0.125mOhm"/>
<attribute name="VALUE" value="0.07uH"/>
</technology>
<technology name="_74431012010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431012010.pdf"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="125A"/>
<attribute name="LR" value="0.099uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74431012010 "/>
<attribute name="RDC" value="0.125mOhm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_74431012012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431012012.pdf"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="118A"/>
<attribute name="LR" value="0.119uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74431012012 "/>
<attribute name="RDC" value="0.125mOhm"/>
<attribute name="VALUE" value="0.12uH"/>
</technology>
<technology name="_74431012015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431012015.pdf"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="88A"/>
<attribute name="LR" value="0.144uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74431012015 "/>
<attribute name="RDC" value="0.125mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1088B" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-01-14&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1088B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443082010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443082010B.pdf"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="70A"/>
<attribute name="ISAT" value="100A"/>
<attribute name="LR" value="0.104uH"/>
<attribute name="MATERIAL" value=""/>
<attribute name="MOUNT" value=""/>
<attribute name="PART-NUMBER" value="7443082010B"/>
<attribute name="RDC" value="0.114mOhm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_7443082010B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443082010B.pdf"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="70A"/>
<attribute name="ISAT" value="100A"/>
<attribute name="LR" value="0.104uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443082010B"/>
<attribute name="RDC" value="0.114mOhm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_7443082012">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443082012B.pdf"/>
<attribute name="FRES" value="64MHz"/>
<attribute name="IR" value="70A"/>
<attribute name="ISAT" value="90A"/>
<attribute name="LR" value="0.117uH"/>
<attribute name="MATERIAL" value=""/>
<attribute name="MOUNT" value=""/>
<attribute name="PART-NUMBER" value="7443082012B"/>
<attribute name="RDC" value="0.114mOhm"/>
<attribute name="VALUE" value="0.12uH"/>
</technology>
<technology name="_7443082012B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443082012B.pdf"/>
<attribute name="FRES" value="64MHz"/>
<attribute name="IR" value="70A"/>
<attribute name="ISAT" value="90A"/>
<attribute name="LR" value="0.117uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443082012B"/>
<attribute name="RDC" value="0.114mOhm"/>
<attribute name="VALUE" value="0.12uH"/>
</technology>
<technology name="_7443082015">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443082015B.pdf"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="IR" value="70A"/>
<attribute name="ISAT" value="72A"/>
<attribute name="LR" value="0.143uH"/>
<attribute name="MATERIAL" value=""/>
<attribute name="MOUNT" value=""/>
<attribute name="PART-NUMBER" value="7443082015B"/>
<attribute name="RDC" value="0.114mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
<technology name="_7443082015B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443082015B.pdf"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="IR" value="70A"/>
<attribute name="ISAT" value="72A"/>
<attribute name="LR" value="0.143uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443082015B"/>
<attribute name="RDC" value="0.114mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_7070" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;


Updated by  Yingchun,Shan 2019-08-08&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_7070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744307012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744307012.pdf"/>
<attribute name="FRES" value="66MHz"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="48A"/>
<attribute name="LR" value="0.118uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744307012"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="VALUE" value="0.12uH"/>
</technology>
<technology name="_744307016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744307016.pdf"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="41A"/>
<attribute name="LR" value="0.155uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744307016"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="VALUE" value="0.16uH"/>
</technology>
<technology name="_744307022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744307022.pdf"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="29A"/>
<attribute name="LR" value="0.174uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744307022"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1820_PARALLEL" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2019-06-22&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HCM_1820_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-HCM_1820_PARALLEL">
<connects>
<connect gate="G$1" pin="IN" pad="1 2 3" route="any"/>
<connect gate="G$1" pin="OUT" pad="4 5 6" route="any"/>
</connects>
<technologies>
<technology name="_74431821100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431821100.pdf"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="28A"/>
<attribute name="LR" value="0.09uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74431821100"/>
<attribute name="RDC" value="0.33mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1411" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2019-01-14&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1411">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443091062">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443091062.pdf"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="62A"/>
<attribute name="LR" value="0.62uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443091062"/>
<attribute name="RDC" value="0.42mOhm"/>
<attribute name="VALUE" value="0.62uH"/>
</technology>
<technology name="_7443091080">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443091080.pdf"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="56A"/>
<attribute name="LR" value="0.78uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443091080"/>
<attribute name="RDC" value="0.42mOhm"/>
<attribute name="VALUE" value="0.8uH"/>
</technology>
<technology name="_7443091100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443091100.pdf"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="37A"/>
<attribute name="LR" value="0.95uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443091100"/>
<attribute name="RDC" value="0.42mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7443091120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443091120.pdf"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="36A"/>
<attribute name="LR" value="1.02uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443091120"/>
<attribute name="RDC" value="0.42mOhm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_7443091150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443091150.pdf"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="25A"/>
<attribute name="LR" value="0.18uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443091150"/>
<attribute name="RDC" value="0.42mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1820_TWO-TURNS" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2019-06-22&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HCM_1820_TWO-TURNS"/>
</gates>
<devices>
<device name="" package="WE-HCM_1820_TWO-TURNS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="_74431821100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74431821100.pdf"/>
<attribute name="FRES" value="41MHz"/>
<attribute name="IR" value="21A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="LR" value="0.37uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74431821100"/>
<attribute name="RDC" value="0.33mOhm"/>
<attribute name="VALUE" value="0.5uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1088A" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2019-01-14&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1088A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443082015">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443082015A.pdf"/>
<attribute name="FRES" value="56MHz"/>
<attribute name="IR" value="65A"/>
<attribute name="ISAT" value="74A"/>
<attribute name="LR" value="0.136uH"/>
<attribute name="MATERIAL" value=""/>
<attribute name="MOUNT" value=""/>
<attribute name="PART-NUMBER" value="7443082015A"/>
<attribute name="RDC" value="0.15mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
<technology name="_7443082015A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443082015A.pdf"/>
<attribute name="FRES" value="56MHz"/>
<attribute name="IR" value="65A"/>
<attribute name="ISAT" value="74A"/>
<attribute name="LR" value="0.136uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443082015A"/>
<attribute name="RDC" value="0.15mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
<technology name="_7443082018">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443082018A.pdf"/>
<attribute name="FRES" value="47MHz"/>
<attribute name="IR" value="65A"/>
<attribute name="ISAT" value="68A"/>
<attribute name="LR" value="0.157uH"/>
<attribute name="MATERIAL" value=""/>
<attribute name="MOUNT" value=""/>
<attribute name="PART-NUMBER" value="7443082018A"/>
<attribute name="RDC" value="0.15mOhm"/>
<attribute name="VALUE" value="0.18uH"/>
</technology>
<technology name="_7443082018A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7443082018A.pdf"/>
<attribute name="FRES" value="47MHz"/>
<attribute name="IR" value="65A"/>
<attribute name="ISAT" value="68A"/>
<attribute name="LR" value="0.157uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443082018A"/>
<attribute name="RDC" value="0.15mOhm"/>
<attribute name="VALUE" value="0.18uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_5030" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2020-5-13&lt;br&gt;
2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74435030010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74435030010.pdf"/>
<attribute name="FRES" value="83MHz"/>
<attribute name="IR" value="27A"/>
<attribute name="ISAT" value="17A"/>
<attribute name="LR" value="0.01uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74435030010"/>
<attribute name="RDC" value="0.31mOhm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_9065" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2020-5-13&lt;br&gt;
2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_9065">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744300006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744300006.pdf"/>
<attribute name="FRES" value="124MHz"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="63A"/>
<attribute name="LR" value="0.059uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744300006"/>
<attribute name="RDC" value="0.22mOhm"/>
<attribute name="VALUE" value="0.06uH"/>
</technology>
<technology name="_744300008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744300008.pdf"/>
<attribute name="FRES" value="94MHz"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="51A"/>
<attribute name="LR" value="0.078uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744300008"/>
<attribute name="RDC" value="0.22mOhm"/>
<attribute name="VALUE" value="0.08uH"/>
</technology>
<technology name="_744300010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744300010.pdf"/>
<attribute name="FRES" value="74MHz"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="42A"/>
<attribute name="LR" value="0.093uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744300010"/>
<attribute name="RDC" value="0.22mOhm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_744300015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744300015.pdf"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="29A"/>
<attribute name="LR" value="0.034uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744300015"/>
<attribute name="RDC" value="0.22mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
<technology name="_744300022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744300022.pdf"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="19A"/>
<attribute name="LR" value="0.034uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744300022"/>
<attribute name="RDC" value="0.22mOhm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_7050" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun,Shan 2019-08-08&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_7050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744302007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744302007.pdf"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="IR" value="30A"/>
<attribute name="ISAT" value="60A"/>
<attribute name="LR" value="0.071uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744302007"/>
<attribute name="RDC" value="0.235mOhm"/>
<attribute name="VALUE" value="0.072uH"/>
</technology>
<technology name="_744302010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744302010.pdf"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="30A"/>
<attribute name="ISAT" value="45A"/>
<attribute name="LR" value="0.104uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744302010"/>
<attribute name="RDC" value="0.235mOhm"/>
<attribute name="VALUE" value="0.105uH"/>
</technology>
<technology name="_744302015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744302015.pdf"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="30A"/>
<attribute name="ISAT" value="32A"/>
<attribute name="LR" value="0.125uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744302015"/>
<attribute name="RDC" value="0.235mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1052" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;


Updated by  Yingchun,Shan 2019-08-08&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1052">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744306020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744306020.pdf"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="36A"/>
<attribute name="LR" value="0.195uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744306020"/>
<attribute name="RDC" value="0.26mOhm"/>
<attribute name="VALUE" value="0.2uH"/>
</technology>
<technology name="_744306025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744306025.pdf"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="32A"/>
<attribute name="LR" value="0.24uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744306025"/>
<attribute name="RDC" value="0.26mOhm"/>
<attribute name="VALUE" value="0.25uH"/>
</technology>
<technology name="_744306030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744306030.pdf"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="24A"/>
<attribute name="LR" value="0.22uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744306030"/>
<attribute name="RDC" value="0.26mOhm"/>
<attribute name="VALUE" value="0.3uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1240" prefix="L">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14798v209%20Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HCM/"&gt;https://www.we-online.com/catalog/en/WE-HCM/&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun,Shan 2019-08-08&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCM_1240">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744304010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744304010.pdf"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="IR" value="24A"/>
<attribute name="ISAT" value="52A"/>
<attribute name="LR" value="0.1uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744304010"/>
<attribute name="RDC" value="0.17mOhm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_744304016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744304016.pdf"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="24A"/>
<attribute name="ISAT" value="32A"/>
<attribute name="LR" value="0.155uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744304016"/>
<attribute name="RDC" value="0.17mOhm"/>
<attribute name="VALUE" value="0.16uH"/>
</technology>
<technology name="_744304022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744304022.pdf"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="24A"/>
<attribute name="ISAT" value="23A"/>
<attribute name="LR" value="0.16uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744304022"/>
<attribute name="RDC" value="0.17mOhm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
