<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-LHMI&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2023-03-12&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-LHMI_4012">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 4012, SMT, 2pins
&lt;br&gt;LXWXH = 4.06x4.06x1.0mm</description>
</package>
<package name="WE-LHMI_1365">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 1365, SMT, 2pins
&lt;br&gt;LXWXH = 12.5x12.5x6.2mm</description>
</package>
<package name="WE-LHMI_4020">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 4012, SMT, 2pins
&lt;br&gt;LXWXH = 4.06x4.06x1.8mm</description>
</package>
<package name="WE-LHMI_5020">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 5020, SMT, 2pins
&lt;br&gt;LXWXH = 5.2x5.2x1.8mm</description>
</package>
<package name="WE-LHMI_1335">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 1040, SMT, 2pins
&lt;br&gt;LXWXH = 12.6x12.6x3.3mm</description>
</package>
<package name="WE-LHMI_7030HT">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 7030HT, SMT, 2pins
&lt;br&gt;LXWXH = 6.6x6.6x2.8mm</description>
</package>
<package name="WE-LHMI_8030">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 8030, SMT, 2pins
&lt;br&gt;LXWXH = 9.2x8.5x3.0mm</description>
</package>
<package name="WE-LHMI_7050HT">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 7030HT, SMT, 2pins
&lt;br&gt;LXWXH = 6.6x6.6x4.8mm</description>
</package>
<package name="WE-LHMI_5020HT">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 5020HT, SMT, 2pins
&lt;br&gt;LXWXH = 5.2x5.2x1.8mm</description>
</package>
<package name="WE-LHMI_5030">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 5030, SMT, 2pins
&lt;br&gt;LXWXH = 5.2x5.2x2.8mm</description>
</package>
<package name="WE-LHMI_4020HT">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 4012HT, SMT, 2pins
&lt;br&gt;LXWXH = 4.06x4.06x1.8mm</description>
</package>
<package name="WE-LHMI_7050">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 7050, SMT, 2pins
&lt;br&gt;LXWXH = 6.6x6.6x2.8mm</description>
</package>
<package name="WE-LHMI_8040_PW3">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 8040, SMT, 2pins
&lt;br&gt;LXWXH = 9.2x8.5x3.0mm
&lt;br&gt;
&lt;br&gt;PW3 means the width of the pin is 3.0 mm</description>
</package>
<package name="WE-LHMI_8040_PW5">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 8040, SMT, 2pins
&lt;br&gt;LXWXH = 9.2x8.5x3.0mm
&lt;br&gt;
&lt;br&gt;PW3 means the width of the pin is 3.0 mm</description>
</package>
<package name="WE-LHMI_1040">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 1040, SMT, 2pins
&lt;br&gt;LXWXH = 10x10x3.8mm</description>
</package>
<package name="WE-LHMI_7030">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 7030, SMT, 2pins
&lt;br&gt;LXWXH = 6.6x6.6x2.8mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-LHMI_4012" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-LHMI_4012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373210010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373210010?ae"/>
<attribute name="FRES" value="365MHz"/>
<attribute name="IR" value="14.1A"/>
<attribute name="ISAT" value="16.1A"/>
<attribute name="ISAT2" value="29.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373210010 "/>
<attribute name="RDC-MAX" value="5.5mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_744373210022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373210022?ae"/>
<attribute name="FRES" value="230MHz"/>
<attribute name="IR" value="11.4A"/>
<attribute name="ISAT" value="11.1A"/>
<attribute name="ISAT2" value="11.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373210022 "/>
<attribute name="RDC-MAX" value="21.5mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744373210047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373210047?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="IR" value="6.9A"/>
<attribute name="ISAT" value="6.8A"/>
<attribute name="ISAT2" value="6.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373210047 "/>
<attribute name="RDC-MAX" value="12.5mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74437321010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437321010?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="4.5A"/>
<attribute name="ISAT" value="5.65A"/>
<attribute name="ISAT2" value="4.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437321010 "/>
<attribute name="RDC-MAX" value="10mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74437321015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437321015?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="3.9A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="ISAT2" value="3.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437321015 "/>
<attribute name="RDC-MAX" value="5.1mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74437321022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437321022?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="ISAT2" value="3.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437321022 "/>
<attribute name="RDC-MAX" value="6.2mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74437321033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437321033?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="3.15A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="ISAT2" value="3.15A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437321033 "/>
<attribute name="RDC-MAX" value="4.8mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74437321047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437321047?ae"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="IR" value="2.55A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="ISAT2" value="2.55A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437321047 "/>
<attribute name="RDC-MAX" value="4.1mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74437321056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437321056?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="2.15A"/>
<attribute name="ISAT" value="1.95A"/>
<attribute name="ISAT2" value="2.15A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437321056 "/>
<attribute name="RDC-MAX" value="3.65mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74437321068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437321068?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="1.65A"/>
<attribute name="ISAT" value="1.65A"/>
<attribute name="ISAT2" value="1.65A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437321068 "/>
<attribute name="RDC-MAX" value="3.05mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74437321082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437321082?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="1.65A"/>
<attribute name="ISAT2" value="1.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437321082 "/>
<attribute name="RDC-MAX" value="2.85mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74437321100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437321100?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="ISAT2" value="1.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437321100 "/>
<attribute name="RDC-MAX" value="2.65mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_1365" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-LHMI_1365">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443739650022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443739650022?ae"/>
<attribute name="FRES" value="112.3MHz"/>
<attribute name="IR" value="54.9A"/>
<attribute name="ISAT" value="81.5A"/>
<attribute name="ISAT2" value="54.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443739650022 "/>
<attribute name="RDC-MAX" value="120mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_7443739650033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443739650033?ae"/>
<attribute name="FRES" value="74.7MHz"/>
<attribute name="IR" value="49A"/>
<attribute name="ISAT" value="57.5A"/>
<attribute name="ISAT2" value="49A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443739650033 "/>
<attribute name="RDC-MAX" value="108.6mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_7443739650047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443739650047?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="40.7A"/>
<attribute name="ISAT" value="49.7A"/>
<attribute name="ISAT2" value="40.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443739650047 "/>
<attribute name="RDC-MAX" value="99.4mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_7443739650056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443739650056?ae"/>
<attribute name="FRES" value="51.7MHz"/>
<attribute name="IR" value="37.1A"/>
<attribute name="ISAT" value="36.3A"/>
<attribute name="ISAT2" value="37.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443739650056 "/>
<attribute name="RDC-MAX" value="68.3mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_7443739650068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443739650068?ae"/>
<attribute name="FRES" value="51.1MHz"/>
<attribute name="IR" value="35.6A"/>
<attribute name="ISAT" value="35.7A"/>
<attribute name="ISAT2" value="35.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443739650068 "/>
<attribute name="RDC-MAX" value="67.4mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_744373965010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965010?ae"/>
<attribute name="FRES" value="43.5MHz"/>
<attribute name="IR" value="28.2A"/>
<attribute name="ISAT" value="32.7A"/>
<attribute name="ISAT2" value="28.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965010 "/>
<attribute name="RDC-MAX" value="59.9mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_744373965015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965015?ae"/>
<attribute name="FRES" value="29.5MHz"/>
<attribute name="IR" value="25.7A"/>
<attribute name="ISAT" value="28.9A"/>
<attribute name="ISAT2" value="25.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965015 "/>
<attribute name="RDC-MAX" value="55.2mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_744373965022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965022?ae"/>
<attribute name="FRES" value="21.6MHz"/>
<attribute name="IR" value="21.6A"/>
<attribute name="ISAT" value="20.7A"/>
<attribute name="ISAT2" value="21.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965022 "/>
<attribute name="RDC-MAX" value="41.1mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744373965033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965033?ae"/>
<attribute name="FRES" value="20.3MHz"/>
<attribute name="IR" value="16.2A"/>
<attribute name="ISAT" value="20.3A"/>
<attribute name="ISAT2" value="16.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965033 "/>
<attribute name="RDC-MAX" value="41.5mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744373965047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965047?ae"/>
<attribute name="FRES" value="13.9MHz"/>
<attribute name="IR" value="15.1A"/>
<attribute name="ISAT" value="18.4A"/>
<attribute name="ISAT2" value="15.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965047 "/>
<attribute name="RDC-MAX" value="35.8mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744373965056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965056?ae"/>
<attribute name="FRES" value="13.7MHz"/>
<attribute name="IR" value="13.3A"/>
<attribute name="ISAT" value="18.3A"/>
<attribute name="ISAT2" value="13.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965056 "/>
<attribute name="RDC-MAX" value="33mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_744373965068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965068?ae"/>
<attribute name="FRES" value="11.6MHz"/>
<attribute name="IR" value="12.7A"/>
<attribute name="ISAT" value="15.8A"/>
<attribute name="ISAT2" value="12.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965068 "/>
<attribute name="RDC-MAX" value="28.9mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744373965100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965100?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="11.8A"/>
<attribute name="ISAT" value="13.2A"/>
<attribute name="ISAT2" value="11.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965100 "/>
<attribute name="RDC-MAX" value="23.9mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744373965101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965101?ae"/>
<attribute name="FRES" value="2.4MHz"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT" value="3.45A"/>
<attribute name="ISAT2" value="3.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965101 "/>
<attribute name="RDC-MAX" value="6.8mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744373965120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965120?ae"/>
<attribute name="FRES" value="7.6MHz"/>
<attribute name="IR" value="9.1A"/>
<attribute name="ISAT" value="12.9A"/>
<attribute name="ISAT2" value="9.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965120 "/>
<attribute name="RDC-MAX" value="26.6mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_744373965150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965150?ae"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="IR" value="7.7A"/>
<attribute name="ISAT" value="10.2A"/>
<attribute name="ISAT2" value="7.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965150 "/>
<attribute name="RDC-MAX" value="18.5mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744373965220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965220?ae"/>
<attribute name="FRES" value="5.4MHz"/>
<attribute name="IR" value="6.5A"/>
<attribute name="ISAT" value="6.7A"/>
<attribute name="ISAT2" value="6.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965220 "/>
<attribute name="RDC-MAX" value="13.9mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744373965330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965330?ae"/>
<attribute name="FRES" value="4.4MHz"/>
<attribute name="IR" value="5.45A"/>
<attribute name="ISAT" value="6.3A"/>
<attribute name="ISAT2" value="5.45A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965330 "/>
<attribute name="RDC-MAX" value="13.2mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744373965470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373965470?ae"/>
<attribute name="FRES" value="3.8MHz"/>
<attribute name="IR" value="4.4A"/>
<attribute name="ISAT" value="6.15A"/>
<attribute name="ISAT2" value="4.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373965470 "/>
<attribute name="RDC-MAX" value="13.1mOhm"/>
<attribute name="SIZE" value=" 1365 "/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_7030HT" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Created by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-LHMI_7030HT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443734648010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734648010?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IR" value="13.5A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="ISAT2" value="13.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734648010 "/>
<attribute name="RDC-MAX" value="18.5mOhm"/>
<attribute name="SIZE" value="7030HT"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7443734648015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734648015?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="IR" value="12A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="ISAT2" value="12A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734648015 "/>
<attribute name="RDC-MAX" value="17mOhm"/>
<attribute name="SIZE" value="7030HT"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7443734648022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734648022?ae"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="IR" value="10.5A"/>
<attribute name="ISAT" value="6.8A"/>
<attribute name="ISAT2" value="10.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734648022 "/>
<attribute name="RDC-MAX" value="14.7mOhm"/>
<attribute name="SIZE" value="7030HT"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7443734648033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734648033?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="8.7A"/>
<attribute name="ISAT" value="5.6A"/>
<attribute name="ISAT2" value="8.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734648033 "/>
<attribute name="RDC-MAX" value="10.8mOhm"/>
<attribute name="SIZE" value="7030HT"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7443734648047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734648047?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="4.4A"/>
<attribute name="ISAT2" value="7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734648047 "/>
<attribute name="RDC-MAX" value="9.8mOhm"/>
<attribute name="SIZE" value="7030HT"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7443734648068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734648068?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="5.6A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="ISAT2" value="5.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734648068 "/>
<attribute name="RDC-MAX" value="7.6mOhm"/>
<attribute name="SIZE" value="7030HT"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7443734648100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734648100?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="ISAT2" value="4.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734648100 "/>
<attribute name="RDC-MAX" value="6mOhm"/>
<attribute name="SIZE" value="7030HT"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_1335" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-LHMI_1335">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373770022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373770022?ae"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="IR" value="45A"/>
<attribute name="ISAT" value="23.9A"/>
<attribute name="ISAT2" value="45A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373770022 "/>
<attribute name="RDC-MAX" value="57.4mOhm"/>
<attribute name="SIZE" value=" 1335 "/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744373770033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373770033?ae"/>
<attribute name="FRES" value="84MHz"/>
<attribute name="IR" value="41.6A"/>
<attribute name="ISAT" value="23.9A"/>
<attribute name="ISAT2" value="41.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373770033 "/>
<attribute name="RDC-MAX" value="65.5mOhm"/>
<attribute name="SIZE" value=" 1335 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744373770047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373770047?ae"/>
<attribute name="FRES" value="77MHz"/>
<attribute name="IR" value="33.8A"/>
<attribute name="ISAT" value="17.2A"/>
<attribute name="ISAT2" value="33.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373770047 "/>
<attribute name="RDC-MAX" value="40.2mOhm"/>
<attribute name="SIZE" value=" 1335 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_744373770056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373770056?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="IR" value="32.9A"/>
<attribute name="ISAT" value="16.8A"/>
<attribute name="ISAT2" value="32.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373770056 "/>
<attribute name="RDC-MAX" value="42.8mOhm"/>
<attribute name="SIZE" value=" 1335 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_744373770068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373770068?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="IR" value="28.8A"/>
<attribute name="ISAT" value="15.7A"/>
<attribute name="ISAT2" value="28.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373770068 "/>
<attribute name="RDC-MAX" value="42.5mOhm"/>
<attribute name="SIZE" value=" 1335 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_74437377010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437377010?ae"/>
<attribute name="FRES" value="41MHz"/>
<attribute name="IR" value="23.5A"/>
<attribute name="ISAT" value="15.4A"/>
<attribute name="ISAT2" value="23.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437377010 "/>
<attribute name="RDC-MAX" value="38mOhm"/>
<attribute name="SIZE" value=" 1335 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74437377015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437377015?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="17.8A"/>
<attribute name="ISAT" value="14.3A"/>
<attribute name="ISAT2" value="17.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437377015 "/>
<attribute name="RDC-MAX" value="33.8mOhm"/>
<attribute name="SIZE" value=" 1335 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74437377022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437377022?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="14.3A"/>
<attribute name="ISAT" value="14.2A"/>
<attribute name="ISAT2" value="14.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437377022 "/>
<attribute name="RDC-MAX" value="31.2mOhm"/>
<attribute name="SIZE" value=" 1335 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74437377033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437377033?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="12.8A"/>
<attribute name="ISAT" value="13.3A"/>
<attribute name="ISAT2" value="12.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437377033 "/>
<attribute name="RDC-MAX" value="30.9mOhm"/>
<attribute name="SIZE" value=" 1335 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74437377047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437377047?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="10.6A"/>
<attribute name="ISAT" value="12A"/>
<attribute name="ISAT2" value="10.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437377047 "/>
<attribute name="RDC-MAX" value="25.1mOhm"/>
<attribute name="SIZE" value=" 1335 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_4020" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-LHMI_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373240010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373240010?ae"/>
<attribute name="FRES" value="323MHz"/>
<attribute name="IR" value="16.5A"/>
<attribute name="ISAT" value="20.9A"/>
<attribute name="ISAT2" value="16.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373240010 "/>
<attribute name="RDC-MAX" value="37.6mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_744373240022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373240022?ae"/>
<attribute name="FRES" value="195MHz"/>
<attribute name="IR" value="11.4A"/>
<attribute name="ISAT" value="10.8A"/>
<attribute name="ISAT2" value="11.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373240022 "/>
<attribute name="RDC-MAX" value="22.3mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744373240033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373240033?ae"/>
<attribute name="FRES" value="143MHz"/>
<attribute name="IR" value="10.5A"/>
<attribute name="ISAT" value="11.2A"/>
<attribute name="ISAT2" value="10.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373240033 "/>
<attribute name="RDC-MAX" value="22mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744373240047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373240047?ae"/>
<attribute name="FRES" value="122MHz"/>
<attribute name="IR" value="8.7A"/>
<attribute name="ISAT" value="10.4A"/>
<attribute name="ISAT2" value="8.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373240047 "/>
<attribute name="RDC-MAX" value="19.6mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_744373240056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373240056?ae"/>
<attribute name="FRES" value="104MHz"/>
<attribute name="IR" value="7.9A"/>
<attribute name="ISAT" value="6.7A"/>
<attribute name="ISAT2" value="7.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373240056 "/>
<attribute name="RDC-MAX" value="13mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_744373240068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373240068?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="7.3A"/>
<attribute name="ISAT" value="7.1A"/>
<attribute name="ISAT2" value="7.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373240068 "/>
<attribute name="RDC-MAX" value="14mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_74437324010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437324010?ae"/>
<attribute name="FRES" value="89MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="ISAT2" value="6.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437324010 "/>
<attribute name="RDC-MAX" value="12.5mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74437324012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437324012?ae"/>
<attribute name="FRES" value="71MHz"/>
<attribute name="IR" value="5.85A"/>
<attribute name="ISAT" value="6.3A"/>
<attribute name="ISAT2" value="5.85A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437324012 "/>
<attribute name="RDC-MAX" value="11.6mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74437324015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437324015?ae"/>
<attribute name="FRES" value="64MHz"/>
<attribute name="IR" value="4.9A"/>
<attribute name="ISAT" value="5.65A"/>
<attribute name="ISAT2" value="4.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437324015 "/>
<attribute name="RDC-MAX" value="10.1mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74437324022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437324022?ae"/>
<attribute name="FRES" value="49MHz"/>
<attribute name="IR" value="4.05A"/>
<attribute name="ISAT" value="4.45A"/>
<attribute name="ISAT2" value="4.05A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437324022 "/>
<attribute name="RDC-MAX" value="8.4mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74437324033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437324033?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="2.75A"/>
<attribute name="ISAT2" value="3.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437324033 "/>
<attribute name="RDC-MAX" value="5.45mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74437324047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437324047?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="IR" value="2.95A"/>
<attribute name="ISAT" value="2.45A"/>
<attribute name="ISAT2" value="2.95A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437324047 "/>
<attribute name="RDC-MAX" value="5.4mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74437324056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437324056?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="ISAT2" value="2.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437324056 "/>
<attribute name="RDC-MAX" value="5.1mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74437324068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437324068?ae"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="IR" value="2.35A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="ISAT2" value="2.35A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437324068 "/>
<attribute name="RDC-MAX" value="4.75mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74437324082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437324082?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="ISAT2" value="2.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437324082 "/>
<attribute name="RDC-MAX" value="3.8mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74437324100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437324100?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="1.95A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="ISAT2" value="1.95A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437324100 "/>
<attribute name="RDC-MAX" value="3.15mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74437324150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437324150?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="1.35A"/>
<attribute name="ISAT2" value="1.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437324150 "/>
<attribute name="RDC-MAX" value="2.75mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74437324220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437324220?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="1.45A"/>
<attribute name="ISAT2" value="1.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437324220 "/>
<attribute name="RDC-MAX" value="2.35mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_7050HT" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Created by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-LHMI_7050HT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443734948010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734948010?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="IR" value="15.7A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="ISAT2" value="15.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734948010 "/>
<attribute name="RDC-MAX" value="17.8mOhm"/>
<attribute name="SIZE" value="7050HT"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7443734948015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734948015?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="13.2A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="ISAT2" value="13.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734948015 "/>
<attribute name="RDC-MAX" value="15.5mOhm"/>
<attribute name="SIZE" value="7050HT"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7443734948022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734948022?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="IR" value="10.5A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="ISAT2" value="10.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734948022 "/>
<attribute name="RDC-MAX" value="12.8mOhm"/>
<attribute name="SIZE" value="7050HT"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7443734948033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734948033?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="8.7A"/>
<attribute name="ISAT" value="5.6A"/>
<attribute name="ISAT2" value="8.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734948033 "/>
<attribute name="RDC-MAX" value="11.8mOhm"/>
<attribute name="SIZE" value="7050HT"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7443734948047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734948047?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="5.2A"/>
<attribute name="ISAT2" value="7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734948047 "/>
<attribute name="RDC-MAX" value="11.4mOhm"/>
<attribute name="SIZE" value="7050HT"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7443734948068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734948068?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="6.6A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="ISAT2" value="6.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734948068 "/>
<attribute name="RDC-MAX" value="8.4mOhm"/>
<attribute name="SIZE" value="7050HT"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7443734948100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443734948100?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="5.2A"/>
<attribute name="ISAT" value="3.7A"/>
<attribute name="ISAT2" value="5.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443734948100 "/>
<attribute name="RDC-MAX" value="8mOhm"/>
<attribute name="SIZE" value="7050HT"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_8030" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-LHMI_8030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373560022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373560022?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="29.5A"/>
<attribute name="ISAT" value="32.1A"/>
<attribute name="ISAT2" value="29.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373560022 "/>
<attribute name="RDC-MAX" value="63.4mOhm"/>
<attribute name="SIZE" value=" 8030 "/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744373560033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373560033?ae"/>
<attribute name="FRES" value="95MHz"/>
<attribute name="IR" value="24.8A"/>
<attribute name="ISAT" value="26.2A"/>
<attribute name="ISAT2" value="24.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373560033 "/>
<attribute name="RDC-MAX" value="51.9mOhm"/>
<attribute name="SIZE" value=" 8030 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744373560047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373560047?ae"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="IR" value="23.2A"/>
<attribute name="ISAT" value="22A"/>
<attribute name="ISAT2" value="23.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373560047 "/>
<attribute name="RDC-MAX" value="44.7mOhm"/>
<attribute name="SIZE" value=" 8030 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_744373560068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373560068?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IR" value="18.5A"/>
<attribute name="ISAT" value="21A"/>
<attribute name="ISAT2" value="18.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373560068 "/>
<attribute name="RDC-MAX" value="43mOhm"/>
<attribute name="SIZE" value=" 8030 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_744373560082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373560082?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="IR" value="17.3A"/>
<attribute name="ISAT" value="19.3A"/>
<attribute name="ISAT2" value="17.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373560082 "/>
<attribute name="RDC-MAX" value="40.9mOhm"/>
<attribute name="SIZE" value=" 8030 "/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_74437356010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437356010?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="IR" value="15.7A"/>
<attribute name="ISAT" value="15.8A"/>
<attribute name="ISAT2" value="15.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437356010 "/>
<attribute name="RDC-MAX" value="34.2mOhm"/>
<attribute name="SIZE" value=" 8030 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74437356015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437356015?ae"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="IR" value="12.2A"/>
<attribute name="ISAT" value="13.5A"/>
<attribute name="ISAT2" value="12.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437356015 "/>
<attribute name="RDC-MAX" value="27.2mOhm"/>
<attribute name="SIZE" value=" 8030 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74437356022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437356022?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="9.5A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="ISAT2" value="9.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437356022 "/>
<attribute name="RDC-MAX" value="19.6mOhm"/>
<attribute name="SIZE" value=" 8030 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74437356033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437356033?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="8A"/>
<attribute name="ISAT" value="8.8A"/>
<attribute name="ISAT2" value="8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437356033 "/>
<attribute name="RDC-MAX" value="16.1mOhm"/>
<attribute name="SIZE" value=" 8030 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74437356047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437356047?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="6.7A"/>
<attribute name="ISAT" value="8.1A"/>
<attribute name="ISAT2" value="6.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437356047 "/>
<attribute name="RDC-MAX" value="15.2mOhm"/>
<attribute name="SIZE" value=" 8030 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74437356068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437356068?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="5.8A"/>
<attribute name="ISAT" value="6.9A"/>
<attribute name="ISAT2" value="5.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437356068 "/>
<attribute name="RDC-MAX" value="14.2mOhm"/>
<attribute name="SIZE" value=" 8030 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74437356082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437356082?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="4.6A"/>
<attribute name="ISAT" value="6.3A"/>
<attribute name="ISAT2" value="4.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437356082 "/>
<attribute name="RDC-MAX" value="14mOhm"/>
<attribute name="SIZE" value=" 8030 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74437356100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437356100?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="4.45A"/>
<attribute name="ISAT" value="6.2A"/>
<attribute name="ISAT2" value="4.45A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437356100 "/>
<attribute name="RDC-MAX" value="13.4mOhm"/>
<attribute name="SIZE" value=" 8030 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_5020" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-LHMI_5020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373340033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373340033?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="12.4A"/>
<attribute name="ISAT" value="14.7A"/>
<attribute name="ISAT2" value="12.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373340033 "/>
<attribute name="RDC-MAX" value="29.3mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744373340047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373340047?ae"/>
<attribute name="FRES" value="95MHz"/>
<attribute name="IR" value="11.5A"/>
<attribute name="ISAT" value="9.6A"/>
<attribute name="ISAT2" value="11.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373340047 "/>
<attribute name="RDC-MAX" value="19.8mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_744373340068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373340068?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="9.4A"/>
<attribute name="ISAT" value="9.8A"/>
<attribute name="ISAT2" value="9.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373340068 "/>
<attribute name="RDC-MAX" value="17.8mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_74437334010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437334010?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="7.4A"/>
<attribute name="ISAT" value="9.2A"/>
<attribute name="ISAT2" value="7.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437334010 "/>
<attribute name="RDC-MAX" value="17.7mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74437334012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437334012?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="6.4A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="ISAT2" value="6.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437334012 "/>
<attribute name="RDC-MAX" value="14mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74437334015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437334015?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="6A"/>
<attribute name="ISAT" value="6.6A"/>
<attribute name="ISAT2" value="6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437334015 "/>
<attribute name="RDC-MAX" value="13.6mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74437334022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437334022?ae"/>
<attribute name="FRES" value="46MHz"/>
<attribute name="IR" value="4.75A"/>
<attribute name="ISAT" value="6.4A"/>
<attribute name="ISAT2" value="4.75A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437334022 "/>
<attribute name="RDC-MAX" value="11.9mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74437334033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437334033?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="3.75A"/>
<attribute name="ISAT" value="5.25A"/>
<attribute name="ISAT2" value="3.75A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437334033 "/>
<attribute name="RDC-MAX" value="9.6mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74437334047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437334047?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="4.1A"/>
<attribute name="ISAT2" value="3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437334047 "/>
<attribute name="RDC-MAX" value="7.5mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74437334056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437334056?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="2.85A"/>
<attribute name="ISAT" value="3.7A"/>
<attribute name="ISAT2" value="2.85A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437334056 "/>
<attribute name="RDC-MAX" value="7mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74437334068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437334068?ae"/>
<attribute name="FRES" value="20.5MHz"/>
<attribute name="IR" value="2.65A"/>
<attribute name="ISAT" value="3.05A"/>
<attribute name="ISAT2" value="2.65A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437334068 "/>
<attribute name="RDC-MAX" value="5.55mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74437334082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437334082?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="ISAT2" value="2.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437334082 "/>
<attribute name="RDC-MAX" value="5.65mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74437334100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437334100?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="2.25A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="ISAT2" value="2.25A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437334100 "/>
<attribute name="RDC-MAX" value="5.15mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_5020HT" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Created by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-LHMI_5020HT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443733448010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443733448010?ae"/>
<attribute name="FRES" value="62MHz"/>
<attribute name="IR" value="7.9A"/>
<attribute name="ISAT" value="5.4A"/>
<attribute name="ISAT2" value="7.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443733448010 "/>
<attribute name="RDC-MAX" value="12mOhm"/>
<attribute name="SIZE" value="5020HT"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7443733448015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443733448015?ae"/>
<attribute name="FRES" value="54MHz"/>
<attribute name="IR" value="6.7A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="ISAT2" value="6.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443733448015 "/>
<attribute name="RDC-MAX" value="9.5mOhm"/>
<attribute name="SIZE" value="5020HT"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7443733448022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443733448022?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="5.5A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="ISAT2" value="5.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443733448022 "/>
<attribute name="RDC-MAX" value="6.7mOhm"/>
<attribute name="SIZE" value="5020HT"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7443733448033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443733448033?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="IR" value="4.8A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="ISAT2" value="4.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443733448033 "/>
<attribute name="RDC-MAX" value="6.5mOhm"/>
<attribute name="SIZE" value="5020HT"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7443733448047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443733448047?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="ISAT2" value="4.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443733448047 "/>
<attribute name="RDC-MAX" value="5.8mOhm"/>
<attribute name="SIZE" value="5020HT"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7443733448068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443733448068?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="3.3A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="ISAT2" value="3.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443733448068 "/>
<attribute name="RDC-MAX" value="4.5mOhm"/>
<attribute name="SIZE" value="5020HT"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7443733448100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443733448100?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="ISAT2" value="2.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443733448100 "/>
<attribute name="RDC-MAX" value="3mOhm"/>
<attribute name="SIZE" value="5020HT"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_5030" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-LHMI_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373360033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373360033?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="IR" value="15.1A"/>
<attribute name="ISAT" value="15A"/>
<attribute name="ISAT2" value="15.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373360033 "/>
<attribute name="RDC-MAX" value="29.3mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744373360047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373360047?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="12.3A"/>
<attribute name="ISAT" value="10.8A"/>
<attribute name="ISAT2" value="12.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373360047 "/>
<attribute name="RDC-MAX" value="21.5mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_744373360068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373360068?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="9.8A"/>
<attribute name="ISAT" value="10.2A"/>
<attribute name="ISAT2" value="9.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373360068 "/>
<attribute name="RDC-MAX" value="19.3mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_74437336010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437336010?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="8.6A"/>
<attribute name="ISAT" value="7.4A"/>
<attribute name="ISAT2" value="8.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437336010 "/>
<attribute name="RDC-MAX" value="14.2mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74437336012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437336012?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="8.3A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="ISAT2" value="8.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437336012 "/>
<attribute name="RDC-MAX" value="13.9mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74437336015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437336015?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="7.8A"/>
<attribute name="ISAT" value="7.7A"/>
<attribute name="ISAT2" value="7.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437336015 "/>
<attribute name="RDC-MAX" value="14.2mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74437336022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437336022?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="ISAT2" value="6.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437336022 "/>
<attribute name="RDC-MAX" value="14mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74437336033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437336033?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="5.45A"/>
<attribute name="ISAT" value="5.55A"/>
<attribute name="ISAT2" value="5.45A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437336033 "/>
<attribute name="RDC-MAX" value="10.9mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74437336047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437336047?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="4.35A"/>
<attribute name="ISAT" value="3.85A"/>
<attribute name="ISAT2" value="4.35A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437336047 "/>
<attribute name="RDC-MAX" value="7.6mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74437336056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437336056?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="4.15A"/>
<attribute name="ISAT" value="3.85A"/>
<attribute name="ISAT2" value="4.15A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437336056 "/>
<attribute name="RDC-MAX" value="7.7mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74437336068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437336068?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="3.75A"/>
<attribute name="ISAT" value="2.9A"/>
<attribute name="ISAT2" value="3.75A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437336068 "/>
<attribute name="RDC-MAX" value="5.9mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74437336100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437336100?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="ISAT2" value="2.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437336100 "/>
<attribute name="RDC-MAX" value="5.35mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_4020HT" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Created by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-LHMI_4020HT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443732448010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443732448010?ae"/>
<attribute name="FRES" value="66MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="ISAT2" value="7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443732448010 "/>
<attribute name="RDC-MAX" value="8.5mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7443732448015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443732448015?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="6.1A"/>
<attribute name="ISAT" value="3.4A"/>
<attribute name="ISAT2" value="6.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443732448015 "/>
<attribute name="RDC-MAX" value="7mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7443732448022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443732448022?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="IR" value="5.2A"/>
<attribute name="ISAT" value="2.9A"/>
<attribute name="ISAT2" value="5.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443732448022 "/>
<attribute name="RDC-MAX" value="6mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7443732448033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443732448033?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="4.1A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="ISAT2" value="4.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443732448033 "/>
<attribute name="RDC-MAX" value="5.6mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7443732448047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443732448047?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="ISAT2" value="3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443732448047 "/>
<attribute name="RDC-MAX" value="4.7mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7443732448068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443732448068?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="ISAT2" value="2.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443732448068 "/>
<attribute name="RDC-MAX" value="3mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7443732448100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443732448100?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="ISAT2" value="2.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443732448100 "/>
<attribute name="RDC-MAX" value="2.4mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_7050" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-LHMI_7050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373490047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373490047?ae"/>
<attribute name="FRES" value="96MHz"/>
<attribute name="IR" value="17.8A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="ISAT2" value="17.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373490047 "/>
<attribute name="RDC-MAX" value="41.6mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_744373490056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373490056?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="17.6A"/>
<attribute name="ISAT" value="19.9A"/>
<attribute name="ISAT2" value="17.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373490056 "/>
<attribute name="RDC-MAX" value="36.4mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_744373490068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373490068?ae"/>
<attribute name="FRES" value="73MHz"/>
<attribute name="IR" value="16.7A"/>
<attribute name="ISAT" value="18.8A"/>
<attribute name="ISAT2" value="16.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373490068 "/>
<attribute name="RDC-MAX" value="33.8mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_744373490082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373490082?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="15.5A"/>
<attribute name="ISAT" value="17.4A"/>
<attribute name="ISAT2" value="15.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373490082 "/>
<attribute name="RDC-MAX" value="31.6mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_74437349010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349010?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="IR" value="13.4A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="ISAT2" value="13.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349010 "/>
<attribute name="RDC-MAX" value="25.8mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74437349012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349012?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="12.4A"/>
<attribute name="ISAT" value="12A"/>
<attribute name="ISAT2" value="12.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349012 "/>
<attribute name="RDC-MAX" value="24mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74437349015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349015?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="11.3A"/>
<attribute name="ISAT" value="9.7A"/>
<attribute name="ISAT2" value="11.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349015 "/>
<attribute name="RDC-MAX" value="18.7mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74437349022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349022?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="9.9A"/>
<attribute name="ISAT" value="10.5A"/>
<attribute name="ISAT2" value="9.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349022 "/>
<attribute name="RDC-MAX" value="19.1mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74437349033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349033?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="7.5A"/>
<attribute name="ISAT" value="7.9A"/>
<attribute name="ISAT2" value="7.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349033 "/>
<attribute name="RDC-MAX" value="15.1mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74437349047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349047?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="ISAT2" value="6.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349047 "/>
<attribute name="RDC-MAX" value="14.6mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74437349056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349056?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="4.9A"/>
<attribute name="ISAT" value="6.6A"/>
<attribute name="ISAT2" value="4.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349056 "/>
<attribute name="RDC-MAX" value="16.5mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74437349068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349068?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="4.8A"/>
<attribute name="ISAT" value="6.3A"/>
<attribute name="ISAT2" value="4.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349068 "/>
<attribute name="RDC-MAX" value="13.1mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74437349082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349082?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="4.35A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="ISAT2" value="4.35A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349082 "/>
<attribute name="RDC-MAX" value="12.2mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74437349100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349100?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="4.05A"/>
<attribute name="ISAT" value="5.6A"/>
<attribute name="ISAT2" value="4.05A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349100 "/>
<attribute name="RDC-MAX" value="10.5mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74437349150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349150?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="3.6A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="ISAT2" value="3.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349150 "/>
<attribute name="RDC-MAX" value="7.2mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74437349220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349220?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="2.75A"/>
<attribute name="ISAT" value="4.15A"/>
<attribute name="ISAT2" value="2.75A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349220 "/>
<attribute name="RDC-MAX" value="8.5mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74437349330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349330?ae"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="IR" value="2.45A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="ISAT2" value="2.45A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349330 "/>
<attribute name="RDC-MAX" value="4.75mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74437349470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349470?ae"/>
<attribute name="FRES" value="7.3MHz"/>
<attribute name="IR" value="1.9A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="ISAT2" value="1.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349470 "/>
<attribute name="RDC-MAX" value="3.4mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74437349560">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349560?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="1.75A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="ISAT2" value="1.75A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349560 "/>
<attribute name="RDC-MAX" value="2.7mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="56uH"/>
</technology>
<technology name="_74437349680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437349680?ae"/>
<attribute name="FRES" value="3.5MHz"/>
<attribute name="IR" value="1.65A"/>
<attribute name="ISAT" value="1.45A"/>
<attribute name="ISAT2" value="1.65A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437349680 "/>
<attribute name="RDC-MAX" value="3.8mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_1040" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-LHMI_1040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373680022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373680022?ae"/>
<attribute name="FRES" value="153MHz"/>
<attribute name="IR" value="41.4A"/>
<attribute name="ISAT" value="46A"/>
<attribute name="ISAT2" value="41.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373680022 "/>
<attribute name="RDC-MAX" value="94.2mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744373680036">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373680036?ae"/>
<attribute name="FRES" value="104MHz"/>
<attribute name="IR" value="36.2A"/>
<attribute name="ISAT" value="44.5A"/>
<attribute name="ISAT2" value="36.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373680036 "/>
<attribute name="RDC-MAX" value="79.4mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="0.36uH"/>
</technology>
<technology name="_744373680039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373680039?ae"/>
<attribute name="FRES" value="101MHz"/>
<attribute name="IR" value="35.3A"/>
<attribute name="ISAT" value="43A"/>
<attribute name="ISAT2" value="35.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373680039 "/>
<attribute name="RDC-MAX" value="77.5mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="0.39uH"/>
</technology>
<technology name="_744373680045">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373680045?ae"/>
<attribute name="FRES" value="82MHz"/>
<attribute name="IR" value="32.6A"/>
<attribute name="ISAT" value="34.9A"/>
<attribute name="ISAT2" value="32.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373680045 "/>
<attribute name="RDC-MAX" value="64.5mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="0.45uH"/>
</technology>
<technology name="_744373680056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373680056?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="29.3A"/>
<attribute name="ISAT" value="31.7A"/>
<attribute name="ISAT2" value="29.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373680056 "/>
<attribute name="RDC-MAX" value="60.9mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_744373680068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373680068?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IR" value="23.8A"/>
<attribute name="ISAT" value="30.6A"/>
<attribute name="ISAT2" value="23.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373680068 "/>
<attribute name="RDC-MAX" value="58.3mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_74437368010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437368010?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="21.3A"/>
<attribute name="ISAT" value="22.7A"/>
<attribute name="ISAT2" value="21.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437368010 "/>
<attribute name="RDC-MAX" value="48.3mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74437368022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437368022?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="14.3A"/>
<attribute name="ISAT" value="18.1A"/>
<attribute name="ISAT2" value="14.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437368022 "/>
<attribute name="RDC-MAX" value="38.7mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74437368033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437368033?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="11.1A"/>
<attribute name="ISAT" value="15.6A"/>
<attribute name="ISAT2" value="11.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437368033 "/>
<attribute name="RDC-MAX" value="31.2mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74437368039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437368039?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="10.3A"/>
<attribute name="ISAT" value="12A"/>
<attribute name="ISAT2" value="10.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437368039 "/>
<attribute name="RDC-MAX" value="26.8mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
<technology name="_74437368047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437368047?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="9.4A"/>
<attribute name="ISAT" value="11.7A"/>
<attribute name="ISAT2" value="9.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437368047 "/>
<attribute name="RDC-MAX" value="26mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74437368056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437368056?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="8.7A"/>
<attribute name="ISAT" value="9.4A"/>
<attribute name="ISAT2" value="8.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437368056 "/>
<attribute name="RDC-MAX" value="19.4mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74437368068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437368068?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="8.6A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="ISAT2" value="8.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437368068 "/>
<attribute name="RDC-MAX" value="17.4mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74437368100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437368100?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="7.9A"/>
<attribute name="ISAT2" value="7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437368100 "/>
<attribute name="RDC-MAX" value="16.8mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74437368150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437368150?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="5.7A"/>
<attribute name="ISAT" value="5.55A"/>
<attribute name="ISAT2" value="5.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437368150 "/>
<attribute name="RDC-MAX" value="11.8mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74437368220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437368220?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="4.5A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="ISAT2" value="4.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437368220 "/>
<attribute name="RDC-MAX" value="10.8mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74437368330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437368330?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="3.75A"/>
<attribute name="ISAT" value="3.3A"/>
<attribute name="ISAT2" value="3.75A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437368330 "/>
<attribute name="RDC-MAX" value="7.4mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74437368470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437368470?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="2.95A"/>
<attribute name="ISAT" value="2.55A"/>
<attribute name="ISAT2" value="2.95A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437368470 "/>
<attribute name="RDC-MAX" value="6.7mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_8040" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="_PW3" package="WE-LHMI_8040_PW3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373580022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373580022?ae"/>
<attribute name="FRES" value="145MHz"/>
<attribute name="IR" value="38.5A"/>
<attribute name="ISAT" value="38.3A"/>
<attribute name="ISAT2" value="38.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373580022 "/>
<attribute name="RDC-MAX" value="80.4mOhm"/>
<attribute name="SIZE" value=" 8040 "/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744373580033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373580033?ae"/>
<attribute name="FRES" value="96MHz"/>
<attribute name="IR" value="29.7A"/>
<attribute name="ISAT" value="31.4A"/>
<attribute name="ISAT2" value="29.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373580033 "/>
<attribute name="RDC-MAX" value="67.2mOhm"/>
<attribute name="SIZE" value=" 8040 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744373580047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373580047?ae"/>
<attribute name="FRES" value="82MHz"/>
<attribute name="IR" value="27.6A"/>
<attribute name="ISAT" value="27.1A"/>
<attribute name="ISAT2" value="27.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373580047 "/>
<attribute name="RDC-MAX" value="56.8mOhm"/>
<attribute name="SIZE" value=" 8040 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
</technologies>
</device>
<device name="_PW5" package="WE-LHMI_8040_PW5">
<technologies>
<technology name="_744373580068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373580068?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="21.5A"/>
<attribute name="ISAT" value="17.5A"/>
<attribute name="ISAT2" value="21.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373580068 "/>
<attribute name="RDC-MAX" value="37.8mOhm"/>
<attribute name="SIZE" value=" 8040 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_744373580082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373580082?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="IR" value="20.7A"/>
<attribute name="ISAT" value="19.7A"/>
<attribute name="ISAT2" value="20.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373580082 "/>
<attribute name="RDC-MAX" value="41.6mOhm"/>
<attribute name="SIZE" value=" 8040 "/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_74437358010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437358010?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="18.6A"/>
<attribute name="ISAT" value="20.6A"/>
<attribute name="ISAT2" value="18.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437358010 "/>
<attribute name="RDC-MAX" value="43.1mOhm"/>
<attribute name="SIZE" value=" 8040 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74437358022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437358022?ae"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="IR" value="12A"/>
<attribute name="ISAT" value="17.2A"/>
<attribute name="ISAT2" value="12A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437358022 "/>
<attribute name="RDC-MAX" value="36.8mOhm"/>
<attribute name="SIZE" value=" 8040 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74437358033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437358033?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="12.4A"/>
<attribute name="ISAT2" value="10A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437358033 "/>
<attribute name="RDC-MAX" value="27mOhm"/>
<attribute name="SIZE" value=" 8040 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74437358047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437358047?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="7.9A"/>
<attribute name="ISAT" value="10.8A"/>
<attribute name="ISAT2" value="7.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437358047 "/>
<attribute name="RDC-MAX" value="22.9mOhm"/>
<attribute name="SIZE" value=" 8040 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74437358068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437358068?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="6.4A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="ISAT2" value="6.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437358068 "/>
<attribute name="RDC-MAX" value="17.7mOhm"/>
<attribute name="SIZE" value=" 8040 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74437358082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437358082?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="5.45A"/>
<attribute name="ISAT" value="8.6A"/>
<attribute name="ISAT2" value="5.45A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437358082 "/>
<attribute name="RDC-MAX" value="16.6mOhm"/>
<attribute name="SIZE" value=" 8040 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74437358100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437358100?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="5.05A"/>
<attribute name="ISAT" value="8.3A"/>
<attribute name="ISAT2" value="5.05A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437358100 "/>
<attribute name="RDC-MAX" value="15.9mOhm"/>
<attribute name="SIZE" value=" 8040 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_7030" prefix="L">
<description>&lt;b&gt;WE-LHMI SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Compact Design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability
&lt;br&gt;Handles high transient current spikes
&lt;br&gt;No acoustic noise and no leakage field
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-LHMI Sizes 4020HT 520HT 7030HT 7050HT
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;Designed to avoid thermal aging degradation

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC Converters for high current power supplies
&lt;br&gt;DC/DC Converters for Field Programmable Gate Arrays (FPGA)
&lt;br&gt;POL Converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/ graphic cards
&lt;br&gt;CPU/ RAM
&lt;br&gt;Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14803v209%20Family_WE-LHMI_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-LHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-03-12&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-LHMI_7030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373460022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373460022?ae"/>
<attribute name="FRES" value="149MHz"/>
<attribute name="IR" value="23A"/>
<attribute name="ISAT" value="29.9A"/>
<attribute name="ISAT2" value="23A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373460022 "/>
<attribute name="RDC-MAX" value="54.3mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744373460033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373460033?ae"/>
<attribute name="FRES" value="124MHz"/>
<attribute name="IR" value="17.8A"/>
<attribute name="ISAT" value="27.1A"/>
<attribute name="ISAT2" value="17.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373460033 "/>
<attribute name="RDC-MAX" value="47mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744373460047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373460047?ae"/>
<attribute name="FRES" value="91MHz"/>
<attribute name="IR" value="16.6A"/>
<attribute name="ISAT" value="21.4A"/>
<attribute name="ISAT2" value="16.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373460047 "/>
<attribute name="RDC-MAX" value="37.8mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_744373460068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373460068?ae"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="IR" value="15.1A"/>
<attribute name="ISAT" value="15.9A"/>
<attribute name="ISAT2" value="15.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373460068 "/>
<attribute name="RDC-MAX" value="31.6mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_744373460082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744373460082?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="12.7A"/>
<attribute name="ISAT" value="15A"/>
<attribute name="ISAT2" value="12.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744373460082 "/>
<attribute name="RDC-MAX" value="31.9mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_74437346010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437346010?ae"/>
<attribute name="FRES" value="54MHz"/>
<attribute name="IR" value="11.4A"/>
<attribute name="ISAT" value="14.7A"/>
<attribute name="ISAT2" value="11.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437346010 "/>
<attribute name="RDC-MAX" value="29mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74437346015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437346015?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="9.1A"/>
<attribute name="ISAT" value="11.2A"/>
<attribute name="ISAT2" value="9.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437346015 "/>
<attribute name="RDC-MAX" value="27.6mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74437346018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437346018?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="8.8A"/>
<attribute name="ISAT" value="10.2A"/>
<attribute name="ISAT2" value="8.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437346018 "/>
<attribute name="RDC-MAX" value="21.4mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_74437346022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437346022?ae"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="IR" value="7.7A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="ISAT2" value="7.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437346022 "/>
<attribute name="RDC-MAX" value="19.1mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74437346025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437346025?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="7.3A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="ISAT2" value="7.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437346025 "/>
<attribute name="RDC-MAX" value="17.3mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="2.5uH"/>
</technology>
<technology name="_74437346033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437346033?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="8.4A"/>
<attribute name="ISAT2" value="6.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437346033 "/>
<attribute name="RDC-MAX" value="16.6mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74437346047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437346047?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="5.35A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="ISAT2" value="5.35A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437346047 "/>
<attribute name="RDC-MAX" value="15.5mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74437346056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437346056?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="5.9A"/>
<attribute name="ISAT2" value="5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437346056 "/>
<attribute name="RDC-MAX" value="12.1mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74437346068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437346068?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="4.45A"/>
<attribute name="ISAT" value="5.45A"/>
<attribute name="ISAT2" value="4.45A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437346068 "/>
<attribute name="RDC-MAX" value="10.6mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74437346082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437346082?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="4.1A"/>
<attribute name="ISAT" value="5.1A"/>
<attribute name="ISAT2" value="4.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437346082 "/>
<attribute name="RDC-MAX" value="10.1mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74437346100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437346100?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="3.75A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="ISAT2" value="3.75A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437346100 "/>
<attribute name="RDC-MAX" value="9.8mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74437346150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437346150?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="3.15A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="ISAT2" value="3.15A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437346150 "/>
<attribute name="RDC-MAX" value="6.1mOhm"/>
<attribute name="SIZE" value=" 7050 "/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74437346220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437346220?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="2.75A"/>
<attribute name="ISAT2" value="2.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74437346220 "/>
<attribute name="RDC-MAX" value="5.95mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
