<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-HCF&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-05-15&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-HCF_2920_ROUND">
<description>&lt;b&gt;WE-HCF SMD High Current Cube Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 2920, SMT, 3pins</description>
</package>
<package name="WE-HCF_2818B">
<description>&lt;b&gt;WE-HCF SMD High Current Cube Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 2818, SMT, 3pins</description>
</package>
<package name="WE-HCF_2013">
<description>&lt;b&gt;WE-HCF SMD High Current Cube Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 2013, SMT, 3pins</description>
</package>
<package name="WE-HCF_2010">
<description>&lt;b&gt;WE-HCF SMD High Current Cube Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 2010, SMT, 3pins</description>
</package>
<package name="WE-HCF_2818">
<description>&lt;b&gt;WE-HCF SMD High Current Cube Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 2818, SMT, 3pins</description>
</package>
<package name="WE-HCF_2815">
<description>&lt;b&gt;WE-HCF SMD High Current Cube Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 2815, SMT, 3pins</description>
</package>
<package name="WE-HCF_2920_LITZ">
<description>&lt;b&gt;WE-HCF SMD High Current Cube Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 2920, SMT, 3pins</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="L_GAP_SHIELD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-HCF_2010" prefix="L">
<description>&lt;b&gt;WE-HCF SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Saturation current up to 125 A
&lt;br&gt;Flat, round and litz wire version to optimize the DC &amp; AC losses
&lt;br&gt;Inductance values ranging from 0.7 µH to 680 µH
&lt;br&gt;Low core losses (MnZn)
&lt;br&gt;Magnetically shielded
&lt;br&gt;Litz and round wire: base for SMD mount and coplanarity
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;&lt;/b&gt;Storage inductor for high efficiency DC/DC converters with high ripple currents
&lt;br&gt;CRM, CCM &amp; DCM PFC Stages
&lt;br&gt;Resonant SMPS
&lt;br&gt;Filter for audio applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-HCF"&gt;www.we-online.com/en/components/products/WE-HCF&lt;/a&gt;&lt;p&gt;


Updated by Ella,Wu 2023-05-15&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_SHIELD"/>
</gates>
<devices>
<device name="" package="WE-HCF_2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="_7443642010100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443642010100?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="IR" value="50.3A"/>
<attribute name="ISAT" value="49A"/>
<attribute name="PART-NUMBER" value=" 7443642010100 "/>
<attribute name="RDC" value="0.92mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7443642010120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443642010120?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="50.3A"/>
<attribute name="ISAT" value="42.5A"/>
<attribute name="PART-NUMBER" value=" 7443642010120 "/>
<attribute name="RDC" value="0.92mOhm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_7443642010200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443642010200?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="50.3A"/>
<attribute name="ISAT" value="25.5A"/>
<attribute name="PART-NUMBER" value=" 7443642010200 "/>
<attribute name="RDC" value="0.92mOhm"/>
<attribute name="VALUE" value="2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCF_2818B" prefix="L">
<description>&lt;b&gt;WE-HCF SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Saturation current up to 125 A
&lt;br&gt;Flat, round and litz wire version to optimize the DC &amp; AC losses
&lt;br&gt;Inductance values ranging from 0.7 µH to 680 µH
&lt;br&gt;Low core losses (MnZn)
&lt;br&gt;Magnetically shielded
&lt;br&gt;Litz and round wire: base for SMD mount and coplanarity
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;&lt;/b&gt;Storage inductor for high efficiency DC/DC converters with high ripple currents
&lt;br&gt;CRM, CCM &amp; DCM PFC Stages
&lt;br&gt;Resonant SMPS
&lt;br&gt;Filter for audio applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-HCF"&gt;www.we-online.com/en/components/products/WE-HCF&lt;/a&gt;&lt;p&gt;


Updated by Ella,Wu 2023-05-15&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCF_2818B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443640100B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443640100B?ae"/>
<attribute name="FRES" value="53.6MHz"/>
<attribute name="IR" value="86.2A"/>
<attribute name="ISAT" value="122A"/>
<attribute name="PART-NUMBER" value="7443640100B"/>
<attribute name="RDC" value="0.48mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7443640150B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443640150B?ae"/>
<attribute name="FRES" value="37.6MHz"/>
<attribute name="IR" value="86.2A"/>
<attribute name="ISAT" value="85A"/>
<attribute name="PART-NUMBER" value="7443640150B"/>
<attribute name="RDC" value="0.48mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7443640330B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443640330B?ae"/>
<attribute name="FRES" value="28.2MHz"/>
<attribute name="IR" value="59.2A"/>
<attribute name="ISAT" value="61.35A"/>
<attribute name="PART-NUMBER" value="7443640330B"/>
<attribute name="RDC" value="0.97mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7443640470B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443640470B?ae"/>
<attribute name="FRES" value="22.6MHz"/>
<attribute name="IR" value="59.2A"/>
<attribute name="ISAT" value="43.85A"/>
<attribute name="PART-NUMBER" value="7443640470B"/>
<attribute name="RDC" value="0.97mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7443640680B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443640680B?ae"/>
<attribute name="FRES" value="18.8MHz"/>
<attribute name="IR" value="59.2A"/>
<attribute name="ISAT" value="31.9A"/>
<attribute name="PART-NUMBER" value="7443640680B"/>
<attribute name="RDC" value="0.97mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7443641000B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443641000B?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="59.2A"/>
<attribute name="ISAT" value="22.9A"/>
<attribute name="PART-NUMBER" value="7443641000B"/>
<attribute name="RDC" value="0.97mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCF_2920_ROUND" prefix="L">
<description>&lt;b&gt;WE-HCF SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Saturation current up to 125 A
&lt;br&gt;Flat, round and litz wire version to optimize the DC &amp; AC losses
&lt;br&gt;Inductance values ranging from 0.7 µH to 680 µH
&lt;br&gt;Low core losses (MnZn)
&lt;br&gt;Magnetically shielded
&lt;br&gt;Litz and round wire: base for SMD mount and coplanarity
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;&lt;/b&gt;Storage inductor for high efficiency DC/DC converters with high ripple currents
&lt;br&gt;CRM, CCM &amp; DCM PFC Stages
&lt;br&gt;Resonant SMPS
&lt;br&gt;Filter for audio applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-HCF"&gt;www.we-online.com/en/components/products/WE-HCF&lt;/a&gt;&lt;p&gt;


Updated by Ella,Wu 2023-05-15&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCF_2920_ROUND">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74437529203101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437529203101?ae"/>
<attribute name="FRES" value="4.3MHz"/>
<attribute name="IR" value="10.5A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="PART-NUMBER" value=" 74437529203101 "/>
<attribute name="RDC" value="25.19mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74437529203151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437529203151?ae"/>
<attribute name="FRES" value="3.2MHz"/>
<attribute name="IR" value="9A"/>
<attribute name="ISAT" value="5.8A"/>
<attribute name="PART-NUMBER" value=" 74437529203151 "/>
<attribute name="RDC" value="33.66mOhm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_74437529203220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437529203220?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="24.05A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="PART-NUMBER" value=" 74437529203220 "/>
<attribute name="RDC" value="5.39mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74437529203221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437529203221?ae"/>
<attribute name="FRES" value="2.8MHz"/>
<attribute name="IR" value="8.15A"/>
<attribute name="ISAT" value="4.1A"/>
<attribute name="PART-NUMBER" value=" 74437529203221 "/>
<attribute name="RDC" value="40.1mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_74437529203330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437529203330?ae"/>
<attribute name="FRES" value="7.1MHz"/>
<attribute name="IR" value="20.05A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="PART-NUMBER" value=" 74437529203330 "/>
<attribute name="RDC" value="7.59mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74437529203331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437529203331?ae"/>
<attribute name="FRES" value="2.4MHz"/>
<attribute name="IR" value="5.75A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="PART-NUMBER" value=" 74437529203331 "/>
<attribute name="RDC" value="77.5mOhm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_74437529203470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437529203470?ae"/>
<attribute name="FRES" value="6.7MHz"/>
<attribute name="IR" value="17.5A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="PART-NUMBER" value=" 74437529203470 "/>
<attribute name="RDC" value="9.68mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74437529203471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437529203471?ae"/>
<attribute name="FRES" value="1.7MHz"/>
<attribute name="IR" value="5.2A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="PART-NUMBER" value=" 74437529203471 "/>
<attribute name="RDC" value="91.8mOhm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_74437529203680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437529203680?ae"/>
<attribute name="FRES" value="5.7MHz"/>
<attribute name="IR" value="16A"/>
<attribute name="ISAT" value="7.2A"/>
<attribute name="PART-NUMBER" value=" 74437529203680 "/>
<attribute name="RDC" value="11.33mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_74437529203681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437529203681?ae"/>
<attribute name="FRES" value="1.1MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="PART-NUMBER" value=" 74437529203681 "/>
<attribute name="RDC" value="130.13mOhm"/>
<attribute name="VALUE" value="680uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCF_2013" prefix="L">
<description>&lt;b&gt;WE-HCF SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Saturation current up to 125 A
&lt;br&gt;Flat, round and litz wire version to optimize the DC &amp; AC losses
&lt;br&gt;Inductance values ranging from 0.7 µH to 680 µH
&lt;br&gt;Low core losses (MnZn)
&lt;br&gt;Magnetically shielded
&lt;br&gt;Litz and round wire: base for SMD mount and coplanarity
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;&lt;/b&gt;Storage inductor for high efficiency DC/DC converters with high ripple currents
&lt;br&gt;CRM, CCM &amp; DCM PFC Stages
&lt;br&gt;Resonant SMPS
&lt;br&gt;Filter for audio applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-HCF"&gt;www.we-online.com/en/components/products/WE-HCF&lt;/a&gt;&lt;p&gt;


Updated by Ella,Wu 2023-05-15&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCF_2013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443630070">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443630070?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="54.7A"/>
<attribute name="ISAT" value="63A"/>
<attribute name="PART-NUMBER" value=" 7443630070 "/>
<attribute name="RDC" value="0.91mOhm"/>
<attribute name="VALUE" value="0.7uH"/>
</technology>
<technology name="_7443630140">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443630140?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="IR" value="47.1A"/>
<attribute name="ISAT" value="55A"/>
<attribute name="PART-NUMBER" value=" 7443630140 "/>
<attribute name="RDC" value="1.19mOhm"/>
<attribute name="VALUE" value="1.4uH"/>
</technology>
<technology name="_7443630220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443630220?ae"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="IR" value="39.5A"/>
<attribute name="ISAT" value="47A"/>
<attribute name="PART-NUMBER" value=" 7443630220 "/>
<attribute name="RDC" value="1.65mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7443630310">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443630310?ae"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="IR" value="33.15A"/>
<attribute name="ISAT" value="41A"/>
<attribute name="PART-NUMBER" value=" 7443630310 "/>
<attribute name="RDC" value="2.3mOhm"/>
<attribute name="VALUE" value="3.1uH"/>
</technology>
<technology name="_7443630420">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443630420?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="27A"/>
<attribute name="ISAT" value="34A"/>
<attribute name="PART-NUMBER" value=" 7443630420 "/>
<attribute name="RDC" value="3.34mOhm"/>
<attribute name="VALUE" value="4.2uH"/>
</technology>
<technology name="_7443630550">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443630550?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="23.35A"/>
<attribute name="ISAT" value="30A"/>
<attribute name="PART-NUMBER" value=" 7443630550 "/>
<attribute name="RDC" value="4.4mOhm"/>
<attribute name="VALUE" value="5.5uH"/>
</technology>
<technology name="_7443630700">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443630700?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="19.5A"/>
<attribute name="ISAT" value="27A"/>
<attribute name="PART-NUMBER" value=" 7443630700 "/>
<attribute name="RDC" value="6.17mOhm"/>
<attribute name="VALUE" value="7uH"/>
</technology>
<technology name="_7443630860">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443630860?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="17.1A"/>
<attribute name="ISAT" value="23.5A"/>
<attribute name="PART-NUMBER" value=" 7443630860 "/>
<attribute name="RDC" value="7.91mOhm"/>
<attribute name="VALUE" value="8.6uH"/>
</technology>
<technology name="_7443631000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443631000?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="16.15A"/>
<attribute name="ISAT" value="22A"/>
<attribute name="PART-NUMBER" value=" 7443631000 "/>
<attribute name="RDC" value="8.76mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7443631500">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443631500?ae"/>
<attribute name="FRES" value="12.8MHz"/>
<attribute name="IR" value="15.4A"/>
<attribute name="ISAT" value="19A"/>
<attribute name="PART-NUMBER" value=" 7443631500 "/>
<attribute name="RDC" value="9.57mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7443632200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443632200?ae"/>
<attribute name="FRES" value="12.5MHz"/>
<attribute name="IR" value="13.8A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="PART-NUMBER" value=" 7443632200 "/>
<attribute name="RDC" value="11.72mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7443633300">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443633300?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="13.3A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="PART-NUMBER" value=" 7443633300 "/>
<attribute name="RDC" value="12.54mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_7443634700">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443634700?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="12.8A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="PART-NUMBER" value=" 7443634700 "/>
<attribute name="RDC" value="13.42mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCF_2818" prefix="L">
<description>&lt;b&gt;WE-HCF SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Saturation current up to 125 A
&lt;br&gt;Flat, round and litz wire version to optimize the DC &amp; AC losses
&lt;br&gt;Inductance values ranging from 0.7 µH to 680 µH
&lt;br&gt;Low core losses (MnZn)
&lt;br&gt;Magnetically shielded
&lt;br&gt;Litz and round wire: base for SMD mount and coplanarity
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;&lt;/b&gt;Storage inductor for high efficiency DC/DC converters with high ripple currents
&lt;br&gt;CRM, CCM &amp; DCM PFC Stages
&lt;br&gt;Resonant SMPS
&lt;br&gt;Filter for audio applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-HCF"&gt;www.we-online.com/en/components/products/WE-HCF&lt;/a&gt;&lt;p&gt;


Updated by Ella,Wu 2023-05-15&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCF_2818">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443640330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443640330?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="34.95A"/>
<attribute name="ISAT" value="89.8A"/>
<attribute name="PART-NUMBER" value=" 7443640330 "/>
<attribute name="RDC" value="2.64mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7443640470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443640470?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="34.95A"/>
<attribute name="ISAT" value="70A"/>
<attribute name="PART-NUMBER" value=" 7443640470 "/>
<attribute name="RDC" value="2.64mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7443640680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443640680?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="34.95A"/>
<attribute name="ISAT" value="49.8A"/>
<attribute name="PART-NUMBER" value=" 7443640680 "/>
<attribute name="RDC" value="2.64mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7443641000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443641000?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="34.95A"/>
<attribute name="ISAT" value="32.6A"/>
<attribute name="PART-NUMBER" value=" 7443641000 "/>
<attribute name="RDC" value="2.64mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7443641500">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443641500?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="34.95A"/>
<attribute name="ISAT" value="22A"/>
<attribute name="PART-NUMBER" value=" 7443641500 "/>
<attribute name="RDC" value="2.64mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7443642200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443642200?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="34.95A"/>
<attribute name="ISAT" value="15.5A"/>
<attribute name="PART-NUMBER" value=" 7443642200 "/>
<attribute name="RDC" value="2.64mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7443643300">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443643300?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="34.95A"/>
<attribute name="ISAT" value="10.5A"/>
<attribute name="PART-NUMBER" value=" 7443643300 "/>
<attribute name="RDC" value="2.64mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCF_2815" prefix="L">
<description>&lt;b&gt;WE-HCF SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Saturation current up to 125 A
&lt;br&gt;Flat, round and litz wire version to optimize the DC &amp; AC losses
&lt;br&gt;Inductance values ranging from 0.7 µH to 680 µH
&lt;br&gt;Low core losses (MnZn)
&lt;br&gt;Magnetically shielded
&lt;br&gt;Litz and round wire: base for SMD mount and coplanarity
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;&lt;/b&gt;Storage inductor for high efficiency DC/DC converters with high ripple currents
&lt;br&gt;CRM, CCM &amp; DCM PFC Stages
&lt;br&gt;Resonant SMPS
&lt;br&gt;Filter for audio applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-HCF"&gt;www.we-online.com/en/components/products/WE-HCF&lt;/a&gt;&lt;p&gt;


Updated by Ella,Wu 2023-05-15&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCF_2815">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74436410150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74436410150?ae"/>
<attribute name="FRES" value="43.24MHz"/>
<attribute name="IR" value="44A"/>
<attribute name="ISAT" value="110A"/>
<attribute name="PART-NUMBER" value=" 74436410150 "/>
<attribute name="RDC" value="1.44mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74436410220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74436410220?ae"/>
<attribute name="FRES" value="32.8MHz"/>
<attribute name="IR" value="44A"/>
<attribute name="ISAT" value="85A"/>
<attribute name="PART-NUMBER" value=" 74436410220 "/>
<attribute name="RDC" value="1.44mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74436410330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74436410330?ae"/>
<attribute name="FRES" value="26.44MHz"/>
<attribute name="IR" value="44A"/>
<attribute name="ISAT" value="57A"/>
<attribute name="PART-NUMBER" value=" 74436410330 "/>
<attribute name="RDC" value="1.44mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74436410470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74436410470?ae"/>
<attribute name="FRES" value="21.56MHz"/>
<attribute name="IR" value="44A"/>
<attribute name="ISAT" value="44A"/>
<attribute name="PART-NUMBER" value=" 74436410470 "/>
<attribute name="RDC" value="1.44mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74436410680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74436410680?ae"/>
<attribute name="FRES" value="17.03MHz"/>
<attribute name="IR" value="44A"/>
<attribute name="ISAT" value="30A"/>
<attribute name="PART-NUMBER" value=" 74436410680 "/>
<attribute name="RDC" value="1.44mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74436411000">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74436411000?ae"/>
<attribute name="FRES" value="13.55MHz"/>
<attribute name="IR" value="44A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="PART-NUMBER" value=" 74436411000 "/>
<attribute name="RDC" value="1.44mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74436411500">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74436411500?ae"/>
<attribute name="FRES" value="10.73MHz"/>
<attribute name="IR" value="44A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="PART-NUMBER" value=" 74436411500 "/>
<attribute name="RDC" value="1.44mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74436412200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74436412200?ae"/>
<attribute name="FRES" value="8.06MHz"/>
<attribute name="IR" value="44A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="PART-NUMBER" value=" 74436412200 "/>
<attribute name="RDC" value="1.44mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74436413300">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74436413300?ae"/>
<attribute name="FRES" value="6.29MHz"/>
<attribute name="IR" value="44A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="PART-NUMBER" value=" 74436413300 "/>
<attribute name="RDC" value="1.44mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCF_2920_LITZ" prefix="L">
<description>&lt;b&gt;WE-HCF SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Saturation current up to 125 A
&lt;br&gt;Flat, round and litz wire version to optimize the DC &amp; AC losses
&lt;br&gt;Inductance values ranging from 0.7 µH to 680 µH
&lt;br&gt;Low core losses (MnZn)
&lt;br&gt;Magnetically shielded
&lt;br&gt;Litz and round wire: base for SMD mount and coplanarity
&lt;br&gt;Operating temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;&lt;/b&gt;Storage inductor for high efficiency DC/DC converters with high ripple currents
&lt;br&gt;CRM, CCM &amp; DCM PFC Stages
&lt;br&gt;Resonant SMPS
&lt;br&gt;Filter for audio applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o107965v209%20Family_WE-HCF_2018_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-HCF"&gt;www.we-online.com/en/components/products/WE-HCF&lt;/a&gt;&lt;p&gt;


Updated by Ella,Wu 2023-05-15&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCF_2920_LITZ">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74437429203101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437429203101?ae"/>
<attribute name="FRES" value="4.3MHz"/>
<attribute name="IR" value="8.2A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="PART-NUMBER" value=" 74437429203101 "/>
<attribute name="RDC" value="39.49mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74437429203151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437429203151?ae"/>
<attribute name="FRES" value="3.8MHz"/>
<attribute name="IR" value="7.9A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="PART-NUMBER" value=" 74437429203151 "/>
<attribute name="RDC" value="42.74mOhm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_74437429203330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437429203330?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="13.25A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="PART-NUMBER" value=" 74437429203330 "/>
<attribute name="RDC" value="16.83mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74437429203470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437429203470?ae"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="IR" value="11.65A"/>
<attribute name="ISAT" value="7.6A"/>
<attribute name="PART-NUMBER" value=" 74437429203470 "/>
<attribute name="RDC" value="21.23mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74437429203680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74437429203680?ae"/>
<attribute name="FRES" value="5.3MHz"/>
<attribute name="IR" value="10.8A"/>
<attribute name="ISAT" value="6.4A"/>
<attribute name="PART-NUMBER" value=" 74437429203680 "/>
<attribute name="RDC" value="24.42mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
