<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Film Capacitors - Interference Suppression - WCAP-FTX2&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-10-30&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-FTX2_P7.5L10W6H12">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 7.5mm, Standard, THT
&lt;BR&gt;7.5X10X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P7.5L11W6H10">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 7.5mm, Standard, THT
&lt;BR&gt;7.5X11X6X10(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W5H11_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W10H16_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X10X16(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W8.5H14.5_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X8.5X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W6H12_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W10H17.5_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X10X17.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W7.5H13.5_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X7.5X13.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P7.5L10W6H12_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 7.5mm, CS, THT
&lt;BR&gt;7.5X10X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W6H11.5_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X6X11.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W8H14_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X8X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W7.5H14.5_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X7.55X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W9H15_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X9X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W13H22_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, CS, THT
&lt;BR&gt;27.5X31X13X22(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W8H17">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, Standard, THT
&lt;BR&gt;27.5X31X8X17(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W10H16">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X10X16(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W10.5H20_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, CS, THT
&lt;BR&gt;27.5X31X10.5X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P7.5L11W6H10_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 7.5mm, CS, THT
&lt;BR&gt;7.5X11X6X10(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W15.5H29_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, CS, THT
&lt;BR&gt;27.5X31X15.5X29(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W13H22">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, Standard, THT
&lt;BR&gt;27.5X31X13X22(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W5H11">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W15.5H29">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, Standard, THT
&lt;BR&gt;27.5X31X15.5X29(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W6H12">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W19H32.5_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, CS, THT
&lt;BR&gt;27.5X31X19X32.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W6H11.5">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X6X11.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W7.5H13.5">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X7.5X13.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W10.5H20">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, Standard, THT
&lt;BR&gt;27.5X31X10.5X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W8H14">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X8X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W7.5H14.5">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X7.55X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W8.5H14.5">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X8.5X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P37.5L41.5W22.5H35.5">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 37.5mm, Standard, THT
&lt;BR&gt;37.5X41.5X22.5X35.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W4.5H9.5">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X4.5X9.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W9H15">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X9X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W5H11">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W7H12">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X7X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W5H10">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X5X10(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W7H13">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X7X13(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W5H10_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, CS, THT
&lt;BR&gt;10X13X5X10(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W5H11_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, CS, THT
&lt;BR&gt;10X13X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W4.5H9.5_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, CS, THT
&lt;BR&gt;10X13X4.5X9.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W7H12_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, CS, THT
&lt;BR&gt;10X13X7X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W8H14_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, CS, THT
&lt;BR&gt;10X13X8X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W7H13_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, CS, THT
&lt;BR&gt;10X13X7X13(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W9H18_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X9X18(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W6H15_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X6X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W7.5H16.5_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X7.5X16.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W7.5H15_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X7.5X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W15H25_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X15X25(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W8H14">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X8X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W11H20_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X11X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W6H12_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W10H21_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X10X21(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W7H14.5_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X7X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W6H11.5">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, Standard, THT
&lt;BR&gt;12.5X15X6X11.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W10H16">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, Standard, THT
&lt;BR&gt;12.5X15X10X16(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W10H21">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X10X21(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P37.5L41.5W22.5H35.5_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 37.5mm, CS, THT
&lt;BR&gt;37.5X41.5X22.5X35.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W8.5H14">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, Standard, THT
&lt;BR&gt;12.5X15X8.5X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W7H12.5">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, Standard, THT
&lt;BR&gt;12.5X15X7X12.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W11H20">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X11X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W8.5H14_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, CS, THT
&lt;BR&gt;12.5X15X8.5X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W15H25">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X15X25(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W6H11.5_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, CS, THT
&lt;BR&gt;12.5X15X6X11.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W7H12.5_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, CS, THT
&lt;BR&gt;12.5X15X7X12.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W10H16_CS">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, CS, THT
&lt;BR&gt;12.5X15X10X16(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W7.5H15">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X7.5X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W7.5H16.5">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X7.5X16.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W6H15">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X6X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W7H14.5">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X7X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W9H18">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X9X18(PitchXLXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-FTX2_P7.5" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L10W6H12" package="WCAP-FTX2_P7.5L10W6H12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324022017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324022017?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="PART-NUMBER" value=" 890324022017 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L11W6H10" package="WCAP-FTX2_P7.5L11W6H10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324022007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324022007?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value=" 890324022007 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P15_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L18W10H16" package="WCAP-FTX2_P15L18W10H16_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025045CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025045CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025045CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L18W5H11" package="WCAP-FTX2_P15L18W5H11_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025004CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025004CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="27 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324025006CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025006CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025006CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="33 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324025007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025007CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025007CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="39 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324025009CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025009CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025009CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324025011CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025011CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025011CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="250V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="56 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W6H11.5" package="WCAP-FTX2_P15L18W6H11.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025027CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025027CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025027CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="180V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L18W6H12" package="WCAP-FTX2_P15L18W6H12_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025013CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025013CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025013CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="270V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890324025015CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025015CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025015CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="290V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="82 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890324025017CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025017CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025017CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890324025022CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025022CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025022CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="210V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890324025025CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025025CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025025CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="180 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L18W7.5H13.5" package="WCAP-FTX2_P15L18W7.5H13.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025020CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025020CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025020CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="120 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W7.5H14.5" package="WCAP-FTX2_P15L18W7.5H14.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025031CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025031CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025031CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="250V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="270 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W8.5H14.5" package="WCAP-FTX2_P15L18W8.5H14.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025034CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025034CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025034CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="260V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W8H14" package="WCAP-FTX2_P15L18W8H14_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025039CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025039CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025039CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
</technologies>
</device>
<device name="_L18W9H15" package="WCAP-FTX2_P15L18W9H15_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025043CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025043CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025043CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="17.86 GOhm"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
<device name="_L18W10H17.5" package="WCAP-FTX2_P15L18W10H17.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025047CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025047CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="17.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890324025047CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="12.20 GOhm"/>
<attribute name="VALUE" value="820 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P7.5_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L10W6H12" package="WCAP-FTX2_P7.5L10W6H12_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324022017CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324022017CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="PART-NUMBER" value="890324022017CS"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L11W6H10" package="WCAP-FTX2_P7.5L11W6H10_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324022007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324022007CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="890324022007CS"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P27.5_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L31W10.5H20" package="WCAP-FTX2_P27.5L31W10.5H20_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027006CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324027006CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890324027006CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
</technologies>
</device>
<device name="_L31W13H22" package="WCAP-FTX2_P27.5L31W13H22_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027012CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324027012CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="22mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890324027012CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="8.33 GOhm"/>
<attribute name="VALUE" value="1.2 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="13mm"/>
</technology>
</technologies>
</device>
<device name="_L31W15.5H29" package="WCAP-FTX2_P27.5L31W15.5H29_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027025CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324027025CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="29mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890324027025CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="3.03 GOhm"/>
<attribute name="VALUE" value="3.3 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="15.5mm"/>
</technology>
</technologies>
</device>
<device name="_L31W19H32.5" package="WCAP-FTX2_P27.5L31W19H32.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027030CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324027030CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="32.5mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890324027030CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="2.13 GOhm"/>
<attribute name="VALUE" value="4.7 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="19mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P27.5" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L31W10.5H20" package="WCAP-FTX2_P27.5L31W10.5H20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324027006?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value=" 890324027006 "/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="VALUE" value="0.68u"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
</technologies>
</device>
<device name="_L31W13H22" package="WCAP-FTX2_P27.5L31W13H22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324027012?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="22mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value=" 890324027012 "/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="8.33 GOhm"/>
<attribute name="VALUE" value="1.2 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="13mm"/>
</technology>
</technologies>
</device>
<device name="_L31W15.5H29" package="WCAP-FTX2_P27.5L31W15.5H29">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324027025?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="29mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value=" 890324027025 "/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="3.03 GOhm"/>
<attribute name="VALUE" value="3.3 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="15.5mm"/>
</technology>
</technologies>
</device>
<device name="_L31W8H17" package="WCAP-FTX2_P27.5L31W8H17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324027009?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value=" 890324027009 "/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="100V/us"/>
<attribute name="RISO" value="10.00 GOhm"/>
<attribute name="VALUE" value="1 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P37.5" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L41.5W22.5H35.5" package="WCAP-FTX2_P37.5L41.5W22.5H35.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324028008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324028008?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="35.5mm"/>
<attribute name="LENGTH" value="41.5mm"/>
<attribute name="PART-NUMBER" value=" 890324028008 "/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="110V/us"/>
<attribute name="RISO" value="1.47 GOhm"/>
<attribute name="VALUE" value="6.8 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="22.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P15" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L18W10H16" package="WCAP-FTX2_P15L18W10H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025045">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025045?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025045 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L18W5H11" package="WCAP-FTX2_P15L18W5H11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025004?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025004 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="27 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324025006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025006?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025006 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="33 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324025007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025007?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025007 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="39 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324025009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025009?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025009 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324025011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025011?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025011 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="250V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="56 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W6H11.5" package="WCAP-FTX2_P15L18W6H11.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025027?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025027 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="180V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L18W6H12" package="WCAP-FTX2_P15L18W6H12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025013?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025013 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="270V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890324025015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025015?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025015 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="290V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="82 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890324025017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025017?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025017 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890324025022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025022?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025022 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="210V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890324025025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025025?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025025 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="180 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L18W7.5H13.5" package="WCAP-FTX2_P15L18W7.5H13.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025020?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025020 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="120 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W7.5H14.5" package="WCAP-FTX2_P15L18W7.5H14.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025031?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025031 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="250V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="270 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W8.5H14.5" package="WCAP-FTX2_P15L18W8.5H14.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025034">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025034?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025034 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="260V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W8H14" package="WCAP-FTX2_P15L18W8H14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025039?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025039 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
</technologies>
</device>
<device name="_L18W9H15" package="WCAP-FTX2_P15L18W9H15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025043">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324025043?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890324025043 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="17.86 GOhm"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P10_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L13W4.5H9.5" package="WCAP-FTX2_P10L13W4.5H9.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023008CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023008CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023008CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
<technology name="_890324023011CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023011CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023011CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
<technology name="_890324023015CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023015CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023015CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
</technologies>
</device>
<device name="_L13W5H10" package="WCAP-FTX2_P10L13W5H10_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023002CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023002CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023002CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="600V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="5.6 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324023003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023003CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023003CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="6.8 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324023004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023004CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023004CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="8.2 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324023017CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023017CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023017CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="56 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L13W5H11" package="WCAP-FTX2_P10L13W5H11_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023006CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023006CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023006CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324023007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023007CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023007CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="12 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324023010CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023010CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023010CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="18 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L13W7H12" package="WCAP-FTX2_P10L13W7H12_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023025CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023025CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023025CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L13W7H13" package="WCAP-FTX2_P10L13W7H13_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023019CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023019CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023019CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_890324023021CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023021CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023021CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="82 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_890324023023CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023023CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023023CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_890324023024CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023024CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023024CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="120 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L13W8H14" package="WCAP-FTX2_P10L13W8H14_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023028CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023028CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890324023028CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P10" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L13W4.5H9.5" package="WCAP-FTX2_P10L13W4.5H9.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023008?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023008 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
<technology name="_890324023011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023011?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023011 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
<technology name="_890324023015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023015?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023015 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
</technologies>
</device>
<device name="_L13W5H10" package="WCAP-FTX2_P10L13W5H10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023002?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023002 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="600V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="5.6 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324023003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023003?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023003 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="6.8 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324023004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023004?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023004 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="8.2 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324023017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023017?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023017 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="56 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L13W5H11" package="WCAP-FTX2_P10L13W5H11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023006?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023006 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324023007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023007?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023007 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="12 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890324023010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023010?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023010 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="18 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L13W7H12" package="WCAP-FTX2_P10L13W7H12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023025?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023025 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L13W7H13" package="WCAP-FTX2_P10L13W7H13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023019?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023019 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_890324023021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023021?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023021 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="82 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_890324023023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023023?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023023 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_890324023024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023024?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023024 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="120 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L13W8H14" package="WCAP-FTX2_P10L13W8H14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324023028?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890324023028 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P22.5_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L26W10H21" package="WCAP-FTX2_P22.5L26W10H21_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026030CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026030CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="21mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890324026030CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="6.67 GOhm"/>
<attribute name="VALUE" value="1.5 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L26W11H20" package="WCAP-FTX2_P22.5L26W11H20_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026027CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026027CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890324026027CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="10.00 GOhm"/>
<attribute name="VALUE" value="1 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
</technologies>
</device>
<device name="_L26W15H25" package="WCAP-FTX2_P22.5L26W15H25_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026034CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026034CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="25mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890324026034CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="4.55 GOhm"/>
<attribute name="VALUE" value="2.2 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_L26W6H15" package="WCAP-FTX2_P22.5L26W6H15_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026003CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890324026003CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L26W7.5H15" package="WCAP-FTX2_P22.5L26W7.5H15_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026020CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026020CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890324026020CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L26W7.5H16.5" package="WCAP-FTX2_P22.5L26W7.5H16.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026018CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026018CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="16.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890324026018CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="17.86 GOhm"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L26W9H18" package="WCAP-FTX2_P22.5L26W9H18_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026024CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026024CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="18mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890324026024CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="12.20 GOhm"/>
<attribute name="VALUE" value="820 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
<device name="_L26W6H12" package="WCAP-FTX2_P22.5L26W6H12_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026007CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890324026007CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L26W7H14.5" package="WCAP-FTX2_P22.5L26W7H14.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026014CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026014CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890324026014CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="VALUE" value="0.47 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P37.5_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L41.5W22.5H35.5" package="WCAP-FTX2_P37.5L41.5W22.5H35.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324028008CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324028008CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="35.5mm"/>
<attribute name="LENGTH" value="41.5mm"/>
<attribute name="PART-NUMBER" value="890324028008CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="110V/us"/>
<attribute name="RISO" value="1.47 GOhm"/>
<attribute name="VALUE" value="6.8 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="22.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P12.5" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L15W10H16" package="WCAP-FTX2_P12.5L15W10H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324024005?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value=" 890324024005 "/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="280V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L15W6H11.5" package="WCAP-FTX2_P12.5L15W6H11.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324024001?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value=" 890324024001 "/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="210V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L15W7H12.5" package="WCAP-FTX2_P12.5L15W7H12.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324024002?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12.5mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value=" 890324024002 "/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="240V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L15W8.5H14" package="WCAP-FTX2_P12.5L15W8.5H14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324024003?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value=" 890324024003 "/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="260V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P12.5_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L15W10H16" package="WCAP-FTX2_P12.5L15W10H16_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324024005CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value="890324024005CS"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="280V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L15W6H11.5" package="WCAP-FTX2_P12.5L15W6H11.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324024001CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value="890324024001CS"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="210V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L15W7H12.5" package="WCAP-FTX2_P12.5L15W7H12.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024002CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324024002CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12.5mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value="890324024002CS"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="240V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L15W8.5H14" package="WCAP-FTX2_P12.5L15W8.5H14_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324024003CS?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value="890324024003CS"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="260V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P22.5" prefix="C">
<description>&lt;b&gt;WCAP-FTX2 Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polypropylene
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF
&lt;BR&gt;Capacitance tolerance: ±10 %
&lt;BR&gt;Voltage range (UR): 275 V(AC)
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt;Filter
&lt;BR&gt;Interference suppression
&lt;BR&gt;e.g. EMI filter for power supplies


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14733v209%20family-WCAP-FTX2-10x13x5x11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;


           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTX2/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTX2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-30&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L26W10H21" package="WCAP-FTX2_P22.5L26W10H21">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026014?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890324026014 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="VALUE" value="0.47 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_890324026030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026030?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="21mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890324026030 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="6.67 GOhm"/>
<attribute name="VALUE" value="1.5 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L26W11H20" package="WCAP-FTX2_P22.5L26W11H20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026027?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890324026027 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="10.00 GOhm"/>
<attribute name="VALUE" value="1 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
</technologies>
</device>
<device name="_L26W15H25" package="WCAP-FTX2_P22.5L26W15H25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026034">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026034?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="25mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890324026034 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="4.55 GOhm"/>
<attribute name="VALUE" value="2.2 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_L26W6H15" package="WCAP-FTX2_P22.5L26W6H15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026003?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890324026003 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L26W7.5H15" package="WCAP-FTX2_P22.5L26W7.5H15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026020?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890324026020 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L26W7.5H16.5" package="WCAP-FTX2_P22.5L26W7.5H16.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026018?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="16.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890324026018 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="17.86 GOhm"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L26W9H18" package="WCAP-FTX2_P22.5L26W9H18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026024?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="18mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890324026024 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="12.20 GOhm"/>
<attribute name="VALUE" value="820 nF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
<device name="_L26W7H14.5" package="WCAP-FTX2_P22.5L26W7H14.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890324026014?ae"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890324026014 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="VALUE" value="0.47 uF"/>
<attribute name="VR" value="275V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
