<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Film Capacitors - WCAP-FTBE&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-11&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-FTBE_27.5X31X14X23.5(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X14X23.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_27.5X31X13X22(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X13X22(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_27.5X31X18X26(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X18X26(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_27.5X31X10X19(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X10X19(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_22.5X26X7X16.5(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,22.5X26X7X16.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_22.5X26X9X18(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt;Film Capacitors,22.5X26X9X18(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_15X18X5X11(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_15X18X6X12(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_15X18X12X21(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X12X21(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_22.5X26X6X15(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,22.5X26X6X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_37.5X42X17X30(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,37.5X42X17X30(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_15X18X8.5X15(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X8.5X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_15X18X7X13(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X7X13(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_37.5X42X20.5X34(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,37.5X42X20.5X34(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_37.5X42X31X43(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,37.5X42X31X43(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_27.5X31X15X24.5(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X15X24.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_27.5X31X11X20PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X11X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_10X13X5.0X11(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,10X13X5.0X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_7.5X10.5X5X11(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,7.5X10.5X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_10X13X5.5X11(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,10X13X5.5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_7.5X10.5X6X12(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,7.5X10.5X6X12(PitchXLXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-FTBE_P15" prefix="C">
<description>&lt;b&gt;WCAP-FTBE Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Boxed Type Metallized Polyester  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;High voltage and volumetric capacity possible 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polyester 
&lt;BR&gt;Capacitance range: 10 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 100 V(DC) ‒ 1 kV(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 85 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering  
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;P15=Pitch 15&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o85130v209%20Family_WE_WCAP-FTBE_4mm+Original.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o85130v209%20Family_WE_WCAP-FTBE_4mm+Original.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-FTBE/"&gt;https://www.we-online.com/catalog/en/WCAP-FTBE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-11
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_W12.0" package="WCAP-FTBE_15X18X12X21(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283425012CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283425012CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.5%@10kHz"/>
<attribute name="DF3" value="4%@100kHz"/>
<attribute name="H" value="21mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890283425012CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="20V/us"/>
<attribute name="RISO" value="2000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP015155K400DCPP35004"/>
<attribute name="VALUE" value="1.5  µF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="12mm"/>
</technology>
</technologies>
</device>
<device name="_W5.0" package="WCAP-FTBE_15X18X5X11(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273425001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890273425001CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.5%@10kHz"/>
<attribute name="DF3" value="4%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890273425001CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="8V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP015334K250DCPP45004"/>
<attribute name="VALUE" value="330  nF "/>
<attribute name="VR" value="250V(DC)"/>
<attribute name="W" value="5mm"/>
</technology>
<technology name="_890283425002CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283425002CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.5%@10kHz"/>
<attribute name="DF3" value="3.6%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890283425002CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="12V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP015224K400DCPP45004"/>
<attribute name="VALUE" value="220  nF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="5mm"/>
</technology>
<technology name="_890493425001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890493425001CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.4%@10kHz"/>
<attribute name="DF3" value="2.5%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890493425001CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="27V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP015223KA00DCPP45004"/>
<attribute name="VALUE" value="22  nF "/>
<attribute name="VR" value="1000V(DC)"/>
<attribute name="W" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_W6.0" package="WCAP-FTBE_15X18X6X12(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890303425004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303425004CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.4%@10kHz"/>
<attribute name="DF3" value="3.2%@100kHz"/>
<attribute name="H" value="12mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890303425004CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="28V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP015104K630DCPP45004"/>
<attribute name="VALUE" value="100  nF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_W7.0" package="WCAP-FTBE_15X18X7X13(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273425007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890273425007CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.5%@10kHz"/>
<attribute name="DF3" value="4.3%@100kHz"/>
<attribute name="H" value="13mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890273425007CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="11V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP015105K250DCPP45004"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="250V(DC)"/>
<attribute name="W" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_W8.5" package="WCAP-FTBE_15X18X8.5X15(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890263425004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890263425004CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.6%@10kHz"/>
<attribute name="DF3" value="5%@100kHz"/>
<attribute name="H" value="15mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890263425004CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="9V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP015225K100DCPP45004"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="W" value="8.5mm"/>
</technology>
<technology name="_890283425008CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283425008CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.5%@10kHz"/>
<attribute name="DF3" value="3.8%@100kHz"/>
<attribute name="H" value="15mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890283425008CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="18V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP015684K400DCPP45004"/>
<attribute name="VALUE" value="680  nF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="8.5mm"/>
</technology>
<technology name="_890493425009CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890493425009CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.4%@10kHz"/>
<attribute name="DF3" value="2.5%@100kHz"/>
<attribute name="H" value="15mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890493425009CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="44V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP015104KA00DCPP45004"/>
<attribute name="VALUE" value="100  nF "/>
<attribute name="VR" value="1000V(DC)"/>
<attribute name="W" value="8.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBE_P37.5" prefix="C">
<description>&lt;b&gt;WCAP-FTBE Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Boxed Type Metallized Polyester  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;High voltage and volumetric capacity possible 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polyester 
&lt;BR&gt;Capacitance range: 10 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 100 V(DC) ‒ 1 kV(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 85 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering  
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;P37.5=Pitch 37.5&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o85130v209%20Family_WE_WCAP-FTBE_4mm+Original.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o85130v209%20Family_WE_WCAP-FTBE_4mm+Original.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-FTBE/"&gt;https://www.we-online.com/catalog/en/WCAP-FTBE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-11
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_W17.0" package="WCAP-FTBE_37.5X42X17X30(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890303428008CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303428008CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="2.1%@10kHz"/>
<attribute name="DF3" value="11%@100kHz"/>
<attribute name="H" value="30mm"/>
<attribute name="L" value="42mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890303428008CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="12V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP375335K630DCPP25004"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="17mm"/>
</technology>
</technologies>
</device>
<device name="_W20.5" package="WCAP-FTBE_37.5X42X20.5X34(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283428007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283428007CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="2.3%@10kHz"/>
<attribute name="DF3" value="13%@100kHz"/>
<attribute name="H" value="34mm"/>
<attribute name="L" value="42mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890283428007CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="9V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP375685K400DCPP25004"/>
<attribute name="VALUE" value="6.8  µF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="20.5mm"/>
</technology>
</technologies>
</device>
<device name="_W31.0" package="WCAP-FTBE_37.5X42X31X43(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890493428013CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890493428013CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="2%@10kHz"/>
<attribute name="DF3" value="10%@100kHz"/>
<attribute name="H" value="43mm"/>
<attribute name="L" value="42mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890493428013CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="16V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP375475KA00DCPP25004"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="1000V(DC)"/>
<attribute name="W" value="31mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBE_P22.5" prefix="C">
<description>&lt;b&gt;WCAP-FTBE Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Boxed Type Metallized Polyester  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;High voltage and volumetric capacity possible 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polyester 
&lt;BR&gt;Capacitance range: 10 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 100 V(DC) ‒ 1 kV(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 85 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering  
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;P22.5=Pitch 22.5&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o85130v209%20Family_WE_WCAP-FTBE_4mm+Original.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o85130v209%20Family_WE_WCAP-FTBE_4mm+Original.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-FTBE/"&gt;https://www.we-online.com/catalog/en/WCAP-FTBE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-11
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_W6.0" package="WCAP-FTBE_22.5X26X6X15(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890263426001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890263426001CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="2%@10kHz"/>
<attribute name="DF3" value="10%@100kHz"/>
<attribute name="H" value="15mm"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890263426001CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="5V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP225225K100DCPP45004"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
<technology name="_890283426004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283426004CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.6%@10kHz"/>
<attribute name="DF3" value="4.6%@100kHz"/>
<attribute name="H" value="15mm"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890283426004CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="11V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP225474K400DCPP45004"/>
<attribute name="VALUE" value="470  nF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_W7.0" package="WCAP-FTBE_22.5X26X7X16.5(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890263426003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890263426003CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="2.1%@10kHz"/>
<attribute name="DF3" value="10%@100kHz"/>
<attribute name="H" value="16.5mm"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890263426003CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="5V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP225335K100DCPP35004"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="W" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_W9.0" package="WCAP-FTBE_22.5X26X9X18(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283426008CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283426008CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.6%@10kHz"/>
<attribute name="DF3" value="4.8%@100kHz"/>
<attribute name="H" value="18mm"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890283426008CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="13V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP225105K400DCPP35004"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="9mm"/>
</technology>
<technology name="_890303426008CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303426008CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.5%@10kHz"/>
<attribute name="DF3" value="4%@100kHz"/>
<attribute name="H" value="18mm"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890303426008CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="20V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP225474K630DCPP35004"/>
<attribute name="VALUE" value="470  nF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="9mm"/>
</technology>
<technology name="_890493426011CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890493426011CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.5%@10kHz"/>
<attribute name="DF3" value="3.6%@100kHz"/>
<attribute name="H" value="18mm"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890493426011CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="27V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP225224KA00DCPP35004"/>
<attribute name="VALUE" value="220  nF "/>
<attribute name="VR" value="1000V(DC)"/>
<attribute name="W" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBE_P27.5" prefix="C">
<description>&lt;b&gt;WCAP-FTBE Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Boxed Type Metallized Polyester  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;High voltage and volumetric capacity possible 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polyester 
&lt;BR&gt;Capacitance range: 10 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 100 V(DC) ‒ 1 kV(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 85 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering  
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;P27.5=Pitch 27.5&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o85130v209%20Family_WE_WCAP-FTBE_4mm+Original.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o85130v209%20Family_WE_WCAP-FTBE_4mm+Original.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-FTBE/"&gt;https://www.we-online.com/catalog/en/WCAP-FTBE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-11
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_W15.0" package="WCAP-FTBE_27.5X31X15X24.5(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283427007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283427007CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="2%@10kHz"/>
<attribute name="DF3" value="9%@100kHz"/>
<attribute name="H" value="24.5mm"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890283427007CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="11V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP275335K400DCPP25004"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="15mm"/>
</technology>
<technology name="_890303427009CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303427009CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.6%@10kHz"/>
<attribute name="DF3" value="5.2%@100kHz"/>
<attribute name="H" value="24.5mm"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890303427009CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="17V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP275155K630DCPP25004"/>
<attribute name="VALUE" value="1.5  µF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_W11.0" package="WCAP-FTBE_27.5X31X11X20PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273427005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890273427005CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="2.2%@10kHz"/>
<attribute name="DF3" value="11%@100kHz"/>
<attribute name="H" value="20mm"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890273427005CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="6V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP275475K250DCPP35004"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="250V(DC)"/>
<attribute name="W" value="11mm"/>
</technology>
<technology name="_890493427007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890493427007CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.5%@10kHz"/>
<attribute name="DF3" value="4.3%@100kHz"/>
<attribute name="H" value="20mm"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890493427007CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="22V/us"/>
<attribute name="RISO" value="3000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP275474KA00DCPP35004"/>
<attribute name="VALUE" value="470  nF "/>
<attribute name="VR" value="1000V(DC)"/>
<attribute name="W" value="11mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBE_P10" prefix="C">
<description>&lt;b&gt;WCAP-FTBE Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Boxed Type Metallized Polyester  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;High voltage and volumetric capacity possible 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polyester 
&lt;BR&gt;Capacitance range: 10 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 100 V(DC) ‒ 1 kV(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 85 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering  
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;P10=Pitch10&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o85130v209%20Family_WE_WCAP-FTBE_4mm+Original.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o85130v209%20Family_WE_WCAP-FTBE_4mm+Original.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-FTBE/"&gt;https://www.we-online.com/catalog/en/WCAP-FTBE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-11
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_W5.0" package="WCAP-FTBE_10X13X5.0X11(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273423002CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890273423002CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.4%@10kHz"/>
<attribute name="DF3" value="3.1%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890273423002CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="23V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP010224K250DCPP55004"/>
<attribute name="VALUE" value="220  nF "/>
<attribute name="VR" value="250V(DC)"/>
<attribute name="W" value="5mm"/>
</technology>
<technology name="_890283423001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283423001CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.4%@10kHz"/>
<attribute name="DF3" value="2.4%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890283423001CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="34V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP010104K400DCPP55004"/>
<attribute name="VALUE" value="100  nF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="5mm"/>
</technology>
<technology name="_890493423001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890493423001CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.4%@10kHz"/>
<attribute name="DF3" value="2.2%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890493423001CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="83V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP010153KA00DCPP55004"/>
<attribute name="VALUE" value="15  nF "/>
<attribute name="VR" value="1000V(DC)"/>
<attribute name="W" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_W5.5" package="WCAP-FTBE_10X13X5.5X11(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890303423005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303423005CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.4%@10kHz"/>
<attribute name="DF3" value="2.3%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890303423005CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="52V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP010683K630DCPP55004"/>
<attribute name="VALUE" value="68  nF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="5.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBE_P7.5" prefix="C">
<description>&lt;b&gt;WCAP-FTBE Film Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Boxed Type Metallized Polyester  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;High voltage and volumetric capacity possible 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polyester 
&lt;BR&gt;Capacitance range: 10 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 100 V(DC) ‒ 1 kV(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 85 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering  
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;P7.5=Pitch 7.5&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o85130v209%20Family_WE_WCAP-FTBE_4mm+Original.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o85130v209%20Family_WE_WCAP-FTBE_4mm+Original.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-FTBE/"&gt;https://www.we-online.com/catalog/en/WCAP-FTBE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-11
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_W5.0" package="WCAP-FTBE_7.5X10.5X5X11(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283422001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283422001CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.4%@10kHz"/>
<attribute name="DF3" value="2.3%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890283422001CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="44V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP075683K400DCPP45004"/>
<attribute name="VALUE" value="68  nF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_W6.0" package="WCAP-FTBE_7.5X10.5X6X12(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273422002CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890273422002CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.4%@10kHz"/>
<attribute name="DF3" value="2.4%@100kHz"/>
<attribute name="H" value="12mm"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890273422002CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="38V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP075224K250DCPP45004"/>
<attribute name="VALUE" value="220  nF "/>
<attribute name="VR" value="250V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
<technology name="_890283422005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283422005CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.4%@10kHz"/>
<attribute name="DF3" value="2.3%@100kHz"/>
<attribute name="H" value="12mm"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890283422005CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="46V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP075154K400DCPP45004"/>
<attribute name="VALUE" value="150  nF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
<technology name="_890303422005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303422005CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.4%@10kHz"/>
<attribute name="DF3" value="2.2%@100kHz"/>
<attribute name="H" value="12mm"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890303422005CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="100V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP075473K630DCPP45004"/>
<attribute name="VALUE" value="47  nF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
<technology name="_890493422002CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890493422002CS.pdf"/>
<attribute name="DF1" value="1%@1kHz"/>
<attribute name="DF2" value="1.4%@10kHz"/>
<attribute name="DF3" value="2.2%@100kHz"/>
<attribute name="H" value="12mm"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="890493422002CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="9000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPSP075103KA00DCPP45004"/>
<attribute name="VALUE" value="10  nF "/>
<attribute name="VR" value="1000V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
