<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Modules (MagI³C Series) - Step Down Converter - Variable Output Voltage - MagI³C-VDRM &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-04-22&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WPME-VDRM_BQFN_171021501">
</package>
<package name="WPME-VDRM_BQFN_1710X0302">
</package>
<package name="WPME-VDRM_TO263-7EP">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module
&lt;br&gt;&lt;/b&gt;Size : TO263-7EP</description>
</package>
</packages>
<symbols>
<symbol name="WPME-VDRM_BQFN">
<pin name="2" direction="pas"/>
<pin name="3" direction="out"/>
<pin name="4" direction="in"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="in"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pwr"/>
<pin name="9" direction="pwr"/>
<pin name="10" direction="pwr"/>
<pin name="20" direction="pwr"/>
<pin name="21" direction="pwr"/>
<pin name="22" direction="pwr"/>
<pin name="23" direction="pwr"/>
<pin name="24" direction="pwr"/>
<pin name="25" direction="pwr"/>
<pin name="26" direction="sup"/>
<pin name="27" direction="out"/>
<pin name="28" direction="in"/>
<pin name="29" direction="in"/>
<pin name="30" direction="pwr"/>
<pin name="32" direction="pwr"/>
<pin name="33" direction="sup"/>
<pin name="34" direction="sup"/>
<pin name="35" direction="in"/>
<pin name="36" direction="in"/>
<pin name="1" direction="pas"/>
<pin name="12" direction="pwr"/>
<pin name="13" direction="pwr"/>
<pin name="14" direction="pwr"/>
<pin name="15" direction="nc"/>
<pin name="16" direction="nc"/>
<pin name="17" direction="pwr"/>
<pin name="18" direction="pwr"/>
<pin name="19" direction="pwr"/>
<pin name="11" direction="pwr"/>
<pin name="38" direction="pwr"/>
<pin name="39" direction="pwr"/>
<pin name="37" direction="pas"/>
<pin name="31" direction="pwr"/>
</symbol>
<symbol name="WPME-VDRM_TO263-7EP_171050601">
<pin name="VIN" direction="pwr"/>
<pin name="SYNC" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="AGND" direction="sup"/>
<pin name="PGND" direction="pwr"/>
<pin name="SS/TRK" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="VOUT" direction="pwr"/>
</symbol>
<symbol name="WPME-VDRM_BQFN_171021501">
<pin name="2" direction="out"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="sup"/>
<pin name="5" direction="sup"/>
<pin name="6" direction="pwr"/>
<pin name="7" direction="pwr"/>
<pin name="8" direction="nc"/>
<pin name="9" direction="nc"/>
<pin name="10" direction="pwr"/>
<pin name="20" direction="pwr"/>
<pin name="21" direction="pwr"/>
<pin name="22" direction="pwr"/>
<pin name="23" direction="pwr"/>
<pin name="24" direction="pwr"/>
<pin name="25" direction="sup"/>
<pin name="26" direction="pwr"/>
<pin name="27" direction="in"/>
<pin name="28" direction="in"/>
<pin name="29" direction="in"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="in"/>
<pin name="32" direction="sup"/>
<pin name="33" direction="sup"/>
<pin name="34" direction="sup"/>
<pin name="35" direction="out"/>
<pin name="36" direction="in"/>
<pin name="1" direction="pas"/>
<pin name="12" direction="pwr"/>
<pin name="13" direction="pwr"/>
<pin name="14" direction="pwr"/>
<pin name="15" direction="pwr"/>
<pin name="16" direction="pwr"/>
<pin name="17" direction="pwr"/>
<pin name="18" direction="pwr"/>
<pin name="19" direction="pwr"/>
<pin name="40" direction="pwr"/>
<pin name="41" direction="pwr"/>
<pin name="11" direction="pwr"/>
<pin name="38" direction="pwr"/>
<pin name="39" direction="pwr"/>
<pin name="37" direction="sup"/>
</symbol>
<symbol name="WPME-VDRM_TO263-7EP">
<pin name="VIN" direction="pwr"/>
<pin name="RON" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="AGND" direction="sup"/>
<pin name="PGND" direction="pwr"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="VOUT" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="171021501" prefix="U">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDRM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-04-22&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDRM_BQFN_171021501"/>
</gates>
<devices>
<device name="" package="WPME-VDRM_BQFN_171021501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171021501?ae"/>
<attribute name="HEIGHT" value="2.85mm"/>
<attribute name="I-OUTPUT" value="2.5A"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171021501"/>
<attribute name="SIZE" value="BQFN"/>
<attribute name="V-INPUT" value="7 - 50Vin"/>
<attribute name="V-OUTPUT" value="2.5 - 15Vout"/>
<attribute name="VALUE" value="7 - 50Vin, 2.5 - 15Vout, 2.5A"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171020302" prefix="U">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDRM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-04-22&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDRM_BQFN"/>
</gates>
<devices>
<device name="" package="WPME-VDRM_BQFN_1710X0302">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171020302?ae"/>
<attribute name="HEIGHT" value="2.85mm"/>
<attribute name="I-OUTPUT" value="2A"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171020302"/>
<attribute name="SIZE" value="BQFN"/>
<attribute name="V-INPUT" value="2.95 - 6Vin"/>
<attribute name="V-OUTPUT" value="0.8 - 3.6Vout"/>
<attribute name="VALUE" value="2.95 - 6Vin, 0.8 - 3.6Vout, 2A"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171060302" prefix="U">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDRM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-04-22&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDRM_BQFN"/>
</gates>
<devices>
<device name="" package="WPME-VDRM_BQFN_1710X0302">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171060302?ae"/>
<attribute name="HEIGHT" value="2.85mm"/>
<attribute name="I-OUTPUT" value="6A"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171060302"/>
<attribute name="SIZE" value="BQFN"/>
<attribute name="V-INPUT" value="2.95 - 6Vin"/>
<attribute name="V-OUTPUT" value="0.8 - 3.6Vout"/>
<attribute name="VALUE" value="2.95 - 6Vin, 0.8 - 3.6Vout, 6A"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171040302" prefix="U">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDRM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-04-22&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDRM_BQFN"/>
</gates>
<devices>
<device name="" package="WPME-VDRM_BQFN_1710X0302">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171040302?ae"/>
<attribute name="HEIGHT" value="2.85mm"/>
<attribute name="I-OUTPUT" value="4A"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171040302"/>
<attribute name="SIZE" value="BQFN"/>
<attribute name="V-INPUT" value="2.95 - 6Vin"/>
<attribute name="V-OUTPUT" value="0.8 - 3.6Vout"/>
<attribute name="VALUE" value="2.95 - 6Vin, 0.8 - 3.6Vout, 4A"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171030601" prefix="U">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDRM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-04-22&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDRM_TO263-7EP"/>
</gates>
<devices>
<device name="" package="WPME-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171030601?ae"/>
<attribute name="HEIGHT" value="4.57mm"/>
<attribute name="I-OUTPUT" value="3A"/>
<attribute name="LENGTH" value="9.85mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171030601"/>
<attribute name="SIZE" value="TO263-7EP"/>
<attribute name="V-INPUT" value="6 - 42Vin"/>
<attribute name="V-OUTPUT" value="0.8 - 6Vout"/>
<attribute name="VALUE" value="6 - 42Vin, 0.8 - 6Vout, 3A"/>
<attribute name="WIDTH" value="10.16mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171032401" prefix="U">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDRM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-04-22&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDRM_TO263-7EP"/>
</gates>
<devices>
<device name="" package="WPME-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171032401?ae"/>
<attribute name="HEIGHT" value="4.57mm"/>
<attribute name="I-OUTPUT" value="3A"/>
<attribute name="LENGTH" value="9.85mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171032401"/>
<attribute name="SIZE" value="TO263-7EP"/>
<attribute name="V-INPUT" value="6 - 42Vin"/>
<attribute name="V-OUTPUT" value="5 - 24Vout"/>
<attribute name="VALUE" value="6 - 42Vin, 5 - 24Vout, 3A"/>
<attribute name="WIDTH" value="10.16mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171012401" prefix="U">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDRM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-04-22&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDRM_TO263-7EP"/>
</gates>
<devices>
<device name="" package="WPME-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171012401?ae"/>
<attribute name="HEIGHT" value="4.57mm"/>
<attribute name="I-OUTPUT" value="1A"/>
<attribute name="LENGTH" value="9.85mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171012401"/>
<attribute name="SIZE" value="TO263-7EP"/>
<attribute name="V-INPUT" value="6 - 42Vin"/>
<attribute name="V-OUTPUT" value="5 - 24Vout"/>
<attribute name="VALUE" value="6 - 42Vin, 5 - 24Vout, 1A"/>
<attribute name="WIDTH" value="10.16mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171010601" prefix="U">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDRM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-04-22&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDRM_TO263-7EP"/>
</gates>
<devices>
<device name="" package="WPME-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171010601?ae"/>
<attribute name="HEIGHT" value="4.57mm"/>
<attribute name="I-OUTPUT" value="1A"/>
<attribute name="LENGTH" value="9.85mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171010601"/>
<attribute name="SIZE" value="TO263-7EP"/>
<attribute name="V-INPUT" value="6 - 42Vin"/>
<attribute name="V-OUTPUT" value="0.8 - 6Vout"/>
<attribute name="VALUE" value="6 - 42Vin, 0.8 - 6Vout, 1A"/>
<attribute name="WIDTH" value="10.16mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171012402" prefix="U">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDRM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-04-22&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDRM_TO263-7EP"/>
</gates>
<devices>
<device name="" package="WPME-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171012402?ae"/>
<attribute name="HEIGHT" value="4.57mm"/>
<attribute name="I-OUTPUT" value="2A"/>
<attribute name="LENGTH" value="9.85mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171012402"/>
<attribute name="SIZE" value="TO263-7EP"/>
<attribute name="V-INPUT" value="6 - 42Vin"/>
<attribute name="V-OUTPUT" value="5 - 24Vout"/>
<attribute name="VALUE" value="6 - 42Vin, 5 - 24Vout, 2A"/>
<attribute name="WIDTH" value="10.16mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171020601" prefix="U">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDRM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-04-22&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDRM_TO263-7EP"/>
</gates>
<devices>
<device name="" package="WPME-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171020601?ae"/>
<attribute name="HEIGHT" value="4.57mm"/>
<attribute name="I-OUTPUT" value="2A"/>
<attribute name="LENGTH" value="9.85mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171020601"/>
<attribute name="SIZE" value="TO263-7EP"/>
<attribute name="V-INPUT" value="6 - 42Vin"/>
<attribute name="V-OUTPUT" value="0.8 - 6Vout"/>
<attribute name="VALUE" value="6 - 42Vin, 0.8 - 6Vout, 2A"/>
<attribute name="WIDTH" value="10.16mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171050601" prefix="U">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33388v209%20Family-MagicVDRM-171010601-171021501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDRM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-04-22&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDRM_TO263-7EP_171050601"/>
</gates>
<devices>
<device name="" package="WPME-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="5"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="SS/TRK" pad="6"/>
<connect gate="G$1" pin="SYNC" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171050601?ae"/>
<attribute name="HEIGHT" value="4.57mm"/>
<attribute name="I-OUTPUT" value="5A"/>
<attribute name="LENGTH" value="9.85mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171050601"/>
<attribute name="SIZE" value="TO263-7EP"/>
<attribute name="V-INPUT" value="6 - 36Vin"/>
<attribute name="V-OUTPUT" value="0.8 - 6Vout"/>
<attribute name="VALUE" value="6 - 36Vin, 0.8 - 6Vout, 5A"/>
<attribute name="WIDTH" value="10.16mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
