<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Aluminum Electrolytic Capacitors - Snap-In - WCAP-AI3H&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2026a, 2026-04-09&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-AI3H_D22L35">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X35mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D22L26">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X26mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D25L31">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X31mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D30L40">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X40mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D25L51">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X51mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L25">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X25mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D30L35">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X35mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D22L36">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X36mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L40">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X40mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D22L31">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X31mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D22L51">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X51mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D25L35">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X35mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D22L41">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X41mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L65">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X65mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D25L36">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X36mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D30L51">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X51mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D22L46">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X46mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L57">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X57mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L42">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X42mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D25L46">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X46mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D25L41">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X41mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D25L30">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X30mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D30L31">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X31mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D30L36">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X36mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D30L30">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X30mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D30L26">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X26mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D30L41">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X41mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L30">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X30mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L37">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X37mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L32">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X32mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D25L26">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X26mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L52">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X52mm(DiameterXLength)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AI3H_D22L35" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D22L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140783006">
<attribute name="C" value="2200 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861140783006?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1116.87 uA"/>
<attribute name="I-RIPPLE" value="1820 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861140783006"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="2200 uF"/>
<attribute name="VR" value="63 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D22L26" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D22L26">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483001">
<attribute name="C" value="68 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141483001?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="524.79 uA"/>
<attribute name="I-RIPPLE" value="520 mA"/>
<attribute name="LENGTH" value="26 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483001"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="68 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L31" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L31">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141484009">
<attribute name="C" value="100 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141484009?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="636.4 uA"/>
<attribute name="I-RIPPLE" value="690 mA"/>
<attribute name="LENGTH" value="31 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141484009"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="100 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861141484010">
<attribute name="C" value="120 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141484010?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="697.14 uA"/>
<attribute name="I-RIPPLE" value="800 mA"/>
<attribute name="LENGTH" value="31 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141484010"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="120 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L51" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L51">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140884001">
<attribute name="C" value="2200 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861140884001?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1407.12 uA"/>
<attribute name="I-RIPPLE" value="2650 mA"/>
<attribute name="LENGTH" value="51 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861140884001"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="2200 uF"/>
<attribute name="VR" value="100 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D30L40" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D30L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141485033">
<attribute name="C" value="470 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141485033?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value=" 4000 "/>
<attribute name="I-LEAK" value="1380 uA"/>
<attribute name="I-RIPPLE" value="1940 mA"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485033"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="470 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L25" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141386015">
<attribute name="C" value="220 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141386015?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="889.94 uA"/>
<attribute name="I-RIPPLE" value="1100 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141386015"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="400 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D30L35" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D30L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141085021">
<attribute name="C" value="1000 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141085021?ae"/>
<attribute name="DF" value="15 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1341.64 uA"/>
<attribute name="I-RIPPLE" value="2300 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141085021"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="1000 uF"/>
<attribute name="VR" value="200 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L40" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141386025">
<attribute name="C" value="470 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141386025?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1300.77 uA"/>
<attribute name="I-RIPPLE" value="1900 mA"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141386025"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="470 uF"/>
<attribute name="VR" value="400 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D22L36" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D22L36">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483003">
<attribute name="C" value="100 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141483003?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="636.4 uA"/>
<attribute name="I-RIPPLE" value="690 mA"/>
<attribute name="LENGTH" value="36 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483003"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="100 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D22L31" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D22L31">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483002">
<attribute name="C" value="82 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141483002?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="576.28 uA"/>
<attribute name="I-RIPPLE" value="640 mA"/>
<attribute name="LENGTH" value="31 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483002"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="82 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D22L51" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D22L51">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483006">
<attribute name="C" value="180 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141483006?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="853.81 uA"/>
<attribute name="I-RIPPLE" value="1000 mA"/>
<attribute name="LENGTH" value="51 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483006"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861141483007">
<attribute name="C" value="220 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141483007?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="943.93 uA"/>
<attribute name="I-RIPPLE" value="1000 mA"/>
<attribute name="LENGTH" value="51 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483007"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D22L41" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D22L41">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483004">
<attribute name="C" value="120 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141483004?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="697.14 uA"/>
<attribute name="I-RIPPLE" value="800 mA"/>
<attribute name="LENGTH" value="41 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483004"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="120 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L35" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140784012">
<attribute name="C" value="3300 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861140784012?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1367.88 uA"/>
<attribute name="I-RIPPLE" value="2270 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861140784012"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="3300 uF"/>
<attribute name="VR" value="63 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L65" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L65">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141386028">
<attribute name="C" value="1000 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141386028?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1897.37 uA"/>
<attribute name="I-RIPPLE" value="2650 mA"/>
<attribute name="LENGTH" value="65 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141386028"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="1000 uF"/>
<attribute name="VR" value="400 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L36" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L36">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141484011">
<attribute name="C" value="150 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141484011?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="779.42 uA"/>
<attribute name="I-RIPPLE" value="880 mA"/>
<attribute name="LENGTH" value="36 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141484011"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="150 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D30L51" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D30L51">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141485019">
<attribute name="C" value="330 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141485019?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1156.07 uA"/>
<attribute name="I-RIPPLE" value="1450 mA"/>
<attribute name="LENGTH" value="51 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485019"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="330 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D22L46" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D22L46">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483005">
<attribute name="C" value="150 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141483005?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="779.42 uA"/>
<attribute name="I-RIPPLE" value="880 mA"/>
<attribute name="LENGTH" value="46 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483005"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="150 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L57" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L57">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141486025">
<attribute name="C" value="560 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141486025?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1505.99 uA"/>
<attribute name="I-RIPPLE" value="2150 mA"/>
<attribute name="LENGTH" value="57 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486025"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="560 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861141486026">
<attribute name="C" value="680 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141486026?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1659.52 uA"/>
<attribute name="I-RIPPLE" value="2200 mA"/>
<attribute name="LENGTH" value="57 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486026"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="680 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L42" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L42">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141486022">
<attribute name="C" value="330 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141486022?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1156.07 uA"/>
<attribute name="I-RIPPLE" value="1450 mA"/>
<attribute name="LENGTH" value="42 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486022"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="330 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861141486023">
<attribute name="C" value="390 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141486023?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1256.78 uA"/>
<attribute name="I-RIPPLE" value="1500 mA"/>
<attribute name="LENGTH" value="42 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486023"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="390 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L46" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L46">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141484013">
<attribute name="C" value="220 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141484013?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="943.93 uA"/>
<attribute name="I-RIPPLE" value="1120 mA"/>
<attribute name="LENGTH" value="46 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141484013"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L41" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L41">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141484012">
<attribute name="C" value="180 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141484012?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="853.81 uA"/>
<attribute name="I-RIPPLE" value="1000 mA"/>
<attribute name="LENGTH" value="41 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141484012"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D30L31" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D30L31">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141485015">
<attribute name="C" value="150 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141485015?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="779.42 uA"/>
<attribute name="I-RIPPLE" value="880 mA"/>
<attribute name="LENGTH" value="31 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485015"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="150 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861141485016">
<attribute name="C" value="180 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141485016?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="853.81 uA"/>
<attribute name="I-RIPPLE" value="1000 mA"/>
<attribute name="LENGTH" value="31 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485016"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D30L36" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D30L36">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141485017">
<attribute name="C" value="220 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141485017?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="943.93 uA"/>
<attribute name="I-RIPPLE" value="1120 mA"/>
<attribute name="LENGTH" value="36 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485017"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L30" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;br&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2026-04-09
&lt;br&gt;2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141084008">
<attribute name="C" value="470 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141084008?ae"/>
<attribute name="DF" value="15 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="919.78 uA"/>
<attribute name="I-RIPPLE" value="1500 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141084008"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="470 uF"/>
<attribute name="VR" value="200 V (DC)"/>
</technology>
<technology name="_861142084015">
<attribute name="C" value="180 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861142084015?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value=" 5000 "/>
<attribute name="I-LEAK" value="900 uA"/>
<attribute name="I-RIPPLE" value="1160 Ma"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861142084015"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="500 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D30L30" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D30L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141085015">
<attribute name="C" value="680 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141085015?ae"/>
<attribute name="DF" value="15 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1106.35 uA"/>
<attribute name="I-RIPPLE" value="1780 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141085015"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="680 uF"/>
<attribute name="VR" value="200 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D30L26" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D30L26">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141485014">
<attribute name="C" value="120 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141485014?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="697.14 uA"/>
<attribute name="I-RIPPLE" value="800 mA"/>
<attribute name="LENGTH" value="26 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485014"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="120 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L30" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140786018">
<attribute name="C" value="4700 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861140786018?ae"/>
<attribute name="DF" value="30 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1632.45 uA"/>
<attribute name="I-RIPPLE" value="2830 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861140786018"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="4700 uF"/>
<attribute name="VR" value="63 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D30L41" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D30L41">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141485018">
<attribute name="C" value="270 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141485018?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1045.71 uA"/>
<attribute name="I-RIPPLE" value="1280 mA"/>
<attribute name="LENGTH" value="41 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485018"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="270 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L37" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L37">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141486021">
<attribute name="C" value="270 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141486021?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1045.71 uA"/>
<attribute name="I-RIPPLE" value="1280 mA"/>
<attribute name="LENGTH" value="37 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486021"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="270 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L32" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L32">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141486020">
<attribute name="C" value="220 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141486020?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="943.93 uA"/>
<attribute name="I-RIPPLE" value="1120 mA"/>
<attribute name="LENGTH" value="32 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486020"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L26" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L26">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141484008">
<attribute name="C" value="82 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141484008?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="576.28 uA"/>
<attribute name="I-RIPPLE" value="640 mA"/>
<attribute name="LENGTH" value="26 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141484008"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="82 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L52" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications
&lt;br&gt;Filtering
&lt;br&gt;Smoothing
&lt;br&gt;Energy storage
&lt;br&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14717v209%20family-wcap-ai3h-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AI3H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AI3H&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L52">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140786024">
<attribute name="C" value="10000 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861140786024?ae"/>
<attribute name="DF" value="30 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="2381.18 uA"/>
<attribute name="I-RIPPLE" value="4690 mA"/>
<attribute name="LENGTH" value="52 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861140786024"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="10000 uF"/>
<attribute name="VR" value="63 V (DC)"/>
</technology>
<technology name="_861141486024">
<attribute name="C" value="470 uF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861141486024?ae"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="1379.67 uA"/>
<attribute name="I-RIPPLE" value="1850 mA"/>
<attribute name="LENGTH" value="52 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486024"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="470 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
