<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<library>
<description>Würth Elektronik - Passive Components - Capacitors - Aluminum Electrolytic Capacitors - Snap-In - WCAP-AI3H

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026b, 2026-07-27
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-AI3H_D22L35">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=22mmX35mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D25L45">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=25mmX45mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D25L40">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=25mmX40mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D22L50">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=22mmX50mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D22L45">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=22mmX45mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D22L40">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=22mmX40mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D35L25">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X25mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L30">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X30mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D30L40">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X40mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L55">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=35mmX55mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D22L30">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=22mmX30mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D30L25">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=30mmX25mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D25L30">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X30mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D25L51">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X51mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D25L25">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=25mmX25mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D30L50">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=30mmX50mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D30L30">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X30mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L35">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=35mmX35mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D25L35">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X35mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L52">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=35mmX52mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D30L35">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X35mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L50">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=35mmX50mm, THT, 2pins</description>
</package>
<package name="WCAP-AI3H_D35L40">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X40mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D35L65">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X65mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_D22L25">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors

DiameterXLength=22mmX25mm, THT, 2pins</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AI3H_D22L35" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D22L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140783006">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861140783006?ae"/>
<attribute name="C" value="2200 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1117 uA"/>
<attribute name="I-RIPPLE" value="1830 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861140783006"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="2200 uF"/>
<attribute name="VR" value="63 V (DC)"/>
</technology>
<technology name="_861141483003">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141483003?ae"/>
<attribute name="C" value="100 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="636 uA"/>
<attribute name="I-RIPPLE" value="730 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483003"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="100 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L45" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L45">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141484013">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141484013?ae"/>
<attribute name="C" value="220 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="945 uA"/>
<attribute name="I-RIPPLE" value="1190 mA"/>
<attribute name="LENGTH" value="45 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141484013"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L40" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141484012">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141484012?ae"/>
<attribute name="C" value="180 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="854 uA"/>
<attribute name="I-RIPPLE" value="1110 mA"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141484012"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D22L50" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D22L50">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483006">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141483006?ae"/>
<attribute name="C" value="180 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="854 uA"/>
<attribute name="I-RIPPLE" value="1160 mA"/>
<attribute name="LENGTH" value="50 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483006"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861141483007">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141483007?ae"/>
<attribute name="C" value="220 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="945 uA"/>
<attribute name="I-RIPPLE" value="1160 mA"/>
<attribute name="LENGTH" value="50 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483007"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D22L45" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D22L45">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483005">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141483005?ae"/>
<attribute name="C" value="150 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="779 uA"/>
<attribute name="I-RIPPLE" value="990 mA"/>
<attribute name="LENGTH" value="45 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483005"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="150 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D22L40" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D22L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483004">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141483004?ae"/>
<attribute name="C" value="120 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="697 uA"/>
<attribute name="I-RIPPLE" value="840 mA"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483004"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="120 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L25" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors 

Long Life +105 °C   

Characteristics

Long life product series

Mounting style: Snap-In

Recommended soldering: Wave soldering

Applications

Long life &amp; high operating temperature applications

Filtering

Smoothing

Energy storage

e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2025-09-08

2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141386015">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141386015?ae"/>
<attribute name="C" value="220 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="890 uA"/>
<attribute name="I-RIPPLE" value="1160 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141386015"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="400 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L30" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140786018">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861140786018?ae"/>
<attribute name="C" value="4700 uF"/>
<attribute name="DF" value="30 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1632 uA"/>
<attribute name="I-RIPPLE" value="3050 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861140786018"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="4700 uF"/>
<attribute name="VR" value="63 V (DC)"/>
</technology>
<technology name="_861141486020">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141486020?ae"/>
<attribute name="C" value="220 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="944 uA"/>
<attribute name="I-RIPPLE" value="1250 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486020"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D30L40" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D30L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141485018">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141485018?ae"/>
<attribute name="C" value="270 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1046 uA"/>
<attribute name="I-RIPPLE" value="1390 mA"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485018"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="270 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861141485033">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141485033?ae"/>
<attribute name="C" value="470 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="4000"/>
<attribute name="I-LEAK" value="1380 uA"/>
<attribute name="I-RIPPLE" value="1940 mA"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485033"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="470 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L55" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L55">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141486025">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141486025?ae"/>
<attribute name="C" value="560 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1506 uA"/>
<attribute name="I-RIPPLE" value="2510 mA"/>
<attribute name="LENGTH" value="55 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486025"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="560 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861141486026">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141486026?ae"/>
<attribute name="C" value="680 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1660 uA"/>
<attribute name="I-RIPPLE" value="2760 mA"/>
<attribute name="LENGTH" value="55 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486026"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="680 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D22L30" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D22L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483002">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141483002?ae"/>
<attribute name="C" value="82 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="577 uA"/>
<attribute name="I-RIPPLE" value="640 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483002"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="82 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D30L25" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D30L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141485014">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141485014?ae"/>
<attribute name="C" value="120 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="697 uA"/>
<attribute name="I-RIPPLE" value="860 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485014"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="120 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L30" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141084008">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141084008?ae"/>
<attribute name="C" value="470 uF"/>
<attribute name="DF" value="15 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="920 uA"/>
<attribute name="I-RIPPLE" value="1580 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141084008"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="470 uF"/>
<attribute name="VR" value="200 V (DC)"/>
</technology>
<technology name="_861141484009">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141484009?ae"/>
<attribute name="C" value="100 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="636 uA"/>
<attribute name="I-RIPPLE" value="760 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141484009"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="100 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861141484010">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141484010?ae"/>
<attribute name="C" value="120 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="697 uA"/>
<attribute name="I-RIPPLE" value="840 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141484010"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="120 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861142084015">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861142084015?ae"/>
<attribute name="C" value="180 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="5000"/>
<attribute name="I-LEAK" value="900 uA"/>
<attribute name="I-RIPPLE" value="1160 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861142084015"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="500 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L51" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors 

Long Life +105 °C   

Characteristics

Long life product series

Mounting style: Snap-In

Recommended soldering: Wave soldering

Applications

Long life &amp; high operating temperature applications

Filtering

Smoothing

Energy storage

e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2025-09-08

2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L51">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140884001">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861140884001?ae"/>
<attribute name="C" value="2200 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1407 uA"/>
<attribute name="I-RIPPLE" value="2650 mA"/>
<attribute name="LENGTH" value="51 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861140884001"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="2200 uF"/>
<attribute name="VR" value="100 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L25" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141484008">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141484008?ae"/>
<attribute name="C" value="82 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="576 uA"/>
<attribute name="I-RIPPLE" value="640 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141484008"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="82 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D30L50" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D30L50">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141485019">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141485019?ae"/>
<attribute name="C" value="330 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1156 uA"/>
<attribute name="I-RIPPLE" value="1690 mA"/>
<attribute name="LENGTH" value="50 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485019"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="330 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D30L30" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D30L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141085015">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141085015?ae"/>
<attribute name="C" value="680 uF"/>
<attribute name="DF" value="15 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1106 uA"/>
<attribute name="I-RIPPLE" value="2150 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141085015"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="680 uF"/>
<attribute name="VR" value="200 V (DC)"/>
</technology>
<technology name="_861141485015">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141485015?ae"/>
<attribute name="C" value="150 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="779 uA"/>
<attribute name="I-RIPPLE" value="1010 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485015"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="150 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861141485016">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141485016?ae"/>
<attribute name="C" value="180 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="854 uA"/>
<attribute name="I-RIPPLE" value="1120 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485016"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L35" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141486021">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141486021?ae"/>
<attribute name="C" value="270 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1046 uA"/>
<attribute name="I-RIPPLE" value="1470 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486021"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="270 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D25L35" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D25L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140784012">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861140784012?ae"/>
<attribute name="C" value="3300 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1368 uA"/>
<attribute name="I-RIPPLE" value="2330 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861140784012"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="3300 uF"/>
<attribute name="VR" value="63 V (DC)"/>
</technology>
<technology name="_861141484011">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141484011?ae"/>
<attribute name="C" value="150 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="779 uA"/>
<attribute name="I-RIPPLE" value="990 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141484011"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="150 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L52" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors 
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L52">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140786024">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861140786024?ae"/>
<attribute name="C" value="10000 uF"/>
<attribute name="DF" value="30 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="2381 uA"/>
<attribute name="I-RIPPLE" value="4690 mA"/>
<attribute name="LENGTH" value="52 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861140786024"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="10000 uF"/>
<attribute name="VR" value="63 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D30L35" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D30L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141085021">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141085021?ae"/>
<attribute name="C" value="1000 uF"/>
<attribute name="DF" value="15 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1342 uA"/>
<attribute name="I-RIPPLE" value="2300 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141085021"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="1000 uF"/>
<attribute name="VR" value="200 V (DC)"/>
</technology>
<technology name="_861141485017">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141485017?ae"/>
<attribute name="C" value="220 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="944 uA"/>
<attribute name="I-RIPPLE" value="1190 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141485017"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L50" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L50">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140786024">
<attribute name="DATASHEET" value=""/>
<attribute name="C" value="10000 uF"/>
<attribute name="DF" value="30 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value=" 3000 "/>
<attribute name="I-LEAK" value="2381.18 uA"/>
<attribute name="I-RIPPLE" value="4690 mA"/>
<attribute name="LENGTH" value="52 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861140786024"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="10000 uF"/>
<attribute name="VR" value="63 V (DC)"/>
</technology>
<technology name="_861141486024">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141486024?ae"/>
<attribute name="C" value="470 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1380 uA"/>
<attribute name="I-RIPPLE" value="2210 mA"/>
<attribute name="LENGTH" value="50 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486024"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="470 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L40" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141386025">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141386025?ae"/>
<attribute name="C" value="470 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1301 uA"/>
<attribute name="I-RIPPLE" value="2010 mA"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141386025"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="470 uF"/>
<attribute name="VR" value="400 V (DC)"/>
</technology>
<technology name="_861141486022">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141486022?ae"/>
<attribute name="C" value="330 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1156 uA"/>
<attribute name="I-RIPPLE" value="1700 mA"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486022"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="330 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861141486023">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141486023?ae"/>
<attribute name="C" value="390 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1257 uA"/>
<attribute name="I-RIPPLE" value="1860 mA"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141486023"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="390 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D35L65" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors 

Long Life +105 °C   

Characteristics

Long life product series

Mounting style: Snap-In

Recommended soldering: Wave soldering

Applications

Long life &amp; high operating temperature applications

Filtering

Smoothing

Energy storage

e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2025-09-08

2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D35L65">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141386028">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141386028?ae"/>
<attribute name="C" value="1000 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="1897 uA"/>
<attribute name="I-RIPPLE" value="3110 mA"/>
<attribute name="LENGTH" value="65 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141386028"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="1000 uF"/>
<attribute name="VR" value="400 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_D22L25" prefix="C">
<description>WCAP-AI3H Aluminum Electrolytic Capacitors
Long Life +105 °C   

Characteristics
Long life product series
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
Long life &amp; high operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AI3H

Updated by Ella 2026-07-24
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_D22L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483001">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861141483001?ae"/>
<attribute name="C" value="68 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="3000"/>
<attribute name="I-LEAK" value="525 uA"/>
<attribute name="I-RIPPLE" value="520 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="861141483001"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="68 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
