<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-AI3H&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-04-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-AI3H_35X25(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X25mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_22X25(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X25mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_25X40(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X40mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_30X50(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X50mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_35X55(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X55mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_25X35(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X35mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_35X65(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X65mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_22X40(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X40mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_35X50(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X50mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_35X35(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X35mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_22X35(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X35mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_30X40(DXL)_PINLENGTH_6MM">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X40mm(DiameterXLength), Pin Length=6mm</description>
</package>
<package name="WCAP-AI3H_25X45(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X45mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_25X30(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X30mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_30X40(DXL)_PINLENGTH_4MM">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X40mm(DiameterXLength), Pin Length=4mm</description>
</package>
<package name="WCAP-AI3H_35X30(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X30mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_30X35(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X35mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_35X52(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X52mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_22X30(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X30mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_22X45(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X45mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_35X40(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X40mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_30X30(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X30mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_22X50(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X50mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_25X25(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X25mm(DiameterXLength)</description>
</package>
<package name="WCAP-AI3H_30X25(DXL)">
<description>&lt;B&gt;WCAP-AI3H Aluminum Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X25mm(DiameterXLength)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AI3H_35X25" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_35X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141386015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141386015.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="889.94uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141386015 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ250221M400DSIC2C000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_22X25" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_22X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141483001.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="524.79uA"/>
<attribute name="I-RIPPLE" value="520mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141483001 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN250680M450DSIC3C000"/>
<attribute name="VALUE" value="68uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_25X40" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_25X40(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141484012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141484012.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="853.81uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141484012 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO400181M450DSIC3C000"/>
<attribute name="VALUE" value="180uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_30X50" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_30X50(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141485019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141485019.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="1156.07uA"/>
<attribute name="I-RIPPLE" value="1450mA"/>
<attribute name="L" value="50mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141485019 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP500331M450DSIC2C000"/>
<attribute name="VALUE" value="330uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_35X55" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_35X55(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141486025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141486025.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1505.99uA"/>
<attribute name="I-RIPPLE" value="2150mA"/>
<attribute name="L" value="55mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141486025 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ550561M450DSIC2C000"/>
<attribute name="VALUE" value="560uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861141486026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141486026.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1659.52uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="L" value="55mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141486026 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ550681M450DSIC2C000"/>
<attribute name="VALUE" value="680uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_25X35" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_25X35(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140784012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861140784012.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="1367.88uA"/>
<attribute name="I-RIPPLE" value="2270mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861140784012 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDO350332M063DSIC3C000"/>
<attribute name="VALUE" value="3300uF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_861141484011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141484011.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="779.42uA"/>
<attribute name="I-RIPPLE" value="880mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141484011 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO350151M450DSIC3C000"/>
<attribute name="VALUE" value="150uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_35X65" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_35X65(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141386028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141386028.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1897.37uA"/>
<attribute name="I-RIPPLE" value="2650mA"/>
<attribute name="L" value="65mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141386028 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ650102M400DSIC2C000"/>
<attribute name="VALUE" value="1000uF"/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_35X50" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) W��rth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_35X50(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141486024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141486024.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1379.67uA"/>
<attribute name="I-RIPPLE" value="1850mA"/>
<attribute name="L" value="50mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141486024 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ500471M450DSIC2C000"/>
<attribute name="VALUE" value="470uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_35X35" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_35X35(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141486021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141486021.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1045.71uA"/>
<attribute name="I-RIPPLE" value="1280mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141486021 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ350271M450DSIC2C000"/>
<attribute name="VALUE" value="270uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_22X40" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_22X40(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141483004.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="697.14uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141483004 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN400121M450DSIC3C000"/>
<attribute name="VALUE" value="120uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_22X35" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_22X35(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140783006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861140783006.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="1116.87uA"/>
<attribute name="I-RIPPLE" value="1820mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861140783006 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDN350222M063DSIC3C000"/>
<attribute name="VALUE" value="2200uF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_861141483003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141483003.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="636.4uA"/>
<attribute name="I-RIPPLE" value="690mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141483003 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN350101M450DSIC3C000"/>
<attribute name="VALUE" value="100uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_30X40" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;&lt;br&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
        
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2020-04-23
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="_PINLENGTH_4MM" package="WCAP-AI3H_30X40(DXL)_PINLENGTH_4MM">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141485033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141485033.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="1380uA"/>
<attribute name="I-RIPPLE" value="1940mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141485033 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDP400471M450DSIC2D0T2"/>
<attribute name="VALUE" value="470uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
<device name="_PINLENGTH_6MM" package="WCAP-AI3H_30X40(DXL)_PINLENGTH_6MM">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141485018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141485018.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="1045.71uA"/>
<attribute name="I-RIPPLE" value="1280mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141485018 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP400271M450DSIC2C000"/>
<attribute name="VALUE" value="270uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_25X45" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_25X45(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141484013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141484013.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="943.93uA"/>
<attribute name="I-RIPPLE" value="1120mA"/>
<attribute name="L" value="45mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141484013 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO450221M450DSIC3C000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_25X30" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_25X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141084008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141084008.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="919.78uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141084008 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDO300471M200DSIC3C000"/>
<attribute name="VALUE" value="470uF"/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_861141484009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141484009.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="636.4uA"/>
<attribute name="I-RIPPLE" value="690mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141484009 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO300101M450DSIC3C000"/>
<attribute name="VALUE" value="100uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861141484010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141484010.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="697.14uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141484010 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO300121M450DSIC3C000"/>
<attribute name="VALUE" value="120uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_35X30" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_35X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140786018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861140786018.pdf"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1632.45uA"/>
<attribute name="I-RIPPLE" value="2830mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861140786018 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDQ300472M063DSIC2C000"/>
<attribute name="VALUE" value="4700uF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_861141486020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141486020.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="943.93uA"/>
<attribute name="I-RIPPLE" value="1120mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141486020 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ300221M450DSIC2C000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_30X35" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_30X35(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141085021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141085021.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="1341.64uA"/>
<attribute name="I-RIPPLE" value="2300mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141085021 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDP350102M200DSIC2C000"/>
<attribute name="VALUE" value="1000uF"/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_861141485017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141485017.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="943.93uA"/>
<attribute name="I-RIPPLE" value="1120mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141485017 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP350221M450DSIC2C000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_35X52" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu, 2020-03-20
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_35X52(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861140786024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861140786024.pdf"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="2381.18uA"/>
<attribute name="I-RIPPLE" value="4690mA"/>
<attribute name="L" value="52mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861140786024 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDQ520103M063DSIC2C000"/>
<attribute name="VALUE" value="10000uF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_22X30" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR �� 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_22X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141483002.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="576.28uA"/>
<attribute name="I-RIPPLE" value="640mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141483002 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN300820M450DSIC3C000"/>
<attribute name="VALUE" value="82uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_22X45" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_22X45(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141483005.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="779.42uA"/>
<attribute name="I-RIPPLE" value="880mA"/>
<attribute name="L" value="45mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141483005 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN450151M450DSIC3C000"/>
<attribute name="VALUE" value="150uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_35X40" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_35X40(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141386025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141386025.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1300.77uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141386025 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ400471M400DSIC2C000"/>
<attribute name="VALUE" value="470uF"/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_861141486022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141486022.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1156.07uA"/>
<attribute name="I-RIPPLE" value="1450mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141486022 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ400331M450DSIC2C000"/>
<attribute name="VALUE" value="330uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861141486023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141486023.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1256.78uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141486023 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ400391M450DSIC2C000"/>
<attribute name="VALUE" value="390uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_30X30" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_30X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141085015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141085015.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="1106.35uA"/>
<attribute name="I-RIPPLE" value="1780mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141085015 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDP300681M200DSIC2C000"/>
<attribute name="VALUE" value="680uF"/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_861141485015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141485015.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="779.42uA"/>
<attribute name="I-RIPPLE" value="880mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141485015 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP300151M450DSIC2C000"/>
<attribute name="VALUE" value="150uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861141485016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141485016.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="853.81uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141485016 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP300181M450DSIC2C000"/>
<attribute name="VALUE" value="180uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_22X50" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_22X50(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141483006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141483006.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="853.81uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="L" value="50mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141483006 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN500181M450DSIC3C000"/>
<attribute name="VALUE" value="180uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861141483007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141483007.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="943.93uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="L" value="50mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141483007 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN500221M450DSIC3C000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_25X25" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_25X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141484008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141484008.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="576.28uA"/>
<attribute name="I-RIPPLE" value="640mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141484008 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO250820M450DSIC3C000"/>
<attribute name="VALUE" value="82uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AI3H_30X25" prefix="C">
<description>&lt;b&gt;WCAP-AI3H Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 68 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 3000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 25.0 up to 35.0 x 65.0 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life &amp; high operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14717v209%20Family_WCAP-AI3H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AI3H/"&gt;https://www.we-online.com/catalog/en/WCAP-AI3H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-17
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AI3H_30X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861141485014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861141485014.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="697.14uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C  up to+105°C"/>
<attribute name="PART-NUMBER" value=" 861141485014 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP250121M450DSIC2C000"/>
<attribute name="VALUE" value="120uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
