<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Aluminum Electrolytic Capacitors - Snap-In - WCAP-AIE8&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2026a, 2026-01-19&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-AIE8_D35L35">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X35(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D30L35">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X35(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D25L40">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X40(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D22L45">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X45(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D25L30">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X30(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D35L30">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X30(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D22L40">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X40(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D22L30">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X30(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D22L35">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X35(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D30L40">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X40(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D35L40">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X40(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D25L35">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X35(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D22L25">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;22X25(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D30L30">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X30(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D35L25">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X25(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D35L45">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X45(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D30L25">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X25(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D25L25">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;25X25(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D30L45">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;30X45(DiameterXLength), THT, 2pins</description>
</package>
<package name="WCAP-AIE8_D35L50">
<description>&lt;B&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;35X50(DiameterXLength), THT, 2pins</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AIE8_D35L35" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D35L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221386021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="1300.8uA"/>
<attribute name="I-RIPPLE" value="2710mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221386021 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="470 uF"/>
<attribute name="VR" value="400VDC"/>
</technology>
<technology name="_861221486021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="1156.1uA"/>
<attribute name="I-RIPPLE" value="2630mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221486021 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="330 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D30L35" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D30L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221485016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="1045.8uA"/>
<attribute name="I-RIPPLE" value="2290mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221485016 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="270 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D25L40" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D25L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221084017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="1341.7uA"/>
<attribute name="I-RIPPLE" value="3280mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221084017 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="1000 uF"/>
<attribute name="VR" value="200VDC"/>
</technology>
<technology name="_861221484011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="944uA"/>
<attribute name="I-RIPPLE" value="2020mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221484011 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D25L30" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D25L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861220784007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="1367.9uA"/>
<attribute name="I-RIPPLE" value="2740mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861220784007 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="3300 uF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_861221484008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="697.2uA"/>
<attribute name="I-RIPPLE" value="1170mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221484008 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="120 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861221484009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="779.5uA"/>
<attribute name="I-RIPPLE" value="1310mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221484009 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="150 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D22L40" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D22L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221483005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="779.5uA"/>
<attribute name="I-RIPPLE" value="1380mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221483005 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="150 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D35L30" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D35L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861220786020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="1963.6uA"/>
<attribute name="I-RIPPLE" value="4950mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861220786020 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="6800 uF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_861221486020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="1045.8uA"/>
<attribute name="I-RIPPLE" value="2410mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221486020 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="270 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D22L30" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D22L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221483003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="636.4uA"/>
<attribute name="I-RIPPLE" value="950mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221483003 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="100 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D22L35" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D22L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221483004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="697.2uA"/>
<attribute name="I-RIPPLE" value="1140mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221483004 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="120 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D30L40" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D30L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221485017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="1156.1uA"/>
<attribute name="I-RIPPLE" value="2650mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221485017 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="330 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D35L40" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D35L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221486022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="1256.8uA"/>
<attribute name="I-RIPPLE" value="3150mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221486022 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="390 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D22L45" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D22L45">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221483006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="853.9uA"/>
<attribute name="I-RIPPLE" value="1560mA"/>
<attribute name="LENGTH" value="45mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221483006 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D25L35" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D25L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221484010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="853.9uA"/>
<attribute name="I-RIPPLE" value="1510mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221484010 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D22L25" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D22L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221483001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="524.8uA"/>
<attribute name="I-RIPPLE" value="710mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221483001 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="68 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861221483002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="576.3uA"/>
<attribute name="I-RIPPLE" value="860mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221483002 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="82 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D30L30" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D30L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861220785014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="1632.5uA"/>
<attribute name="I-RIPPLE" value="3700mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861220785014 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="4700 uF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_861221385012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="890uA"/>
<attribute name="I-RIPPLE" value="1660mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221385012 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="400VDC"/>
</technology>
<technology name="_861221485014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="853.9uA"/>
<attribute name="I-RIPPLE" value="1450mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221485014 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861221485015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="944uA"/>
<attribute name="I-RIPPLE" value="1910mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221485015 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D35L25" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D35L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221486019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="944uA"/>
<attribute name="I-RIPPLE" value="1920mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221486019 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D35L45" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D35L45">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221486023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="1379.7uA"/>
<attribute name="I-RIPPLE" value="3310mA"/>
<attribute name="LENGTH" value="45mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221486023 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="470 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D30L25" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D30L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221485012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="697.2uA"/>
<attribute name="I-RIPPLE" value="1210mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221485012 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="120 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861221485013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="779.5uA"/>
<attribute name="I-RIPPLE" value="1340mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221485013 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="150 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D25L25" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D25L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221084006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="919.8uA"/>
<attribute name="I-RIPPLE" value="1990mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221084006 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="470 uF"/>
<attribute name="VR" value="200VDC"/>
</technology>
<technology name="_861221484007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="636.4uA"/>
<attribute name="I-RIPPLE" value="970mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221484007 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="100 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D30L45" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D30L45">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221485018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="1256.8uA"/>
<attribute name="I-RIPPLE" value="3030mA"/>
<attribute name="LENGTH" value="45mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221485018 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="390 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIE8_D35L50" prefix="C">
<description>&lt;b&gt;WCAP-AIE8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;

&lt;B&gt;Long Life +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;br&gt;
&lt;Br&gt;Long life applications (industry, medical)
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14718v209%20family-wcap-aie8-22x25.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIE8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIE8&lt;/a&gt;&lt;p&gt;
Updated by Ella 2026-01-19&lt;br&gt;
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIE8_D35L50">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861221486024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="3000h"/>
<attribute name="I-LEAK" value="1506uA"/>
<attribute name="I-RIPPLE" value="3580mA"/>
<attribute name="LENGTH" value="50mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 861221486024 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="560 uF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
