<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Aluminum Electrolytic Capacitors - Snap-In - WCAP-AIG5&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-09-08&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-AIG5_D22L46">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X46(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L32">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X32(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D22L51">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt;Aluminum Electrolytic Capacitors,22X51(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D25L31">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X31(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D30L41">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X41(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D30L26">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X26(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L45">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X45(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L27">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X27(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D22L36">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X36(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D22L41">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X41(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L50">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X50(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D30L30">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X30(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D25L36">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X36(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D25L41">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X41(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L30">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X30(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L42">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X42(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D25L25">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X25(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L35">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X35(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D25L46">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X46(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D30L31">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt;Aluminum Electrolytic Capacitors,30X31(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D22L31">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X31(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L60">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X60(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L52">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X52(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D30L25">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X25(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D22L26">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X26(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L37">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X37(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D30L36">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt;Aluminum Electrolytic Capacitors,30X36(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D30L51">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X51(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D25L26">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X26(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L47">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X47(DiameterXLength)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AIG5_D22L46" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D22L46">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483007">
<attribute name="C" value="120 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021483007?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1080uA"/>
<attribute name="I-RIPPLE" value="820mA"/>
<attribute name="LENGTH" value="46mm"/>
<attribute name="PART-NUMBER" value="861021483007"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="120 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L32" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L32">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486028">
<attribute name="C" value="180 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021486028?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1620uA"/>
<attribute name="I-RIPPLE" value="1140mA"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="PART-NUMBER" value="861021486028"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="180 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D22L51" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D22L51">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483008">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021483008?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="960mA"/>
<attribute name="LENGTH" value="51mm"/>
<attribute name="PART-NUMBER" value="861021483008"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D25L31" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D25L31">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484011">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021484011?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="612uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="861021484011"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861021484012">
<attribute name="C" value="82 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021484012?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="738uA"/>
<attribute name="I-RIPPLE" value="640mA"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="861021484012"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="82 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861021484013">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021484013?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="900uA"/>
<attribute name="I-RIPPLE" value="740mA"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="861021484013"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D30L41" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D30L41">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021485024">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021485024?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1980uA"/>
<attribute name="I-RIPPLE" value="1240mA"/>
<attribute name="LENGTH" value="41mm"/>
<attribute name="PART-NUMBER" value="861021485024"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D30L26" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D30L26">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021485018">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021485018?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="612uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="861021485018"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861021485019">
<attribute name="C" value="82 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021485019?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="738uA"/>
<attribute name="I-RIPPLE" value="640mA"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="861021485019"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="82 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L45" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L45">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861020786030">
<attribute name="C" value="10000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861020786030?ae"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="12600uA"/>
<attribute name="I-RIPPLE" value="5510mA"/>
<attribute name="LENGTH" value="45mm"/>
<attribute name="PART-NUMBER" value="861020786030"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="10000 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L27" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L27">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486027">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021486027?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="960mA"/>
<attribute name="LENGTH" value="27mm"/>
<attribute name="PART-NUMBER" value="861021486027"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D22L36" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D22L36">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483004">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021483004?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="612uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="LENGTH" value="36mm"/>
<attribute name="PART-NUMBER" value="861021483004"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861021483005">
<attribute name="C" value="82 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021483005?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="738uA"/>
<attribute name="I-RIPPLE" value="640mA"/>
<attribute name="LENGTH" value="36mm"/>
<attribute name="PART-NUMBER" value="861021483005"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="82 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D22L41" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D22L41">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483006">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021483006?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="900uA"/>
<attribute name="I-RIPPLE" value="740mA"/>
<attribute name="LENGTH" value="41mm"/>
<attribute name="PART-NUMBER" value="861021483006"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D30L30" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D30L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861020785017">
<attribute name="C" value="3300 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861020785017?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="4158uA"/>
<attribute name="I-RIPPLE" value="2480mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="861020785017"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="3300 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_861021085019">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021085019?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2720uA"/>
<attribute name="I-RIPPLE" value="2040mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="861021085019"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L50" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L50">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_S861021486042">
<attribute name="C" value="560 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/S861021486042?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1506uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="LENGTH" value="50mm"/>
<attribute name="PART-NUMBER" value="S861021486042"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="560 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D25L36" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D25L36">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484014">
<attribute name="C" value="120 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021484014?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1080uA"/>
<attribute name="I-RIPPLE" value="820mA"/>
<attribute name="LENGTH" value="36mm"/>
<attribute name="PART-NUMBER" value="861021484014"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="120 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D25L41" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D25L41">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484015">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021484015?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="960mA"/>
<attribute name="LENGTH" value="41mm"/>
<attribute name="PART-NUMBER" value="861021484015"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L30" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861020786024">
<attribute name="C" value="4700 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861020786024?ae"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="5922uA"/>
<attribute name="I-RIPPLE" value="3430mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="861020786024"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="4700 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_861021086027">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021086027?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="4000uA"/>
<attribute name="I-RIPPLE" value="2480mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PART-NUMBER" value="861021086027"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L42" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L42">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486030">
<attribute name="C" value="270 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021486030?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2430uA"/>
<attribute name="I-RIPPLE" value="1480mA"/>
<attribute name="LENGTH" value="42mm"/>
<attribute name="PART-NUMBER" value="861021486030"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="270 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D25L25" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D25L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021084013">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021084013?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1880uA"/>
<attribute name="I-RIPPLE" value="1390mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="861021084013"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L35" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021386031">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021386031?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3760uA"/>
<attribute name="I-RIPPLE" value="1760mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PART-NUMBER" value="861021386031"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D25L46" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D25L46">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484016">
<attribute name="C" value="180 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021484016?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1620uA"/>
<attribute name="I-RIPPLE" value="1140mA"/>
<attribute name="LENGTH" value="46mm"/>
<attribute name="PART-NUMBER" value="861021484016"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="180 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861021484017">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021484017?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1980uA"/>
<attribute name="I-RIPPLE" value="1240mA"/>
<attribute name="LENGTH" value="46mm"/>
<attribute name="PART-NUMBER" value="861021484017"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D30L31" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D30L31">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021485020">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021485020?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="900uA"/>
<attribute name="I-RIPPLE" value="740mA"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="861021485020"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861021485021">
<attribute name="C" value="120 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021485021?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1080uA"/>
<attribute name="I-RIPPLE" value="820mA"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="861021485021"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="120 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D22L31" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D22L31">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483002">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021483002?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="423uA"/>
<attribute name="I-RIPPLE" value="350mA"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="861021483002"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861021483003">
<attribute name="C" value="56 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021483003?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="504uA"/>
<attribute name="I-RIPPLE" value="410mA"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="861021483003"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L60" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L60">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021386035">
<attribute name="C" value="1000 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021386035?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="8000uA"/>
<attribute name="I-RIPPLE" value="2850mA"/>
<attribute name="LENGTH" value="60mm"/>
<attribute name="PART-NUMBER" value="861021386035"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D30L25" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D30L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021385017">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021385017?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1760uA"/>
<attribute name="I-RIPPLE" value="1110mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value="861021385017"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L52" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L52">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486032">
<attribute name="C" value="390 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021486032?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3510uA"/>
<attribute name="I-RIPPLE" value="1860mA"/>
<attribute name="LENGTH" value="52mm"/>
<attribute name="PART-NUMBER" value="861021486032"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="390 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D22L26" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D22L26">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483001">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021483001?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="297uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="861021483001"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L37" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L37">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486029">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021486029?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1980uA"/>
<attribute name="I-RIPPLE" value="1240mA"/>
<attribute name="LENGTH" value="37mm"/>
<attribute name="PART-NUMBER" value="861021486029"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D30L36" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D30L36">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021485022">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021485022?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="960mA"/>
<attribute name="LENGTH" value="36mm"/>
<attribute name="PART-NUMBER" value="861021485022"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861021485023">
<attribute name="C" value="180 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021485023?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1620uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="LENGTH" value="36mm"/>
<attribute name="PART-NUMBER" value="861021485023"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="180 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D30L51" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D30L51">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021485025">
<attribute name="C" value="270 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021485025?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2430uA"/>
<attribute name="I-RIPPLE" value="1480mA"/>
<attribute name="LENGTH" value="51mm"/>
<attribute name="PART-NUMBER" value="861021485025"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="270 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861021485026">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021485026?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2970uA"/>
<attribute name="I-RIPPLE" value="1640mA"/>
<attribute name="LENGTH" value="51mm"/>
<attribute name="PART-NUMBER" value="861021485026"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D25L26" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D25L26">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484009">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021484009?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="423uA"/>
<attribute name="I-RIPPLE" value="350mA"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="861021484009"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861021484010">
<attribute name="C" value="56 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021484010?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="504uA"/>
<attribute name="I-RIPPLE" value="410mA"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="861021484010"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L47" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C
&lt;BR&gt;High permissible ripple current
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;High operating temperature applications
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14719v209%20family-wcap-aig5-22x31.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG5/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-AIG5&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-09-08
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L47">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486031">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861021486031?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2970uA"/>
<attribute name="I-RIPPLE" value="1640mA"/>
<attribute name="LENGTH" value="47mm"/>
<attribute name="PART-NUMBER" value="861021486031"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
