<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-AIG5&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-17&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-AIG5_35X60(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X60(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_35X45(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X45(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_25X41(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X41(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_25X36(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X36(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_35X27(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X27(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_35X52(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X52(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_35X35(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X35(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_35X32(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X32(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_35X42(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X42(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_35X47(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X47(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_35X37(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X37(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_25X31(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X31(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_35X30(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X30(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_30X41(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X41(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_30X51(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X51(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_30X31(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt;Aluminum Electrolytic Capacitors,30X31(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_30X30(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X30(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_25X25(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X25(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_30X25(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X25(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_22X36(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X36(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_25X46(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X46(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_30X36(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt;Aluminum Electrolytic Capacitors,30X36(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_30X26(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X26(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_22X31(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X31(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_22X41(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X41(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_25X26(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X26(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_22X46(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X46(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_22X51(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt;Aluminum Electrolytic Capacitors,22X51(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_22X26(DXL)">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X26(DiameterXLength)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AIG5_35X60" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_35X60(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021386035">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021386035.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="2850mA"/>
<attribute name="L" value="60mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021386035 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ600102M400DSIC2B000"/>
<attribute name="VALUE" value="1000uF"/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_35X45" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_35X45(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861020786030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861020786030.pdf"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="30uA"/>
<attribute name="I-RIPPLE" value="5510mA"/>
<attribute name="L" value="45mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861020786030 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDQ450103M063DSIC2B000"/>
<attribute name="VALUE" value="10000uF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_25X41" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_25X41(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021484015.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="960mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021484015 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO410151M450DSIC3B000"/>
<attribute name="VALUE" value="150uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_25X36" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_25X36(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021484014.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="820mA"/>
<attribute name="L" value="36mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021484014 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO360121M450DSIC3B000"/>
<attribute name="VALUE" value="120uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_35X27" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_35X27(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021486027.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="960mA"/>
<attribute name="L" value="27mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021486027 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ270151M450DSIC2B000"/>
<attribute name="VALUE" value="150uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_35X52" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_35X52(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486032">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021486032.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="1860mA"/>
<attribute name="L" value="52mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021486032 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ520391M450DSIC2B000"/>
<attribute name="VALUE" value="390uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_35X32" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_35X32(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021486028.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="1140mA"/>
<attribute name="L" value="32mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021486028 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ320181M450DSIC2B000"/>
<attribute name="VALUE" value="180uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_35X42" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_35X42(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021486030.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="1480mA"/>
<attribute name="L" value="42mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021486030 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ420271M450DSIC2B000"/>
<attribute name="VALUE" value="270uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_35X47" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_35X47(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021486031.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="1640mA"/>
<attribute name="L" value="47mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021486031 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ470331M450DSIC2B000"/>
<attribute name="VALUE" value="330uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_35X35" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_35X35(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021386031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021386031.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="1760mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021386031 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ350471M400DSIC2B000"/>
<attribute name="VALUE" value="470uF"/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_25X31" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_25X31(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021484011.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021484011 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO310680M450DSIC3B000"/>
<attribute name="VALUE" value="68uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861021484012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021484012.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="640mA"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021484012 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO310820M450DSIC3B000"/>
<attribute name="VALUE" value="82uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861021484013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021484013.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="740mA"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021484013 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO310101M450DSIC3B000"/>
<attribute name="VALUE" value="100uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_30X41" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_30X41(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021485024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021485024.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="1240mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021485024 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP410221M450DSIC2B000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_35X37" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_35X37(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021486029.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="1240mA"/>
<attribute name="L" value="37mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021486029 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJQ370221M450DSIC2B000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_30X31" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_30X31(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021485020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021485020.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="740mA"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021485020 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP310101M450DSIC2B000"/>
<attribute name="VALUE" value="100uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861021485021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021485021.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="820mA"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021485021 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP310121M450DSIC2B000"/>
<attribute name="VALUE" value="120uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_30X30" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_30X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861020785017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861020785017.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="2480mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861020785017 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDP300332M063DSIC2B000"/>
<attribute name="VALUE" value="3300uF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_861021085019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021085019.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="15uA"/>
<attribute name="I-RIPPLE" value="2040mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021085019 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDP300681M200DSIC2B000"/>
<attribute name="VALUE" value="680uF"/>
<attribute name="VR" value="200V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_30X25" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_30X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021385017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021385017.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="1110mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021385017 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP250221M400DSIC2B000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_25X25" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_25X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021084013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021084013.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="15uA"/>
<attribute name="I-RIPPLE" value="1390mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021084013 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDO250471M200DSIC3B000"/>
<attribute name="VALUE" value="470uF"/>
<attribute name="VR" value="200V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_30X51" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_30X51(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021485025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021485025.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="1480mA"/>
<attribute name="L" value="51mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021485025 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP510271M450DSIC2B000"/>
<attribute name="VALUE" value="270uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861021485026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021485026.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="1640mA"/>
<attribute name="L" value="51mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021485026 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP510331M450DSIC2B000"/>
<attribute name="VALUE" value="330uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_22X36" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_22X36(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021483004.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="36mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021483004 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN360680M450DSIC3B000"/>
<attribute name="VALUE" value="68uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861021483005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021483005.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="640mA"/>
<attribute name="L" value="36mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021483005 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN360820M450DSIC3B000"/>
<attribute name="VALUE" value="82uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_25X46" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_25X46(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021484016.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="1140mA"/>
<attribute name="L" value="46mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021484016 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO460181M450DSIC3B000"/>
<attribute name="VALUE" value="180uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861021484017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021484017.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="1240mA"/>
<attribute name="L" value="46mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021484017 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO460221M450DSIC3B000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_30X36" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_30X36(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021485022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021485022.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="960mA"/>
<attribute name="L" value="36mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021485022 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP360151M450DSIC2B000"/>
<attribute name="VALUE" value="150uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861021485023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021485023.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="L" value="36mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021485023 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP360181M450DSIC2B000"/>
<attribute name="VALUE" value="180uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_30X26" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_30X26(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021485018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021485018.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021485018 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP260680M450DSIC2B000"/>
<attribute name="VALUE" value="68uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861021485019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021485019.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="640mA"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021485019 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJP260820M450DSIC2B000"/>
<attribute name="VALUE" value="82uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_22X31" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_22X31(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021483002.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="350mA"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021483002 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN310470M450DSIC3B000"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861021483003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021483003.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="410mA"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021483003 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN310560M450DSIC3B000"/>
<attribute name="VALUE" value="56uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_22X41" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_22X41(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021483006.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="740mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021483006 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN410101M450DSIC3B000"/>
<attribute name="VALUE" value="100uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_35X30" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_35X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861020786024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861020786024.pdf"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="30uA"/>
<attribute name="I-RIPPLE" value="3430mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861020786024 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDQ300472M063DSIC2B000"/>
<attribute name="VALUE" value="4700uF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_861021086027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021086027.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="15uA"/>
<attribute name="I-RIPPLE" value="2480mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 40°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021086027 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANDQ300102M200DSIC2B000"/>
<attribute name="VALUE" value="1000uF"/>
<attribute name="VR" value="200V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_25X26" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_25X26(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021484009.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="350mA"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021484009 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO260470M450DSIC3B000"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861021484010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021484010.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="410mA"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021484010 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJO260560M450DSIC3B000"/>
<attribute name="VALUE" value="56uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_22X51" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_22X51(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021483008.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="960mA"/>
<attribute name="L" value="51mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021483008 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN510151M450DSIC3B000"/>
<attribute name="VALUE" value="150uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_22X46" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_22X46(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021483007.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="820mA"/>
<attribute name="L" value="46mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021483007 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN460121M450DSIC3B000"/>
<attribute name="VALUE" value="120uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_22X26" prefix="C">
<description>&lt;b&gt;WCAP-AIG5 Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 33 µF ‒ 10000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 35.0 x 60.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14719v209%20Family_WCAP-AIG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG5/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-017
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_22X26(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861021483001.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="20uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="- 25°C   up to105°C"/>
<attribute name="PART-NUMBER" value=" 861021483001 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANJN260330M450DSIC3B000"/>
<attribute name="VALUE" value="33uF"/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
