<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<library>
<description>Würth Elektronik - Passive Components - Capacitors - Aluminum Electrolytic Capacitors - Snap-In - WCAP-AIG5

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026a, 2026-07-27
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-AIG5_D35L30">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X30(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D25L45">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=25mmX45mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D25L35">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=25mmX35mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D30L40">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=30mmX40mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D22L35">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=22mmX35mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D35L25">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=35mmX25mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D30L50">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=30mmX50mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D25L40">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=25mmX40mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D22L45">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=22mmX45mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D22L40">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=22mmX40mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D25L30">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=25mmX30mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D30L25">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X25(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D22L25">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=22mmX25mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D22L30">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=22mmX30mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D35L35">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X35(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L40">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=35mmX40mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D25L25">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X25(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L45">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X45(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L50">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=35mmX50mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D22L50">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors

DiameterXLength=22mmX50mm,THT,2pins</description>
</package>
<package name="WCAP-AIG5_D30L30">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X30(DiameterXLength)</description>
</package>
<package name="WCAP-AIG5_D35L60">
<description>&lt;B&gt;WCAP-AIG5&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X60(DiameterXLength)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AIG5_D35L30" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861020786024">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861020786024?ae"/>
<attribute name="C" value="4700 uF"/>
<attribute name="DF" value="30 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="5922 uA"/>
<attribute name="I-RIPPLE" value="3430 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="PART-NUMBER" value="861020786024"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="4700 uF"/>
<attribute name="VR" value="63 V (DC)"/>
</technology>
<technology name="_861021086027">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021086027?ae"/>
<attribute name="C" value="1000 uF"/>
<attribute name="DF" value="15 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="4000 uA"/>
<attribute name="I-RIPPLE" value="2580 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="PART-NUMBER" value="861021086027"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="1000 uF"/>
<attribute name="VR" value="200 V (DC)"/>
</technology>
<technology name="_861021486028">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021486028?ae"/>
<attribute name="C" value="180 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1620 uA"/>
<attribute name="I-RIPPLE" value="1280 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="PART-NUMBER" value="861021486028"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D25L45" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D25L45">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484016">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021484016?ae"/>
<attribute name="C" value="180 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1620 uA"/>
<attribute name="I-RIPPLE" value="1240 mA"/>
<attribute name="LENGTH" value="45 mm"/>
<attribute name="PART-NUMBER" value="861021484016"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861021484017">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021484017?ae"/>
<attribute name="C" value="220 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1980 uA"/>
<attribute name="I-RIPPLE" value="1330 mA"/>
<attribute name="LENGTH" value="45 mm"/>
<attribute name="PART-NUMBER" value="861021484017"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D25L35" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D25L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484014">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021484014?ae"/>
<attribute name="C" value="120 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1080 uA"/>
<attribute name="I-RIPPLE" value="930 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="PART-NUMBER" value="861021484014"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="120 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D30L40" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D30L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021485024">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021485024?ae"/>
<attribute name="C" value="220 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1980 uA"/>
<attribute name="I-RIPPLE" value="1410 mA"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="PART-NUMBER" value="861021485024"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D22L35" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D22L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483004">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021483004?ae"/>
<attribute name="C" value="68 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="612 uA"/>
<attribute name="I-RIPPLE" value="620 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="PART-NUMBER" value="861021483004"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="68 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861021483005">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021483005?ae"/>
<attribute name="C" value="82 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="738 uA"/>
<attribute name="I-RIPPLE" value="770 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="PART-NUMBER" value="861021483005"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="82 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L25" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486027">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021486027?ae"/>
<attribute name="C" value="150 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1350 uA"/>
<attribute name="I-RIPPLE" value="1080 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="PART-NUMBER" value="861021486027"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="150 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D30L50" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D30L50">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021485025">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021485025?ae"/>
<attribute name="C" value="270 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2430 uA"/>
<attribute name="I-RIPPLE" value="1670 mA"/>
<attribute name="LENGTH" value="50 mm"/>
<attribute name="PART-NUMBER" value="861021485025"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="270 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861021485026">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021485026?ae"/>
<attribute name="C" value="330 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2970 uA"/>
<attribute name="I-RIPPLE" value="1860 mA"/>
<attribute name="LENGTH" value="50 mm"/>
<attribute name="PART-NUMBER" value="861021485026"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="330 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D25L40" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D25L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484015">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021484015?ae"/>
<attribute name="C" value="150 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1350 uA"/>
<attribute name="I-RIPPLE" value="1040 mA"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="PART-NUMBER" value="861021484015"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="150 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D22L45" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D22L45">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483007">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021483007?ae"/>
<attribute name="C" value="120 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1080 uA"/>
<attribute name="I-RIPPLE" value="960 mA"/>
<attribute name="LENGTH" value="45 mm"/>
<attribute name="PART-NUMBER" value="861021483007"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="120 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D22L40" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D22L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483006">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021483006?ae"/>
<attribute name="C" value="100 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="900 uA"/>
<attribute name="I-RIPPLE" value="860 mA"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="PART-NUMBER" value="861021483006"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="100 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D25L30" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D25L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021484011">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021484011?ae"/>
<attribute name="C" value="68 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="612 uA"/>
<attribute name="I-RIPPLE" value="500 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="PART-NUMBER" value="861021484011"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="68 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861021484012">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021484012?ae"/>
<attribute name="C" value="82 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="738 uA"/>
<attribute name="I-RIPPLE" value="780 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="PART-NUMBER" value="861021484012"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="82 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861021484013">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021484013?ae"/>
<attribute name="C" value="100 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="900 uA"/>
<attribute name="I-RIPPLE" value="820 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="PART-NUMBER" value="861021484013"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="100 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D30L25" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D30L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021385017">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021385017?ae"/>
<attribute name="C" value="220 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1760 uA"/>
<attribute name="I-RIPPLE" value="1110 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="PART-NUMBER" value="861021385017"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="400 V (DC)"/>
</technology>
<technology name="_861021485018">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021485018?ae"/>
<attribute name="C" value="68 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="612 uA"/>
<attribute name="I-RIPPLE" value="570 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="PART-NUMBER" value="861021485018"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="68 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861021485019">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021485019?ae"/>
<attribute name="C" value="82 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="738 uA"/>
<attribute name="I-RIPPLE" value="790 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="PART-NUMBER" value="861021485019"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="82 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861021485022">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021485022?ae"/>
<attribute name="C" value="150 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1350 uA"/>
<attribute name="I-RIPPLE" value="980 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="PART-NUMBER" value="861021485022"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="150 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861021485023">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021485023?ae"/>
<attribute name="C" value="180 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1620 uA"/>
<attribute name="I-RIPPLE" value="1100 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="PART-NUMBER" value="861021485023"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="180 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D22L25" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D22L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483001">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021483001?ae"/>
<attribute name="C" value="33 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="297 uA"/>
<attribute name="I-RIPPLE" value="360 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="PART-NUMBER" value="861021483001"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="33 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D22L30" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D22L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483002">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021483002?ae"/>
<attribute name="C" value="47 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="423 uA"/>
<attribute name="I-RIPPLE" value="420 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="PART-NUMBER" value="861021483002"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="47 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861021483003">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021483003?ae"/>
<attribute name="C" value="56 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="504 uA"/>
<attribute name="I-RIPPLE" value="490 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="PART-NUMBER" value="861021483003"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="56 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L35" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021386031">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021386031?ae"/>
<attribute name="C" value="470 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3760 uA"/>
<attribute name="I-RIPPLE" value="1950 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="PART-NUMBER" value="861021386031"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="470 uF"/>
<attribute name="VR" value="400 V (DC)"/>
</technology>
<technology name="_861021486029">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021486029?ae"/>
<attribute name="C" value="220 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1980 uA"/>
<attribute name="I-RIPPLE" value="1410 mA"/>
<attribute name="LENGTH" value="35 mm"/>
<attribute name="PART-NUMBER" value="861021486029"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="220 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L40" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486030">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021486030?ae"/>
<attribute name="C" value="270 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2430 uA"/>
<attribute name="I-RIPPLE" value="1630 mA"/>
<attribute name="LENGTH" value="40 mm"/>
<attribute name="PART-NUMBER" value="861021486030"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="270 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D25L25" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D25L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021084013">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021084013?ae"/>
<attribute name="C" value="470 uF"/>
<attribute name="DF" value="15 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1880 uA"/>
<attribute name="I-RIPPLE" value="1490 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="PART-NUMBER" value="861021084013"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="470 uF"/>
<attribute name="VR" value="200 V (DC)"/>
</technology>
<technology name="_861021484009">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021484009?ae"/>
<attribute name="C" value="47 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="423 uA"/>
<attribute name="I-RIPPLE" value="420 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="PART-NUMBER" value="861021484009"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="47 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861021484010">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021484010?ae"/>
<attribute name="C" value="56 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="25 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="504 uA"/>
<attribute name="I-RIPPLE" value="470 mA"/>
<attribute name="LENGTH" value="25 mm"/>
<attribute name="PART-NUMBER" value="861021484010"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="56 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L45" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L45">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861020786030">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861020786030?ae"/>
<attribute name="C" value="10000 uF"/>
<attribute name="DF" value="30 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="12600 uA"/>
<attribute name="I-RIPPLE" value="5510 mA"/>
<attribute name="LENGTH" value="45 mm"/>
<attribute name="PART-NUMBER" value="861020786030"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="10000 uF"/>
<attribute name="VR" value="63 V (DC)"/>
</technology>
<technology name="_861021486031">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021486031?ae"/>
<attribute name="C" value="330 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2970 uA"/>
<attribute name="I-RIPPLE" value="2070 mA"/>
<attribute name="LENGTH" value="45 mm"/>
<attribute name="PART-NUMBER" value="861021486031"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="330 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L50" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L50">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021486032">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021486032?ae"/>
<attribute name="C" value="390 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3510 uA"/>
<attribute name="I-RIPPLE" value="2270 mA"/>
<attribute name="LENGTH" value="50 mm"/>
<attribute name="PART-NUMBER" value="861021486032"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="390 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_S861021486042">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/S861021486042?ae"/>
<attribute name="C" value="560 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1506 uA"/>
<attribute name="I-RIPPLE" value="2800 mA"/>
<attribute name="LENGTH" value="50 mm"/>
<attribute name="PART-NUMBER" value="S861021486042"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="560 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D22L50" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D22L50">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021483008">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021483008?ae"/>
<attribute name="C" value="150 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="22 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1350 uA"/>
<attribute name="I-RIPPLE" value="1060 mA"/>
<attribute name="LENGTH" value="50 mm"/>
<attribute name="PART-NUMBER" value="861021483008"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="150 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D30L30" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D30L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861020785017">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861020785017?ae"/>
<attribute name="C" value="3300 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="4158 uA"/>
<attribute name="I-RIPPLE" value="2480 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="PART-NUMBER" value="861020785017"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="3300 uF"/>
<attribute name="VR" value="63 V (DC)"/>
</technology>
<technology name="_861021085019">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021085019?ae"/>
<attribute name="C" value="680 uF"/>
<attribute name="DF" value="15 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2720 uA"/>
<attribute name="I-RIPPLE" value="2150 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="PART-NUMBER" value="861021085019"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="680 uF"/>
<attribute name="VR" value="200 V (DC)"/>
</technology>
<technology name="_861021485020">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021485020?ae"/>
<attribute name="C" value="100 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="900 uA"/>
<attribute name="I-RIPPLE" value="900 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="PART-NUMBER" value="861021485020"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="100 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
<technology name="_861021485021">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021485021?ae"/>
<attribute name="C" value="120 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="30 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1080 uA"/>
<attribute name="I-RIPPLE" value="940 mA"/>
<attribute name="LENGTH" value="30 mm"/>
<attribute name="PART-NUMBER" value="861021485021"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="120 uF"/>
<attribute name="VR" value="450 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG5_D35L60" prefix="C">
<description>WCAP-AIG5 Aluminum Electrolytic Capacitors 
General Purpose +105 °C  

Characteristics
General purpose product series with max. operating temperature of +105 °C
High permissible ripple current
Mounting style: Snap-In
Recommended soldering: Wave soldering

Applications
High operating temperature applications
Filtering
Smoothing
Energy storage
e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter

Details see: www.we-online.com/en/components/products/WCAP-AIG5

Updated by Ella 2026-07-27
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG5_D35L60">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861021386035">
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/861021386035?ae"/>
<attribute name="C" value="1000 uF"/>
<attribute name="DF" value="20 %"/>
<attribute name="DIAMETER" value="35 mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="8000 uA"/>
<attribute name="I-RIPPLE" value="3410 mA"/>
<attribute name="LENGTH" value="60 mm"/>
<attribute name="PART-NUMBER" value="861021386035"/>
<attribute name="PITCH" value="10 mm"/>
<attribute name="VALUE" value="1000 uF"/>
<attribute name="VR" value="400 V (DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
