<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Aluminum Electrolytic Capacitors - Snap-In - WCAP-AIG8&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-07-25&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-AIG8_D25L30">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=25X30mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D40L35">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=40X35mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D22L25">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=22X25mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D22L30">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=22X30mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D30L35">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=30X35mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D25L40">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=25X40mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D30L30">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=30X30mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D25L25">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=25X25mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D35L40">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=35X40mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D35L35">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=35X35mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D35L25">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=35X25mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D25L35">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=25X35mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D30L45">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=30X45mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D25L50">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=25X50mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D22L35">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=22X35mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D35L30">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=35X30mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D40L40">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=40X40mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D30L40">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=30X40mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D22L40">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=22X40mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D25L20">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=25X20mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D35L45">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=35X45mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D25L45">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=25X45mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D22L50">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=22X50mm, 2pins, THT</description>
</package>
<package name="WCAP-AIG8_D40L50">
<description>&lt;B&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;DXL=40X50mm, 2pins, THT</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AIG8_D25L30" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D25L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861010784009">
<attribute name="C" value="3300 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861010784009?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="4158uA"/>
<attribute name="I-RIPPLE" value="3250mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861010784009"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="3300 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
<technology name="_861011084015">
<attribute name="C" value="680 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011084015?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2720uA"/>
<attribute name="I-RIPPLE" value="2980mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011084015"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
<technology name="_861011384014">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011384014?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1760uA"/>
<attribute name="I-RIPPLE" value="1720mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011384014"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
<technology name="_861011484009">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011484009?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="900uA"/>
<attribute name="I-RIPPLE" value="1060mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011484009"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D40L35" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D40L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011487025">
<attribute name="C" value="390 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011487025?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="40mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3510uA"/>
<attribute name="I-RIPPLE" value="2670mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011487025"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="390 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D22L25" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D22L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011483001">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011483001?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="423uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011483001"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D22L30" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D22L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011483002">
<attribute name="C" value="68 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011483002?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="612uA"/>
<attribute name="I-RIPPLE" value="750mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011483002"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861011483003">
<attribute name="C" value="82 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011483003?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="738uA"/>
<attribute name="I-RIPPLE" value="930mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011483003"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="82 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D30L35" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D30L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011485015">
<attribute name="C" value="180 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011485015?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1620uA"/>
<attribute name="I-RIPPLE" value="1580mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011485015"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="180 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D25L40" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D25L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011484011">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011484011?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="1740mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011484011"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D30L30" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D30L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011385023">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011385023?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2640uA"/>
<attribute name="I-RIPPLE" value="2050mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011385023"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
<technology name="_861011485014">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011485014?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="1470mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011485014"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D25L25" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D25L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011084009">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011084009?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1880uA"/>
<attribute name="I-RIPPLE" value="2080mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011084009"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
<technology name="_861011484008">
<attribute name="C" value="82 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011484008?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="738uA"/>
<attribute name="I-RIPPLE" value="900mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011484008"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="82 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D35L40" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D35L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011486023">
<attribute name="C" value="390 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011486023?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3510uA"/>
<attribute name="I-RIPPLE" value="2540mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011486023"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="390 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D35L35" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D35L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011086027">
<attribute name="C" value="1500 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011086027?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="6000uA"/>
<attribute name="I-RIPPLE" value="4770mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011086027"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="1500 µF"/>
<attribute name="VR" value="200VDC"/>
</technology>
<technology name="_861011386030">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011386030?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3760uA"/>
<attribute name="I-RIPPLE" value="2760mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011386030"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="400VDC"/>
</technology>
<technology name="_861011486020">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011486020?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1980uA"/>
<attribute name="I-RIPPLE" value="1920mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011486020"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861011486021">
<attribute name="C" value="270 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011486021?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2430uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011486021"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="270 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861011486022">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011486022?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2970uA"/>
<attribute name="I-RIPPLE" value="2290mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011486022"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D35L25" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D35L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861010786015">
<attribute name="C" value="4700 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861010786015?ae"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="5922uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861010786015"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="4700 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D25L35" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D25L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011484010">
<attribute name="C" value="120 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011484010?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1080uA"/>
<attribute name="I-RIPPLE" value="1340mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011484010"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="120 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D30L45" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D30L45">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011485017">
<attribute name="C" value="270 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011485017?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2430uA"/>
<attribute name="I-RIPPLE" value="2250mA"/>
<attribute name="LENGTH" value="45mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011485017"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="270 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861011485018">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011485018?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="2970uA"/>
<attribute name="I-RIPPLE" value="2290mA"/>
<attribute name="LENGTH" value="45mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011485018"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861011485019">
<attribute name="C" value="390 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011485019?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3510uA"/>
<attribute name="I-RIPPLE" value="2540mA"/>
<attribute name="LENGTH" value="45mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011485019"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="390 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D25L50" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D25L50">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011484013">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011484013?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1980uA"/>
<attribute name="I-RIPPLE" value="1820mA"/>
<attribute name="LENGTH" value="50mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011484013"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D35L30" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D35L30">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861010786021">
<attribute name="C" value="6800 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861010786021?ae"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="8568uA"/>
<attribute name="I-RIPPLE" value="5400mA"/>
<attribute name="LENGTH" value="30mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861010786021"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="6800 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D22L35" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D22L35">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011483004">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011483004?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="900uA"/>
<attribute name="I-RIPPLE" value="1030mA"/>
<attribute name="LENGTH" value="35mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011483004"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D40L40" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D40L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011487026">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011487026?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="40mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="4230uA"/>
<attribute name="I-RIPPLE" value="2890mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011487026"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D30L40" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D30L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011485016">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011485016?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1980uA"/>
<attribute name="I-RIPPLE" value="1860mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011485016"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D22L40" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D22L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011483005">
<attribute name="C" value="120 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011483005?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1080uA"/>
<attribute name="I-RIPPLE" value="1260mA"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011483005"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="120 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D25L20" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D25L20">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_S861011784003">
<attribute name="C" value="1100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/S861011784003?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="890uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="S861011784003"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="1100 µF"/>
<attribute name="VR" value="80VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D35L45" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D35L45">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011486024">
<attribute name="C" value="470 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011486024?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="4230uA"/>
<attribute name="I-RIPPLE" value="2890mA"/>
<attribute name="LENGTH" value="45mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011486024"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D25L45" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D25L45">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011484012">
<attribute name="C" value="180 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011484012?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1620uA"/>
<attribute name="I-RIPPLE" value="1570mA"/>
<attribute name="LENGTH" value="45mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011484012"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="180 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D22L50" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D22L50">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011483006">
<attribute name="C" value="150 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011483006?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="1690mA"/>
<attribute name="LENGTH" value="50mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011483006"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
<technology name="_861011483007">
<attribute name="C" value="180 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011483007?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="1620uA"/>
<attribute name="I-RIPPLE" value="1580mA"/>
<attribute name="LENGTH" value="50mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011483007"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="180 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_D40L50" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose +85 °C 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Mounting style: Snap-In
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;Energy storage
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14720v209%20family-wcap-aig8-_35x47.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
         
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AIG8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-AIG8&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_D40L50">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011487027">
<attribute name="C" value="560 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/861011487027?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="40mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="5040uA"/>
<attribute name="I-RIPPLE" value="3470mA"/>
<attribute name="LENGTH" value="50mm"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="861011487027"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="VALUE" value="560 µF"/>
<attribute name="VR" value="450VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
