<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-AIG8&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-04&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-AIG8_30X31(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X31(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_25X51(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X51(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_30X36(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X36(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_40X52(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,40X52(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_40X42(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,40X42(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_25X30(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X30(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_25X46(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X46(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_22X51(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X51(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_30X30(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X30(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_25X41(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X41(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_25X31(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X31(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_35X25(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X25(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_22X26(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X26(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_25X26(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X26(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_35X37(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X37(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_22X36(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X36(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_35X47(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X47(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_30X46(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X46(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_35X30(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X30(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_25X36(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X36(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_22X31(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X31(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_35X35(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X35(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_30X41(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,30X41(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_35X42(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,35X42(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_40X37(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,40X37(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_25X25(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,25X25(DiameterXLength)</description>
</package>
<package name="WCAP-AIG8_22X41(DXL)">
<description>&lt;B&gt;WCAP-AIG8&lt;/B&gt;&lt;BR&gt; Aluminum Electrolytic Capacitors,22X41(DiameterXLength)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AIG8_30X31" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_30X31(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011485014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011485014.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="1390mA"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011485014 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP310151M450DSIC2B000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_25X51" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_25X51(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011484013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011484013.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="1980uA"/>
<attribute name="I-RIPPLE" value="1760mA"/>
<attribute name="L" value="51mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011484013 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO510221M450DSIC3B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_40X52" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_40X52(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011487027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011487027.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="40mm"/>
<attribute name="I-LEAK" value="5040uA"/>
<attribute name="I-RIPPLE" value="3260mA"/>
<attribute name="L" value="52mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011487027 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAR520561M450DSIC1B000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_30X36" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_30X36(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011485015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011485015.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="1620uA"/>
<attribute name="I-RIPPLE" value="1520mA"/>
<attribute name="L" value="36mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011485015 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP360181M450DSIC2B000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_40X42" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_40X42(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011487026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011487026.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="40mm"/>
<attribute name="I-LEAK" value="4230uA"/>
<attribute name="I-RIPPLE" value="2890mA"/>
<attribute name="L" value="42mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011487026 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAR420471M450DSIC1B000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_25X46" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_25X46(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011484012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011484012.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="1620uA"/>
<attribute name="I-RIPPLE" value="1520mA"/>
<attribute name="L" value="46mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011484012 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO460181M450DSIC3B000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_22X51" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_22X51(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011483006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011483006.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="1390mA"/>
<attribute name="L" value="51mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011483006 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAN510151M450DSIC3B000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861011483007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011483007.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="1620uA"/>
<attribute name="I-RIPPLE" value="1520mA"/>
<attribute name="L" value="51mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011483007 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAN510181M450DSIC3B000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_30X30" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_30X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011385023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011385023.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="2640uA"/>
<attribute name="I-RIPPLE" value="2050mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011385023 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP300331M400DSIC2B000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_25X41" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_25X41(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011484011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011484011.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="1390mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011484011 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO410151M450DSIC3B000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_25X31" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_25X31(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011484009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011484009.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="900uA"/>
<attribute name="I-RIPPLE" value="1030mA"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011484009 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO310101M450DSIC3B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_22X26" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_22X26(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011483001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011483001.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="423uA"/>
<attribute name="I-RIPPLE" value="360mA"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011483001 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAN260470M450DSIC3B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_35X25" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_35X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861010786015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861010786015.pdf"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="5922uA"/>
<attribute name="I-RIPPLE" value="3280mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861010786015 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANBQ250472M063DSIC2B000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_35X37" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_35X37(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011486020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011486020.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="1980uA"/>
<attribute name="I-RIPPLE" value="1760mA"/>
<attribute name="L" value="37mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011486020 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ370221M450DSIC2B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861011486021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011486021.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="2430uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="37mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011486021 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ370271M450DSIC2B000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861011486022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011486022.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="2970uA"/>
<attribute name="I-RIPPLE" value="2290mA"/>
<attribute name="L" value="37mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011486022 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ370331M450DSIC2B000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_25X26" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_25X26(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011484008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011484008.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="738uA"/>
<attribute name="I-RIPPLE" value="890mA"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011484008 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO260820M450DSIC3B000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_25X30" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_25X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861010784009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861010784009.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="4158uA"/>
<attribute name="I-RIPPLE" value="3120mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861010784009 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANBO300332M063DSIC3B000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_861011084015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011084015.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="2720uA"/>
<attribute name="I-RIPPLE" value="2980mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011084015 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO300681M200DSIC3B000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_861011384014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011384014.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="1760uA"/>
<attribute name="I-RIPPLE" value="1550mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011384014 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO300221M400DSIC3B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_22X36" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_22X36(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011483004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011483004.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="900uA"/>
<attribute name="I-RIPPLE" value="1030mA"/>
<attribute name="L" value="36mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011483004 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAN360101M450DSIC3B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_35X47" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_35X47(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011486024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011486024.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="4230uA"/>
<attribute name="I-RIPPLE" value="2890mA"/>
<attribute name="L" value="47mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011486024 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ470471M450DSIC2B000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_30X46" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_30X46(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011485017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011485017.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="2430uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="46mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011485017 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP460271M450DSIC2B000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861011485018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011485018.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="2970uA"/>
<attribute name="I-RIPPLE" value="2290mA"/>
<attribute name="L" value="46mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011485018 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP460331M450DSIC2B000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861011485019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011485019.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="3510uA"/>
<attribute name="I-RIPPLE" value="2540mA"/>
<attribute name="L" value="46mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011485019 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP460391M450DSIC2B000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_25X36" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_25X36(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011484010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011484010.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="1080uA"/>
<attribute name="I-RIPPLE" value="1190mA"/>
<attribute name="L" value="36mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011484010 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO360121M450DSIC3B000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_22X31" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_22X31(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011483002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011483002.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="612uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011483002 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAN310680M450DSIC3B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_861011483003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011483003.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="738uA"/>
<attribute name="I-RIPPLE" value="890mA"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011483003 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAN310820M450DSIC3B000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_35X35" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_35X35(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011086027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011086027.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="6000uA"/>
<attribute name="I-RIPPLE" value="4770mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011086027 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ350152M200DSIC2B000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_861011386030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011386030.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="3760uA"/>
<attribute name="I-RIPPLE" value="2420mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011386030 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ350471M400DSIC2B000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_35X30" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_35X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861010786021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861010786021.pdf"/>
<attribute name="DF" value="30%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="8568uA"/>
<attribute name="I-RIPPLE" value="4320mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861010786021 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANBQ300682M063DSIC2B000"/>
<attribute name="VALUE" value="6800  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_30X41" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_30X41(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011485016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011485016.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="30mm"/>
<attribute name="I-LEAK" value="1980uA"/>
<attribute name="I-RIPPLE" value="1760mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011485016 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAP410221M450DSIC2B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_35X42" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_35X42(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011486023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011486023.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="35mm"/>
<attribute name="I-LEAK" value="3510uA"/>
<attribute name="I-RIPPLE" value="2540mA"/>
<attribute name="L" value="42mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011486023 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAQ420391M450DSIC2B000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_40X37" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_40X37(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011487025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011487025.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="40mm"/>
<attribute name="I-LEAK" value="3510uA"/>
<attribute name="I-RIPPLE" value="2540mA"/>
<attribute name="L" value="37mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011487025 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAR370391M450DSIC1B000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_25X25" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_25X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011084009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011084009.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="25mm"/>
<attribute name="I-LEAK" value="1880uA"/>
<attribute name="I-RIPPLE" value="2080mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011084009 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAO250471M200DSIC3B000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AIG8_22X41" prefix="C">
<description>&lt;b&gt;WCAP-AIG8 Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Mounting style: Snap-In 
&lt;BR&gt;Capacitance range: 47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 63 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 22.0 x 26.0 up to 40.0 x 52.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;e.g. Personal and industrial computer power supply, server power supply, drive circuit, DC/AC inverter
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;DXL=DiameterxLength&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14720v209%20Family_WCAP-AIG8.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AIG8/"&gt;https://www.we-online.com/catalog/en/WCAP-AIG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-04
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AIG8_22X41(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_861011483005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/861011483005.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="1080uA"/>
<attribute name="I-RIPPLE" value="1190mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 861011483005 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ANAN410121M450DSIC3B000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
