<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-AS5H&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020b, 2020-12-14&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-AS5H_6.3X7.7(DXL)">
<description>&lt;B&gt;WCAP-AS5H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X7.7X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-AS5H_6.3X5.5(DXL)">
<description>&lt;B&gt;WCAP-AS5H&lt;/B&gt;&lt;BR&gt;Aluminium Electrolytic Capacitors,6.3X5.5X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-AS5H_5X5.5(DXL)">
<description>&lt;B&gt;WCAP-AS5H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X5.5X1.4(DiameterXLengthXP)</description>
</package>
<package name="WCAP-AS5H_10X10.5(DXL)">
<description>&lt;B&gt;WCAP-AS5H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X10.5X4.5(DiameterXLengthXP)</description>
</package>
<package name="WCAP-AS5H_8X10.5(DXL)">
<description>&lt;B&gt;WCAP-AS5H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X10.5X3.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-AS5H_4X5.5(DXL)">
<description>&lt;B&gt;WCAP-AS5H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,4X5.5X1(DiameterXLengthXPitch)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AS5H_6.3X7.7" prefix="C">
<description>&lt;b&gt;WCAP-AS5H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55801v209%20Family_WCAP-AS5H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55801v209%20Family_WCAP-AS5H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AS5H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-AS5H&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-07-27
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AS5H_6.3X7.7(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865230145005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230145005?ae"/>
<attribute name="DF" value="32%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="7.7mm"/>
<attribute name="I-LEAK" value="13.86uA"/>
<attribute name="I-RIPPLE" value="110mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230145005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD077221M6R3DVCTCE000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865230245004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230245004?ae"/>
<attribute name="DF" value="28%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="7.7mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="79mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230245004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD077101M010DVCTCE000"/>
<attribute name="VALUE" value="100uF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865230345005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230345005?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="7.7mm"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="81mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230345005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD077101M016DVCTCE000"/>
<attribute name="VALUE" value="100uF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865230445005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230445005?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="7.7mm"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="63mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230445005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD077470M025DVCTCE000"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865230545004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230545004?ae"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="7.7mm"/>
<attribute name="I-LEAK" value="11.55uA"/>
<attribute name="I-RIPPLE" value="57mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230545004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD077330M035DVCTCE000"/>
<attribute name="VALUE" value="33uF"/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865230645010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230645010?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="7.7mm"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="52mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230645010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD077220M050DVCTCE000"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AS5H_6.3X5.5" prefix="C">
<description>&lt;b&gt;WCAP-AS5H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55801v209%20Family_WCAP-AS5H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55801v209%20Family_WCAP-AS5H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AS5H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-AS5H&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-07-27
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AS5H_6.3X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865230143004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230143004?ae"/>
<attribute name="DF" value="32%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="6.3uA"/>
<attribute name="I-RIPPLE" value="60mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230143004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD055101M6R3DVCTBE000"/>
<attribute name="VALUE" value="100uF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865230243003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230243003?ae"/>
<attribute name="DF" value="28%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="48mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230243003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD055470M010DVCTBE000"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865230343003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230343003?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="5.28uA"/>
<attribute name="I-RIPPLE" value="44mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230343003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD055330M016DVCTBE000"/>
<attribute name="VALUE" value="33uF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865230343004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230343004?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="7.52uA"/>
<attribute name="I-RIPPLE" value="50mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230343004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD055470M016DVCTBE000"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865230443003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230443003?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="5.5uA"/>
<attribute name="I-RIPPLE" value="40mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230443003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD055220M025DVCTBE000"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865230443004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230443004?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="8.25uA"/>
<attribute name="I-RIPPLE" value="48mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230443004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD055330M025DVCTBE000"/>
<attribute name="VALUE" value="33uF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865230543003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230543003?ae"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="7.7uA"/>
<attribute name="I-RIPPLE" value="42mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230543003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD055220M035DVCTBE000"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865230643009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230643009?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="30mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230643009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDD055100M050DVCTBE000"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AS5H_10X10.5" prefix="C">
<description>&lt;b&gt;WCAP-AS5H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55801v209%20Family_WCAP-AS5H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55801v209%20Family_WCAP-AS5H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AS5H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-AS5H&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-07-27
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AS5H_10X10.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865230157007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230157007?ae"/>
<attribute name="DF" value="32%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="29.61uA"/>
<attribute name="I-RIPPLE" value="260mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230157007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDF105471M6R3DVCTEE000"/>
<attribute name="VALUE" value="470uF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865230157008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230157008?ae"/>
<attribute name="DF" value="32%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="340mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230157008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDF105102M6R3DVCTEE000"/>
<attribute name="VALUE" value="1000uF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865230257006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230257006?ae"/>
<attribute name="DF" value="28%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230257006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDF105331M010DVCTEE000"/>
<attribute name="VALUE" value="330uF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865230257007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230257007?ae"/>
<attribute name="DF" value="28%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230257007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDF105471M010DVCTEE000"/>
<attribute name="VALUE" value="470uF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865230357006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230357006?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="216mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230357006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDF105221M016DVCTEE000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865230357007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230357007?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230357007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDF105331M016DVCTEE000"/>
<attribute name="VALUE" value="330uF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865230357008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230357008?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="320mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230357008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDF105471M016DVCTEE000"/>
<attribute name="VALUE" value="470uF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865230457007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230457007?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230457007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDF105221M025DVCTEE000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865230457008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230457008?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="375mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230457008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDF105331M025DVCTEE000"/>
<attribute name="VALUE" value="330uF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865230557006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230557006?ae"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="150mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230557006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDF105101M035DVCTEE000"/>
<attribute name="VALUE" value="100uF"/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865230557007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230557007?ae"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230557007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDF105221M035DVCTEE000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865230657013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230657013?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230657013 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDF105101M050DVCTEE000"/>
<attribute name="VALUE" value="100uF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865230657014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230657014?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="900mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230657014 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105331M050DVCTEE000"/>
<attribute name="VALUE" value="330uF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AS5H_8X10.5" prefix="C">
<description>&lt;b&gt;WCAP-AS5H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55801v209%20Family_WCAP-AS5H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55801v209%20Family_WCAP-AS5H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AS5H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-AS5H&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-07-27
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AS5H_8X10.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865230153006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230153006?ae"/>
<attribute name="DF" value="32%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230153006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDE105331M6R3DVCTEE000"/>
<attribute name="VALUE" value="330uF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865230253005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230253005?ae"/>
<attribute name="DF" value="28%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="140mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230253005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDE105221M010DVCTEE000"/>
<attribute name="VALUE" value="220uF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865230453006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230453006?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="116mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230453006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDE105101M025DVCTEE000"/>
<attribute name="VALUE" value="100uF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865230553005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230553005?ae"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="16.45uA"/>
<attribute name="I-RIPPLE" value="92mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230553005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDE105470M035DVCTEE000"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865230653011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230653011?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230653011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDE105330M050DVCTEE000"/>
<attribute name="VALUE" value="33uF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865230653012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230653012?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="95mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230653012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDE105470M050DVCTEE000"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AS5H_5X5.5" prefix="C">
<description>&lt;b&gt;WCAP-AS5H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55801v209%20Family_WCAP-AS5H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55801v209%20Family_WCAP-AS5H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AS5H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-AS5H&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-07-27
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AS5H_5X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865230142002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230142002?ae"/>
<attribute name="DF" value="32%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="32mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230142002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDC055330M6R3DVCTBE000"/>
<attribute name="VALUE" value="33uF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865230142003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230142003?ae"/>
<attribute name="DF" value="32%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="36mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230142003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDC055470M6R3DVCTBE000"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865230242001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230242001?ae"/>
<attribute name="DF" value="28%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="28mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230242001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDC055220M010DVCTBE000"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865230242002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230242002?ae"/>
<attribute name="DF" value="28%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="34mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230242002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDC055330M010DVCTBE000"/>
<attribute name="VALUE" value="33uF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_865230342002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230342002?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3.52uA"/>
<attribute name="I-RIPPLE" value="30mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230342002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDC055220M016DVCTBE000"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865230542002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230542002?ae"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3.5uA"/>
<attribute name="I-RIPPLE" value="25mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230542002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDC055100M035DVCTBE000"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865230642008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230642008?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="19mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230642008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDC0554R7M050DVCTBE000"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AS5H_4X5.5" prefix="C">
<description>&lt;b&gt;WCAP-AS5H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o55801v209%20Family_WCAP-AS5H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o55801v209%20Family_WCAP-AS5H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-AS5H/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-AS5H&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-07-27
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AS5H_4X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865230140001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230140001?ae"/>
<attribute name="DF" value="32%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="22mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230140001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDB055220M6R3DVCTAE000"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_865230340001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230340001?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="17mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230340001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDB055100M016DVCTAE000"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_865230440001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230440001?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="13mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230440001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDB0554R7M025DVCTAE000"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865230440002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230440002?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="23mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230440002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDB055100M025DVCTAE000"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_865230540001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230540001?ae"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="15mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230540001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDB0554R7M035DVCTAE000"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_865230640004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230640004?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="3.8mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230640004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDB055R47M050DVCTAE000"/>
<attribute name="VALUE" value="0.47uF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865230640005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230640005?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="6.2mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230640005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDB055010M050DVCTAE000"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865230640006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230640006?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="11mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230640006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDB0552R2M050DVCTAE000"/>
<attribute name="VALUE" value="2.2uf"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_865230640007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865230640007?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="14mA"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865230640007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDB0553R3M050DVCTAE000"/>
<attribute name="VALUE" value="3.3uF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
