<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Aluminum Electrolytic Capacitors - V-Chip SMT - WCAP-ASLU&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-10-30&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-ASLU_D8L6.5">
<description>&lt;B&gt;WCAP-ASLU&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X6.5X2.3(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLU_D6.3L7.7">
<description>&lt;B&gt;WCAP-ASLU&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X7.7X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLU_D12.5L16">
<description>&lt;B&gt;WCAP-ASLU Aluminium Electrolytic Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
DiameterXLengthXPitch=12.5X16X4.5mm</description>
</package>
<package name="WCAP-ASLU_D5L5.5">
<description>&lt;B&gt;WCAP-ASLU&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X5.5X1.4(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLU_D4L5.5">
<description>&lt;B&gt;WCAP-ASLU&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,4X5.5X1(DiameterXLengthXPitch)</description>
</package>
<package name="WCAP-ASLU_D3L5.5">
<description>&lt;B&gt;WCAP-ASLU&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,3X5.5X0.8(DiameterXLengthXPitch)</description>
</package>
<package name="WCAP-ASLU_D6.3L5.5">
<description>&lt;B&gt;WCAP-ASLU&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X5.5X2.1(DiameterXLengthXP)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-ASLU_D8L6.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLU Aluminum Electrolytic Capacitor &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current product series
&lt;BR&gt;Mounting style: V-Chip SMT
&lt;BR&gt;Recommended soldering: Reflow soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications and small handheld devices
&lt;BR&gt;Input and output capacitor for switched-mode power supply
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLU/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ASLU&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLU_D8L6.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865090149007">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090149007?ae"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="2.8uA"/>
<attribute name="I-RIPPLE" value="110mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865090149007"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="6.3VDC"/>
</technology>
<technology name="_865090149009">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090149009?ae"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="4.2uA"/>
<attribute name="I-RIPPLE" value="170mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865090149009"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="6.3VDC"/>
</technology>
<technology name="_865090249006">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090249006?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="2uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865090249006"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_865090249008">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090249008?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="4.4uA"/>
<attribute name="I-RIPPLE" value="135mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865090249008"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_865090349007">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090349007?ae"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="3.2uA"/>
<attribute name="I-RIPPLE" value="92mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865090349007"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_865090449007">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090449007?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="2.4uA"/>
<attribute name="I-RIPPLE" value="70mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865090449007"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_865090449009">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090449009?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="110mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865090449009"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_865090549007">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090549007?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="2.4uA"/>
<attribute name="I-RIPPLE" value="62mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865090549007"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_865090549009">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090549009?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865090549009"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_865090649011">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090649011?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="2.2uA"/>
<attribute name="I-RIPPLE" value="52mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865090649011"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_865090649013">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090649013?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="71mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865090649013"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_865090749001">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090749001?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="14uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="PART-NUMBER" value="865090749001"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="63VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLU_D6.3L7.7" prefix="C">
<description>&lt;b&gt;WCAP-ASLU Aluminum Electrolytic Capacitor &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current product series
&lt;BR&gt;Mounting style: V-Chip SMT
&lt;BR&gt;Recommended soldering: Reflow soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications and small handheld devices
&lt;BR&gt;Input and output capacitor for switched-mode power supply
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLU/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ASLU&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLU_D6.3L7.7">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865090145006">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090145006?ae"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="2.8uA"/>
<attribute name="I-RIPPLE" value="102mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865090145006"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="6.3VDC"/>
</technology>
<technology name="_865090145008">
<attribute name="C" value="330 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090145008?ae"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="4.2uA"/>
<attribute name="I-RIPPLE" value="155mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865090145008"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="6.3VDC"/>
</technology>
<technology name="_865090245005">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090245005?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="2uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865090245005"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_865090245007">
<attribute name="C" value="220 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090245007?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="4.4uA"/>
<attribute name="I-RIPPLE" value="125mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865090245007"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_865090345006">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090345006?ae"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="3.2uA"/>
<attribute name="I-RIPPLE" value="85mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865090345006"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_865090445006">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090445006?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="2.4uA"/>
<attribute name="I-RIPPLE" value="65mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865090445006"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_865090445008">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090445008?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="102mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865090445008"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_865090545006">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090545006?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="2.4uA"/>
<attribute name="I-RIPPLE" value="58mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865090545006"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_865090545008">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090545008?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865090545008"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_865090645010">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090645010?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="2.2uA"/>
<attribute name="I-RIPPLE" value="48mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865090645010"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_865090645012">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090645012?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="66mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value="865090645012"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLU_D4L5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLU Aluminum Electrolytic Capacitor &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current product series
&lt;BR&gt;Mounting style: V-Chip SMT
&lt;BR&gt;Recommended soldering: Reflow soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications and small handheld devices
&lt;BR&gt;Input and output capacitor for switched-mode power supply
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLU/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ASLU&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLU_D4L5.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865090140001">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090140001?ae"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="15mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090140001"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="6.3VDC"/>
</technology>
<technology name="_865090140002">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090140002?ae"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="28mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090140002"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="6.3VDC"/>
</technology>
<technology name="_865090140003">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090140003?ae"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.5uA"/>
<attribute name="I-RIPPLE" value="37mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090140003"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="6.3VDC"/>
</technology>
<technology name="_865090140004">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090140004?ae"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.6uA"/>
<attribute name="I-RIPPLE" value="45mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090140004"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="6.3VDC"/>
</technology>
<technology name="_865090240001">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090240001?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="23mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090240001"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_865090240002">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090240002?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.5uA"/>
<attribute name="I-RIPPLE" value="33mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090240002"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_865090340001">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090340001?ae"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="10mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090340001"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_865090340002">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090340002?ae"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="23mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090340002"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_865090440001">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090440001?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="10mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090440001"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_865090440002">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090440002?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="16mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090440002"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_865090440003">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090440003?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.5uA"/>
<attribute name="I-RIPPLE" value="27mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090440003"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_865090540001">
<attribute name="C" value="2.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090540001?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="8.4mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090540001"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_865090540002">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090540002?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="15mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090540002"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_865090540003">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090540003?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="18mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090540003"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_865090640004">
<attribute name="C" value="0.47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090640004?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="4mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090640004"/>
<attribute name="VALUE" value="0.47 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_865090640005">
<attribute name="C" value="1 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090640005?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="8.4mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090640005"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_865090640006">
<attribute name="C" value="2.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090640006?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="13mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090640006"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_865090640007">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090640007?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.4uA"/>
<attribute name="I-RIPPLE" value="17mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090640007"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLU_D5L5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLU Aluminum Electrolytic Capacitor &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current product series
&lt;BR&gt;Mounting style: V-Chip SMT
&lt;BR&gt;Recommended soldering: Reflow soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications and small handheld devices
&lt;BR&gt;Input and output capacitor for switched-mode power supply
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLU/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ASLU&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLU_D5L5.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865090142005">
<attribute name="C" value="100 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090142005?ae"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="1.3uA"/>
<attribute name="I-RIPPLE" value="70mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090142005"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="6.3VDC"/>
</technology>
<technology name="_865090242003">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090242003?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.7uA"/>
<attribute name="I-RIPPLE" value="41mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090242003"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_865090342003">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090342003?ae"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.8uA"/>
<attribute name="I-RIPPLE" value="37mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090342003"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_865090442004">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090442004?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="1.1uA"/>
<attribute name="I-RIPPLE" value="42mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090442004"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLU_D3L5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLU Aluminum Electrolytic Capacitor &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current product series
&lt;BR&gt;Mounting style: V-Chip SMT
&lt;BR&gt;Recommended soldering: Reflow soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications and small handheld devices
&lt;BR&gt;Input and output capacitor for switched-mode power supply
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLU/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ASLU&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLU_D3L5.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865090168010">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090168010?ae"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="25mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090168010"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="6.3VDC"/>
</technology>
<technology name="_865090268009">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090268009?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="18mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090268009"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_865090368008">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090368008?ae"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="20mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090368008"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_865090468010">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090468010?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="11mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090468010"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_865090468011">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090468011?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="15mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090468011"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLU_D6.3L5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLU Aluminum Electrolytic Capacitor &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current product series
&lt;BR&gt;Mounting style: V-Chip SMT
&lt;BR&gt;Recommended soldering: Reflow soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications and small handheld devices
&lt;BR&gt;Input and output capacitor for switched-mode power supply
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLU/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ASLU&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLU_D6.3L5.5">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865090243004">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090243004?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="1uA"/>
<attribute name="I-RIPPLE" value="52mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090243004"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="10VDC"/>
</technology>
<technology name="_865090343004">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090343004?ae"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="1.1uA"/>
<attribute name="I-RIPPLE" value="49mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090343004"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_865090343005">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090343005?ae"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="1.6uA"/>
<attribute name="I-RIPPLE" value="58mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090343005"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="16VDC"/>
</technology>
<technology name="_865090443005">
<attribute name="C" value="33 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090443005?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="1.7uA"/>
<attribute name="I-RIPPLE" value="52mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090443005"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="25VDC"/>
</technology>
<technology name="_865090543004">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090543004?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.7uA"/>
<attribute name="I-RIPPLE" value="29mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090543004"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_865090543005">
<attribute name="C" value="22 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090543005?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="1.6uA"/>
<attribute name="I-RIPPLE" value="46mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090543005"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="35VDC"/>
</technology>
<technology name="_865090643008">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090643008?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="0.5uA"/>
<attribute name="I-RIPPLE" value="20mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090643008"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
<technology name="_865090643009">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090643009?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="1000h"/>
<attribute name="I-LEAK" value="1uA"/>
<attribute name="I-RIPPLE" value="33mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="PART-NUMBER" value="865090643009"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="50VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLU_D12.5L16" prefix="C">
<description>&lt;b&gt;WCAP-ASLU Aluminum Electrolytic Capacitor &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current product series
&lt;BR&gt;Mounting style: V-Chip SMT
&lt;BR&gt;Recommended soldering: Reflow soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications and small handheld devices
&lt;BR&gt;Input and output capacitor for switched-mode power supply
&lt;BR&gt;Filtering
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14725v209%206.3x7.7x2.2_Group.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLU/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-ASLU&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella 2025-10-28
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLU_D12.5L16">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865090969001">
<attribute name="C" value="47 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865090969001?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="401uA"/>
<attribute name="I-RIPPLE" value="370mA"/>
<attribute name="LENGTH" value="16mm"/>
<attribute name="PART-NUMBER" value="865090969001"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="160VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
