<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-ASNP&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-03&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-ASNP_6.3X7.7(DXL)">
<description>&lt;B&gt;WCAP-ASNP&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X7.7X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASNP_6.3X5.5(DXL)">
<description>&lt;B&gt;WCAP-ASNP&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X5.5X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASNP_5X5.5(DXL)">
<description>&lt;B&gt;WCAP-ASNP&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X5.5X1.4(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASNP_8X6.5(DXL)">
<description>&lt;B&gt;WCAP-ASNP&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X6.5X2.3(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASNP_4X5.5(DXL)">
<description>&lt;B&gt;WCAP-ASNP&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,4X5.5X1(DiameterXLengthXPitch)</description>
</package>
<package name="WCAP-ASNP_10X10.5(DXL)">
<description>&lt;B&gt;WCAP-ASNP&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X10.5X4.5(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASNP_8X10.5(DXL)">
<description>&lt;B&gt;WCAP-ASNP&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X10.5X3.1(DiameterXLengthXP)</description>
</package>
</packages>
<symbols>
<symbol name="C">
<description>C</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-ASNP_6.3X5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASNP Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Non-Polar +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Non-polarized product series with max. operating temperature of +85°C 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 560 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +85 °C 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Reverse polarity protected 
&lt;BR&gt;Filtering 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. TV, audio, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASNP/"&gt;https://www.we-online.com/catalog/en/WCAP-ASNP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-ASNP_6.3X5.5(DXL)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_865250143004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250143004.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="14.805uA"/>
<attribute name="I-RIPPLE" value="45mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250143004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055470M6R3DVCTBB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="0.990213Ohm"/>
</technology>
<technology name="_865250243003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250243003.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="41mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250243003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055330M010DVCTBB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="1.07989Ohm"/>
</technology>
<technology name="_865250243004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250243004.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="50mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250243004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055470M010DVCTBB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="0.996059Ohm"/>
</technology>
<technology name="_865250343005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250343005.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="26.4uA"/>
<attribute name="I-RIPPLE" value="49mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250343005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055330M016DVCTBB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="1.89848Ohm"/>
</technology>
<technology name="_865250443004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250443004.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="27.5uA"/>
<attribute name="I-RIPPLE" value="40mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250443004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055220M025DVCTBB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="1.08894Ohm"/>
</technology>
<technology name="_865250543004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250543004.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="17.5uA"/>
<attribute name="I-RIPPLE" value="29mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250543004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055100M035DVCTBB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="1.27833Ohm"/>
</technology>
<technology name="_865250543005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250543005.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="38.5uA"/>
<attribute name="I-RIPPLE" value="45mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250543005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055220M035DVCTBB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="1.10653Ohm"/>
</technology>
<technology name="_865250643009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250643009.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="32mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250643009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD055100M050DVCTBB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="2.52664Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASNP_6.3X7.7" prefix="C">
<description>&lt;b&gt;WCAP-ASNP Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Non-Polar +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Non-polarized product series with max. operating temperature of +85°C 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 560 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +85 °C 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Reverse polarity protected 
&lt;BR&gt;Filtering 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. TV, audio, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASNP/"&gt;https://www.we-online.com/catalog/en/WCAP-ASNP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-ASNP_6.3X7.7(DXL)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_865250145005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250145005.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="31.5uA"/>
<attribute name="I-RIPPLE" value="65mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250145005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077101M6R3DVCTCB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="0.463097Ohm"/>
</technology>
<technology name="_865250245005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250245005.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250245005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077101M010DVCTCB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="0.442638Ohm"/>
</technology>
<technology name="_865250345006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250345006.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="37.6uA"/>
<attribute name="I-RIPPLE" value="51mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250345006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077470M016DVCTCB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="0.67708Ohm"/>
</technology>
<technology name="_865250445005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250445005.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="41.25uA"/>
<attribute name="I-RIPPLE" value="51mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250445005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077330M025DVCTCB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="0.761286Ohm"/>
</technology>
<technology name="_865250445007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250445007.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="58.75uA"/>
<attribute name="I-RIPPLE" value="56mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250445007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBD077470M025DVCTCB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="0.624706Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASNP_8X6.5" prefix="C">
<description>&lt;b&gt;WCAP-ASNP Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Non-Polar +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Non-polarized product series with max. operating temperature of +85°C 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 560 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +85 °C 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Reverse polarity protected 
&lt;BR&gt;Filtering 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. TV, audio, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASNP/"&gt;https://www.we-online.com/catalog/en/WCAP-ASNP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-ASNP_8X6.5(DXL)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_865250149006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250149006.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="31.5uA"/>
<attribute name="I-RIPPLE" value="70mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250149006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065101M6R3DVCTBB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="0.592638Ohm"/>
</technology>
<technology name="_865250249006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250249006.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250249006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065101M010DVCTBB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="0.603224Ohm"/>
</technology>
<technology name="_865250349007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250349007.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="37.6uA"/>
<attribute name="I-RIPPLE" value="55mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250349007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065470M016DVCTBB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="0.592421Ohm"/>
</technology>
<technology name="_865250449006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250449006.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="41.25uA"/>
<attribute name="I-RIPPLE" value="55mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250449006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065330M025DVCTBB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="0.711226Ohm"/>
</technology>
<technology name="_865250449008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250449008.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="58.75uA"/>
<attribute name="I-RIPPLE" value="60mA"/>
<attribute name="L" value="6.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250449008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE065470M025DVCTBB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="0.896552Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASNP_5X5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASNP Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Non-Polar +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Non-polarized product series with max. operating temperature of +85°C 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 560 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +85 °C 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Reverse polarity protected 
&lt;BR&gt;Filtering 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. TV, audio, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASNP/"&gt;https://www.we-online.com/catalog/en/WCAP-ASNP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-ASNP_5X5.5(DXL)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_865250142003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250142003.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="10.395uA"/>
<attribute name="I-RIPPLE" value="37mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250142003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBC055330M6R3DVCTBB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="1.37241Ohm"/>
</technology>
<technology name="_865250242002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250242002.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="33mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250242002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBC055220M010DVCTBB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="1.7538Ohm"/>
</technology>
<technology name="_865250342004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250342004.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="17.6uA"/>
<attribute name="I-RIPPLE" value="37mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250342004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBC055220M016DVCTBB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="1.45067Ohm"/>
</technology>
<technology name="_865250442003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250442003.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="12.5uA"/>
<attribute name="I-RIPPLE" value="27mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250442003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBC055100M025DVCTBB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="2.34491Ohm"/>
</technology>
<technology name="_865250642008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250642008.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="20mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250642008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBC0554R7M050DVCTBB000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="2.61794Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASNP_4X5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASNP Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Non-Polar +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Non-polarized product series with max. operating temperature of +85°C 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 560 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +85 °C 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Reverse polarity protected 
&lt;BR&gt;Filtering 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. TV, audio, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASNP/"&gt;https://www.we-online.com/catalog/en/WCAP-ASNP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-ASNP_4X5.5(DXL)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_865250140001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250140001.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="15mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250140001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055100M6R3DVCTAB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="3.8354Ohm"/>
</technology>
<technology name="_865250140002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250140002.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="28mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250140002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055220M6R3DVCTAB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="3.86425Ohm"/>
</technology>
<technology name="_865250240001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250240001.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="17mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250240001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055100M010DVCTAB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="3.8754Ohm"/>
</technology>
<technology name="_865250340001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250340001.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="12mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250340001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0553R3M016DVCTAB000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="4.00216Ohm"/>
</technology>
<technology name="_865250340002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250340002.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="12mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250340002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0554R7M016DVCTAB000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865250340003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250340003.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="23mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250340003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055100M016DVCTAB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="3.68257Ohm"/>
</technology>
<technology name="_865250440001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250440001.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="12mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250440001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0553R3M025DVCTAB000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="3.93557Ohm"/>
</technology>
<technology name="_865250440002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250440002.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="16mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250440002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0554R7M025DVCTAB000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="3.37198Ohm"/>
</technology>
<technology name="_865250540001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250540001.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="8.4mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250540001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0552R2M035DVCTAB000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="5.31872Ohm"/>
</technology>
<technology name="_865250540002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250540002.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="16mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250540002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0553R3M035DVCTAB000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="3.34078Ohm"/>
</technology>
<technology name="_865250540003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250540003.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="18mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250540003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0554R7M035DVCTAB000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="3.47818Ohm"/>
</technology>
<technology name="_865250640001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250640001.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="1mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250640001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055R10M050DVCTAB000"/>
<attribute name="VALUE" value="0.1  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="20.6814Ohm"/>
</technology>
<technology name="_865250640002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250640002.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="2mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250640002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055R22M050DVCTAB000"/>
<attribute name="VALUE" value="0.22  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value=""/>
</technology>
<technology name="_865250640003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250640003.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="2.8mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250640003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055R33M050DVCTAB000"/>
<attribute name="VALUE" value="0.33  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="8.79148Ohm"/>
</technology>
<technology name="_865250640004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250640004.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="4mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250640004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055R47M050DVCTAB000"/>
<attribute name="VALUE" value="0.47  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="7.8069Ohm"/>
</technology>
<technology name="_865250640005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250640005.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="8.4mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250640005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB055010M050DVCTAB000"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="6.11584Ohm"/>
</technology>
<technology name="_865250640006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250640006.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="13mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250640006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0552R2M050DVCTAB000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="5.54928Ohm"/>
</technology>
<technology name="_865250640007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250640007.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="17mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250640007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBB0553R3M050DVCTAB000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="5.77566Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASNP_10X10.5" prefix="C">
<description>&lt;b&gt;WCAP-ASNP Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Non-Polar +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Non-polarized product series with max. operating temperature of +85°C 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 560 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +85 °C 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Reverse polarity protected 
&lt;BR&gt;Filtering 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. TV, audio, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASNP/"&gt;https://www.we-online.com/catalog/en/WCAP-ASNP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-ASNP_10X10.5(DXL)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_865250157009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250157009.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="148.05uA"/>
<attribute name="I-RIPPLE" value="190mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250157009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBF105471M6R3DVCTEB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="0.154707Ohm"/>
</technology>
<technology name="_865250157010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250157010.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="176.4uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250157010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBF105561M6R3DVCTEB000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="0.138049Ohm"/>
</technology>
<technology name="_865250257008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250257008.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="180mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250257008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBF105331M010DVCTEB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="0.151124Ohm"/>
</technology>
<technology name="_865250357009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250357009.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="176uA"/>
<attribute name="I-RIPPLE" value="170mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250357009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBF105221M016DVCTEB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="0.152594Ohm"/>
</technology>
<technology name="_865250657011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250657011.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250657011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBF105330M050DVCTEB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="0.214878Ohm"/>
</technology>
<technology name="_865250657012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250657012.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="100mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250657012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBF105470M050DVCTEB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="0.214467Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASNP_8X10.5" prefix="C">
<description>&lt;b&gt;WCAP-ASNP Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Non-Polar +85 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Non-polarized product series with max. operating temperature of +85°C 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 560 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +85 °C 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Reverse polarity protected 
&lt;BR&gt;Filtering 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. TV, audio, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14726v209%20Family_WCAP-ASNP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ASNP/"&gt;https://www.we-online.com/catalog/en/WCAP-ASNP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-03
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-ASNP_8X10.5(DXL)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_865250153007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250153007.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="69.3uA"/>
<attribute name="I-RIPPLE" value="120mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250153007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE105221M6R3DVCTEB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="0.258878Ohm"/>
</technology>
<technology name="_865250153008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250153008.pdf"/>
<attribute name="DF" value="24%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="103.95uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250153008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE105331M6R3DVCTEB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="Z" value="0.246094Ohm"/>
</technology>
<technology name="_865250253007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250253007.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="150mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250253007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE105221M010DVCTEB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="Z" value="0.249444Ohm"/>
</technology>
<technology name="_865250353008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250353008.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="80uA"/>
<attribute name="I-RIPPLE" value="100mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250353008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE105101M016DVCTEB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="Z" value="0.298562Ohm"/>
</technology>
<technology name="_865250453009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250453009.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="125uA"/>
<attribute name="I-RIPPLE" value="130mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250453009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE105101M025DVCTEB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="Z" value="0.308167Ohm"/>
</technology>
<technology name="_865250553006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250553006.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="57.75uA"/>
<attribute name="I-RIPPLE" value="58mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250553006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE105330M035DVCTEB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="0.356225Ohm"/>
</technology>
<technology name="_865250553007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250553007.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="82.25uA"/>
<attribute name="I-RIPPLE" value="64mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250553007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE105470M035DVCTEB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="35V(DC)"/>
<attribute name="Z" value="0.351603Ohm"/>
</technology>
<technology name="_865250653010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865250653010.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="60mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 865250653010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASBE105220M050DVCTEB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="Z" value="0.415783Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
