<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-AT1H&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-02-28&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-AT1H_18X35.5(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X35.5X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_18X31.5(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,18X31.5X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_13X25(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X25X5X0.6(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_8X16(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,8X16X3.5X0.5(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_18X25(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,18X25X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_18X21(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X21X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_10X20(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,10X20X5X0.6(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_8X11.5(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,8X11.5X3.5X0.5(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_16X21(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,16X21X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_10X16(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,10X16X5X0.6(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_5X11(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X11X2X0.5(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_16X35.5(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X35.5X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_13X20(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X20X5X0.6(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_16X31.5(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,16X31.5X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_10X12.5(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X12.5X5X0.6(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_6.3X11(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,6.3X11X2.5X0.5(DiameteXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-AT1H_16X25(DXL)">
<description>&lt;B&gt;WCAP-AT1H&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X25X7.5X0.8(DiameteXLengthX PitchXØPin)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-AT1H_18X35.5" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_18X35.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860241081001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241081001.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="2740uA"/>
<attribute name="I-RIPPLE" value="3220mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241081001 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL355331M200DSPAEK000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_18X31.5" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_18X31.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240681012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240681012.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="500uA"/>
<attribute name="I-RIPPLE" value="2093mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240681012 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL315102M050DSPAEK000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860241081009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241081009.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1860uA"/>
<attribute name="I-RIPPLE" value="2350mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241081009 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL315221M200DSPAEK000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_860241181007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241181007.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1600uA"/>
<attribute name="I-RIPPLE" value="1870mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241181007 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL315151M250DSPAEK000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
<technology name="_860241381006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241381006.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1188uA"/>
<attribute name="I-RIPPLE" value="1460mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241381006 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL315680M400DSPAEK000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860241481007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241481007.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="946uA"/>
<attribute name="I-RIPPLE" value="1120mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241481007 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL315470M450DSPAEK000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_13X25" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_13X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240478010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240478010.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="1552mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240478010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250102M025DSPACK000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860240578010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240578010.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="164.5uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240578010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250471M035DSPACK000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860240678010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240678010.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="1150mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240678010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250331M050DSPACK000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860240978005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240978005.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="535.2uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240978005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJI250680M160DSPACK000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="160V(DC)"/>
</technology>
<technology name="_860241178003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241178003.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="430uA"/>
<attribute name="I-RIPPLE" value="750mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241178003 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJI250330M250DSPACK000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
<technology name="_860241478004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241478004.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="496uA"/>
<attribute name="I-RIPPLE" value="632mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241478004 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJI250220M450DSPACK000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_8X16" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_8X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240374007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240374007.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240374007 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE160331M016DSPA7H000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_18X25" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_18X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240981007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240981007.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1060uA"/>
<attribute name="I-RIPPLE" value="1780mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240981007 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL250151M160DSPAEK000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="160V(DC)"/>
</technology>
<technology name="_860240981008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240981008.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1508uA"/>
<attribute name="I-RIPPLE" value="2290mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240981008 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL250221M160DSPAEK000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="160V(DC)"/>
</technology>
<technology name="_860241081008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241081008.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1300uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241081008 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL250151M200DSPAEK000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_860241181006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241181006.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1100uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241181006 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL250101M250DSPAEK000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
<technology name="_860241381008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241381008.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1412uA"/>
<attribute name="I-RIPPLE" value="1530mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value=""/>
<attribute name="PART-NUMBER" value=" 860241381008 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL250820M400DSPAEK0R1"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_18X21" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_18X21(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240981006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240981006.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="740uA"/>
<attribute name="I-RIPPLE" value="1310mA"/>
<attribute name="L" value="21mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240981006 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL210101M160DSPAEK000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="160V(DC)"/>
</technology>
<technology name="_860241081007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241081007.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="900uA"/>
<attribute name="I-RIPPLE" value="1380mA"/>
<attribute name="L" value="21mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241081007 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL210101M200DSPAEK000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_860241181005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241181005.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="780uA"/>
<attribute name="I-RIPPLE" value="1300mA"/>
<attribute name="L" value="21mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241181005 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL210680M250DSPAEK000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
<technology name="_860241381004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241381004.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="628uA"/>
<attribute name="I-RIPPLE" value="870mA"/>
<attribute name="L" value="21mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241381004 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL210330M400DSPAEK000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860241381005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241381005.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="852uA"/>
<attribute name="I-RIPPLE" value="1050mA"/>
<attribute name="L" value="21mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241381005 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL210470M400DSPAEK000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860241481006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241481006.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="694uA"/>
<attribute name="I-RIPPLE" value="883mA"/>
<attribute name="L" value="21mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241481006 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJL210330M450DSPAEK000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_10X20" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_10X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240475008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240475008.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="805mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240475008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200331M025DSPAAK000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860240475009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240475009.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="950mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240475009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200471M025DSPAAK000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860240575008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240575008.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="760mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240575008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200221M035DSPAAK000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860240675008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240675008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75uA"/>
<attribute name="I-RIPPLE" value="747mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240675008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200151M050DSPAAK000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860240975001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240975001.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="164uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240975001 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJF160100M160DSPAAK000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="160V(DC)"/>
</technology>
<technology name="_860240975002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240975002.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="240.8uA"/>
<attribute name="I-RIPPLE" value="450mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240975002 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJF200220M160DSPAAK000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="160V(DC)"/>
</technology>
<technology name="_860241075003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241075003.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="180uA"/>
<attribute name="I-RIPPLE" value="310mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241075003 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJF200100M200DSPAAK000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_860241075004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241075004.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="276uA"/>
<attribute name="I-RIPPLE" value="470mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241075004 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJF200220M200DSPAAK000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_860241175001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241175001.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="200uA"/>
<attribute name="I-RIPPLE" value="320mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241175001 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJF200100M250DSPAAK000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
<technology name="_860241175002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241175002.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="320uA"/>
<attribute name="I-RIPPLE" value="420mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241175002 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJF200220M250DSPAAK000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_8X11.5" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_8X11.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240274006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240274006.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="390mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240274006 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115331M010DSPA7H000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860240374004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240374004.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="245mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240374004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115101M016DSPA7H000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860240374005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240374005.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="24uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240374005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115151M016DSPA7H000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860240374006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240374006.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="420mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240374006 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115221M016DSPA7H000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860240474004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240474004.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="17uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240474004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115680M025DSPA7H000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860240474005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240474005.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="327mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240474005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115101M025DSPA7H000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860240574004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240574004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="16.45uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240574004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115470M035DSPA7H000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860240574005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240574005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="23.8uA"/>
<attribute name="I-RIPPLE" value="270mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240574005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115680M035DSPA7H000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860240674004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240674004.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="241mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240674004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115330M050DSPA7H000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860240674005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240674005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="287mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240674005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115470M050DSPA7H000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_16X21" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_16X21(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860241180004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241180004.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="570uA"/>
<attribute name="I-RIPPLE" value="930mA"/>
<attribute name="L" value="21mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241180004 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJK210470M250DSPAEK000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_10X16" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_10X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240275008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240275008.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="900mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240275008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160102M010DSPAAK000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860240375008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240375008.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="730mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240375008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160471M016DSPAAK000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860240475007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240475007.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="580mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240475007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160221M025DSPAAK000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860240575007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240575007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="52.5uA"/>
<attribute name="I-RIPPLE" value="632mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240575007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160151M035DSPAAK000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860240675007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240675007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240675007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160101M050DSPAAK000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860241375002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241375002.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="260uA"/>
<attribute name="I-RIPPLE" value="274mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241375002 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJF160100M400DSPAAK000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_16X35.5" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_16X35.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860241480001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241480001.pdf"/>
<attribute name="DF" value="17%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1900uA"/>
<attribute name="I-RIPPLE" value="610mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241480001 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJK355101M450DSPADE000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_13X20" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_13X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240278009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240278009.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1540mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240278009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200222M010DSPACK000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860240378009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240378009.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="1173mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240378009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200102M016DSPACK000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860240578009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240578009.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="1035mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240578009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200331M035DSPACK000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860240678009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240678009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="977mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240678009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200221M050DSPACK000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860240978003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240978003.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="311.2uA"/>
<attribute name="I-RIPPLE" value="610mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240978003 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJI200330M160DSPACK000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="160V(DC)"/>
</technology>
<technology name="_860240978004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240978004.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="400.8uA"/>
<attribute name="I-RIPPLE" value="680mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240978004 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJI200470M160DSPACK000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="160V(DC)"/>
</technology>
<technology name="_860241078002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241078002.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="476uA"/>
<attribute name="I-RIPPLE" value="980mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241078002 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJI200470M200DSPACK000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_860241078005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241078005.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="364uA"/>
<attribute name="I-RIPPLE" value="620mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241078005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJI200330M200DSPACK000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_860241178002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241178002.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="320uA"/>
<attribute name="I-RIPPLE" value="490mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241178002 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJI200220M250DSPACK000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
<technology name="_860241378003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241378003.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="452uA"/>
<attribute name="I-RIPPLE" value="557mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241378003 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJI200220M400DSPACK000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860241478002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241478002.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="222.4uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241478002 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJI2006R8M450DSPACK000"/>
<attribute name="VALUE" value="6.8  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
<technology name="_860241478003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241478003.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="280uA"/>
<attribute name="I-RIPPLE" value="390mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241478003 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJI200100M450DSPACK000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="450V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_5X11" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_5X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240272001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240272001.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="100mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240272001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110470M010DSPA3E000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860240272002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240272002.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="6.8uA"/>
<attribute name="I-RIPPLE" value="130mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240272002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110680M010DSPA3E000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860240372001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240372001.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5.28uA"/>
<attribute name="I-RIPPLE" value="115mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240372001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110330M016DSPA3E000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860240372002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240372002.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="7.52uA"/>
<attribute name="I-RIPPLE" value="145mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240372002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110470M016DSPA3E000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860240472001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240472001.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5.5uA"/>
<attribute name="I-RIPPLE" value="100mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240472001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110220M025DSPA3E000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860240472002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240472002.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="8.25uA"/>
<attribute name="I-RIPPLE" value="130mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240472002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110330M025DSPA3E000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860240572001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240572001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.5uA"/>
<attribute name="I-RIPPLE" value="65mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240572001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110100M035DSPA3E000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860240572002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240572002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="7.7uA"/>
<attribute name="I-RIPPLE" value="125mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240572002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110220M035DSPA3E000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860240672001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240672001.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.4uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240672001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC1106R8M050DSPA3E000"/>
<attribute name="VALUE" value="6.8  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860240672002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240672002.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="97mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240672002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110100M050DSPA3E000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_16X31.5" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_16X31.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240480011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240480011.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="550uA"/>
<attribute name="I-RIPPLE" value="2400mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240480011 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK315222M025DSPADK000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860240580011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240580011.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="350uA"/>
<attribute name="I-RIPPLE" value="1932mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240580011 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK315102M035DSPADK000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_10X12.5" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_10X12.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240275007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240275007.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="540mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240275007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125471M010DSPA9K000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860240475006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240475006.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="37.5uA"/>
<attribute name="I-RIPPLE" value="460mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240475006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125151M025DSPA9K000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860240575006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240575006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="390mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240575006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125101M035DSPA9K000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860240675006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240675006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="34uA"/>
<attribute name="I-RIPPLE" value="356mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240675006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125680M050DSPA9K000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860241375001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241375001.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="208.8uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241375001 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJF1256R8M400DSPA9K000"/>
<attribute name="VALUE" value="6.8  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_6.3X11" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_6.3X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240273003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240273003.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="190mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240273003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110101M010DSPA4E000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860240273004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240273004.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="15uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240273004 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110151M010DSPA4E000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860240273005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240273005.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="270mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240273005 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110221M010DSPA4E000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860240373003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240373003.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="10.88uA"/>
<attribute name="I-RIPPLE" value="200mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240373003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110680M016DSPA4E000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860240473003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240473003.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240473003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110470M025DSPA4E000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860240573003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240573003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="11.55uA"/>
<attribute name="I-RIPPLE" value="178mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240573003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110330M035DSPA4E000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860240673003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240673003.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="130mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240673003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110220M050DSPA4E000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-AT1H_16X25" prefix="C">
<description>&lt;b&gt;WCAP-AT1H Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 3300 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +105 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 5000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14727v209%20Family_WCAP-AT1H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-AT1H/"&gt;https://www.we-online.com/catalog/en/WCAP-AT1H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-AT1H_16X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860240280010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240280010.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="330uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240280010 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250332M010DSPAEK000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860240380010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240380010.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="352uA"/>
<attribute name="I-RIPPLE" value="2093mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240380010 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250222M016DSPAEK000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860240680011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860240680011.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="1552mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860240680011 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250471M050DSPAEK000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860241080006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241080006.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="644uA"/>
<attribute name="I-RIPPLE" value="1190mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860241080006 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATJK250680M200DSPAEK000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="200V(DC)"/>
</technology>
<technology name="_860241380015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860241380015.pdf"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="852uA"/>
<attribute name="I-RIPPLE" value="1200mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value=""/>
<attribute name="PART-NUMBER" value=" 860241380015 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250470M400DSPAEK0B0"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
