<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-ATET&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-02-28&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-ATET_16X31.5(DXL)">
<description>&lt;B&gt;WCAP-ATET&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X31.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATET_6.3X11(DXL)">
<description>&lt;B&gt;WCAP-ATET&lt;/B&gt;&lt;BR&gt;Aluminium Electrolytic Capacitors,6.3X11X2.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATET_13X25(DXL)">
<description>&lt;B&gt;WCAP-ATET&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,13X25X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATET_13X20(DXL)">
<description>&lt;B&gt;WCAP-ATET&lt;/B&gt;&lt;BR&gt;Aluminium Electrolytic Capacitors,13X20X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATET_10X16(DXL)">
<description>&lt;B&gt;WCAP-ATET&lt;/B&gt;&lt;BR&gt;Aluminium Electrolytic Capacitors,10X16X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATET_10X12.5(DXL)">
<description>&lt;B&gt;WCAP-ATET&lt;/B&gt;&lt;BR&gt;Aluminium Electrolytic Capacitors,10X12.5X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATET_8X11.5(DXL)">
<description>&lt;B&gt;WCAP-ATET&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X11.5X3.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATET_10X25(DXL)">
<description>&lt;B&gt;WCAP-ATET&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X25X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATET_5X11(DXL)">
<description>&lt;B&gt;WCAP-ATET&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X11X2X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATET_16X25(DXL)">
<description>&lt;B&gt;WCAP-ATET&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X25X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-ATET_16X31.5" prefix="C">
<description>&lt;b&gt;WCAP-ATET Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Temperature +125 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 350 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +125 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +125 °C for UR &gt;100 V(DC) 
&lt;BR&gt;Endurance: 1000 ‒ 2000 h @ +125 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 16.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATET/"&gt;https://www.we-online.com/catalog/en/WCAP-ATET/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATET_16X31.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860131280009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131280009.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="329uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131280009 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCK315470M350DSPADB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="350V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATET_6.3X11" prefix="C">
<description>&lt;b&gt;WCAP-ATET Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Temperature +125 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 350 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +125 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +125 °C for UR &gt;100 V(DC) 
&lt;BR&gt;Endurance: 1000 ‒ 2000 h @ +125 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 16.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATET/"&gt;https://www.we-online.com/catalog/en/WCAP-ATET/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATET_6.3X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860130273002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130273002.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="145mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130273002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD110101M010DSPA4A000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860130373001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130373001.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="5.28uA"/>
<attribute name="I-RIPPLE" value="91mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130373001 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD110330M016DSPA4A000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860130373002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130373002.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="7.52uA"/>
<attribute name="I-RIPPLE" value="110mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130373002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD110470M016DSPA4A000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860130373003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130373003.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="175mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130373003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD110101M016DSPA4A000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860130473001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130473001.pdf"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="5.5uA"/>
<attribute name="I-RIPPLE" value="70mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130473001 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD110220M025DSPA4A000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860130473002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130473002.pdf"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="8.25uA"/>
<attribute name="I-RIPPLE" value="100mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130473002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD110330M025DSPA4A000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860130473003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130473003.pdf"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="110mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130473003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD110470M025DSPA4A000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860130573001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130573001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="7.7uA"/>
<attribute name="I-RIPPLE" value="82mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130573001 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD110220M035DSPA4A000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860130673001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130673001.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="48mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130673001 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD110100M050DSPA4A000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860130673002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130673002.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="75mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130673002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD110220M050DSPA4A000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860130873001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130873001.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="14mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130873001 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD110R47M100DSPA4A000"/>
<attribute name="VALUE" value="0.47  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_860130873002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130873002.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="24mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130873002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD110010M100DSPA4A000"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_860130873003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130873003.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="31mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130873003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD1102R2M100DSPA4A000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_860130873004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130873004.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="36mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130873004 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD1103R3M100DSPA4A000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_860130873005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130873005.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="38mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130873005 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGD1104R7M100DSPA4A000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_860131173001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131173001.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="41mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131173001 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCD110010M250DSPA4A000"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
<technology name="_860131173002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131173002.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="42mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131173002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCD1102R2M250DSPA4A000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATET_13X25" prefix="C">
<description>&lt;b&gt;WCAP-ATET Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Temperature +125 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 350 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +125 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +125 °C for UR &gt;100 V(DC) 
&lt;BR&gt;Endurance: 1000 ‒ 2000 h @ +125 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 16.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATET/"&gt;https://www.we-online.com/catalog/en/WCAP-ATET/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATET_13X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860130478010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130478010.pdf"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="970mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130478010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGI250102M025DSPACB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860130678010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130678010.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="900mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130678010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGI250471M050DSPACB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860130878011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130878011.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="270mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130878011 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGI250101M100DSPACB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_860131178007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131178007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="164mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131178007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCI250330M250DSPACB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
<technology name="_860131278007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131278007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="154uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131278007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCI250220M350DSPACB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="350V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATET_13X20" prefix="C">
<description>&lt;b&gt;WCAP-ATET Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Temperature +125 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 350 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +125 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +125 °C for UR &gt;100 V(DC) 
&lt;BR&gt;Endurance: 1000 ‒ 2000 h @ +125 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 16.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATET/"&gt;https://www.we-online.com/catalog/en/WCAP-ATET/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATET_13X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860130378009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130378009.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130378009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGI200102M016DSPACB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860130478009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130478009.pdf"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="810mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130478009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGI200471M025DSPACB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860130578007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130578007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="718mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130578007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGI200331M035DSPACB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860130578008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130578008.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="164.5uA"/>
<attribute name="I-RIPPLE" value="810mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130578008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGI200471M035DSPACB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860130678008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130678008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="587mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130678008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGI200221M050DSPACB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860130678009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130678009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="810mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130678009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGI200331M050DSPACB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860130878010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130878010.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="185mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130878010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGI200470M100DSPACB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_860131178006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131178006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="145mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131178006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCI200220M250DSPACB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
<technology name="_860131278006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131278006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="70uA"/>
<attribute name="I-RIPPLE" value="110mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131278006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCI200100M350DSPACB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="350V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATET_10X12.5" prefix="C">
<description>&lt;b&gt;WCAP-ATET Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Temperature +125 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 350 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +125 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +125 °C for UR &gt;100 V(DC) 
&lt;BR&gt;Endurance: 1000 ‒ 2000 h @ +125 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 16.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATET/"&gt;https://www.we-online.com/catalog/en/WCAP-ATET/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATET_10X12.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860130275005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130275005.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="505mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130275005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF125471M010DSPA9B000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860130375005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130375005.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="400mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130375005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF125221M016DSPA9B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860130375006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130375006.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="470mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130375006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF125331M016DSPA9B000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860130475005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130475005.pdf"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="250mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130475005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF125101M025DSPA9B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860130475006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130475006.pdf"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="420mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130475006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF125221M025DSPA9B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860130575004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130575004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130575004 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF125101M035DSPA9B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860130675005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130675005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="164mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130675005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF125470M050DSPA9B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860130875007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130875007.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="90mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130875007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF125220M100DSPA9B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_860131175004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131175004.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="60mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131175004 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCF1254R7M250DSPA9B000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
<technology name="_860131275003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131275003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="23.1uA"/>
<attribute name="I-RIPPLE" value="55mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131275003 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCF1253R3M350DSPA9B000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="350V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATET_10X25" prefix="C">
<description>&lt;b&gt;WCAP-ATET Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Temperature +125 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 350 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +125 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +125 °C for UR &gt;100 V(DC) 
&lt;BR&gt;Endurance: 1000 ‒ 2000 h @ +125 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 16.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATET/"&gt;https://www.we-online.com/catalog/en/WCAP-ATET/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATET_10X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860130375008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130375008.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="950mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130375008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF250102M016DSPAAB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860130475008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130475008.pdf"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="770mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130475008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF250471M025DSPAAB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860130575006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130575006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="680mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130575006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF250331M035DSPAAB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860130675007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130675007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="560mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130675007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF250221M050DSPAAB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860130875009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130875009.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="175mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130875009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF250470M100DSPAAB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_860131275005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131275005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="70uA"/>
<attribute name="I-RIPPLE" value="105mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131275005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCF250100M350DSPAAB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="350V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATET_8X11.5" prefix="C">
<description>&lt;b&gt;WCAP-ATET Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Temperature +125 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 350 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +125 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +125 °C for UR &gt;100 V(DC) 
&lt;BR&gt;Endurance: 1000 ‒ 2000 h @ +125 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 16.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATET/"&gt;https://www.we-online.com/catalog/en/WCAP-ATET/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATET_8X11.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860130274003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130274003.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="330mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130274003 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGE115221M010DSPA7A000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860130274004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130274004.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="340mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130274004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGE115331M010DSPA7A000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860130374004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130374004.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="340mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130374004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGE115221M016DSPA7A000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860130474004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130474004.pdf"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="210mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130474004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGE115101M025DSPA7A000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860130574002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130574002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="11.55uA"/>
<attribute name="I-RIPPLE" value="108mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130574002 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGE115330M035DSPA7A000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860130574003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130574003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="16.45uA"/>
<attribute name="I-RIPPLE" value="130mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130574003 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGE115470M035DSPA7A000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860130674003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130674003.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="122mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130674003 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGE115330M050DSPA7A000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860130674004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130674004.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="140mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130674004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGE115470M050DSPA7A000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860130874006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130874006.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="60mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130874006 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGE115100M100DSPA7A000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_860131174003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131174003.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="50mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131174003 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCE1153R3M250DSPA7A000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
<technology name="_860131274001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131274001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="7uA"/>
<attribute name="I-RIPPLE" value="45mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131274001 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCE115010M350DSPA7A000"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="350V(DC)"/>
</technology>
<technology name="_860131274002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131274002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="15.4uA"/>
<attribute name="I-RIPPLE" value="47mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131274002 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCE1152R2M350DSPA7A000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="350V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATET_5X11" prefix="C">
<description>&lt;b&gt;WCAP-ATET Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Temperature +125 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 350 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +125 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +125 °C for UR &gt;100 V(DC) 
&lt;BR&gt;Endurance: 1000 ‒ 2000 h @ +125 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 16.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATET/"&gt;https://www.we-online.com/catalog/en/WCAP-ATET/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATET_5X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860130272001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130272001.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="92mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130272001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGC110470M010DSPA3A000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATET_16X25" prefix="C">
<description>&lt;b&gt;WCAP-ATET Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Temperature +125 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 350 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +125 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +125 °C for UR &gt;100 V(DC) 
&lt;BR&gt;Endurance: 1000 ‒ 2000 h @ +125 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 16.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATET/"&gt;https://www.we-online.com/catalog/en/WCAP-ATET/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATET_16X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860130580009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130580009.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="350uA"/>
<attribute name="I-RIPPLE" value="1080mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130580009 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGK250102M035DSPAEB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860131180008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131180008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="205mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131180008 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCK250470M250DSPAEB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
<technology name="_860131280008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131280008.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="231uA"/>
<attribute name="I-RIPPLE" value="180mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131280008 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCK250330M350DSPAEB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="350V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATET_10X16" prefix="C">
<description>&lt;b&gt;WCAP-ATET Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Temperature +125 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 1000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 350 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +125 °C for UR ≤100 V(DC) 
&lt;BR&gt;-25 °C up to +125 °C for UR &gt;100 V(DC) 
&lt;BR&gt;Endurance: 1000 ‒ 2000 h @ +125 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 16.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High operating temperature applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14728v209%20Family_WCAP-ATET.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATET/"&gt;https://www.we-online.com/catalog/en/WCAP-ATET/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATET_10X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860130275006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130275006.pdf"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="870mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130275006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF160102M010DSPAAB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860130375007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130375007.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="650mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130375007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF160471M016DSPAAB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860130475007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130475007.pdf"/>
<attribute name="DF" value="13%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="570mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130475007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF160331M025DSPAAB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860130575005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130575005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="480mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130575005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF160221M035DSPAAB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860130675006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130675006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="250mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130675006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF160101M050DSPAAB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860130875008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860130875008.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="140mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860130875008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATGF160330M100DSPAAB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_860131175005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131175005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="83mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131175005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCF160100M250DSPAAB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="250V(DC)"/>
</technology>
<technology name="_860131275004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860131275004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="32.9uA"/>
<attribute name="I-RIPPLE" value="68mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-25 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 860131275004 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATCF1604R7M350DSPAAB000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="350V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
