<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-ATG8&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-02-27&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-ATG8_22X51(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,22X51X10X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_16X25(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X25X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_10X12.5(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X12.5X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_13X25(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,13X25X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_16X35.5(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X35.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_18X25(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X25X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_10X16(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X16X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_18X41X7.5(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X41X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_10X20(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X20X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_6.3X11(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X11X2.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_22X41(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,22X41X10X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_16X31.5(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X31.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_13X20(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,13X20X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_8X11.5(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X11.5X3.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_8X16(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X16X3.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_18X31.5(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X31.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_18X35.5(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X35.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATG8_5X11(DXL)">
<description>&lt;B&gt;WCAP-ATG8&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X11X2X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-ATG8_22X51" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_22X51(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010283033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010283033.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="3300uA"/>
<attribute name="I-RIPPLE" value="4620mA"/>
<attribute name="L" value="51mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010283033"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBN510333M010DSPS2B000"/>
<attribute name="VALUE" value="33000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_16X25" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_16X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010280025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010280025.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="560uA"/>
<attribute name="I-RIPPLE" value="2189mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010280025"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK250562M010DSPAEB000"/>
<attribute name="VALUE" value="5600  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010280026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010280026.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="680uA"/>
<attribute name="I-RIPPLE" value="2475mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010280026"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK250682M010DSPAEB000"/>
<attribute name="VALUE" value="6800  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010380024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010380024.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="624uA"/>
<attribute name="I-RIPPLE" value="2002mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010380024"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK250392M016DSPAEB000"/>
<attribute name="VALUE" value="3900  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010380025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010380025.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="752uA"/>
<attribute name="I-RIPPLE" value="2310mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010380025"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK250472M016DSPAEB000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010480022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010480022.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="675uA"/>
<attribute name="I-RIPPLE" value="1804mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010480022"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK250272M025DSPAEB000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010480023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010480023.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="825uA"/>
<attribute name="I-RIPPLE" value="1870mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010480023"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK250332M025DSPAEB000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010580020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010580020.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="1749mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010580020"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK250182M035DSPAEB000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010580021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010580021.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="770uA"/>
<attribute name="I-RIPPLE" value="1870mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010580021"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK250222M035DSPAEB000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010680025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010680025.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="1617mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010680025"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK250122M050DSPAEB000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010780022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010780022.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="428.4uA"/>
<attribute name="I-RIPPLE" value="1265mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010780022"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK250681M063DSPAEB000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010780023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010780023.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="516.6uA"/>
<attribute name="I-RIPPLE" value="1430mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010780023"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK250821M063DSPAEB000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010780024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010780024.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="1540mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010780024"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK250102M063DSPAEB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860011380009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860011380009.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="564uA"/>
<attribute name="I-RIPPLE" value="270mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860011380009"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATAK250470M400DSPAEB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_10X12.5" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_10X12.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010275014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010275014.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="82uA"/>
<attribute name="I-RIPPLE" value="671mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010275014"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF125821M010DSPA9B000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010275016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010275016.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="726mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010275016"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF125102M010DSPA9B000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010375013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010375013.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="89.6uA"/>
<attribute name="I-RIPPLE" value="572mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010375013"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF125561M016DSPA9B000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010375015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010375015.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="108.8uA"/>
<attribute name="I-RIPPLE" value="682mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010375015"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF125681M016DSPA9B000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010575012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010575012.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="528mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010575012"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF125331M035DSPA9B000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010675016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010675016.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75uA"/>
<attribute name="I-RIPPLE" value="363mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010675016"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF125151M050DSPA9B000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010675017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010675017.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="90uA"/>
<attribute name="I-RIPPLE" value="418mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010675017"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF125181M050DSPA9B000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010675018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010675018.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="468mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010675018"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF125221M050DSPA9B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010775014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010775014.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="330mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010775014"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF125101M063DSPA9B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_13X25" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_13X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010278024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010278024.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="1980mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010278024"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI250472M010DSPACB000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010478021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010478021.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="550uA"/>
<attribute name="I-RIPPLE" value="1705mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010478021"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI250222M025DSPACB000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010578019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010578019.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="525uA"/>
<attribute name="I-RIPPLE" value="1570mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010578019"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI250152M035DSPACB000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010678023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010678023.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="410uA"/>
<attribute name="I-RIPPLE" value="1287mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010678023"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI250821M050DSPACB000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010678024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010678024.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="500uA"/>
<attribute name="I-RIPPLE" value="1485mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010678024"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI250102M050DSPACB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010778021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010778021.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="352.8uA"/>
<attribute name="I-RIPPLE" value="1056mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010778021"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI250561M063DSPACB000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860011378008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860011378008.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="396uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860011378008"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATAI250330M400DSPACB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_16X35.5" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_16X35.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010280028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010280028.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1000uA"/>
<attribute name="I-RIPPLE" value="2640mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010280028"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK355103M010DSPADB000"/>
<attribute name="VALUE" value="10000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010380028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010380028.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1312uA"/>
<attribute name="I-RIPPLE" value="2893mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010380028"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK355822M016DSPADB000"/>
<attribute name="VALUE" value="8200  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010680028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010680028.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1100uA"/>
<attribute name="I-RIPPLE" value="2310mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010680028"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK355222M050DSPADB000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010780026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010780026.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="2090mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010780026"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK355152M063DSPADB000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010780027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010780027.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1134uA"/>
<attribute name="I-RIPPLE" value="2255mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010780027"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK355182M063DSPADB000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860011380010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860011380010.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="816uA"/>
<attribute name="I-RIPPLE" value="410mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860011380010"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATAK355680M400DSPADB000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_18X41" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_18X41X7.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010281031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010281031.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1800uA"/>
<attribute name="I-RIPPLE" value="3410mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010281031"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL410183M010DSPS1B000"/>
<attribute name="VALUE" value="18000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010581026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010581026.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1960uA"/>
<attribute name="I-RIPPLE" value="2915mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010581026"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL410562M035DSPS1B000"/>
<attribute name="VALUE" value="5600  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010681031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010681031.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1950uA"/>
<attribute name="I-RIPPLE" value="2871mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010681031"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL410392M050DSPS1B000"/>
<attribute name="VALUE" value="3900  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860011381013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860011381013.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1440uA"/>
<attribute name="I-RIPPLE" value="520mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860011381013"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATAL410121M400DSPS1B000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_18X25" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_18X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860011381011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860011381011.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="816uA"/>
<attribute name="I-RIPPLE" value="380mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860011381011"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATAL250680M400DSPAEB000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_10X20" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_10X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010275019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010275019.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="180uA"/>
<attribute name="I-RIPPLE" value="1089mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010275019"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF200182M010DSPAAB000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010275020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010275020.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1210mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010275020"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF200222M010DSPAAB000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010375019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010375019.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="240uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010375019"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF200152M016DSPAAB000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010475016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010475016.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="205uA"/>
<attribute name="I-RIPPLE" value="891mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010475016"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF200821M025DSPAAB000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010475017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010475017.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="1050mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010475017"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF200102M025DSPAAB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010575014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010575014.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="196uA"/>
<attribute name="I-RIPPLE" value="847mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010575014"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF200561M035DSPAAB000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010575015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010575015.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="238uA"/>
<attribute name="I-RIPPLE" value="891mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010575015"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF200681M035DSPAAB000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010675020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010675020.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="828mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010675020"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF200471M050DSPAAB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010775019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010775019.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="207.9uA"/>
<attribute name="I-RIPPLE" value="759mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010775019"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF200331M063DSPAAB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_10X16" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_10X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010275017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010275017.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="120uA"/>
<attribute name="I-RIPPLE" value="902mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010275017"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF160122M010DSPAAB000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010275018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010275018.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="150uA"/>
<attribute name="I-RIPPLE" value="1001mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010275018"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF160152M010DSPAAB000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010375016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010375016.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="131.2uA"/>
<attribute name="I-RIPPLE" value="803mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010375016"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF160821M016DSPAAB000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010375017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010375017.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="869mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010375017"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF160102M016DSPAAB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010375018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010375018.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="192uA"/>
<attribute name="I-RIPPLE" value="979mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010375018"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF160122M016DSPAAB000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010475014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010475014.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="140uA"/>
<attribute name="I-RIPPLE" value="693mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010475014"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF160561M025DSPAAB000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010475015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010475015.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="170uA"/>
<attribute name="I-RIPPLE" value="792mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010475015"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF160681M025DSPAAB000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010575013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010575013.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="164.5uA"/>
<attribute name="I-RIPPLE" value="693mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010575013"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF160471M035DSPAAB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010675019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010675019.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="649mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010675019"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF160331M050DSPAAB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010775015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010775015.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75.6uA"/>
<attribute name="I-RIPPLE" value="396mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010775015"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF160121M063DSPAAB000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010775016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010775016.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="94.5uA"/>
<attribute name="I-RIPPLE" value="462mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010775016"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF160151M063DSPAAB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010775017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010775017.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="113.4uA"/>
<attribute name="I-RIPPLE" value="528mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010775017"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF160181M063DSPAAB000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010775018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010775018.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="138.6uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010775018"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBF160221M063DSPAAB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860011375006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860011375006.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="120uA"/>
<attribute name="I-RIPPLE" value="100mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860011375006"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATAF160100M400DSPAAB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_22X41" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_22X41(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010283032">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010283032.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="2200uA"/>
<attribute name="I-RIPPLE" value="4092mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010283032"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBN410223M010DSPS2B000"/>
<attribute name="VALUE" value="22000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010383031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010383031.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="2400uA"/>
<attribute name="I-RIPPLE" value="3905mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010383031"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBN410153M016DSPS2B000"/>
<attribute name="VALUE" value="15000  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010483029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010483029.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="2500uA"/>
<attribute name="I-RIPPLE" value="3960mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010483029"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBN410103M025DSPS2B000"/>
<attribute name="VALUE" value="10000  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010583027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010583027.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="2380uA"/>
<attribute name="I-RIPPLE" value="3630mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010583027"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBN410682M035DSPS2B000"/>
<attribute name="VALUE" value="6800  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010683032">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010683032.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="2350uA"/>
<attribute name="I-RIPPLE" value="3355mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010683032"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBN410472M050DSPS2B000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010783029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010783029.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="1701uA"/>
<attribute name="I-RIPPLE" value="2860mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010783029"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBN410272M063DSPS2B000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010783030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010783030.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="22mm"/>
<attribute name="I-LEAK" value="2079uA"/>
<attribute name="I-RIPPLE" value="3080mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010783030"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBN410332M063DSPS2B000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_8X16" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_8X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010274015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010274015.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="725mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010274015"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE160102M010DSPA7B000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010374014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010374014.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="108.8uA"/>
<attribute name="I-RIPPLE" value="640mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010374014"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE160681M016DSPA7B000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_8X11.5" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_8X11.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010274012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010274012.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="56uA"/>
<attribute name="I-RIPPLE" value="506mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010274012"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115561M010DSPA7B000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010274013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010274013.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="572mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010274013"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115681M010DSPA7B000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010374011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010374011.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="407mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010374011"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115331M016DSPA7B000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010374012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010374012.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="517mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010374012"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115471M016DSPA7B000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010474012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010474012.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="451mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010474012"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115331M025DSPA7B000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010474013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010474013.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="561mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010474013"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115471M025DSPA7B000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010574008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010574008.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="42uA"/>
<attribute name="I-RIPPLE" value="275mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010574008"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115121M035DSPA7B000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010574009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010574009.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="52.5uA"/>
<attribute name="I-RIPPLE" value="308mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010574009"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115151M035DSPA7B000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010574010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010574010.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="352mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010574010"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115181M035DSPA7B000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010574011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010574011.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="385mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010574011"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115221M035DSPA7B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010674013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010674013.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="34uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010674013"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115680M050DSPA7B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010674014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010674014.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="286mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010674014"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115101M050DSPA7B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010674015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010674015.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="60uA"/>
<attribute name="I-RIPPLE" value="319mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010674015"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115121M050DSPA7B000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010774013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010774013.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="42.84uA"/>
<attribute name="I-RIPPLE" value="253mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010774013"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBE115680M063DSPA7B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860011374003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860011374003.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="26.4uA"/>
<attribute name="I-RIPPLE" value="32mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860011374003"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATAE1152R2M400DSPA7B000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860011374004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860011374004.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="39.6uA"/>
<attribute name="I-RIPPLE" value="45mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860011374004"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATAE1153R3M400DSPA7B000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860011374005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860011374005.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="56.4uA"/>
<attribute name="I-RIPPLE" value="55mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860011374005"/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATAE1154R7M400DSPA7B000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_13X20" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_13X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010278021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010278021.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="270uA"/>
<attribute name="I-RIPPLE" value="1419mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010278021"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200272M010DSPACB000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010278022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010278022.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="330uA"/>
<attribute name="I-RIPPLE" value="1540mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010278022"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200332M010DSPACB000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010278023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010278023.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="390uA"/>
<attribute name="I-RIPPLE" value="1760mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010278023"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200392M010DSPACB000"/>
<attribute name="VALUE" value="3900  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010378020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010378020.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="288uA"/>
<attribute name="I-RIPPLE" value="1298mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010378020"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200182M016DSPACB000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010378021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010378021.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="352uA"/>
<attribute name="I-RIPPLE" value="1485mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010378021"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200222M016DSPACB000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010378022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010378022.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="432uA"/>
<attribute name="I-RIPPLE" value="1716mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010378022"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200272M016DSPACB000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010378023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010378023.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="1750mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010378023"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200332M016DSPACB000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010478018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010478018.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1155mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010478018"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200122M025DSPACB000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010478019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010478019.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="375uA"/>
<attribute name="I-RIPPLE" value="1353mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010478019"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200152M025DSPACB000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010478020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010478020.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="450uA"/>
<attribute name="I-RIPPLE" value="1496mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010478020"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200182M025DSPACB000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010578016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010578016.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="287uA"/>
<attribute name="I-RIPPLE" value="1045mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010578016"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200821M035DSPACB000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010578017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010578017.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="350uA"/>
<attribute name="I-RIPPLE" value="1265mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010578017"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200102M035DSPACB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010578018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010578018.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="420uA"/>
<attribute name="I-RIPPLE" value="1375mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010578018"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200122M035DSPACB000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010678021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010678021.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="280uA"/>
<attribute name="I-RIPPLE" value="902mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010678021"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200561M050DSPACB000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010678022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010678022.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="340uA"/>
<attribute name="I-RIPPLE" value="1056mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010678022"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200681M050DSPACB000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010778020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010778020.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="296.1uA"/>
<attribute name="I-RIPPLE" value="968mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010778020"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBI200471M063DSPACB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860011378007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860011378007.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="264uA"/>
<attribute name="I-RIPPLE" value="190mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860011378007"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATAI200220M400DSPACB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_18X31.5" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_18X31.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010481026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010481026.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1400uA"/>
<attribute name="I-RIPPLE" value="2816mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010481026"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL315562M025DSPAEB000"/>
<attribute name="VALUE" value="5600  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010581024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010581024.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1365uA"/>
<attribute name="I-RIPPLE" value="2640mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010581024"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL315392M035DSPAEB000"/>
<attribute name="VALUE" value="3900  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010681029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010681029.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="2420mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010681029"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL315272M050DSPAEB000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860011381012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860011381012.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1200uA"/>
<attribute name="I-RIPPLE" value="440mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860011381012"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATAL315101M400DSPAEB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_16X31.5" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_16X31.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010280027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010280027.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="820uA"/>
<attribute name="I-RIPPLE" value="2541mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010280027"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK315822M010DSPADB000"/>
<attribute name="VALUE" value="8200  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010380026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010380026.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="896uA"/>
<attribute name="I-RIPPLE" value="2453mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010380026"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK315562M016DSPADB000"/>
<attribute name="VALUE" value="5600  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010380027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010380027.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1088uA"/>
<attribute name="I-RIPPLE" value="2805mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010380027"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK315682M016DSPADB000"/>
<attribute name="VALUE" value="6800  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010480024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010480024.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="975uA"/>
<attribute name="I-RIPPLE" value="2343mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010480024"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK315392M025DSPADB000"/>
<attribute name="VALUE" value="3900  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010480025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010480025.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1175uA"/>
<attribute name="I-RIPPLE" value="2640mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010480025"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK315472M025DSPADB000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010580022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010580022.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="2178mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010580022"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK315272M035DSPADB000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010580023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010580023.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="1155uA"/>
<attribute name="I-RIPPLE" value="2365mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010580023"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK315332M035DSPADB000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010680026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010680026.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="750uA"/>
<attribute name="I-RIPPLE" value="1848mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010680026"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK315152M050DSPADB000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010680027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010680027.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="900uA"/>
<attribute name="I-RIPPLE" value="2112mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010680027"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK315182M050DSPADB000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010780025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010780025.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="756uA"/>
<attribute name="I-RIPPLE" value="1837mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010780025"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBK315122M063DSPADB000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_18X35.5" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_18X35.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010281029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010281029.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1200uA"/>
<attribute name="I-RIPPLE" value="3025mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010281029"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL355123M010DSPAEB000"/>
<attribute name="VALUE" value="12000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010281030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010281030.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1500uA"/>
<attribute name="I-RIPPLE" value="3310mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010281030"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL355153M010DSPAEB000"/>
<attribute name="VALUE" value="15000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010381029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010381029.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1600uA"/>
<attribute name="I-RIPPLE" value="2970mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010381029"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL355103M016DSPAEB000"/>
<attribute name="VALUE" value="10000  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010381030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010381030.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1920uA"/>
<attribute name="I-RIPPLE" value="3058mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010381030"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL355123M016DSPAEB000"/>
<attribute name="VALUE" value="12000  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010481027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010481027.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1700uA"/>
<attribute name="I-RIPPLE" value="2970mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010481027"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL355682M025DSPAEB000"/>
<attribute name="VALUE" value="6800  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010481028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010481028.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="2050uA"/>
<attribute name="I-RIPPLE" value="2981mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010481028"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL355822M025DSPAEB000"/>
<attribute name="VALUE" value="8200  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010581025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010581025.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1645uA"/>
<attribute name="I-RIPPLE" value="2860mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010581025"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL355472M035DSPAEB000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010681030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010681030.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1650uA"/>
<attribute name="I-RIPPLE" value="2750mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010681030"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL355332M050DSPAEB000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010781028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010781028.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1386uA"/>
<attribute name="I-RIPPLE" value="2475mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010781028"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBL355222M063DSPAEB000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_5X11" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_5X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010272001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010272001.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="66mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010272001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110220M010DSPA3B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010272002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010272002.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="88mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010272002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110330M010DSPA3B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010272003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010272003.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="105mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010272003"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110470M010DSPA3B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010272004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010272004.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="6.8uA"/>
<attribute name="I-RIPPLE" value="132mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010272004"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110680M010DSPA3B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010272005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010272005.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="198mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010272005"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110101M010DSPA3B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010272006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010272006.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="12uA"/>
<attribute name="I-RIPPLE" value="209mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010272006"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110121M010DSPA3B000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010272007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010272007.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="15uA"/>
<attribute name="I-RIPPLE" value="231mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010272007"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110151M010DSPA3B000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010372001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010372001.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="44mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010372001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110100M016DSPA3B000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010372002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010372002.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.52uA"/>
<attribute name="I-RIPPLE" value="83mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010372002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110220M016DSPA3B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010372003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010372003.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5.28uA"/>
<attribute name="I-RIPPLE" value="84mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010372003"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110330M016DSPA3B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010372004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010372004.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="7.52uA"/>
<attribute name="I-RIPPLE" value="132mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010372004"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110470M016DSPA3B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010372005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010372005.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="10.88uA"/>
<attribute name="I-RIPPLE" value="149mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010372005"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110680M016DSPA3B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010372006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010372006.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="176mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010372006"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110101M016DSPA3B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010472001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010472001.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="34mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010472001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC1104R7M025DSPA3B000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010472002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010472002.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="50mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010472002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110100M025DSPA3B000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010472003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010472003.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5.5uA"/>
<attribute name="I-RIPPLE" value="94mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010472003"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110220M025DSPA3B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010472004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010472004.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="8.25uA"/>
<attribute name="I-RIPPLE" value="105mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010472004"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110330M025DSPA3B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010472005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010472005.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="132mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010472005"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110470M025DSPA3B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010572001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010572001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="44mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010572001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC1104R7M035DSPA3B000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010572002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010572002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.5uA"/>
<attribute name="I-RIPPLE" value="66mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010572002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110100M035DSPA3B000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010572003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010572003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="7.7uA"/>
<attribute name="I-RIPPLE" value="108mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010572003"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110220M035DSPA3B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010572004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010572004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11.55uA"/>
<attribute name="I-RIPPLE" value="121mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010572004"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110330M035DSPA3B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010572005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010572005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="16.45uA"/>
<attribute name="I-RIPPLE" value="143mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010572005"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110470M035DSPA3B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010672001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010672001.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="3.3mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010672001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110R10M050DSPA3B000"/>
<attribute name="VALUE" value="0.1  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010672002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010672002.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="3.3mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010672002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110R22M050DSPA3B000"/>
<attribute name="VALUE" value="0.22  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010672003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010672003.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="5.5mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010672003"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110R33M050DSPA3B000"/>
<attribute name="VALUE" value="0.33  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010672004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010672004.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="7.5mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010672004"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110R47M050DSPA3B000"/>
<attribute name="VALUE" value="0.47  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010672005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010672005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="17mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010672005"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110010M050DSPA3B000"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010672006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010672006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="28mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010672006"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC1102R2M050DSPA3B000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010672007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010672007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="39mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010672007"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC1103R3M050DSPA3B000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010672008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010672008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="46mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010672008"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC1104R7M050DSPA3B000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010672009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010672009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="72mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010672009"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110100M050DSPA3B000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010672010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010672010.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="110mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010672010"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110220M050DSPA3B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010672011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010672011.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="132mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010672011"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110330M050DSPA3B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010772001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010772001.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="4mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010772001"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110R10M063DSPA3B000"/>
<attribute name="VALUE" value="0.1  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010772002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010772002.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="4mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010772002"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110R22M063DSPA3B000"/>
<attribute name="VALUE" value="0.22  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010772003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010772003.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="6mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010772003"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110R33M063DSPA3B000"/>
<attribute name="VALUE" value="0.33  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010772004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010772004.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="8mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010772004"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110R47M063DSPA3B000"/>
<attribute name="VALUE" value="0.47  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010772005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010772005.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="17mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010772005"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110010M063DSPA3B000"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010772006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010772006.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="31mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010772006"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC1102R2M063DSPA3B000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010772007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010772007.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="39mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010772007"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC1103R3M063DSPA3B000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010772008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010772008.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="50mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010772008"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC1104R7M063DSPA3B000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010772009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010772009.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="6.3uA"/>
<attribute name="I-RIPPLE" value="77mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010772009"/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBC110100M063DSPA3B000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATG8_6.3X11" prefix="C">
<description>&lt;b&gt;WCAP-ATG8 Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +85 °C &lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C 
&lt;BR&gt;Wide range of capacitance value 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.1 µF ‒ 33000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 400 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-40 °C up to +85 °C for UR &lt; 400 V(DC) 
&lt;BR&gt;-25 °C up to +85 °C for UR ≥ 400 V(DC) 
&lt;BR&gt;Endurance: 2000 h @ +85 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 22.0 x 51.0 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o35732v209%20WCAP-ATG8_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATG8/"&gt;https://www.we-online.com/catalog/en/WCAP-ATG8/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-27
&lt;br&gt;2020(C) W��rth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATG8_6.3X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860010273008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010273008.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="18uA"/>
<attribute name="I-RIPPLE" value="253mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010273008"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110181M010DSPA4B000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010273009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010273009.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="294mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010273009"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110221M010DSPA4B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010273010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010273010.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="363mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010273010"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110331M010DSPA4B000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010273011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010273011.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="418mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010273011"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110471M010DSPA4B000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860010373007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010373007.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="19.2uA"/>
<attribute name="I-RIPPLE" value="231mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010373007"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110121M016DSPA4B000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010373008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010373008.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="24uA"/>
<attribute name="I-RIPPLE" value="253mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010373008"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110151M016DSPA4B000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010373009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010373009.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="28.8uA"/>
<attribute name="I-RIPPLE" value="275mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010373009"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110181M016DSPA4B000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010373010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010373010.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="308mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010373010"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110221M016DSPA4B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860010473006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010473006.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="17uA"/>
<attribute name="I-RIPPLE" value="176mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010473006"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110680M025DSPA4B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010473007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010473007.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="209mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010473007"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110101M025DSPA4B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010473008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010473008.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="30uA"/>
<attribute name="I-RIPPLE" value="253mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010473008"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110121M025DSPA4B000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010473009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010473009.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="37.5uA"/>
<attribute name="I-RIPPLE" value="275mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010473009"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110151M025DSPA4B000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010473010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010473010.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="45uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010473010"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110181M025DSPA4B000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010473011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010473011.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="310mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010473011"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110221M025DSPA4B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860010573006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010573006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="23.8uA"/>
<attribute name="I-RIPPLE" value="198mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010573006"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110680M035DSPA4B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010573007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010573007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="231mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010573007"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110101M035DSPA4B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860010673012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010673012.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="165mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010673012"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110470M050DSPA4B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860010773010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010773010.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="13.86uA"/>
<attribute name="I-RIPPLE" value="127mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010773010"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110220M063DSPA4B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010773011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010773011.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="149mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010773011"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110330M063DSPA4B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860010773012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860010773012.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="29.61uA"/>
<attribute name="I-RIPPLE" value="198mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860010773012"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATBD110470M063DSPA4B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860011373001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860011373001.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="5.64uA"/>
<attribute name="I-RIPPLE" value="12mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860011373001"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATAD110R47M400DSPA4B000"/>
<attribute name="VALUE" value="0.47  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
<technology name="_860011373002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860011373002.pdf"/>
<attribute name="DF" value="15%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="12uA"/>
<attribute name="I-RIPPLE" value="20mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="860011373002"/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATAD110010M400DSPA4B000"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="400V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
