<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-ATLI&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-02-28&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-ATLI_6.3X15(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,6.3X15X2.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_16X35.5(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X35.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_13X25(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,13X25X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_5X11(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X11X2X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_6.3X11(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,6.3X11X2.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_16X31.5(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt;Aluminium Electrolytic Capacitors,16X31.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_8X20(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,8X20X3.5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_8X16(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt;   Aluminium Electrolytic Capacitors,8X16X3.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_13X30(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,13X30X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_13X20(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,13X20X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_10X16(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X16X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_18X31.5(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X31.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_10X12.5(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X12.5X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_10X20(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X20X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_13X35(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,13X35X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_16X21(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X21X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_10X30(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X30X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_8X11.5X(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,8X11.5X3.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_16X25(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X25X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLI_10X25(DXL)">
<description>&lt;B&gt;WCAP-ATLI&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X25X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-ATLI_6.3X15" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_6.3X15(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080273008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080273008.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="27uA"/>
<attribute name="I-RIPPLE" value="460mA"/>
<attribute name="L" value="15mm"/>
<attribute name="PART-NUMBER" value=" 860080273008 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150271M010DSPA4B000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080473007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080473007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="30uA"/>
<attribute name="I-RIPPLE" value="490mA"/>
<attribute name="L" value="15mm"/>
<attribute name="PART-NUMBER" value=" 860080473007 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150121M025DSPA4B000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_16X35.5" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_16X35.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080580027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080580027.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="770uA"/>
<attribute name="I-RIPPLE" value="3750mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="PART-NUMBER" value=" 860080580027 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK355222M035DSPADE000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080780028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080780028.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="2780mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="PART-NUMBER" value=" 860080780028 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK355102M063DSPADE000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_13X25" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_13X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080278022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080278022.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="330uA"/>
<attribute name="I-RIPPLE" value="2720mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080278022 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250332M010DSPACE000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080378024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080378024.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="352uA"/>
<attribute name="I-RIPPLE" value="2750mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080378024 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250222M016DSPACE000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080378025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080378025.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="432uA"/>
<attribute name="I-RIPPLE" value="3000mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080378025 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250272M016DSPACE000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080478022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080478022.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="375uA"/>
<attribute name="I-RIPPLE" value="2710mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080478022 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250152M025DSPACE000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080578020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080578020.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="287uA"/>
<attribute name="I-RIPPLE" value="2630mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080578020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250821M035DSPACE000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080578021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080578021.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="350uA"/>
<attribute name="I-RIPPLE" value="2780mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080578021 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250102M035DSPACE000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080678021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080678021.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="340uA"/>
<attribute name="I-RIPPLE" value="2490mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080678021 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250681M050DSPACE000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080778021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080778021.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="207.9uA"/>
<attribute name="I-RIPPLE" value="1870mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080778021 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250331M063DSPACE000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860080778022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080778022.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="245.7uA"/>
<attribute name="I-RIPPLE" value="1920mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080778022 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250391M063DSPACE000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_5X11" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_5X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080272001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080272001.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="6.8uA"/>
<attribute name="I-RIPPLE" value="190mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080272001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110680M010DSPA3B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080272002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080272002.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="8.2uA"/>
<attribute name="I-RIPPLE" value="210mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080272002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110820M010DSPA3B000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080272003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080272003.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="242mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080272003 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110101M010DSPA3B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080272004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080272004.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="12uA"/>
<attribute name="I-RIPPLE" value="261mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080272004 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110121M010DSPA3B000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080372001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080372001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="7.52uA"/>
<attribute name="I-RIPPLE" value="200mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080372001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110470M016DSPA3B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080372002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080372002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="8.96uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080372002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110560M016DSPA3B000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080372003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080372003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="10.88uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080372003 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110680M016DSPA3B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080372004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080372004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="13.12uA"/>
<attribute name="I-RIPPLE" value="260mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080372004 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110820M016DSPA3B000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080472001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080472001.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="9.75uA"/>
<attribute name="I-RIPPLE" value="210mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080472001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110390M025DSPA3B000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080472002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080472002.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080472002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110470M025DSPA3B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080472003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080472003.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="14uA"/>
<attribute name="I-RIPPLE" value="256mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080472003 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110560M025DSPA3B000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080572001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080572001.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11.55uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080572001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110330M035DSPA3B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080672001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080672001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080672001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110220M050DSPA3B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080772001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080772001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="6.3uA"/>
<attribute name="I-RIPPLE" value="135mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080772001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110100M063DSPA3B000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860080872002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080872002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="125mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080872002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC1104R7M100DSPA3B0RE"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_6.3X11" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_6.3X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080273005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080273005.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="15uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080273005 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110151M010DSPA4B000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080273006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080273006.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="18uA"/>
<attribute name="I-RIPPLE" value="350mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080273006 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110181M010DSPA4B000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080273007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080273007.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="390mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080273007 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110221M010DSPA4B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080373005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080373005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="360mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080373005 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110101M016DSPA4B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080373006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080373006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="19.2uA"/>
<attribute name="I-RIPPLE" value="365mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080373006 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110121M016DSPA4B000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080373007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080373007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="24uA"/>
<attribute name="I-RIPPLE" value="385mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080373007 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110151M016DSPA4B000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080473004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080473004.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="17uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080473004 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110680M025DSPA4B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080473005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080473005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="20.5uA"/>
<attribute name="I-RIPPLE" value="350mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080473005 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110820M025DSPA4B000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080473006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080473006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="410mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080473006 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110101M025DSPA4B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080573002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080573002.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="13.65uA"/>
<attribute name="I-RIPPLE" value="277mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080573002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110390M035DSPA4B000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080573003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080573003.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="16.45uA"/>
<attribute name="I-RIPPLE" value="340mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080573003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110470M035DSPA4B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080573004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080573004.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="19.6uA"/>
<attribute name="I-RIPPLE" value="375mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080573004 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110560M035DSPA4B000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080573005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080573005.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="23.8uA"/>
<attribute name="I-RIPPLE" value="400mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080573005 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110680M035DSPA4B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080673002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080673002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="13.5uA"/>
<attribute name="I-RIPPLE" value="265mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080673002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110270M050DSPA4B000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080673003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080673003.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080673003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110330M050DSPA4B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080673004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080673004.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="19.5uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080673004 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110390M050DSPA4B000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080773002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080773002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="9.45uA"/>
<attribute name="I-RIPPLE" value="168mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080773002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110150M063DSPA4B000"/>
<attribute name="VALUE" value="15  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860080773003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080773003.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="11.34uA"/>
<attribute name="I-RIPPLE" value="170mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080773003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110180M063DSPA4B000"/>
<attribute name="VALUE" value="18  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860080773004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080773004.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="13.86uA"/>
<attribute name="I-RIPPLE" value="250mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080773004 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110220M063DSPA4B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860080773005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080773005.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="17.01uA"/>
<attribute name="I-RIPPLE" value="260mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080773005 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110270M063DSPA4B000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860080773006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080773006.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="270mA"/>
<attribute name="L" value="11mm"/>
<attribute name="PART-NUMBER" value=" 860080773006 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110330M063DSPA4B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_16X31.5" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_16X31.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080280025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080280025.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="560uA"/>
<attribute name="I-RIPPLE" value="3460mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="PART-NUMBER" value=" 860080280025 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315562M010DSPADE000"/>
<attribute name="VALUE" value="5600  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080280026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080280026.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="680uA"/>
<attribute name="I-RIPPLE" value="3630mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="PART-NUMBER" value=" 860080280026 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315682M010DSPADE000"/>
<attribute name="VALUE" value="6800  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080380028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080380028.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="752uA"/>
<attribute name="I-RIPPLE" value="3770mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="PART-NUMBER" value=" 860080380028 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315472M016DSPADE000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080480025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080480025.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="675uA"/>
<attribute name="I-RIPPLE" value="3480mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="PART-NUMBER" value=" 860080480025 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315272M025DSPADE000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080480026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080480026.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="825uA"/>
<attribute name="I-RIPPLE" value="3600mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="PART-NUMBER" value=" 860080480026 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315332M025DSPADE000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080580025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080580025.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="525uA"/>
<attribute name="I-RIPPLE" value="3600mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="PART-NUMBER" value=" 860080580025 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315152M035DSPADE000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080580026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080580026.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="3670mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="PART-NUMBER" value=" 860080580026 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315182M035DSPADE000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080780026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080780026.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="428.4uA"/>
<attribute name="I-RIPPLE" value="2600mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="PART-NUMBER" value=" 860080780026 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315681M063DSPADE000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860080780027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080780027.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="516.6uA"/>
<attribute name="I-RIPPLE" value="2650mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="PART-NUMBER" value=" 860080780027 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315821M063DSPADE000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_8X16" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_8X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080274012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080274012.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="56uA"/>
<attribute name="I-RIPPLE" value="870mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080274012 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160561M010DSPA7C000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080374012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080374012.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="62.4uA"/>
<attribute name="I-RIPPLE" value="790mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080374012 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160391M016DSPA7C000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080374013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080374013.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="990mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080374013 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160471M016DSPA7C000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080474011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080474011.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="67.5uA"/>
<attribute name="I-RIPPLE" value="850mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080474011 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160271M025DSPA7C000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080474012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080474012.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="990mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080474012 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160331M025DSPA7C000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080574010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080574010.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="810mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080574010 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160181M035DSPA7C000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080574011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080574011.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080574011 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160221M035DSPA7C000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080674010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080674010.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="60uA"/>
<attribute name="I-RIPPLE" value="770mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080674010 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160121M050DSPA7C000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080774011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080774011.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="51.66uA"/>
<attribute name="I-RIPPLE" value="540mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080774011 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160820M063DSPA7C000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_8X20" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_8X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080274013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080274013.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="1010mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080274013 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200681M010DSPA7C000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080274014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080274014.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="82uA"/>
<attribute name="I-RIPPLE" value="1030mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080274014 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200821M010DSPA7C000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080274015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080274015.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="1220mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080274015 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200102M010DSPA7C000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080374015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080374015.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="89.6uA"/>
<attribute name="I-RIPPLE" value="1070mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080374015 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200561M016DSPA7C000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080374016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080374016.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="108.8uA"/>
<attribute name="I-RIPPLE" value="1120mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080374016 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200681M016DSPA7C000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080474015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080474015.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="1260mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080474015 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200471M025DSPA7C000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080574014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080574014.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="1210mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080574014 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200331M035DSPA7C000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080674013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080674013.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="90uA"/>
<attribute name="I-RIPPLE" value="1060mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080674013 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200181M050DSPA7C000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080774014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080774014.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="75.6uA"/>
<attribute name="I-RIPPLE" value="790mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080774014 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200121M063DSPA7C000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_13X30" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_13X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080278023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080278023.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="390uA"/>
<attribute name="I-RIPPLE" value="3000mA"/>
<attribute name="L" value="30mm"/>
<attribute name="PART-NUMBER" value=" 860080278023 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI300392M010DSPACE000"/>
<attribute name="VALUE" value="3900  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080478023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080478023.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="450uA"/>
<attribute name="I-RIPPLE" value="3150mA"/>
<attribute name="L" value="30mm"/>
<attribute name="PART-NUMBER" value=" 860080478023 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI300182M025DSPACE000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080578022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080578022.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="420uA"/>
<attribute name="I-RIPPLE" value="2950mA"/>
<attribute name="L" value="30mm"/>
<attribute name="PART-NUMBER" value=" 860080578022 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI300122M035DSPACE000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080678022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080678022.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="410uA"/>
<attribute name="I-RIPPLE" value="2770mA"/>
<attribute name="L" value="30mm"/>
<attribute name="PART-NUMBER" value=" 860080678022 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI300821M050DSPACE000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080778023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080778023.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="296.1uA"/>
<attribute name="I-RIPPLE" value="2225mA"/>
<attribute name="L" value="30mm"/>
<attribute name="PART-NUMBER" value=" 860080778023 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI300471M063DSPACE000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_13X20" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_13X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080278020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080278020.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="2370mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080278020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200222M010DSPACE000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080278021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080278021.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="270uA"/>
<attribute name="I-RIPPLE" value="2400mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080278021 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200272M010DSPACE000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080378022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080378022.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="240uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080378022 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200152M016DSPACE000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080378023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080378023.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="288uA"/>
<attribute name="I-RIPPLE" value="2380mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080378023 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200182M016DSPACE000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080478020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080478020.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="2340mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080478020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200102M025DSPACE000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080478021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080478021.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="2390mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080478021 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200122M025DSPACE000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080578019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080578019.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="238uA"/>
<attribute name="I-RIPPLE" value="2260mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080578019 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200681M035DSPACE000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080678018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080678018.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="195uA"/>
<attribute name="I-RIPPLE" value="1910mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080678018 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200391M050DSPACE000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080678019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080678019.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080678019 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200471M050DSPACE000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080678020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080678020.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="280uA"/>
<attribute name="I-RIPPLE" value="2150mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080678020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200561M050DSPACE000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080778019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080778019.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="170.1uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080778019 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200271M063DSPACE000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_10X16" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_10X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080275016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080275016.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080275016 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160102M010DSPAAE000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080375017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080375017.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="108.8uA"/>
<attribute name="I-RIPPLE" value="1280mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080375017 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160681M016DSPAAE000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080475016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080475016.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="1415mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080475016 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160471M025DSPAAE000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080575013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080575013.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="94.5uA"/>
<attribute name="I-RIPPLE" value="1190mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080575013 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160271M035DSPAAE000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080575015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080575015.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080575015 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160331M035DSPAAE000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080675014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080675014.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="90uA"/>
<attribute name="I-RIPPLE" value="1090mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080675014 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160181M050DSPAAE000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080675015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080675015.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="1385mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080675015 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160221M050DSPAAE000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080775015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080775015.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75.6uA"/>
<attribute name="I-RIPPLE" value="835mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080775015 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160121M063DSPAAE000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860080775016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080775016.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="94.5uA"/>
<attribute name="I-RIPPLE" value="900mA"/>
<attribute name="L" value="16mm"/>
<attribute name="PART-NUMBER" value=" 860080775016 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160151M063DSPAAE000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_18X31.5" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_18X31.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080581028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080581028.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="3850mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="PART-NUMBER" value=" 860080581028 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEL315272M035DSPAEE000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080781029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080781029.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="3230mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="PART-NUMBER" value=" 860080781029 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEL315102M063DSPAEE000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_10X12.5" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_10X12.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080375014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080375014.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="PART-NUMBER" value=" 860080375014 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125471M016DSPA9E000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080475013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080475013.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="1010mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="PART-NUMBER" value=" 860080475013 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125331M025DSPA9E000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080475014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080475014.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="97.5uA"/>
<attribute name="I-RIPPLE" value="1050mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="PART-NUMBER" value=" 860080475014 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125391M025DSPA9E000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080575012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080575012.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="1060mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="PART-NUMBER" value=" 860080575012 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125221M035DSPA9E000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080675011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080675011.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="60uA"/>
<attribute name="I-RIPPLE" value="790mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="PART-NUMBER" value=" 860080675011 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125121M050DSPA9E000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080675012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080675012.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75uA"/>
<attribute name="I-RIPPLE" value="870mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="PART-NUMBER" value=" 860080675012 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125151M050DSPA9E000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080775010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080775010.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="42.84uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="PART-NUMBER" value=" 860080775010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125680M063DSPA9E000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860080775012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080775012.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="51.66uA"/>
<attribute name="I-RIPPLE" value="570mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="PART-NUMBER" value=" 860080775012 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125820M063DSPA9E000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860080775013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080775013.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="720mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="PART-NUMBER" value=" 860080775013 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125101M063DSPA9E000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_13X35" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_13X35(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080278024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080278024.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="3450mA"/>
<attribute name="L" value="35mm"/>
<attribute name="PART-NUMBER" value=" 860080278024 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI350472M010DSPABE000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080378026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080378026.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="3490mA"/>
<attribute name="L" value="35mm"/>
<attribute name="PART-NUMBER" value=" 860080378026 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI350332M016DSPABE000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080478024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080478024.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="550uA"/>
<attribute name="I-RIPPLE" value="3420mA"/>
<attribute name="L" value="35mm"/>
<attribute name="PART-NUMBER" value=" 860080478024 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI350222M025DSPABE000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080578024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080578024.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="525uA"/>
<attribute name="I-RIPPLE" value="3350mA"/>
<attribute name="L" value="35mm"/>
<attribute name="PART-NUMBER" value=" 860080578024 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI350152M035DSPABE000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_16X21" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_16X21(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080780024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080780024.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="296.1uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="L" value="21mm"/>
<attribute name="PART-NUMBER" value=" 860080780024 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK210471M063DSPAEE000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_10X30" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_10X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080775020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080775020.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="207.9uA"/>
<attribute name="I-RIPPLE" value="1750mA"/>
<attribute name="L" value="30mm"/>
<attribute name="PART-NUMBER" value=" 860080775020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF300331M063DSPAAE000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_10X20" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_10X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080275017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080275017.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="120uA"/>
<attribute name="I-RIPPLE" value="1560mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080275017 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200122M010DSPAAE000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080275018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080275018.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="150uA"/>
<attribute name="I-RIPPLE" value="1670mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080275018 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200152M010DSPAAE000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080375018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080375018.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="131.2uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080375018 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200821M016DSPAAE000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080375019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080375019.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="1840mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080375019 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200102M016DSPAAE000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080475017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080475017.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="140uA"/>
<attribute name="I-RIPPLE" value="1450mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080475017 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200561M025DSPAAE000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080475018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080475018.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="170uA"/>
<attribute name="I-RIPPLE" value="1570mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080475018 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200681M025DSPAAE000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080575016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080575016.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="136.5uA"/>
<attribute name="I-RIPPLE" value="1550mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080575016 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200391M035DSPAAE000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080575017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080575017.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="164.5uA"/>
<attribute name="I-RIPPLE" value="1850mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080575017 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200471M035DSPAAE000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080675016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080675016.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="135uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080675016 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200271M050DSPAAE000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080775017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080775017.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="113.4uA"/>
<attribute name="I-RIPPLE" value="1200mA"/>
<attribute name="L" value="20mm"/>
<attribute name="PART-NUMBER" value=" 860080775017 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200181M063DSPAAE000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_8X11.5" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_8X11.5X(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080274009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080274009.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="540mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080274009 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115331M010DSPA7C000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080274010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080274010.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="39uA"/>
<attribute name="I-RIPPLE" value="620mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080274010 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115391M010DSPA7C000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080274011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080274011.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="750mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080274011 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115471M010DSPA7C000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080374008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080374008.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="28.8uA"/>
<attribute name="I-RIPPLE" value="520mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080374008 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115181M016DSPA7C000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080374009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080374009.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="575mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080374009 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115221M016DSPA7C000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080374010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080374010.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="43.2uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080374010 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115271M016DSPA7C000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080374011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080374011.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="740mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080374011 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115331M016DSPA7C000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080474008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080474008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="37.5uA"/>
<attribute name="I-RIPPLE" value="540mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080474008 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115151M025DSPA7C000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080474009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080474009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="45uA"/>
<attribute name="I-RIPPLE" value="620mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080474009 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115181M025DSPA7C000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080474010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080474010.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="750mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080474010 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115221M025DSPA7C000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080574006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080574006.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="28.7uA"/>
<attribute name="I-RIPPLE" value="480mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080574006 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115820M035DSPA7C000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080574007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080574007.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="560mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080574007 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115101M035DSPA7C000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080574008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080574008.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="42uA"/>
<attribute name="I-RIPPLE" value="585mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080574008 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115121M035DSPA7C000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080574009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080574009.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="52.5uA"/>
<attribute name="I-RIPPLE" value="680mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080574009 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115151M035DSPA7C000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080674005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080674005.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="360mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080674005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115470M050DSPA7C000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080674006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080674006.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="28uA"/>
<attribute name="I-RIPPLE" value="375mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080674006 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115560M050DSPA7C000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080674007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080674007.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="34uA"/>
<attribute name="I-RIPPLE" value="400mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080674007 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115680M050DSPA7C000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080674008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080674008.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="41uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080674008 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115820M050DSPA7C000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080674009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080674009.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="730mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080674009 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115101M050DSPA7C000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080774007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080774007.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="24.57uA"/>
<attribute name="I-RIPPLE" value="320mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080774007 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115390M063DSPA7C000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860080774008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080774008.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="29.61uA"/>
<attribute name="I-RIPPLE" value="400mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080774008 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115470M063DSPA7C000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860080774009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080774009.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="35.28uA"/>
<attribute name="I-RIPPLE" value="420mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 860080774009 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115560M063DSPA7C000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_10X25" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_10X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080275019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080275019.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="180uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080275019 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250182M010DSPAAE000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860080375020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080375020.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="192uA"/>
<attribute name="I-RIPPLE" value="1920mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080375020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250122M016DSPAAE000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080375021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080375021.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="240uA"/>
<attribute name="I-RIPPLE" value="2050mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080375021 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250152M016DSPAAE000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080475019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080475019.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="205uA"/>
<attribute name="I-RIPPLE" value="1910mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080475019 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250821M025DSPAAE000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860080575018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080575018.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="196uA"/>
<attribute name="I-RIPPLE" value="2040mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080575018 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250561M035DSPAAE000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080675017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080675017.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="1850mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080675017 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250331M050DSPAAE000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080775018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080775018.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="138.6uA"/>
<attribute name="I-RIPPLE" value="1315mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080775018 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250221M063DSPAAE000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLI_16X25" prefix="C">
<description>&lt;b&gt;WCAP-ATLI Aluminium Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Impedance +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 63 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 31.5 
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance, especially for filtering applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14729v209%20Family_WCAP-ATLI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLI/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLI/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-28
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLI_16X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860080380027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080380027.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="624uA"/>
<attribute name="I-RIPPLE" value="3520mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080380027 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK250392M016DSPAEE000"/>
<attribute name="VALUE" value="3900  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860080580023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080580023.pdf"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="420uA"/>
<attribute name="I-RIPPLE" value="3150mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080580023 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK250122M035DSPAEE000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860080680023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080680023.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="410uA"/>
<attribute name="I-RIPPLE" value="2960mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080680023 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK250821M050DSPAEE000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080680024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080680024.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="500uA"/>
<attribute name="I-RIPPLE" value="3000mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080680024 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK250102M050DSPAEE000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860080780025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860080780025.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="352.8uA"/>
<attribute name="I-RIPPLE" value="2350mA"/>
<attribute name="L" value="25mm"/>
<attribute name="PART-NUMBER" value=" 860080780025 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK250561M063DSPAEE000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
