<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-ATLL&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-02&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-ATLL_18X31.5(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X31.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_18X35.5(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X35.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_18X25(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X25X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_13X35(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,13X35X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_16X25(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X25X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_13X30(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,13X30X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_10X30(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X30X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_10X25(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X25X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_16X35.5(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X35.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_13X20(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt;Aluminium Electrolytic Capacitors,13X20X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_10X20(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,10X20X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_13X25(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,13X25X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_16X31.5(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt;Aluminium Electrolytic Capacitors,16X31.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_8X20(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,8X20X3.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_8X11.5(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,8X11.5X3.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_6.3X11(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,6.3X11X2.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_10X12.5(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X12.5X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_5X11(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X11X2X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_10X16(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,10X16X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_6.3X15(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,6.3X15X2.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATLL_8X16(DXL)">
<description>&lt;B&gt;WCAP-ATLL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,8X16X3.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-ATLL_18X31.5" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_18X31.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160381046">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160381046.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="896uA"/>
<attribute name="I-RIPPLE" value="3084mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160381046 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEL315562M016DSPAEG000"/>
<attribute name="VALUE" value="5600  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160581040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160581040.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="3336mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160581040 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEL315272M035DSPAEG000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_18X35.5" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_18X35.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160381047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160381047.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1088uA"/>
<attribute name="I-RIPPLE" value="3252mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160381047 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEL355682M016DSPAEG000"/>
<attribute name="VALUE" value="6800  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_18X25" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_18X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160381045">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160381045.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="752uA"/>
<attribute name="I-RIPPLE" value="2844mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160381045 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEL250472M016DSPAEG000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160481038">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160481038.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="825uA"/>
<attribute name="I-RIPPLE" value="3156mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160481038 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEL250332M025DSPAEG000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160581039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160581039.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="770uA"/>
<attribute name="I-RIPPLE" value="3132mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160581039 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEL250222M035DSPAEG000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_13X35" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_13X35(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160278046">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160278046.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="560uA"/>
<attribute name="I-RIPPLE" value="2640mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160278046 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI350562M010DSPABG000"/>
<attribute name="VALUE" value="5600  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160378042">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160378042.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="624uA"/>
<attribute name="I-RIPPLE" value="2664mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160378042 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI350392M016DSPABG000"/>
<attribute name="VALUE" value="3900  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160478035">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160478035.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="675uA"/>
<attribute name="I-RIPPLE" value="2850mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160478035 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI350272M025DSPABK000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160578034">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160578034.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="525uA"/>
<attribute name="I-RIPPLE" value="2820mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160578034 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI350152M035DSPABG000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160578036">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160578036.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="2976mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160578036 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI350182M035DSPABG000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_16X25" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_16X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160280045">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160280045.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="2634mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160280045 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK250472M010DSPAEG000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160380041">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160380041.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="2700mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160380041 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK250332M016DSPAEG000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160380043">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160380043.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="624uA"/>
<attribute name="I-RIPPLE" value="2736mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160380043 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK250392M016DSPAEG000"/>
<attribute name="VALUE" value="3900  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160480032">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160480032.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="450uA"/>
<attribute name="I-RIPPLE" value="2340mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160480032 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK250182M025DSPAEK000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160480034">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160480034.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="550uA"/>
<attribute name="I-RIPPLE" value="2712mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160480034 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK250222M025DSPAEK000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160680034">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160680034.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="500uA"/>
<attribute name="I-RIPPLE" value="2676mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160680034 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK250102M050DSPAEG000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_13X30" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_13X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160278044">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160278044.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="2484mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160278044 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI300472M010DSPACG000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160378040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160378040.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="2562mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160378040 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI300332M016DSPACG000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160478031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160478031.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="450uA"/>
<attribute name="I-RIPPLE" value="2310mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160478031 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI300182M025DSPACK000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160478033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160478033.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="550uA"/>
<attribute name="I-RIPPLE" value="2592mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160478033 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI300222M025DSPACG000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160678033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160678033.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="410uA"/>
<attribute name="I-RIPPLE" value="2412mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160678033 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI300821M050DSPACG000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_10X30" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_10X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160275039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160275039.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="270uA"/>
<attribute name="I-RIPPLE" value="2076mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160275039 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF300272M010DSPAAG000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160275041">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160275041.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="330uA"/>
<attribute name="I-RIPPLE" value="2232mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160275041 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF300332M010DSPAAF000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160375036">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160375036.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="288uA"/>
<attribute name="I-RIPPLE" value="1776mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160375036 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF300182M016DSPAAF000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160575031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160575031.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="350uA"/>
<attribute name="I-RIPPLE" value="2136mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160575031 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF300102M035DSPAAF000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_10X25" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_10X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160275035">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160275035.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="180uA"/>
<attribute name="I-RIPPLE" value="1650mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160275035 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250182M010DSPAAG000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160275037">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160275037.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1776mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160275037 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250222M010DSPAAF000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160375034">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160375034.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="240uA"/>
<attribute name="I-RIPPLE" value="1620mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160375034 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250152M016DSPAAF000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160475027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160475027.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="1812mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160475027 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250102M025DSPAAF000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160575026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160575026.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="196uA"/>
<attribute name="I-RIPPLE" value="1572mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160575026 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250561M035DSPAAF000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160575028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160575028.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="238uA"/>
<attribute name="I-RIPPLE" value="1680mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160575028 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250681M035DSPAAF000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160675028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160675028.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="1404mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160675028 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF250331M050DSPAAF000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_16X35.5" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_16X35.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160680036">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160680036.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="750uA"/>
<attribute name="I-RIPPLE" value="3216mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160680036 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK355152M050DSPADG000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_10X20" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_10X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160275034">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160275034.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="150uA"/>
<attribute name="I-RIPPLE" value="1536mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160275034 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200152M010DSPAAG000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160375033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160375033.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="192uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160375033 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200122M016DSPAAF000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160475025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160475025.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="170uA"/>
<attribute name="I-RIPPLE" value="1470mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160475025 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200681M025DSPAAG000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160475026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160475026.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="205uA"/>
<attribute name="I-RIPPLE" value="1668mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160475026 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200821M025DSPAAF000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160575025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160575025.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="164.5uA"/>
<attribute name="I-RIPPLE" value="1302mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160575025 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200471M035DSPAAF000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160675027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160675027.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="135uA"/>
<attribute name="I-RIPPLE" value="1212mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160675027 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF200271M050DSPAAF000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_13X25" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_13X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160278042">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160278042.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="330uA"/>
<attribute name="I-RIPPLE" value="2268mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160278042 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250332M010DSPACG000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160278043">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160278043.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="390uA"/>
<attribute name="I-RIPPLE" value="2304mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160278043 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250392M010DSPACG000"/>
<attribute name="VALUE" value="3900  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160378039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160378039.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="432uA"/>
<attribute name="I-RIPPLE" value="2436mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160378039 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250272M016DSPACG000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160578032">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160578032.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="350uA"/>
<attribute name="I-RIPPLE" value="2184mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160578032 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250102M035DSPACG000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160578033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160578033.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="420uA"/>
<attribute name="I-RIPPLE" value="2292mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160578033 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250122M035DSPACG000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160678032">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160678032.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="340uA"/>
<attribute name="I-RIPPLE" value="2304mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160678032 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI250681M050DSPACG000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_13X20" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_13X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160278036">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160278036.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="180uA"/>
<attribute name="I-RIPPLE" value="1704mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160278036 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200182M010DSPACK000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160278038">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160278038.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1872mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160278038 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200222M010DSPACK000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160278040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160278040.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="270uA"/>
<attribute name="I-RIPPLE" value="2028mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160278040 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200272M010DSPACG000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160378035">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160378035.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="240uA"/>
<attribute name="I-RIPPLE" value="1728mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160378035 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200152M016DSPACK000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160378037">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160378037.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="288uA"/>
<attribute name="I-RIPPLE" value="1854mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160378037 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200182M016DSPACG000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160378038">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160378038.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="352uA"/>
<attribute name="I-RIPPLE" value="2082mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160378038 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200222M016DSPACG000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160478028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160478028.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="1872mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160478028 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200102M025DSPACK000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160478029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160478029.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="2028mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160478029 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200122M025DSPACK000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160478030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160478030.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="375uA"/>
<attribute name="I-RIPPLE" value="2124mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160478030 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200152M025DSPACG000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160578027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160578027.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="196uA"/>
<attribute name="I-RIPPLE" value="1584mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160578027 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200561M035DSPACK000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160578029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160578029.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="238uA"/>
<attribute name="I-RIPPLE" value="1692mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160578029 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200681M035DSPACK000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160578030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160578030.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="287uA"/>
<attribute name="I-RIPPLE" value="1818mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160578030 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200821M035DSPACG000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160678029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160678029.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160678029 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200331M050DSPACK000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160678030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160678030.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="1776mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160678030 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200471M050DSPACG000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160678031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160678031.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="280uA"/>
<attribute name="I-RIPPLE" value="2094mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160678031 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEI200561M050DSPACG000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_8X20" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_8X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160274032">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160274032.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="120uA"/>
<attribute name="I-RIPPLE" value="1248mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160274032 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200122M010DSPA7D000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160374028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160374028.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="108.8uA"/>
<attribute name="I-RIPPLE" value="960mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160374028 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200681M016DSPA7D000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160374030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160374030.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="131.2uA"/>
<attribute name="I-RIPPLE" value="1104mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160374030 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200821M016DSPA7D000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160474021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160474021.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="1056mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160474021 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200471M025DSPA7G000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160474023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160474023.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="140uA"/>
<attribute name="I-RIPPLE" value="1224mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160474023 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200561M025DSPA7D000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160574021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160574021.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="94.5uA"/>
<attribute name="I-RIPPLE" value="1056mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160574021 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200271M035DSPA7D000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160574023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160574023.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="1140mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160574023 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200331M035DSPA7D000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160674024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160674024.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="90uA"/>
<attribute name="I-RIPPLE" value="864mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160674024 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE200181M050DSPA7D000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_16X31.5" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_16X31.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160280047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160280047.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="560uA"/>
<attribute name="I-RIPPLE" value="2736mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160280047 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315562M010DSPADK000"/>
<attribute name="VALUE" value="5600  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160280048">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160280048.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="680uA"/>
<attribute name="I-RIPPLE" value="2964mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160280048 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315682M010DSPADK000"/>
<attribute name="VALUE" value="6800  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160380044">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160380044.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="752uA"/>
<attribute name="I-RIPPLE" value="2886mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160380044 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315472M016DSPADK000"/>
<attribute name="VALUE" value="4700  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160480036">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160480036.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="675uA"/>
<attribute name="I-RIPPLE" value="2958mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160480036 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315272M025DSPADK000"/>
<attribute name="VALUE" value="2700  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160480037">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160480037.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="825uA"/>
<attribute name="I-RIPPLE" value="3204mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160480037 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315332M025DSPADG000"/>
<attribute name="VALUE" value="3300  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160580035">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160580035.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="525uA"/>
<attribute name="I-RIPPLE" value="2928mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160580035 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315152M035DSPADK000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160580037">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160580037.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="3012mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160580037 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315182M035DSPADK000"/>
<attribute name="VALUE" value="1800  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160580038">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160580038.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="770uA"/>
<attribute name="I-RIPPLE" value="3228mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160580038 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315222M035DSPADG000"/>
<attribute name="VALUE" value="2200  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160680035">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160680035.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2952mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160680035 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEK315122M050DSPADG000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_8X11.5" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_8X11.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160274015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160274015.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="27uA"/>
<attribute name="I-RIPPLE" value="420mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160274015 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115271M010DSPA7G000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160274017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160274017.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="492mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160274017 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115331M010DSPA7G000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160274019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160274019.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="39uA"/>
<attribute name="I-RIPPLE" value="516mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160274019 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115391M010DSPA7G000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160274021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160274021.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="552mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160274021 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115471M010DSPA7G000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160274022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160274022.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="56uA"/>
<attribute name="I-RIPPLE" value="588mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160274022 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115561M010DSPA7D000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160374015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160374015.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="28.8uA"/>
<attribute name="I-RIPPLE" value="426mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160374015 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115181M016DSPA7G000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160374017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160374017.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="540mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160374017 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115221M016DSPA7G000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160374019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160374019.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="43.2uA"/>
<attribute name="I-RIPPLE" value="582mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160374019 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115271M016DSPA7G000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160374020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160374020.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="588mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160374020 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115331M016DSPA7D000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160374022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160374022.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="62.4uA"/>
<attribute name="I-RIPPLE" value="612mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160374022 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115391M016DSPA7D000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160474014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160474014.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="37.5uA"/>
<attribute name="I-RIPPLE" value="528mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160474014 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115151M025DSPA7G000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160474016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160474016.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="45uA"/>
<attribute name="I-RIPPLE" value="552mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160474016 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115181M025DSPA7G000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160474017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160474017.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="618mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160474017 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115221M025DSPA7G000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160474018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160474018.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="67.5uA"/>
<attribute name="I-RIPPLE" value="750mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160474018 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115271M025DSPA7D000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160574011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160574011.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="28.7uA"/>
<attribute name="I-RIPPLE" value="384mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160574011 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115820M035DSPA7G000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160574013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160574013.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="414mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160574013 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115101M035DSPA7G000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160574014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160574014.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="42uA"/>
<attribute name="I-RIPPLE" value="546mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160574014 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115121M035DSPA7D000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160674016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160674016.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="366mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160674016 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115470M050DSPA7G000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160674017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160674017.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="28uA"/>
<attribute name="I-RIPPLE" value="378mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160674017 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115560M050DSPA7G000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160674018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160674018.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="34uA"/>
<attribute name="I-RIPPLE" value="420mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160674018 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115680M050DSPA7G000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160674020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160674020.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="41uA"/>
<attribute name="I-RIPPLE" value="492mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160674020 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115820M050DSPA7D000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160674021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160674021.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="540mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160674021 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE115101M050DSPA7D000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_10X12.5" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_10X12.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160275023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160275023.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="56uA"/>
<attribute name="I-RIPPLE" value="636mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160275023 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125561M010DSPA9G000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160275025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160275025.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="684mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160275025 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125681M010DSPA9G000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160275027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160275027.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="82uA"/>
<attribute name="I-RIPPLE" value="876mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160275027 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125821M010DSPA9F000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160275030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160275030.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="1032mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160275030 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125102M010DSPA9F000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160375023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160375023.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="62.4uA"/>
<attribute name="I-RIPPLE" value="648mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160375023 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125391M016DSPA9G000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160375025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160375025.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="882mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160375025 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125471M016DSPA9G000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160375027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160375027.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="89.6uA"/>
<attribute name="I-RIPPLE" value="882mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160375027 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125561M016DSPA9F000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160475020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160475020.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="924mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160475020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125331M025DSPA9G000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160475022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160475022.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="1020mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160475022 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125471M025DSPA9F000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160575016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160575016.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="52.5uA"/>
<attribute name="I-RIPPLE" value="720mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160575016 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125151M035DSPA9G000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160575018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160575018.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="804mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160575018 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125181M035DSPA9G000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160575020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160575020.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="888mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160575020 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125221M035DSPA9F000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160575022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160575022.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="94.5uA"/>
<attribute name="I-RIPPLE" value="984mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160575022 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF125271M035DSPA9F000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_6.3X11" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_6.3X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160273011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160273011.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="15uA"/>
<attribute name="I-RIPPLE" value="282mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160273011 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110151M010DSPA4D000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160273012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160273012.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="18uA"/>
<attribute name="I-RIPPLE" value="318mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160273012 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110181M010DSPA4D000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160273013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160273013.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="366mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160273013 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110221M010DSPA4C000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160373010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160373010.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="13.12uA"/>
<attribute name="I-RIPPLE" value="264mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160373010 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110820M016DSPA4D000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160373012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160373012.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="19.2uA"/>
<attribute name="I-RIPPLE" value="312mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160373012 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110121M016DSPA4D000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160373013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160373013.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="24uA"/>
<attribute name="I-RIPPLE" value="336mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160373013 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110151M016DSPA4C000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160473009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160473009.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="17uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160473009 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110680M025DSPA4D000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160473010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160473010.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="20.5uA"/>
<attribute name="I-RIPPLE" value="312mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160473010 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110820M025DSPA4D000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160473011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160473011.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="360mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160473011 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110101M025DSPA4D000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160473012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160473012.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="30uA"/>
<attribute name="I-RIPPLE" value="402mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160473012 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110121M025DSPA4D000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160573006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160573006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="13.65uA"/>
<attribute name="I-RIPPLE" value="252mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160573006 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110390M035DSPA4D000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160573007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160573007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="16.45uA"/>
<attribute name="I-RIPPLE" value="264mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160573007 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110470M035DSPA4D000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160573008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160573008.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="19.6uA"/>
<attribute name="I-RIPPLE" value="282mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160573008 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110560M035DSPA4C000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160573009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160573009.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="23.8uA"/>
<attribute name="I-RIPPLE" value="312mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160573009 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110680M035DSPA4C000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160673012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160673012.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="13.5uA"/>
<attribute name="I-RIPPLE" value="192mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160673012 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110270M050DSPA4D000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160673013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160673013.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="282mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160673013 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110330M050DSPA4C000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160673014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160673014.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="19.5uA"/>
<attribute name="I-RIPPLE" value="306mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160673014 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED110390M050DSPA4C000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_10X16" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_10X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160275028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160275028.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="82uA"/>
<attribute name="I-RIPPLE" value="936mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160275028 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160821M010DSPAAG000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160275031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160275031.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="1140mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160275031 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160102M010DSPAAG000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160275033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160275033.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="120uA"/>
<attribute name="I-RIPPLE" value="1272mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160275033 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160122M010DSPAAF000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160375029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160375029.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="108.8uA"/>
<attribute name="I-RIPPLE" value="1044mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160375029 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160681M016DSPAAG000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160375031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160375031.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="131.2uA"/>
<attribute name="I-RIPPLE" value="1254mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160375031 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160821M016DSPAAF000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160375032">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160375032.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="1404mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160375032 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160102M016DSPAAF000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160475024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160475024.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="140uA"/>
<attribute name="I-RIPPLE" value="1260mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160475024 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160561M025DSPAAG000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160575024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160575024.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="1176mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160575024 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160331M035DSPAAF000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160675025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160675025.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="90uA"/>
<attribute name="I-RIPPLE" value="912mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160675025 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160181M050DSPAAG000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160675026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160675026.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="1056mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160675026 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEF160221M050DSPAAF000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_5X11" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_5X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160272001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160272001.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="66mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160272001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110220M010DSPA3D000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160272002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160272002.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="72mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160272002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110270M010DSPA3D000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160272003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160272003.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="72mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160272003 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110330M010DSPA3D000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160272004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160272004.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.9uA"/>
<attribute name="I-RIPPLE" value="120mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160272004 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110390M010DSPA3D000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160272005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160272005.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="132mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160272005 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110470M010DSPA3D000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160272006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160272006.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5.6uA"/>
<attribute name="I-RIPPLE" value="144mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160272006 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110560M010DSPA3D000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160272007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160272007.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="6.8uA"/>
<attribute name="I-RIPPLE" value="162mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160272007 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110680M010DSPA3D000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160272008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160272008.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="8.2uA"/>
<attribute name="I-RIPPLE" value="192mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160272008 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110820M010DSPA3D000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160272009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160272009.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="222mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160272009 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110101M010DSPA3D000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160272010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160272010.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="12uA"/>
<attribute name="I-RIPPLE" value="246mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160272010 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110121M010DSPA3C000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160372001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160372001.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="36mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160372001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110100M016DSPA3D000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160372002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160372002.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="72mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160372002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110150M016DSPA3D000"/>
<attribute name="VALUE" value="15  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160372003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160372003.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.52uA"/>
<attribute name="I-RIPPLE" value="72mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160372003 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110220M016DSPA3D000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160372004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160372004.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="4.32uA"/>
<attribute name="I-RIPPLE" value="132mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160372004 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110270M016DSPA3D000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160372005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160372005.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5.28uA"/>
<attribute name="I-RIPPLE" value="144mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160372005 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110330M016DSPA3D000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160372006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160372006.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="6.24uA"/>
<attribute name="I-RIPPLE" value="168mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160372006 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110390M016DSPA3D000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160372007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160372007.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="7.52uA"/>
<attribute name="I-RIPPLE" value="186mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160372007 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110470M016DSPA3D000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160372008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160372008.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="8.96uA"/>
<attribute name="I-RIPPLE" value="210mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160372008 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110560M016DSPA3D000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160372009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160372009.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="10.88uA"/>
<attribute name="I-RIPPLE" value="228mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160372009 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110680M016DSPA3D000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160372011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160372011.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="228mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160372011 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110101M016DSPA3C000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160472001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160472001.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="66mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160472001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110100M025DSPA3D000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160472002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160472002.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.75uA"/>
<attribute name="I-RIPPLE" value="120mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160472002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110150M025DSPA3D000"/>
<attribute name="VALUE" value="15  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160472003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160472003.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5.5uA"/>
<attribute name="I-RIPPLE" value="144mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160472003 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110220M025DSPA3D000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160472004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160472004.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="6.75uA"/>
<attribute name="I-RIPPLE" value="156mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160472004 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110270M025DSPA3D000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160472005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160472005.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="8.25uA"/>
<attribute name="I-RIPPLE" value="174mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160472005 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110330M025DSPA3D000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160472006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160472006.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="9.75uA"/>
<attribute name="I-RIPPLE" value="174mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160472006 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110390M025DSPA3D000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160472007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160472007.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="222mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160472007 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110470M025DSPA3D000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160472008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160472008.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="14uA"/>
<attribute name="I-RIPPLE" value="264mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160472008 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110560M025DSPA3D000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160572001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160572001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.5uA"/>
<attribute name="I-RIPPLE" value="84mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160572001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110100M035DSPA3D000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160572002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160572002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5.25uA"/>
<attribute name="I-RIPPLE" value="144mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160572002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110150M035DSPA3D000"/>
<attribute name="VALUE" value="15  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160572003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160572003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="7.7uA"/>
<attribute name="I-RIPPLE" value="162mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160572003 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110220M035DSPA3D000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160572004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160572004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="9.45uA"/>
<attribute name="I-RIPPLE" value="174mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160572004 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110270M035DSPA3C000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160572005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160572005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11.55uA"/>
<attribute name="I-RIPPLE" value="222mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160572005 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110330M035DSPA3C000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160672001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160672001.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="12mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160672001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110R47M050DSPA3D000"/>
<attribute name="VALUE" value="0.47  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160672002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160672002.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="24mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160672002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110010M050DSPA3D000"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160672003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160672003.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="36mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160672003 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC1102R2M050DSPA3D000"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160672004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160672004.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="48mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160672004 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC1103R3M050DSPA3D000"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160672005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160672005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="66mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160672005 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC1104R7M050DSPA3D000"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160672006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160672006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="96mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160672006 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC1105R6M050DSPA3D000"/>
<attribute name="VALUE" value="5.6  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160672007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160672007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="3.4uA"/>
<attribute name="I-RIPPLE" value="96mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160672007 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC1106R8M050DSPA3D000"/>
<attribute name="VALUE" value="6.8  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160672008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160672008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="4.1uA"/>
<attribute name="I-RIPPLE" value="108mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160672008 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC1108R2M050DSPA3D000"/>
<attribute name="VALUE" value="8.2  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160672009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160672009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="120mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160672009 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110100M050DSPA3D000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160672010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160672010.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="7.5uA"/>
<attribute name="I-RIPPLE" value="150mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160672010 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110150M050DSPA3D000"/>
<attribute name="VALUE" value="15  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160672011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160672011.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="162mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160672011 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEC110220M050DSPA3C000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_6.3X15" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_6.3X15(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160273014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160273014.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="27uA"/>
<attribute name="I-RIPPLE" value="414mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160273014 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150271M010DSPA4D000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160273016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160273016.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="462mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160273016 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150331M010DSPA4D000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160273018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160273018.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="39uA"/>
<attribute name="I-RIPPLE" value="456mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160273018 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150391M010DSPA4C000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160273020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160273020.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="480mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160273020 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150471M010DSPA4C000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160373014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160373014.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="28.8uA"/>
<attribute name="I-RIPPLE" value="420mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160373014 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150181M016DSPA4D000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160373016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160373016.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="504mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160373016 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150221M016DSPA4D000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160373018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160373018.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="43.2uA"/>
<attribute name="I-RIPPLE" value="540mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160373018 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150271M016DSPA4C000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160373021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160373021.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="588mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160373021 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150331M016DSPA4C000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160473013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160473013.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="37.5uA"/>
<attribute name="I-RIPPLE" value="510mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160473013 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150151M025DSPA4D000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160473015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160473015.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="45uA"/>
<attribute name="I-RIPPLE" value="546mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160473015 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150181M025DSPA4D000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160573010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160573010.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="28.7uA"/>
<attribute name="I-RIPPLE" value="354mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160573010 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150820M035DSPA4D000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160573012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160573012.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="378mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160573012 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150101M035DSPA4C000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160673015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160673015.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="348mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160673015 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150470M050DSPA4D000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160673019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160673019.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="41uA"/>
<attribute name="I-RIPPLE" value="462mA"/>
<attribute name="L" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160673019 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATED150820M050DSPA4C000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATLL_8X16" prefix="C">
<description>&lt;b&gt;WCAP-ATLL Aluminum Electrolytic Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life +105 °C   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 0.47 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 3000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 35.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14730v209%20Family_WCAP-ATLL.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-ATLL/"&gt;https://www.we-online.com/catalog/en/WCAP-ATLL/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATLL_8X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860160274024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160274024.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="660mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160274024 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160681M010DSPA7G000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160274026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160274026.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="82uA"/>
<attribute name="I-RIPPLE" value="732mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160274026 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160821M010DSPA7D000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160274029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160274029.pdf"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="1020mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160274029 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160102M010DSPA7D000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860160374024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160374024.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="846mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160374024 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160471M016DSPA7D000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160374026">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160374026.pdf"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="89.6uA"/>
<attribute name="I-RIPPLE" value="864mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160374026 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160561M016DSPA7D000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860160474019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160474019.pdf"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="960mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160474019 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160331M025DSPA7G000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860160574015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160574015.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="52.5uA"/>
<attribute name="I-RIPPLE" value="714mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160574015 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160151M035DSPA7G000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160574017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160574017.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="792mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160574017 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160181M035DSPA7G000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160574019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160574019.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="864mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160574019 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160221M035DSPA7D000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860160674022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160674022.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="60uA"/>
<attribute name="I-RIPPLE" value="630mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160674022 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160121M050DSPA7G000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860160674023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/860160674023.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="75uA"/>
<attribute name="I-RIPPLE" value="696mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860160674023 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATEE160151M050DSPA7D000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
