<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-ATUL&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-12-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-ATUL_10X25(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X25X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_13X35(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X35X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_8X20(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X20X3.5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_16X35.5(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X35.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_13X30(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X30X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_13X25(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X25X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_18X31.5(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,18X31.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_16X41(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X41X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_5X11(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X11X2X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_18X35.5(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X35.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_18X25(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,18X25X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_6.3X11(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,6.3X11X2.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_16X21(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,16X21X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_13X20(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X20X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_13X40(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X40X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_10X20(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X20X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_18X41(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X41X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_8X16(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,8X16X3.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_16X25(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X25X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_16X31.5(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,16X31.5X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_10X12.5(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X12.5X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_18X40(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,18X40X7.5X0.8(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_10X16(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X16X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_10X30(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X30X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_8X11.5(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,8X11.5X3.5X0.5(DiameterXLengthX PitchXØPin)</description>
</package>
<package name="WCAP-ATUL_13X16(DXL)">
<description>&lt;B&gt;WCAP-ATUL&lt;/B&gt;&lt;BR&gt;  Aluminium Electrolytic Capacitors,13X16X5X0.6(DiameterXLengthX PitchXØPin)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-ATUL_13X35" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_13X35(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040378017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040378017?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="2860mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040378017 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI350332M016DSPABK000"/>
<attribute name="VALUE" value="3300uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040478015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040478015?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="550uA"/>
<attribute name="I-RIPPLE" value="2880mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040478015 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI350222M025DSPABK000"/>
<attribute name="VALUE" value="2200uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040578017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040578017?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="525uA"/>
<attribute name="I-RIPPLE" value="3000mA"/>
<attribute name="L" value="35mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040578017 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI350152M035DSPABK000"/>
<attribute name="VALUE" value="1500uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_8X20" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_8X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040274008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040274008?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="1050mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040274008 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE200102M010DSPA7F000"/>
<attribute name="VALUE" value="1000uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040374008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040374008?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="108.8uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040374008 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE200681M016DSPA7G000"/>
<attribute name="VALUE" value="680uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040474007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040474007?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="1020mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040474007 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE200471M025DSPA7G000"/>
<attribute name="VALUE" value="470uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040574008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040574008?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="94.5uA"/>
<attribute name="I-RIPPLE" value="1180mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040574008 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE200271M035DSPA7G000"/>
<attribute name="VALUE" value="270uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040674007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040674007?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="90uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040674007 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE200181M050DSPA7G000"/>
<attribute name="VALUE" value="180uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860040774007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040774007?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="75.6uA"/>
<attribute name="I-RIPPLE" value="700mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040774007 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE200121M063DSPA7G000"/>
<attribute name="VALUE" value="120uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_13X30" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_13X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040278015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040278015?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="390uA"/>
<attribute name="I-RIPPLE" value="2400mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040278015 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI300392M010DSPACH000"/>
<attribute name="VALUE" value="3900uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040378016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040378016?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="432uA"/>
<attribute name="I-RIPPLE" value="2600mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040378016 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI300272M016DSPACK000"/>
<attribute name="VALUE" value="2700uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040478014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040478014?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="450uA"/>
<attribute name="I-RIPPLE" value="2640mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040478014 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI300182M025DSPACK000"/>
<attribute name="VALUE" value="1800uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040578015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040578015?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="420uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040578015 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI300122M035DSPACK000"/>
<attribute name="VALUE" value="1200uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040778013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040778013?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="296.1uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040778013 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI300471M063DSPACK000"/>
<attribute name="VALUE" value="470uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_18X31.5" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_18X31.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040581020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040581020?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="3850mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040581020 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL315272M035DSPAEK000"/>
<attribute name="VALUE" value="2700uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040781018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040781018?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040781018 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL315102M063DSPAEK000"/>
<attribute name="VALUE" value="1000uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040881012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040881012?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040881012 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL315471M100DSPAEK000"/>
<attribute name="VALUE" value="470uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_16X35.5" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_16X35.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040580019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040580019?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040580019 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK355272M035DSPADK000"/>
<attribute name="VALUE" value="2700uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040780017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040780017?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="2500mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040780017 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK355102M063DSPADK000"/>
<attribute name="VALUE" value="1000uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040880011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040880011?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="1880mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040880011 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK355471M100DSPADK000"/>
<attribute name="VALUE" value="470uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_13X25" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_13X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040278014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040278014?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="330uA"/>
<attribute name="I-RIPPLE" value="2120mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040278014 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250332M010DSPACH000"/>
<attribute name="VALUE" value="3300uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040378014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040378014?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="288uA"/>
<attribute name="I-RIPPLE" value="2030mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040378014 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250182M016DSPACK000"/>
<attribute name="VALUE" value="1800uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040378015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040378015?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="352uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040378015 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250222M016DSPACK000"/>
<attribute name="VALUE" value="2200uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040478013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040478013?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="375uA"/>
<attribute name="I-RIPPLE" value="2240mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040478013 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250152M025DSPACK000"/>
<attribute name="VALUE" value="1500uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040578014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040578014?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="350uA"/>
<attribute name="I-RIPPLE" value="2400mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040578014 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250102M035DSPACK000"/>
<attribute name="VALUE" value="1000uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040678012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040678012?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="280uA"/>
<attribute name="I-RIPPLE" value="1950mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040678012 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250561M050DSPACK000"/>
<attribute name="VALUE" value="560uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860040778012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040778012?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="207.9uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040778012 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI250331M063DSPACK000"/>
<attribute name="VALUE" value="330uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040878017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040878017?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="2220mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860040878017"/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value=""/>
<attribute name="VALUE" value="220uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_16X41" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_16X41(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040780019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040780019?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="756uA"/>
<attribute name="I-RIPPLE" value="2920mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040780019 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK410122M063DSPS3K000"/>
<attribute name="VALUE" value="1200uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_6.3X11" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_6.3X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040273002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040273002?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="340mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040273002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110221M010DSPA4D000"/>
<attribute name="VALUE" value="220uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040273003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040273003?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="380mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040273003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110331M010DSPA4D000"/>
<attribute name="VALUE" value="330uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040373002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040373002?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040373002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110101M016DSPA4E000"/>
<attribute name="VALUE" value="100uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040373003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040373003?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="19.2uA"/>
<attribute name="I-RIPPLE" value="310mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040373003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110121M016DSPA4E000"/>
<attribute name="VALUE" value="120uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040473003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040473003?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="350mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040473003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110101M025DSPA4E000"/>
<attribute name="VALUE" value="100uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040573003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040573003?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="19.6uA"/>
<attribute name="I-RIPPLE" value="360mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040573003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110560M035DSPA4E000"/>
<attribute name="VALUE" value="56uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040573004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040573004?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="450mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040573004 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110101M035DSPA4E000"/>
<attribute name="VALUE" value="100uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040673002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040673002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="260mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040673002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110470M050DSPA4E000"/>
<attribute name="VALUE" value="47uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860040673003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040673003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="28uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040673003 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110560M050DSPA4E000"/>
<attribute name="VALUE" value="56uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860040773001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040773001?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="260mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040773001 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDD110330M063DSPA4E000"/>
<attribute name="VALUE" value="33uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_5X11" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_5X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040272001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040272001?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="215mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040272001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110560M016DSPA3E000"/>
<attribute name="VALUE" value="100uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040372001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040372001?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="8.96uA"/>
<attribute name="I-RIPPLE" value="200mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040372001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110470M025DSPA3E000"/>
<attribute name="VALUE" value="56uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040472001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040472001?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040472001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110560M025DSPA3E000"/>
<attribute name="VALUE" value="47uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040472002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040472002?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="14uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040472002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110220M050DSPA3E000"/>
<attribute name="VALUE" value="56uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040572001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040572001?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11.55uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040572001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110101M010DSPA3D000"/>
<attribute name="VALUE" value="33uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040572002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040572002?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="16.45uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040572002 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110330M035DSPA3E000"/>
<attribute name="VALUE" value="47uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040672001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040672001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="220mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040672001 "/>
<attribute name="PITCH" value="2mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDC110470M035DSPA3E000"/>
<attribute name="VALUE" value="22uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_18X35.5" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_18X35.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040781020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040781020?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="756uA"/>
<attribute name="I-RIPPLE" value="3000mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040781020 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL355122M063DSPAEK000"/>
<attribute name="VALUE" value="1200uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040881013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040881013?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="680uA"/>
<attribute name="I-RIPPLE" value="1720mA"/>
<attribute name="L" value="35.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040881013 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL355681M100DSPAEK000"/>
<attribute name="VALUE" value="680uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_18X25" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_18X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040381018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040381018?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="752uA"/>
<attribute name="I-RIPPLE" value="3000mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040381018 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL250472M016DSPAEK000"/>
<attribute name="VALUE" value="4700uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040881010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040881010?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="390uA"/>
<attribute name="I-RIPPLE" value="1740mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040881010 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL250391M100DSPAEK000"/>
<attribute name="VALUE" value="390uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_13X40" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_13X40(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040778015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040778015?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="428.4uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040778015 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI400681M063DSPS4K000"/>
<attribute name="VALUE" value="680uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040878008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040878008?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="330uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040878008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI400331M100DSPS4K000"/>
<attribute name="VALUE" value="330uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_16X21" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_16X21(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040580016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040580016?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="420uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="L" value="21mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040580016 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK210122M035DSPAEK000"/>
<attribute name="VALUE" value="1200uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_10X20" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_10X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040275010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040275010?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="120uA"/>
<attribute name="I-RIPPLE" value="1380mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040275010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200122M010DSPAAF000"/>
<attribute name="VALUE" value="1200uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040375009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040375009?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="131.2uA"/>
<attribute name="I-RIPPLE" value="1280mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040375009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200821M016DSPAAG000"/>
<attribute name="VALUE" value="820uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040375010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040375010?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="1380mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040375010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200102M016DSPAAG000"/>
<attribute name="VALUE" value="1000uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040475009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040475009?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="170uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040475009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200681M025DSPAAG000"/>
<attribute name="VALUE" value="680uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040575010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040575010?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="164.5uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040575010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200471M035DSPAAG000"/>
<attribute name="VALUE" value="470uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040675009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040675009?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="135uA"/>
<attribute name="I-RIPPLE" value="1350mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040675009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200271M050DSPAAG000"/>
<attribute name="VALUE" value="270uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860040775009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040775009?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="113.4uA"/>
<attribute name="I-RIPPLE" value="880mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040775009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200181M063DSPAAG000"/>
<attribute name="VALUE" value="180uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040875004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040875004?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="82uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040875004 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF200820M100DSPAAG000"/>
<attribute name="VALUE" value="82uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_10X25" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_10X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040275011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040275011?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="150uA"/>
<attribute name="I-RIPPLE" value="1550mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040275011 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF250152M010DSPAAF000"/>
<attribute name="VALUE" value="1500uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040375012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040375012?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="192uA"/>
<attribute name="I-RIPPLE" value="1560mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040375012 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF250122M016DSPAAG000"/>
<attribute name="VALUE" value="1200uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040475010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040475010?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="205uA"/>
<attribute name="I-RIPPLE" value="1580mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040475010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF250821M025DSPAAG000"/>
<attribute name="VALUE" value="820uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040575011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040575011?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="196uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040575011 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF250561M035DSPAAG000"/>
<attribute name="VALUE" value="560uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040675010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040675010?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="165uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040675010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF250331M050DSPAAG000"/>
<attribute name="VALUE" value="330uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860040775010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040775010?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="138.6uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040775010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF250221M063DSPAAG000"/>
<attribute name="VALUE" value="220uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040875005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040875005?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040875005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF250101M100DSPAAG000"/>
<attribute name="VALUE" value="100uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_13X20" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_13X20(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040278013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040278013?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040278013 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200152M016DSPACK000"/>
<attribute name="VALUE" value="2200uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040378013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040378013?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="240uA"/>
<attribute name="I-RIPPLE" value="1720mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040378013 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200102M025DSPACK000"/>
<attribute name="VALUE" value="1500uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040478012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040478012?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040478012 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200222M010DSPACH000"/>
<attribute name="VALUE" value="1000uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040578013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040578013?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="238uA"/>
<attribute name="I-RIPPLE" value="2100mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040578013 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200681M035DSPACK000"/>
<attribute name="VALUE" value="680uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040778011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040778011?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="170.1uA"/>
<attribute name="I-RIPPLE" value="1200mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040778011 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200271M063DSPACK000"/>
<attribute name="VALUE" value="270uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040878006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040878006?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="120uA"/>
<attribute name="I-RIPPLE" value="900mA"/>
<attribute name="L" value="20mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040878006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI200121M100DSPACK000"/>
<attribute name="VALUE" value="120uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_18X41" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_18X41(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040581021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040581021?ae"/>
<attribute name="DF" value="18%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1645uA"/>
<attribute name="I-RIPPLE" value="5350mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040581021 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL410472M035DSPAEK000"/>
<attribute name="VALUE" value="4700uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040781021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040781021?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="3200mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040781021 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL410152M063DSPS1K000"/>
<attribute name="VALUE" value="1500uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040881014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040881014?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="820uA"/>
<attribute name="I-RIPPLE" value="2340mA"/>
<attribute name="L" value="41mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040881014 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL410821M100DSPS1K000"/>
<attribute name="VALUE" value="820uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_8X16" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_8X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040274005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040274005?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="770mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040274005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE160681M010DSPA7F000"/>
<attribute name="VALUE" value="680uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040374006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040374006?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="780mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040374006 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE160471M016DSPA7G000"/>
<attribute name="VALUE" value="470uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040474005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040474005?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="810mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040474005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE160331M025DSPA7G000"/>
<attribute name="VALUE" value="330uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040574006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040574006?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040574006 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE160221M035DSPA7G000"/>
<attribute name="VALUE" value="220uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040674005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040674005?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="60uA"/>
<attribute name="I-RIPPLE" value="760mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040674005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE160121M050DSPA7G000"/>
<attribute name="VALUE" value="120uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860040774004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040774004?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="51.66uA"/>
<attribute name="I-RIPPLE" value="460mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040774004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE160820M063DSPA7G000"/>
<attribute name="VALUE" value="82uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_16X25" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_16X25(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040480016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040480016?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="675uA"/>
<attribute name="I-RIPPLE" value="2820mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040480016 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250272M025DSPAEK000"/>
<attribute name="VALUE" value="2700uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040580018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040580018?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040580018 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250182M035DSPAEK000"/>
<attribute name="VALUE" value="1800uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040780014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040780014?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="352.8uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040780014 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250561M063DSPAEK000"/>
<attribute name="VALUE" value="560uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040880007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040880007?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="270uA"/>
<attribute name="I-RIPPLE" value="1480mA"/>
<attribute name="L" value="25mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040880007 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK250271M100DSPAEK000"/>
<attribute name="VALUE" value="270uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_16X31.5" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_16X31.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040680013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040680013?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2870mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040680013 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK315122M050DSPADK000"/>
<attribute name="VALUE" value="1200uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860040780016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040780016?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="516.6uA"/>
<attribute name="I-RIPPLE" value="2400mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040780016 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK315821M063DSPADK000"/>
<attribute name="VALUE" value="820uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040880009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040880009?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="I-LEAK" value="390uA"/>
<attribute name="I-RIPPLE" value="1700mA"/>
<attribute name="L" value="31.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040880009 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDK315391M100DSPADK000"/>
<attribute name="VALUE" value="390uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_10X12.5" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_10X12.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040275006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040275006?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040275006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125681M010DSPA9F000"/>
<attribute name="VALUE" value="680uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040375007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040375007?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040375007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125471M016DSPA9G000"/>
<attribute name="VALUE" value="470uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040475006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040475006?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="826mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040475006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125331M025DSPA9G000"/>
<attribute name="VALUE" value="330uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040575007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040575007?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="1060mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040575007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125221M035DSPA9G000"/>
<attribute name="VALUE" value="220uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040675006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040675006?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040675006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125151M050DSPA9G000"/>
<attribute name="VALUE" value="150uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860040775005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040775005?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="51.66uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040775005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125820M063DSPA9G000"/>
<attribute name="VALUE" value="82uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040775006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040775006?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="640mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040775006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125101M063DSPA9G000"/>
<attribute name="VALUE" value="100uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040875002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040875002?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="400mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040875002 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF125470M100DSPA9G000"/>
<attribute name="VALUE" value="47uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_18X40" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2022-12-23
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_18X40(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040381001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040381001?ae"/>
<attribute name="DF" value="34%"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="I-LEAK" value="1600uA"/>
<attribute name="I-RIPPLE" value="4290mA"/>
<attribute name="L" value="40mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="860040381001"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDL400103M016DSPS1K0L0"/>
<attribute name="VALUE" value="10000uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_10X16" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_10X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040275007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040275007?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="82uA"/>
<attribute name="I-RIPPLE" value="920mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040275007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160821M010DSPAAF000"/>
<attribute name="VALUE" value="820uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040275009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040275009?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="1110mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040275009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160102M010DSPAAF000"/>
<attribute name="VALUE" value="1000uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040475008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040475008?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="1210mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040475008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160471M025DSPAAG000"/>
<attribute name="VALUE" value="470uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040575009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040575009?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="115.5uA"/>
<attribute name="I-RIPPLE" value="1380mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040575009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160331M035DSPAAG000"/>
<attribute name="VALUE" value="330uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040675008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040675008?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="1300mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040675008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160221M050DSPAAG000"/>
<attribute name="VALUE" value="220uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860040775008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040775008?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75.6uA"/>
<attribute name="I-RIPPLE" value="760mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040775008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160121M063DSPAAG000"/>
<attribute name="VALUE" value="120uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040875003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040875003?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="460mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040875003 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF160680M100DSPAAG000"/>
<attribute name="VALUE" value="68uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_10X30" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_10X30(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040275012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040275012?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1880mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040275012 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF300222M010DSPAAF000"/>
<attribute name="VALUE" value="2200uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040475011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040475011?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="1820mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040475011 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF300102M025DSPAAG000"/>
<attribute name="VALUE" value="1000uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040575012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040575012?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="238uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040575012 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF300681M035DSPAAG000"/>
<attribute name="VALUE" value="680uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040675011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040675011?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="30mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040675011 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDF300471M050DSPAAG000"/>
<attribute name="VALUE" value="470uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_8X11.5" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_8X11.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040274004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040274004?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040274004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115471M010DSPA7F000"/>
<attribute name="VALUE" value="470uF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_860040374004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040374004?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="480mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040374004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115221M016DSPA7G000"/>
<attribute name="VALUE" value="220uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040374005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040374005?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040374005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115331M016DSPA7G000"/>
<attribute name="VALUE" value="330uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_860040474004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040474004?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="590mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040474004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115221M025DSPA7G000"/>
<attribute name="VALUE" value="220uF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_860040574005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040574005?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="52.5uA"/>
<attribute name="I-RIPPLE" value="680mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040574005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115151M035DSPA7G000"/>
<attribute name="VALUE" value="150uF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_860040674004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040674004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="680mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040674004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115101M050DSPA7G000"/>
<attribute name="VALUE" value="100uF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_860040774002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040774002?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="29.61uA"/>
<attribute name="I-RIPPLE" value="360mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040774002 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115470M063DSPA7G000"/>
<attribute name="VALUE" value="47uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040774003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040774003?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="35.28uA"/>
<attribute name="I-RIPPLE" value="380mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040774003 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115560M063DSPA7G000"/>
<attribute name="VALUE" value="56uF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_860040874001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040874001?ae"/>
<attribute name="DF" value="9%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="27uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040874001 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDE115270M100DSPA7G000"/>
<attribute name="VALUE" value="27uF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ATUL_13X16" prefix="C">
<description>&lt;b&gt;WCAP-ATUL Aluminum Electrolytic Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low Leakage &amp; Long Life &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low leakage current and long life product series 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 4700 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 10 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to +105 °C 
&lt;BR&gt;Endurance: 4000 ‒ 10000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 5.0 x 11.0 up to 18.0 x 41 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Durable battery applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Energy storage 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. Switched-mode power supply, AC/DC converter, adapter, charger, digital camera 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683655v209%20family-wcap-atul-860040672001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-ATUL"&gt;www.we-online.com/components/products/WCAP-ATUL&lt;/a&gt;&lt;p&gt;

Updated by yingchun,Shan;2020-03-02
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ATUL_13X16(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_860040378011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/860040378011?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="1420mA"/>
<attribute name="L" value="16mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 860040378011 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="ATDI160102M016DSPACK000"/>
<attribute name="VALUE" value="1000uF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
