<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - MLCCs-Multilayer Ceramic Chip Capacitors - WCAP-CSMH&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-05-12&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-CSMH_0805_H0.8_W">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;Solder type: Wave,2 x 1.25x0.8( LxWxH) ;</description>
</package>
<package name="WCAP-CSMH_0805_H0.8_R">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;Solder type: Reflow,2 x 1.25x0.8( LxWxH) ;</description>
</package>
<package name="WCAP-CSMH_1812_H2.0">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;4.5X3.2X2.0(LXWXH)</description>
</package>
<package name="WCAP-CSMH_2220_H2.0">
<description>&lt;b&gt;WCAP-CSMH MLCCs 2220&lt;/b&gt;&lt;br&gt;5.7X5X2.0(LXWXH)</description>
</package>
<package name="WCAP-CSMH_0805_H0.6_R">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;Solder type: Reflow,2x1.25x0.6( LxWxH) ;</description>
</package>
<package name="WCAP-CSMH_1812_H2.5">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;4.5X3.2X2.5(LXWXH)</description>
</package>
<package name="WCAP-CSMH_1210_H1.25">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;3.2x2.5x1.25(LXWXH);</description>
</package>
<package name="WCAP-CSMH_0805_H0.6_W">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;Solder type: Wave,2x1.25x0.6( LxWxH) ;</description>
</package>
<package name="WCAP-CSMH_0805_H1.25_R">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;Solder type: Reflow,2 x 1.25x1.25( LxWxH) ;</description>
</package>
<package name="WCAP-CSMH_2220_H2.8">
<description>&lt;b&gt;WCAP-CSMH MLCCs 2220&lt;/b&gt;&lt;br&gt;5.7X5X2.8(LXWXH)</description>
</package>
<package name="WCAP-CSMH_1206_H0.8_R">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;Solder type: Reflow,3.2X1.6X0.8(LXWXH) ;</description>
</package>
<package name="WCAP-CSMH_1210_H2.5">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;3.2x2.5x2.5(LXWXH);</description>
</package>
<package name="WCAP-CSMH_1210_H0.95">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;3.2x2.5x0.95(LXWXH);</description>
</package>
<package name="WCAP-CSMH_1206_H1.6_R">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;Solder type:Reflow,3.2x1.6x1.6(LXWXH)</description>
</package>
<package name="WCAP-CSMH_1206_H1.25">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;3.2X1.6X1.25(LXWXH) ;</description>
</package>
<package name="WCAP-CSMH_0603_R">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;Solder type: Reflow,size code1.6X0.8X0.8(LXWXH) ;</description>
</package>
<package name="WCAP-CSMH_0603_W">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;Solder type: Wave,1.6X0.8X0.8(LXWXH);</description>
</package>
<package name="WCAP-CSMH_2220_H2.5">
<description>&lt;b&gt;WCAP-CSMH MLCCs 2220&lt;/b&gt;&lt;br&gt;5.7X5X2.5(LXWXH)</description>
</package>
<package name="WCAP-CSMH_1206_H0.8_W">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;Solder type:Wave,3.2x1.6x0.8(LXWXH)</description>
</package>
<package name="WCAP-CSMH_1808_H2.0">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;4.5x2.03x2.0(LXWXH);</description>
</package>
<package name="WCAP-CSMH_1812_H1.25">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;4.5X3.2X1.25(LXWXH)</description>
</package>
<package name="WCAP-CSMH_1210_H2.0">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;3.2x2.5x2.0LXWXH);</description>
</package>
<package name="WCAP-CSMH_1808_H1.25">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;4.5x2.03x1.25(LXWXH);</description>
</package>
<package name="WCAP-CSMH_1210_H1.6">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/b&gt;&lt;br&gt;3.2x2.5x1.6(LXWXH);</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-CSMH_0805_H0.8" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_R" package="WCAP-CSMH_0805_H0.8_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342207001">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207001?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207001"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207002">
<attribute name="C" value="470 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207002"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470 pF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207003">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207003?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207003"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207004">
<attribute name="C" value="4.7 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207004?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207004"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207007">
<attribute name="C" value="470 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207007?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207007"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207008">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207008?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207008"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207009">
<attribute name="C" value="4.7 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207009?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207009"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207012">
<attribute name="C" value="470 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207012?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207012"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470 pF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207013">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207013?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207013"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_W" package="WCAP-CSMH_0805_H0.8_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342207001">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207001?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207001"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207002">
<attribute name="C" value="470 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207002"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470 pF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207003">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207003?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207003"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207004">
<attribute name="C" value="4.7 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207004?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207004"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207007">
<attribute name="C" value="470 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207007?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207007"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207008">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207008?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207008"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207009">
<attribute name="C" value="4.7 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207009?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207009"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207012">
<attribute name="C" value="470 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207012?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207012"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470 pF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207013">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207013?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207013"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_1812_H2.0" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_1812_H2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342011003">
<attribute name="C" value="1.5 nF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342011003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342011003"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1.5 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885342211003">
<attribute name="C" value="470 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342211003?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342211003"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.213 GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885342211005">
<attribute name="C" value="100 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342211005?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342211005"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1 GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885342211006">
<attribute name="C" value="100 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342211006?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342211006"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1 GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885342211008">
<attribute name="C" value="4.7 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342211008?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342211008"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="4.7 nF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885342211009">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342211009?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342211009"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="3000VDC"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_2220_H2.0" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_2220_H2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342014230">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342014230?ae"/>
<attribute name="DF" value="1000%"/>
<attribute name="FI" value="0.85mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342014230"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="2220"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_885342214002">
<attribute name="C" value="1 µF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342214002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.85mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342214002"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1 GOhm"/>
<attribute name="SIZE" value="2220"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_885342214142">
<attribute name="C" value="220 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342214142?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.85mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342214142"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5 GOhm"/>
<attribute name="SIZE" value="2220"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_1812_H2.5" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_1812_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342211010">
<attribute name="C" value="2.2 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342211010?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342211010"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="2.2 nF"/>
<attribute name="VR" value="3000VDC"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_1210_H1.25" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_1210_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342209006">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342209006?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342209006"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885342209008">
<attribute name="C" value="220 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342209008?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342209008"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="220 pF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885342209009">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342209009?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342209009"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_0805_H0.6" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_R" package="WCAP-CSMH_0805_H0.6_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342007004">
<attribute name="C" value="15 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342007004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342007004"/>
<attribute name="QMIN" value="700"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342007006">
<attribute name="C" value="47 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342007006?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342007006"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47 pF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_W" package="WCAP-CSMH_0805_H0.6_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342007004">
<attribute name="C" value="15 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342007004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342007004"/>
<attribute name="QMIN" value="700"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342007006">
<attribute name="C" value="47 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342007006?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342007006"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47 pF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_0805_H1.25" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_0805_H1.25_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342007001">
<attribute name="C" value="220 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342007001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342007001"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220 pF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342007002">
<attribute name="C" value="330 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342007002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342007002"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330 pF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342007003">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342007003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342007003"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342007005">
<attribute name="C" value="2.2 nF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342007005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342007005"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207005">
<attribute name="C" value="10 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207005?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207005"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207006">
<attribute name="C" value="22 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207006?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207006"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="4.545 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207010">
<attribute name="C" value="10 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207010?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207010"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207011">
<attribute name="C" value="22 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207011?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207011"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="4.545 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207014">
<attribute name="C" value="10 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207014?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207014"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207015">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207015?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207015"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885342207016">
<attribute name="C" value="2.2 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342207016?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342207016"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_2220_H2.8" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_2220_H2.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342214001">
<attribute name="C" value="1 µF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342214001?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.85mm"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342214001"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1 GOhm"/>
<attribute name="SIZE" value="2220"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_885342214216">
<attribute name="C" value="22 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342214216?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.85mm"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342214216"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5 GOhm"/>
<attribute name="SIZE" value="2220"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_1210_H2.5" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_1210_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342209003">
<attribute name="C" value="220 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342209003?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342209003"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.455 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_1210_H0.95" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_1210_H0.95">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342009002">
<attribute name="C" value="22 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342009002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342009002"/>
<attribute name="QMIN" value="840"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="22 pF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885342009004">
<attribute name="C" value="10 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342009004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342009004"/>
<attribute name="QMIN" value="600"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="10 pF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885342209001">
<attribute name="C" value="15 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342209001?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342209001"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="6.667 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_1206_H1.6" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-08-09&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_1206_H1.6_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342008003">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008003"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342008005">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008005"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342008006">
<attribute name="C" value="1.5 nF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008006?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008006"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1.5 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342008007">
<attribute name="C" value="2.2 nF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008007?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008007"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208002">
<attribute name="C" value="100 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208002"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208004">
<attribute name="C" value="100 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208004?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208004"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208010">
<attribute name="C" value="22 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208010?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208010"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="4.545 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208014">
<attribute name="C" value="22 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208014?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208014"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="4.545 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208015">
<attribute name="C" value="33 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208015?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208015"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.03 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="33 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208024">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208024?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208024"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208026">
<attribute name="C" value="47 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208026?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208026"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.127 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_1206_H1.25" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_1206_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342008009">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008009?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008009"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342008010">
<attribute name="C" value="68 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008010?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008010"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="68 pF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342008011">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008011?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008011"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208001">
<attribute name="C" value="22 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208001?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208001"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="4.545 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208003">
<attribute name="C" value="10 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208003?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208003"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208005">
<attribute name="C" value="470 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208005?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208005"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470 pF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208006">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208006?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208006"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208007">
<attribute name="C" value="2.2 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208007?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208007"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2 nF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208008">
<attribute name="C" value="4.7 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208008?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208008"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7 nF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208009">
<attribute name="C" value="10 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208009?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208009"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208011">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208011?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208011"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208012">
<attribute name="C" value="10 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208012?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208012"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208013">
<attribute name="C" value="15 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208013?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208013"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="6.667 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208016">
<attribute name="C" value="150 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208016?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208016"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="150 pF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208017">
<attribute name="C" value="470 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208017?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208017"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470 pF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208018">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208018?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208018"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208019">
<attribute name="C" value="2.2 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208019?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208019"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208020">
<attribute name="C" value="4.7 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208020?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208020"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208021">
<attribute name="C" value="10 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208021?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208021"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208022">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208022?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208022"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342208023">
<attribute name="C" value="470 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342208023?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342208023"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470 pF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_0603" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_R" package="WCAP-CSMH_0603_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342006001">
<attribute name="C" value="10 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342006001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342006001"/>
<attribute name="QMIN" value="600"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342006002">
<attribute name="C" value="33 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342006002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342006002"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342006003">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342006003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342006003"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342006004">
<attribute name="C" value="220 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342006004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342006004"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342006005">
<attribute name="C" value="470 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342006005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342006005"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342206001">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342206001?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342206001"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342206002">
<attribute name="C" value="330 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342206002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342206002"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342206003">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342206003?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342206003"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342206004">
<attribute name="C" value="1.5 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342206004?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342206004"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342206005">
<attribute name="C" value="3.3 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342206005?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342206005"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342206006">
<attribute name="C" value="10 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342206006?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342206006"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_W" package="WCAP-CSMH_0603_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342006001">
<attribute name="C" value="10 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342006001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342006001"/>
<attribute name="QMIN" value="600"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342006002">
<attribute name="C" value="33 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342006002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342006002"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342006003">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342006003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342006003"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342006004">
<attribute name="C" value="220 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342006004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342006004"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342006005">
<attribute name="C" value="470 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342006005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342006005"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342206001">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342206001?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342206001"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342206002">
<attribute name="C" value="330 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342206002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342206002"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330 pF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342206003">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342206003?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342206003"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342206004">
<attribute name="C" value="1.5 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342206004?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342206004"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342206005">
<attribute name="C" value="3.3 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342206005?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342206005"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885342206006">
<attribute name="C" value="10 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342206006?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342206006"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_2220_H2.5" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_2220_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342214003">
<attribute name="C" value="2.2 µF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342214003?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.85mm"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342214003"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05 GOhm"/>
<attribute name="SIZE" value="2220"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_885342214173">
<attribute name="C" value="100 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342214173?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.85mm"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342214173"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1 GOhm"/>
<attribute name="SIZE" value="2220"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_1206_H0.8" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_R" package="WCAP-CSMH_1206_H0.8_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342008001">
<attribute name="C" value="47 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008001"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="47 pF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342008002">
<attribute name="C" value="220 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008002"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="220 pF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342008004">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008004"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342008008">
<attribute name="C" value="22 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008008?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008008"/>
<attribute name="QMIN" value="840"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22 pF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_W" package="WCAP-CSMH_1206_H0.8_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342008001">
<attribute name="C" value="47 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008001"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="47 pF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342008002">
<attribute name="C" value="220 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008002"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="220 pF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342008004">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008004"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885342008008">
<attribute name="C" value="22 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342008008?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342008008"/>
<attribute name="QMIN" value="840"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22 pF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_1808_H2.0" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_1808_H2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342010003">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342010003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342010003"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="3000VDC"/>
<attribute name="WIDTH" value="2.03mm"/>
</technology>
<technology name="_885342210002">
<attribute name="C" value="2.2 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342210002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342210002"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="2.2 nF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="2.03mm"/>
</technology>
<technology name="_885342210003">
<attribute name="C" value="470 pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342210003?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342210003"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="470 pF"/>
<attribute name="VR" value="3000VDC"/>
<attribute name="WIDTH" value="2.03mm"/>
</technology>
<technology name="_885342210004">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342210004?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342210004"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="3000VDC"/>
<attribute name="WIDTH" value="2.03mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_1812_H1.25" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_1812_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342011001">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342011001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342011001"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885342011002">
<attribute name="C" value="100 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342011002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342011002"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="100 pF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885342211001">
<attribute name="C" value="4.7 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342211001?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342211001"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="4.7 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885342211002">
<attribute name="C" value="100 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342211002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342211002"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1 GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885342211004">
<attribute name="C" value="10 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342211004?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342211004"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="500VDC"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885342211007">
<attribute name="C" value="2.2 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342211007?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342211007"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="2.2 nF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_1210_H2.0" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_1210_H2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342209005">
<attribute name="C" value="68 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342209005?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342209005"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.471 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_1808_H1.25" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-19&lt;br&gt;
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_1808_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342010001">
<attribute name="C" value="10 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342010001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342010001"/>
<attribute name="QMIN" value="600"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="10 pF"/>
<attribute name="VR" value="3000VDC"/>
<attribute name="WIDTH" value="2.03mm"/>
</technology>
<technology name="_885342010002">
<attribute name="C" value="68 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342010002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342010002"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="68 pF"/>
<attribute name="VR" value="3000VDC"/>
<attribute name="WIDTH" value="2.03mm"/>
</technology>
<technology name="_885342210001">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342210001?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342210001"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="2.03mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSMH_1210_H1.6" prefix="C">
<description>&lt;b&gt;WCAP-CSMH MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Mid and High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;Product series for mid and high voltage up to 3 kV(DC) &lt;/B&gt;
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II) 
&lt;BR&gt;Capacitance range: 10 pF ‒ 470 nF 
&lt;BR&gt;Temperature Coefficient: 
&lt;BR&gt;±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt;±15 % for X7R 
&lt;BR&gt;Voltage range (UR): 200 V(DC) ‒ 3 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 / 1808 / 1812 
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering only valid for 0603, 0805; thickness &lt; 0.85 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Ports protection against EFT and surge 
&lt;BR&gt;Blocking 
&lt;BR&gt;High voltage coupling 
Snubber 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166505v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSMH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSMH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-12&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSMH_1210_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885342009001">
<attribute name="C" value="4.7 nF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342009001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342009001"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="4.7 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885342009003">
<attribute name="C" value="1 nF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342009003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342009003"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885342009005">
<attribute name="C" value="220 pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342009005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342009005"/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="220 pF"/>
<attribute name="VR" value="2000VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885342009007">
<attribute name="C" value="5.6 nF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342009007?ae"/>
<attribute name="DF" value="-"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342009007"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="5.6 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885342209002">
<attribute name="C" value="100 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342209002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342209002"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="200VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885342209004">
<attribute name="C" value="33 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342209004?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342209004"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.03 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="33 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885342209007">
<attribute name="C" value="22 nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885342209007?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="885342209007"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="4.55 GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
