<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - MLCCs-Multilayer Ceramic Chip Capacitors - WCAP-CSRF&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-01-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-CSRF_0201">
<description>&lt;b&gt;WCAP-CSRF High Frequency
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt; Size: 0201, SMT, 2pins
&lt;BR&gt;0.6X0.3X0.3(LXWXH)</description>
</package>
<package name="WCAP-CSRF_0402">
<description>&lt;b&gt;WCAP-CSRF High Frequency
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt; Size: 0402, SMT, 2pins
&lt;BR&gt;1X0.5X0.5(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-CSRF_0201" prefix="C">
<description>&lt;b&gt;WCAP-CSRF MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;High Frequency&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High frequency product series 
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I) 
&lt;BR&gt;Capacitance range: 0.2 pF ‒ 33 pF 
&lt;BR&gt;Temperature Coefficient: ±30 ppm/°C 
&lt;BR&gt;Voltage range (UR): 25 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0201
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;THigh frequency applications 
&lt;BR&gt;Antenna matching 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o164338v209%20Family_WE-MLCC_0805_weiss.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o164338v209%20Family_WE-MLCC_0805_weiss.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSRF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSRF&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-18
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSRF_0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885392004001">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392004001?ae"/>
<attribute name="FI" value="0.15mm"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392004001 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="0.2 pF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885392004002">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392004002?ae"/>
<attribute name="FI" value="0.15mm"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392004002 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="1 pF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885392004003">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392004003?ae"/>
<attribute name="FI" value="0.15mm"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392004003 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="1.2 pF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885392004004">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392004004?ae"/>
<attribute name="FI" value="0.15mm"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392004004 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="1.5 pF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885392004005">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392004005?ae"/>
<attribute name="FI" value="0.15mm"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392004005 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="2.2 pF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885392004006">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392004006?ae"/>
<attribute name="FI" value="0.15mm"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392004006 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="2.7 pF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885392004007">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392004007?ae"/>
<attribute name="FI" value="0.15mm"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392004007 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="3.3 pF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885392004008">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392004008?ae"/>
<attribute name="FI" value="0.15mm"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392004008 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="4.7 pF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885392004009">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392004009?ae"/>
<attribute name="FI" value="0.15mm"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392004009 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="5.6 pF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885392004010">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392004010?ae"/>
<attribute name="FI" value="0.15mm"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392004010 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="9 pF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885392004011">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392004011?ae"/>
<attribute name="FI" value="0.15mm"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392004011 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="33 pF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSRF_0402" prefix="C">
<description>&lt;b&gt;WCAP-CSRF MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;High Frequency&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High frequency product series 
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Ceramic: NP0 (Class I) 
&lt;BR&gt;Capacitance range: 0.2 pF ‒ 33 pF 
&lt;BR&gt;Temperature Coefficient: ±30 ppm/°C 
&lt;BR&gt;Voltage range (UR): 25 ‒ 50 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0201
&lt;BR&gt;Termination: Cu/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;THigh frequency applications 
&lt;BR&gt;Antenna matching 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o164338v209%20Family_WE-MLCC_0805_weiss.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o164338v209%20Family_WE-MLCC_0805_weiss.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSRF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSRF&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-18
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSRF_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885392005001">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005001?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005001 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="0.3 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005002">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005002?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005002 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="0.4 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005003">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005003?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005003 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="0.4 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005004">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005004?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005004 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="0.5 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005005">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005005?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005005 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005006">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005006?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005006 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005007">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005007?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005007 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1.5 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005008">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005008?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005008 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1.8 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005009">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005009?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005009 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.3 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005010">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005010?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005010 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="3 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005011">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005011?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005011 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="3.3 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005012">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005012?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005012 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="4.7 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005013">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005013?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005013 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="5.6 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005014">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005014?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005014 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="9 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005019">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005019?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005019 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="0.7 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005022">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005022?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005022 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="0.9 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005024">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005024?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005024 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1.2 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005030">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005030?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005030 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005032">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005032?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005032 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.2 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005034">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005034?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005034 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.4 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005037">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005037?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005037 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.7 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005044">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005044?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005044 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="3.6 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005047">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005047?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005047 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="3.9 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005051">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005051?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005051 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="4.3 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005058">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005058?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005058 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="5.1 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005068">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005068?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005068 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="6.2 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005074">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005074?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005074 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="6.8 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005081">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005081?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005081 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="7.5 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005088">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005088?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005088 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="8.2 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005097">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005097?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005097 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="9.1 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005106">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005106?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005106 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="10 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005110">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005110?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005110 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="15 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005114">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005114?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005114 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="22 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005116">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005116?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005116 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="27 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005127">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005127?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005127 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="12 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005130">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005130?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005130 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="0.8 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005131">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005131?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005131 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="20 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005146">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005146?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005146 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="0.2 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885392005147">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885392005147?ae"/>
<attribute name="FI" value="0.25mm"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885392005147 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="18 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
