<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - MLCCs-Multilayer Ceramic Chip Capacitors - WCAP-CSSA&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-03-13&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-CSSA_1812_X1/Y2_H1.6">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 1808, SMT, 2pins
&lt;br&gt;LXWXH=4.5X3.2X1.6mm</description>
</package>
<package name="WCAP-CSSA_1812_X1/Y2_H2">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 1808, SMT, 2pins
&lt;br&gt;LXWXH=4.5X3.2X2mm</description>
</package>
<package name="WCAP-CSSA_2211">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 2211, SMT, 2pins
&lt;br&gt;LXWXH=5.7X4.0X2.5mm</description>
</package>
<package name="WCAP-CSSA_1812_X2_H1.6">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 1808, SMT, 2pins
&lt;br&gt;LXWXH=4.5X3.2X1.6mm</description>
</package>
<package name="WCAP-CSSA_1812_X2_H2.5">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 1808, SMT, 2pins
&lt;br&gt;LXWXH=4.5X3.2X2.5mm</description>
</package>
<package name="WCAP-CSSA_1812_X1/Y2_H2.5">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 1808, SMT, 2pins
&lt;br&gt;LXWXH=4.5X3.2X2.5mm</description>
</package>
<package name="WCAP-CSSA_2220">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 2220, SMT, 2pins
&lt;br&gt;LXWXH=5.7X5.0X2.5mm</description>
</package>
<package name="WCAP-CSSA_1808_X1/Y2_H2">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 1808, SMT, 2pins
&lt;br&gt;LXWXH=4.5X2X2mm</description>
</package>
<package name="WCAP-CSSA_1808_X1/Y2_H1.6">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 1808, SMT, 2pins
&lt;br&gt;LXWXH=4.5X2X1.6mm</description>
</package>
<package name="WCAP-CSSA_1808_X1/Y2_H1.4">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 1808, SMT, 2pins
&lt;br&gt;LXWXH=4.5X2X1.4mm</description>
</package>
<package name="WCAP-CSSA_1808_X2_H1.6">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 1808, SMT, 2pins
&lt;br&gt;LXWXH=4.5X2X1.6mm</description>
</package>
<package name="WCAP-CSSA_1808_X2_H1.4">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 1808, SMT, 2pins
&lt;br&gt;LXWXH=4.5X2X1.4mm</description>
</package>
<package name="WCAP-CSSA_1808_X2_H2">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 1808, SMT, 2pins
&lt;br&gt;LXWXH=4.5X2X2mm</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-CSSA_2211" prefix="C">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Safety Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;High capacitance stability
&lt;BR&gt;Certificates: TÜV, cULus
&lt;BR&gt;Safety class: X1/Y2, X2
&lt;BR&gt;Mounting style: SMT-Chip
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II)
&lt;BR&gt;Capacitance range: 33 pF ‒ 4.7 nF
&lt;BR&gt;Temperature Coefficient:
&lt;BR&gt;±30 ppm/°C for NP0
&lt;BR&gt;±15 % for X7R
&lt;BR&gt;Voltage range (UR): 250 V(AC)
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C
&lt;BR&gt;Sizes: 1808 / 1812 / 2211 / 2220
&lt;BR&gt;Recommended soldering: Reflow soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Interference suppression 
&lt;BR&gt;Filter in power supplies 
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166506v209%20Family_WE-MLCC_1812_grau.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166506v209%20Family_WE-MLCC_1812_grau.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;  
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSSA&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-13
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSSA_2211">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8853522130111">
<attribute name="C" value="1nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853522130111?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853522130111"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X1 / Y2"/>
<attribute name="SIZE" value="2211"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VIMP" value="5000 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
<technology name="_8853522130151">
<attribute name="C" value="2.2nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853522130151?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853522130151"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X1 / Y2"/>
<attribute name="SIZE" value="2211"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VIMP" value="5000 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSSA_1812_X1/Y2" prefix="C">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Safety Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;High capacitance stability
&lt;BR&gt;Certificates: TÜV, cULus
&lt;BR&gt;Safety class: X1/Y2, X2
&lt;BR&gt;Mounting style: SMT-Chip
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II)
&lt;BR&gt;Capacitance range: 33 pF ‒ 4.7 nF
&lt;BR&gt;Temperature Coefficient:
&lt;BR&gt;±30 ppm/°C for NP0
&lt;BR&gt;±15 % for X7R
&lt;BR&gt;Voltage range (UR): 250 V(AC)
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C
&lt;BR&gt;Sizes: 1808 / 1812 / 2211 / 2220
&lt;BR&gt;Recommended soldering: Reflow soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Interference suppression 
&lt;BR&gt;Filter in power supplies 
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166506v209%20Family_WE-MLCC_1812_grau.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166506v209%20Family_WE-MLCC_1812_grau.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;  
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSSA&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-13
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_H1.6" package="WCAP-CSSA_1812_X1/Y2_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8853522110011">
<attribute name="C" value="470pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853522110011?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853522110011"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X1 / Y2"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VIMP" value="5000 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
<device name="_H2" package="WCAP-CSSA_1812_X1/Y2_H2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8853522110021">
<attribute name="C" value="680pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853522110021?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853522110021"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X1 / Y2"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VIMP" value="5000 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
<device name="_H2.5" package="WCAP-CSSA_1812_X1/Y2_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8853522110031">
<attribute name="C" value="1nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853522110031?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853522110031"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X1 / Y2"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VIMP" value="5000 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSSA_1812_X2" prefix="C">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Safety Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;High capacitance stability
&lt;BR&gt;Certificates: TÜV, cULus
&lt;BR&gt;Safety class: X1/Y2, X2
&lt;BR&gt;Mounting style: SMT-Chip
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II)
&lt;BR&gt;Capacitance range: 33 pF ‒ 4.7 nF
&lt;BR&gt;Temperature Coefficient:
&lt;BR&gt;±30 ppm/°C for NP0
&lt;BR&gt;±15 % for X7R
&lt;BR&gt;Voltage range (UR): 250 V(AC)
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C
&lt;BR&gt;Sizes: 1808 / 1812 / 2211 / 2220
&lt;BR&gt;Recommended soldering: Reflow soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Interference suppression 
&lt;BR&gt;Filter in power supplies 
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166506v209%20Family_WE-MLCC_1812_grau.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166506v209%20Family_WE-MLCC_1812_grau.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;  
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSSA&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-13
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_H1.6" package="WCAP-CSSA_1812_X2_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8853622110111">
<attribute name="C" value="1nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853622110111?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853622110111"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VIMP" value="2500 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
<device name="_H2.5" package="WCAP-CSSA_1812_X2_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8853622110151">
<attribute name="C" value="2.2nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853622110151?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853622110151"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VIMP" value="2500 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSSA_2220" prefix="C">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Safety Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;High capacitance stability
&lt;BR&gt;Certificates: TÜV, cULus
&lt;BR&gt;Safety class: X1/Y2, X2
&lt;BR&gt;Mounting style: SMT-Chip
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II)
&lt;BR&gt;Capacitance range: 33 pF ‒ 4.7 nF
&lt;BR&gt;Temperature Coefficient:
&lt;BR&gt;±30 ppm/°C for NP0
&lt;BR&gt;±15 % for X7R
&lt;BR&gt;Voltage range (UR): 250 V(AC)
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C
&lt;BR&gt;Sizes: 1808 / 1812 / 2211 / 2220
&lt;BR&gt;Recommended soldering: Reflow soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Interference suppression 
&lt;BR&gt;Filter in power supplies 
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166506v209%20Family_WE-MLCC_1812_grau.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166506v209%20Family_WE-MLCC_1812_grau.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;  
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSSA&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-13
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSSA_2220">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8853522140011">
<attribute name="C" value="4.7nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853522140011?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853522140011"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X1 / Y2"/>
<attribute name="SIZE" value="2220"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VIMP" value="5000 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSSA_1808_X1/Y2" prefix="C">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Safety Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;High capacitance stability
&lt;BR&gt;Certificates: TÜV, cULus
&lt;BR&gt;Safety class: X1/Y2, X2
&lt;BR&gt;Mounting style: SMT-Chip
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II)
&lt;BR&gt;Capacitance range: 33 pF ‒ 4.7 nF
&lt;BR&gt;Temperature Coefficient:
&lt;BR&gt;±30 ppm/°C for NP0
&lt;BR&gt;±15 % for X7R
&lt;BR&gt;Voltage range (UR): 250 V(AC)
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C
&lt;BR&gt;Sizes: 1808 / 1812 / 2211 / 2220
&lt;BR&gt;Recommended soldering: Reflow soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Interference suppression 
&lt;BR&gt;Filter in power supplies 
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166506v209%20Family_WE-MLCC_1812_grau.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166506v209%20Family_WE-MLCC_1812_grau.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;  
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSSA&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-13
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_H1.6" package="WCAP-CSSA_1808_X1/Y2_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8853522100141">
<attribute name="C" value="100pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853522100141?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853522100141"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X1 / Y2"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VIMP" value="5000 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
<device name="_H2" package="WCAP-CSSA_1808_X1/Y2_H2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8853522100131">
<attribute name="C" value="1nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853522100131?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853522100131"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X1 / Y2"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VIMP" value="5000 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
<device name="_H1.4" package="WCAP-CSSA_1808_X1/Y2_H1.4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8853520100071">
<attribute name="C" value="33pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853520100071?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853520100071"/>
<attribute name="RISO" value="100 Gohm"/>
<attribute name="SAFETY-CLASS" value="X1 / Y2"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VIMP" value="5000 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSSA_1808_X2" prefix="C">
<description>&lt;b&gt;WCAP-CSSA Interference Suppression&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Safety Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;High capacitance stability
&lt;BR&gt;Certificates: TÜV, cULus
&lt;BR&gt;Safety class: X1/Y2, X2
&lt;BR&gt;Mounting style: SMT-Chip
&lt;BR&gt;Ceramic: NP0 (Class I), X7R (Class II)
&lt;BR&gt;Capacitance range: 33 pF ‒ 4.7 nF
&lt;BR&gt;Temperature Coefficient:
&lt;BR&gt;±30 ppm/°C for NP0
&lt;BR&gt;±15 % for X7R
&lt;BR&gt;Voltage range (UR): 250 V(AC)
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C
&lt;BR&gt;Sizes: 1808 / 1812 / 2211 / 2220
&lt;BR&gt;Recommended soldering: Reflow soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Interference suppression 
&lt;BR&gt;Filter in power supplies 
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o166506v209%20Family_WE-MLCC_1812_grau.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o166506v209%20Family_WE-MLCC_1812_grau.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;  
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSSA&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-13
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_H1.6" package="WCAP-CSSA_1808_X2_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8853620100111">
<attribute name="C" value="47pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853620100111?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853620100111"/>
<attribute name="RISO" value="100 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VIMP" value="2500 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_8853622100091">
<attribute name="C" value="470pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853622100091?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853622100091"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VIMP" value="2500 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_8853622100131">
<attribute name="C" value="680pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853622100131?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853622100131"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VIMP" value="2500 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_8853622100181">
<attribute name="C" value="150pF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853622100181?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853622100181"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VIMP" value="2500 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
<device name="_H1.4" package="WCAP-CSSA_1808_X2_H1.4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8853620100091">
<attribute name="C" value="33pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853620100091?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853620100091"/>
<attribute name="RISO" value="100 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VIMP" value="2500 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
<device name="_H2" package="WCAP-CSSA_1808_X2_H2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_8853620100171">
<attribute name="C" value="100pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853620100171?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853620100171"/>
<attribute name="RISO" value="100 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VIMP" value="2500 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_8853620100181">
<attribute name="C" value="220pF"/>
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853620100181?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853620100181"/>
<attribute name="RISO" value="100 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VIMP" value="2500 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_8853622100171">
<attribute name="C" value="1nF"/>
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8853622100171?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="8853622100171"/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="SIZE" value="1808"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VIMP" value="2500 V(DC)"/>
<attribute name="VR" value="250 V(AC)"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
