<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Film Capacitors - General Purpose - WCAP-FTBE&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-09-05&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-FTBE_P15L18W12H21">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X12X21(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P37.5L42W17H30">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,37.5X42X17X30(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P37.5L42W20.5H34">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,37.5X42X20.5X34(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P37.5L42W31H43">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,37.5X42X31X43(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P15L18W5H11">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P15L18W6H12">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P15L18W8.5H15">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X8.5X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P15L18W7H13">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X7X13(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P7.5L10.5W6H12">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,7.5X10.5X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P7.5L10.5W5H11">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,7.5X10.5X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P10L13W5.0H11">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,10X13X5.0X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P10L13W5.5H11">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,10X13X5.5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P27.5L31W15H24.5">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X15X24.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P27.5L31W11H20">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X11X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P22.5L26W6H15">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,22.5X26X6X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P22.5L26W7H16.5">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt; Film Capacitors,22.5X26X7X16.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBE_P22.5L26W9H18">
<description>&lt;B&gt;WCAP-FTBE&lt;/B&gt;&lt;BR&gt;Film Capacitors,22.5X26X9X18(PitchXLXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-FTBE_P37.5" prefix="C">
<description>&lt;b&gt;WCAP-FTBE Film Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Boxed Type Metallized Polyester  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Self-healing properties
&lt;BR&gt;High voltage and volumetric capacity possible
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polyester
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o85130v209%20family-WCAP-FTBE-22.5x26x9x18.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o85130v209%20family-WCAP-FTBE-22.5x26x9x18.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTBE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTBE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-05
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L42W17H30" package="WCAP-FTBE_P37.5L42W17H30">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890303428008CS">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890303428008CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="30mm"/>
<attribute name="LENGTH" value="42mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890303428008CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="12V/us"/>
<attribute name="RISO" value="909.09 Mohm"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="VR2" value="504VDC"/>
<attribute name="WIDTH" value="17mm"/>
</technology>
</technologies>
</device>
<device name="_L42W20.5H34" package="WCAP-FTBE_P37.5L42W20.5H34">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283428007CS">
<attribute name="C" value="6.8 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890283428007CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="34mm"/>
<attribute name="LENGTH" value="42mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890283428007CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="9V/us"/>
<attribute name="RISO" value="441.18 Mohm"/>
<attribute name="VALUE" value="6.8 µF"/>
<attribute name="VR" value="400VDC"/>
<attribute name="VR2" value="320VDC"/>
<attribute name="WIDTH" value="20.5mm"/>
</technology>
</technologies>
</device>
<device name="_L42W31H43" package="WCAP-FTBE_P37.5L42W31H43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890493428013CS">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890493428013CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="43mm"/>
<attribute name="LENGTH" value="42mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890493428013CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="16V/us"/>
<attribute name="RISO" value="638.3 Mohm"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="VR2" value="800VDC"/>
<attribute name="WIDTH" value="31mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBE_P7.5" prefix="C">
<description>&lt;b&gt;WCAP-FTBE Film Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Boxed Type Metallized Polyester  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Self-healing properties
&lt;BR&gt;High voltage and volumetric capacity possible
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polyester
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o85130v209%20family-WCAP-FTBE-22.5x26x9x18.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o85130v209%20family-WCAP-FTBE-22.5x26x9x18.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTBE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTBE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-05
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L10.5W5H11" package="WCAP-FTBE_P7.5L10.5W5H11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283422001CS">
<attribute name="C" value="68 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890283422001CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890283422001CS"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="44V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="400VDC"/>
<attribute name="VR2" value="320V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L10.5W6H12" package="WCAP-FTBE_P7.5L10.5W6H12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273422002CS">
<attribute name="C" value="220 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890273422002CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890273422002CS"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="38V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="VR2" value=""/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890283422005CS">
<attribute name="C" value="150 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890283422005CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890283422005CS"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="46V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="400VDC"/>
<attribute name="VR2" value="320V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890303422005CS">
<attribute name="C" value="47 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890303422005CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890303422005CS"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="100V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="VR2" value="504V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890493422002CS">
<attribute name="C" value="10 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890493422002CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890493422002CS"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="VR2" value="800V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBE_P15" prefix="C">
<description>&lt;b&gt;WCAP-FTBE Film Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Boxed Type Metallized Polyester  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Self-healing properties
&lt;BR&gt;High voltage and volumetric capacity possible
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polyester
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o85130v209%20family-WCAP-FTBE-22.5x26x9x18.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o85130v209%20family-WCAP-FTBE-22.5x26x9x18.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTBE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTBE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-05
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L18W5H11" package="WCAP-FTBE_P15L18W5H11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273425001CS">
<attribute name="C" value="330 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890273425001CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890273425001CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="8V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="VR2" value="200V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890283425002CS">
<attribute name="C" value="220 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890283425002CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890283425002CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="12V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="400VDC"/>
<attribute name="VR2" value="320V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890493425001CS">
<attribute name="C" value="22 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890493425001CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890493425001CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="27V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="VR2" value="800V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W6H12" package="WCAP-FTBE_P15L18W6H12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890303425004CS">
<attribute name="C" value="100 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890303425004CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890303425004CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="28V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="VR2" value="504V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L18W7H13" package="WCAP-FTBE_P15L18W7H13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273425007CS">
<attribute name="C" value="1 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890273425007CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890273425007CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="11V/us"/>
<attribute name="RISO" value="3000 ohm*F"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="VR2" value="200V(DC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L18W8.5H15" package="WCAP-FTBE_P15L18W8.5H15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890263425004CS">
<attribute name="C" value="2.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890263425004CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890263425004CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="9V/us"/>
<attribute name="RISO" value="3000 ohm*F"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="100VDC"/>
<attribute name="VR2" value="80V(DC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
<technology name="_890283425008CS">
<attribute name="C" value="680 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890283425008CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890283425008CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="18V/us"/>
<attribute name="RISO" value="3000 ohm*F"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="400VDC"/>
<attribute name="VR2" value="320V(DC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
<technology name="_890493425009CS">
<attribute name="C" value="100 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890493425009CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890493425009CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="44V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="VR2" value="800V(DC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBE_P10" prefix="C">
<description>&lt;b&gt;WCAP-FTBE Film Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Boxed Type Metallized Polyester  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Self-healing properties
&lt;BR&gt;High voltage and volumetric capacity possible
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polyester
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o85130v209%20family-WCAP-FTBE-22.5x26x9x18.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o85130v209%20family-WCAP-FTBE-22.5x26x9x18.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTBE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTBE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-05
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L13W5H11" package="WCAP-FTBE_P10L13W5.0H11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273423002CS">
<attribute name="C" value="220 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890273423002CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890273423002CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="23V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="VR2" value="200V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890283423001CS">
<attribute name="C" value="100 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890283423001CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890283423001CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="34V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="400VDC"/>
<attribute name="VR2" value="320V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890493423001CS">
<attribute name="C" value="15 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890493423001CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890493423001CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="83V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="VR2" value="800V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L13W5.5H11" package="WCAP-FTBE_P10L13W5.5H11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890303423005CS">
<attribute name="C" value="68 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890303423005CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890303423005CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="52V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="VR2" value="504V(DC)"/>
<attribute name="WIDTH" value="5.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBE_P27.5" prefix="C">
<description>&lt;b&gt;WCAP-FTBE Film Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Boxed Type Metallized Polyester  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Self-healing properties
&lt;BR&gt;High voltage and volumetric capacity possible
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polyester
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o85130v209%20family-WCAP-FTBE-22.5x26x9x18.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o85130v209%20family-WCAP-FTBE-22.5x26x9x18.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTBE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTBE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-05
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L31W15H24.5" package="WCAP-FTBE_P27.5L31W15H24.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283427007CS">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890283427007CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="24.5mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890283427007CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="11V/us"/>
<attribute name="RISO" value="3000 ohm*F"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="400VDC"/>
<attribute name="VR2" value="320V(DC)"/>
<attribute name="WIDTH" value="15mm"/>
</technology>
<technology name="_890303427009CS">
<attribute name="C" value="1.5 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890303427009CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="24.5mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890303427009CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="17V/us"/>
<attribute name="RISO" value="3000 ohm*F"/>
<attribute name="VALUE" value="1.5 µF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="VR2" value="504V(DC)"/>
<attribute name="WIDTH" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_L31W11H20" package="WCAP-FTBE_P27.5L31W11H20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273427005CS">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890273427005CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890273427005CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="6V/us"/>
<attribute name="RISO" value="3000 ohm*F"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="250VDC"/>
<attribute name="VR2" value="200V(DC)"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
<technology name="_890493427007CS">
<attribute name="C" value="470 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890493427007CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890493427007CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="22V/us"/>
<attribute name="RISO" value="3000 ohm*F"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="VR2" value="800V(DC)"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBE_P22.5" prefix="C">
<description>&lt;b&gt;WCAP-FTBE Film Capacitors&lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Boxed Type Metallized Polyester  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +85 °C
&lt;BR&gt;Self-healing properties
&lt;BR&gt;High voltage and volumetric capacity possible
&lt;BR&gt;Mounting style: Boxed THT
&lt;BR&gt;Dielectric: Polyester
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 / 37.5 mm
&lt;BR&gt;Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o85130v209%20family-WCAP-FTBE-22.5x26x9x18.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o85130v209%20family-WCAP-FTBE-22.5x26x9x18.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTBE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTBE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-05
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L26W6H15" package="WCAP-FTBE_P22.5L26W6H15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890263426001CS">
<attribute name="C" value="2.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890263426001CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890263426001CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="5V/us"/>
<attribute name="RISO" value="3000 ohm*F"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="100VDC"/>
<attribute name="VR2" value="80V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890283426004CS">
<attribute name="C" value="470 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890283426004CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890283426004CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="11V/us"/>
<attribute name="RISO" value="3000 ohm*F"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="400VDC"/>
<attribute name="VR2" value="320V(DC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L26W7H16.5" package="WCAP-FTBE_P22.5L26W7H16.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890263426003CS">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890263426003CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="16.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890263426003CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="5V/us"/>
<attribute name="RISO" value="3000 ohm*F"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="100VDC"/>
<attribute name="VR2" value="80V(DC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L26W9H18" package="WCAP-FTBE_P22.5L26W9H18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283426008CS">
<attribute name="C" value="1 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890283426008CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="18mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890283426008CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="13V/us"/>
<attribute name="RISO" value="3000 ohm*F"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="400VDC"/>
<attribute name="VR2" value="320V(DC)"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
<technology name="_890303426008CS">
<attribute name="C" value="470 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890303426008CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="18mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890303426008CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="20V/us"/>
<attribute name="RISO" value="3000 ohm*F"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="630VDC"/>
<attribute name="VR2" value="504V(DC)"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
<technology name="_890493426011CS">
<attribute name="C" value="220 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890493426011CS?ae"/>
<attribute name="DF" value="1%@1kHz"/>
<attribute name="HEIGHT" value="18mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890493426011CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="27V/us"/>
<attribute name="RISO" value="9000 Mohm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="1000VDC"/>
<attribute name="VR2" value="800V(DC)"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
