<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Film Capacitors - WCAP-FTDB&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-11-11&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-FTDB_P37.5L42W30H45">
<description>&lt;B&gt;WCAP-FTDB Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=37.5X42X30X45mm</description>
</package>
<package name="WCAP-FTDB_P27.5L32W11H20">
<description>&lt;B&gt;WCAP-FTDB Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=27.5X32X11X20mm</description>
</package>
<package name="WCAP-FTDB_P37.5L42W35H50">
<description>&lt;B&gt;WCAP-FTDB Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=37.5X42X35X50mm</description>
</package>
<package name="WCAP-FTDB_P27.5L32W16H30">
<description>&lt;B&gt;WCAP-FTDB Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=27.5X32X16X30mm</description>
</package>
<package name="WCAP-FTDB_P37.5L42W24H36">
<description>&lt;B&gt;WCAP-FTDB Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=37.5X42X24X36mm</description>
</package>
<package name="WCAP-FTDB_P52.5L57W29.5H43.5">
<description>&lt;B&gt;WCAP-FTDB Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=52.5X57X29.5X43.5mm</description>
</package>
<package name="WCAP-FTDB_P27.5L32W15H24.5">
<description>&lt;B&gt;WCAP-FTDB Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=27.5X32X15X24.5mm</description>
</package>
<package name="WCAP-FTDB_P52.5L57W45H55">
<description>&lt;B&gt;WCAP-FTDB Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=52.5X57X45X55mm</description>
</package>
<package name="WCAP-FTDB_P27.5L32W22H37">
<description>&lt;B&gt;WCAP-FTDB Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=27.5X32X22X37mm</description>
</package>
<package name="WCAP-FTDB_P37.5L42W45H60">
<description>&lt;B&gt;WCAP-FTDB Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=37.5X42X45X60mm</description>
</package>
<package name="WCAP-FTDB_P52.5L57W45H65">
<description>&lt;B&gt;WCAP-FTDB Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=52.5X57X45X65mm</description>
</package>
<package name="WCAP-FTDB_P27.5L32W9H18">
<description>&lt;B&gt;WCAP-FTDB Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=27.5X32X9X18mm</description>
</package>
<package name="WCAP-FTDB_P52.5L57W35H50">
<description>&lt;B&gt;WCAP-FTDB Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=52.5X57X35X50mm</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-FTDB_P37.5" prefix="C">
<description>&lt;b&gt;WCAP-FTDB DC Link  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for DC Link applications
&lt;BR&gt; Self-healing properties
&lt;BR&gt; Support a DC network by supplying periodically currents
&lt;BR&gt; Absorb the high ripple current to prevent the high ripple voltage
&lt;BR&gt; Prevent the instant overload peak voltage
&lt;BR&gt; Mounting style: Boxed THT
&lt;BR&gt; Dielectric: Polypropylene
&lt;BR&gt; Capacitance range: 680 nF ‒ 100 µF
&lt;BR&gt; Capacitance tolerance: ±5 %
&lt;BR&gt; Voltage range (UR): 500 - 1200 V(DC)
&lt;BR&gt; Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt; Pitch: 27.5 / 37.5 / 52.5 mm
&lt;BR&gt; Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;AC/DC converter
&lt;BR&gt; DC/AC converter
 &lt;BR&gt;e.g. for renewable energy, electrical vehicle, hybrid electric vehicle, battery charger, wind power converter, solar low power converter, drives
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14734v209%20Family_WCAP-FTXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14734v209%20Family_WCAP-FTXX.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
        
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTDB/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-FTDB&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-11
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L42W24H36" package="WCAP-FTDB_P37.5L42W24H36">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890484428002CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890484428002CS?ae"/>
<attribute name="DF" value="0.15%"/>
<attribute name="HEIGHT" value="36mm"/>
<attribute name="LENGTH" value="42mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890484428002CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="30V/us"/>
<attribute name="RISO" value="285.71Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP375356J500DCPP15041"/>
<attribute name="VALUE" value="35uF"/>
<attribute name="VR" value="500V"/>
<attribute name="WIDTH" value="24mm"/>
</technology>
</technologies>
</device>
<device name="_L42W30H45" package="WCAP-FTDB_P37.5L42W30H45">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890734428004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890734428004CS?ae"/>
<attribute name="DF" value="0.15%"/>
<attribute name="HEIGHT" value="45mm"/>
<attribute name="LENGTH" value="42mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890734428004CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="40V/us"/>
<attribute name="RISO" value="666.66Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP375156JA10DCPP15040"/>
<attribute name="VALUE" value="15uF"/>
<attribute name="VR" value="1100V"/>
<attribute name="WIDTH" value="30mm"/>
</technology>
<technology name="_890764428004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890764428004CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="45mm"/>
<attribute name="LENGTH" value="42mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890764428004CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="30V/us"/>
<attribute name="RISO" value="250Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP375406J600DCPP15040"/>
<attribute name="VALUE" value="40uF"/>
<attribute name="VR" value="600V"/>
<attribute name="WIDTH" value="30mm"/>
</technology>
</technologies>
</device>
<device name="_L42W35H50" package="WCAP-FTDB_P37.5L42W35H50">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890494428004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890494428004CS?ae"/>
<attribute name="DF" value="0.15%"/>
<attribute name="HEIGHT" value="50mm"/>
<attribute name="LENGTH" value="42mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890494428004CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="37V/us"/>
<attribute name="RISO" value="400Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP375256JA00DCPP15040"/>
<attribute name="VALUE" value="25uF"/>
<attribute name="VR" value="1000V"/>
<attribute name="WIDTH" value="35mm"/>
</technology>
</technologies>
</device>
<device name="_L42W45H60" package="WCAP-FTDB_P37.5L42W45H60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890734428008CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890734428008CS?ae"/>
<attribute name="DF" value="0.15%"/>
<attribute name="HEIGHT" value="60mm"/>
<attribute name="LENGTH" value="42mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890734428008CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="40V/us"/>
<attribute name="RISO" value="333.33Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP375306JA10DCPP15040"/>
<attribute name="VALUE" value="30uF"/>
<attribute name="VR" value="1100V"/>
<attribute name="WIDTH" value="45mm"/>
</technology>
<technology name="_890744428006CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890744428006CS?ae"/>
<attribute name="DF" value="0.13%"/>
<attribute name="HEIGHT" value="60mm"/>
<attribute name="LENGTH" value="42mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890744428006CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="45V/us"/>
<attribute name="RISO" value="400Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP375256JA20DCPP15040"/>
<attribute name="VALUE" value="25uF"/>
<attribute name="VR" value="1200V"/>
<attribute name="WIDTH" value="45mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTDB_P27.5" prefix="C">
<description>&lt;b&gt;WCAP-FTDB DC Link  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for DC Link applications
&lt;BR&gt; Self-healing properties
&lt;BR&gt; Support a DC network by supplying periodically currents
&lt;BR&gt; Absorb the high ripple current to prevent the high ripple voltage
&lt;BR&gt; Prevent the instant overload peak voltage
&lt;BR&gt; Mounting style: Boxed THT
&lt;BR&gt; Dielectric: Polypropylene
&lt;BR&gt; Capacitance range: 680 nF ‒ 100 µF
&lt;BR&gt; Capacitance tolerance: ±5 %
&lt;BR&gt; Voltage range (UR): 500 - 1200 V(DC)
&lt;BR&gt; Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt; Pitch: 27.5 / 37.5 / 52.5 mm
&lt;BR&gt; Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;AC/DC converter
&lt;BR&gt; DC/AC converter
 &lt;BR&gt;e.g. for renewable energy, electrical vehicle, hybrid electric vehicle, battery charger, wind power converter, solar low power converter, drives
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14734v209%20Family_WCAP-FTXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14734v209%20Family_WCAP-FTXX.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
        
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTDB/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-FTDB&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-11
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L32W11H20" package="WCAP-FTDB_P27.5L32W11H20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890484427001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890484427001CS?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890484427001CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="65V/us"/>
<attribute name="RISO" value="2Gohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP275505J500DCPP15020"/>
<attribute name="VALUE" value="5uF"/>
<attribute name="VR" value="500V"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
<technology name="_890744427001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890744427001CS?ae"/>
<attribute name="DF" value="0.07%"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890744427001CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="90V/us"/>
<attribute name="RISO" value="10Gohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP275105JA20DCPP15020"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="1200V"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
</technologies>
</device>
<device name="_L32W15H24.5" package="WCAP-FTDB_P27.5L32W15H24.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890494427003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890494427003CS?ae"/>
<attribute name="DF" value="0.08%"/>
<attribute name="HEIGHT" value="24.5mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890494427003CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="75V/us"/>
<attribute name="RISO" value="3.33Gohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP275305JA00DCPP15020"/>
<attribute name="VALUE" value="3uF"/>
<attribute name="VR" value="1000V"/>
<attribute name="WIDTH" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_L32W16H30" package="WCAP-FTDB_P27.5L32W16H30">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890734427005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890734427005CS?ae"/>
<attribute name="DF" value="0.08%"/>
<attribute name="HEIGHT" value="30mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890734427005CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="80V/us"/>
<attribute name="RISO" value="3.33Gohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP275305JA10DCPP15020"/>
<attribute name="VALUE" value="3uF"/>
<attribute name="VR" value="1100V"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
<technology name="_890764427009CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890764427009CS?ae"/>
<attribute name="DF" value="0.11%"/>
<attribute name="HEIGHT" value="30mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890764427009CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="65V/us"/>
<attribute name="RISO" value="1Gohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP275106J600DCPP15020"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="600V"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
</technologies>
</device>
<device name="_L32W22H37" package="WCAP-FTDB_P27.5L32W22H37">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890724427010CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890724427010CS?ae"/>
<attribute name="DF" value="0.09%"/>
<attribute name="HEIGHT" value="37mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890724427010CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="70V/us"/>
<attribute name="RISO" value="1Gohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP275106J900DCPP15020"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="900V"/>
<attribute name="WIDTH" value="22mm"/>
</technology>
<technology name="_890744427005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890744427005CS?ae"/>
<attribute name="DF" value="0.07%"/>
<attribute name="HEIGHT" value="37mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890744427005CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="90V/us"/>
<attribute name="RISO" value="2Gohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP275505JA20DCPP15020"/>
<attribute name="VALUE" value="5uF"/>
<attribute name="VR" value="1200V"/>
<attribute name="WIDTH" value="22mm"/>
</technology>
</technologies>
</device>
<device name="_L32W9H18" package="WCAP-FTDB_P27.5L32W9H18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890724427001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890724427001CS?ae"/>
<attribute name="DF" value="0.09%"/>
<attribute name="HEIGHT" value="18mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890724427001CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="70V/us"/>
<attribute name="RISO" value="10Gohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP275105J900DCPP15020"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="900V"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTDB_P52.5" prefix="C">
<description>&lt;b&gt;WCAP-FTDB DC Link  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for DC Link applications
&lt;BR&gt; Self-healing properties
&lt;BR&gt; Support a DC network by supplying periodically currents
&lt;BR&gt; Absorb the high ripple current to prevent the high ripple voltage
&lt;BR&gt; Prevent the instant overload peak voltage
&lt;BR&gt; Mounting style: Boxed THT
&lt;BR&gt; Dielectric: Polypropylene
&lt;BR&gt; Capacitance range: 680 nF ‒ 100 µF
&lt;BR&gt; Capacitance tolerance: ±5 %
&lt;BR&gt; Voltage range (UR): 500 - 1200 V(DC)
&lt;BR&gt; Operating temperature: -40 °C up to + 105 °C
&lt;BR&gt; Pitch: 27.5 / 37.5 / 52.5 mm
&lt;BR&gt; Recommended soldering: Wave soldering
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;AC/DC converter
&lt;BR&gt; DC/AC converter
 &lt;BR&gt;e.g. for renewable energy, electrical vehicle, hybrid electric vehicle, battery charger, wind power converter, solar low power converter, drives
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14734v209%20Family_WCAP-FTXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14734v209%20Family_WCAP-FTXX.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
        
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTDB/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-FTDB&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-11
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L57W29.5H43.5" package="WCAP-FTDB_P52.5L57W29.5H43.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890484429001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890484429001CS?ae"/>
<attribute name="DF" value="0.35%"/>
<attribute name="HEIGHT" value="43.5mm"/>
<attribute name="LENGTH" value="57mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890484429001CS"/>
<attribute name="PITCH" value="52.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="15V/us"/>
<attribute name="RISO" value="133.33Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP525756J500DCPP15040"/>
<attribute name="VALUE" value="75uF"/>
<attribute name="VR" value="500V"/>
<attribute name="WIDTH" value="29.5mm"/>
</technology>
<technology name="_890764429002CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890764429002CS?ae"/>
<attribute name="DF" value="0.36%"/>
<attribute name="HEIGHT" value="43.5mm"/>
<attribute name="LENGTH" value="57mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890764429002CS"/>
<attribute name="PITCH" value="52.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="15V/us"/>
<attribute name="RISO" value="166.66Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP525606J600DCPP15040"/>
<attribute name="VALUE" value="60uF"/>
<attribute name="VR" value="600V"/>
<attribute name="WIDTH" value="29.5mm"/>
</technology>
</technologies>
</device>
<device name="_L57W35H50" package="WCAP-FTDB_P52.5L57W35H50">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890494429003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890494429003CS?ae"/>
<attribute name="DF" value="0.28%"/>
<attribute name="HEIGHT" value="50mm"/>
<attribute name="LENGTH" value="57mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890494429003CS"/>
<attribute name="PITCH" value="52.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="17V/us"/>
<attribute name="RISO" value="250Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP525406JA00DCPP15040"/>
<attribute name="VALUE" value="40uF"/>
<attribute name="VR" value="1000V"/>
<attribute name="WIDTH" value="35mm"/>
</technology>
<technology name="_890714429003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890714429003CS?ae"/>
<attribute name="DF" value="0.33%"/>
<attribute name="HEIGHT" value="50mm"/>
<attribute name="LENGTH" value="57mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890714429003CS"/>
<attribute name="PITCH" value="52.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="15V/us"/>
<attribute name="RISO" value="200Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP525506J800DCPP15040"/>
<attribute name="VALUE" value="50uF"/>
<attribute name="VR" value="800V"/>
<attribute name="WIDTH" value="35mm"/>
</technology>
<technology name="_890724429005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890724429005CS?ae"/>
<attribute name="DF" value="0.31%"/>
<attribute name="HEIGHT" value="50mm"/>
<attribute name="LENGTH" value="57mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890724429005CS"/>
<attribute name="PITCH" value="52.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="15V/us"/>
<attribute name="RISO" value="200Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP525506J900DCPP15040"/>
<attribute name="VALUE" value="50uF"/>
<attribute name="VR" value="900V"/>
<attribute name="WIDTH" value="35mm"/>
</technology>
<technology name="_890744429002CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890744429002CS?ae"/>
<attribute name="DF" value="0.24%"/>
<attribute name="HEIGHT" value="50mm"/>
<attribute name="LENGTH" value="57mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890744429002CS"/>
<attribute name="PITCH" value="52.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="23V/us"/>
<attribute name="RISO" value="400Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP525256JA20DCPP15040"/>
<attribute name="VALUE" value="25uF"/>
<attribute name="VR" value="1200V"/>
<attribute name="WIDTH" value="35mm"/>
</technology>
</technologies>
</device>
<device name="_L57W45H55" package="WCAP-FTDB_P52.5L57W45H55">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890494429005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890494429005CS?ae"/>
<attribute name="DF" value="0.28%"/>
<attribute name="HEIGHT" value="55mm"/>
<attribute name="LENGTH" value="57mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890494429005CS"/>
<attribute name="PITCH" value="52.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="17V/us"/>
<attribute name="RISO" value="200Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP525506JA00DCPP15040"/>
<attribute name="VALUE" value="50uF"/>
<attribute name="VR" value="1000V"/>
<attribute name="WIDTH" value="45mm"/>
</technology>
</technologies>
</device>
<device name="_L57W45H65" package="WCAP-FTDB_P52.5L57W45H65">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890724429010CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890724429010CS?ae"/>
<attribute name="DF" value="0.31%"/>
<attribute name="HEIGHT" value="65mm"/>
<attribute name="LENGTH" value="57mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890724429010CS"/>
<attribute name="PITCH" value="52.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="15V/us"/>
<attribute name="RISO" value="133.33Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP525756J900DCPP15040"/>
<attribute name="VALUE" value="75uF"/>
<attribute name="VR" value="900V"/>
<attribute name="WIDTH" value="45mm"/>
</technology>
<technology name="_890734429007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890734429007CS?ae"/>
<attribute name="DF" value="0.27%"/>
<attribute name="HEIGHT" value="65mm"/>
<attribute name="LENGTH" value="57mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890734429007CS"/>
<attribute name="PITCH" value="52.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="20V/us"/>
<attribute name="RISO" value="200Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP525506JA10DCPP15040"/>
<attribute name="VALUE" value="50uF"/>
<attribute name="VR" value="1100V"/>
<attribute name="WIDTH" value="45mm"/>
</technology>
<technology name="_890744429005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890744429005CS?ae"/>
<attribute name="DF" value="0.24%"/>
<attribute name="HEIGHT" value="65mm"/>
<attribute name="LENGTH" value="57mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 up to +105 °C"/>
<attribute name="PART-NUMBER" value="890744429005CS"/>
<attribute name="PITCH" value="52.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="23V/us"/>
<attribute name="RISO" value="250Mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="MDBP525406JA20DCPP15040"/>
<attribute name="VALUE" value="40uF"/>
<attribute name="VR" value="1200V"/>
<attribute name="WIDTH" value="45mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
