<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<library>
<description>Würth Elektronik - Passive Components - Capacitors - Film Capacitors - Interference Suppression - WCAP-FTX2

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026a, 2026-07-20
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-FTX2_P37.5L41.5W22.5H35.5_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 37.5mm, CS, THT

37.5X41.5X22.5X35.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W15.5H29">
<description>WCAP-FTX2 Film Capacitors

Pitch 27.5mm, Standard, THT

27.5X31X15.5X29(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W10.5H20">
<description>WCAP-FTX2 Film Capacitors

Pitch 27.5mm, Standard, THT

27.5X31X10.5X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W13H22">
<description>WCAP-FTX2 Film Capacitors

Pitch 27.5mm, Standard, THT

27.5X31X13X22(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W8H17">
<description>WCAP-FTX2 Film Capacitors

Pitch 27.5mm, Standard, THT

27.5X31X8X17(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W5H11">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, Standard, THT

15X18X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W6H12">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, Standard, THT

15X18X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W6H11.5">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, Standard, THT

15X18X6X11.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W8.5H14.5">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, Standard, THT

15X18X8.5X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W7.5H14.5">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, Standard, THT

15X18X7.55X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W10H16">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, Standard, THT

15X18X10X16(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W8H14">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, Standard, THT

15X18X8X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W9H15">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, Standard, THT

15X18X9X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W7.5H13.5">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, Standard, THT

15X18X7.5X13.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W5H11_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 10mm, CS, THT

10X13X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W7H12_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 10mm, CS, THT

10X13X7X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W5H10_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 10mm, CS, THT

10X13X5X10(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W8H14_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 10mm, CS, THT

10X13X8X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W7H13_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 10mm, CS, THT

10X13X7X13(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W4.5H9.5_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 10mm, CS, THT

10X13X4.5X9.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W19H32.5_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 27.5mm, CS, THT

27.5X31X19X32.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W10.5H20_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 27.5mm, CS, THT

27.5X31X10.5X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W13H22_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 27.5mm, CS, THT

27.5X31X13X22(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P27.5L31W15.5H29_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 27.5mm, CS, THT

27.5X31X15.5X29(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W6H12_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, CS, THT

15X18X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W10H16_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, CS, THT

15X18X10X16(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W7.5H14.5_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, CS, THT

15X18X7.55X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W8.5H14.5_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, CS, THT

15X18X8.5X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W6H11.5_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, CS, THT

15X18X6X11.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W9H15_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, CS, THT

15X18X9X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W5H11_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, CS, THT

15X18X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W7.5H13.5_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, CS, THT

15X18X7.5X13.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W8H14_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, CS, THT

15X18X8X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P15L18W10H17.5_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 15mm, CS, THT

15X18X10X17.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W7H13">
<description>WCAP-FTX2 Film Capacitors

Pitch 10mm, Standard, THT

10X13X7X13(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W8H14">
<description>WCAP-FTX2 Film Capacitors

Pitch 10mm, Standard, THT

10X13X8X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W5H11">
<description>WCAP-FTX2 Film Capacitors

Pitch 10mm, Standard, THT

10X13X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W4.5H9.5">
<description>WCAP-FTX2 Film Capacitors

Pitch 10mm, Standard, THT

10X13X4.5X9.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W7H12">
<description>WCAP-FTX2 Film Capacitors

Pitch 10mm, Standard, THT

10X13X7X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P10L13W5H10">
<description>WCAP-FTX2 Film Capacitors

Pitch 10mm, Standard, THT

10X13X5X10(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W6H11.5">
<description>WCAP-FTX2 Film Capacitors

Pitch 12.5mm, Standard, THT

12.5X15X6X11.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W10H16">
<description>WCAP-FTX2 Film Capacitors

Pitch 12.5mm, Standard, THT

12.5X15X10X16(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W7H12.5">
<description>WCAP-FTX2 Film Capacitors

Pitch 12.5mm, Standard, THT

12.5X15X7X12.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W8.5H14">
<description>WCAP-FTX2 Film Capacitors

Pitch 12.5mm, Standard, THT

12.5X15X8.5X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P7.5L10W6H12">
<description>WCAP-FTX2 Film Capacitors

Pitch 7.5mm, Standard, THT

7.5X10X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P7.5L11W6H10">
<description>WCAP-FTX2 Film Capacitors

Pitch 7.5mm, Standard, THT

7.5X11X6X10(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W10H16_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 12.5mm, CS, THT

12.5X15X10X16(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W6H11.5_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 12.5mm, CS, THT

12.5X15X6X11.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W8.5H14_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 12.5mm, CS, THT

12.5X15X8.5X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P12.5L15W7H12.5_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 12.5mm, CS, THT

12.5X15X7X12.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P37.5L41.5W22.5H35.5">
<description>WCAP-FTX2 Film Capacitors

Pitch 37.5mm, Standard, THT

37.5X41.5X22.5X35.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W11H20">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, Standard, THT

22.5X26X11X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W7.5H15">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, Standard, THT

22.5X26X7.5X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W7.5H16.5">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, Standard, THT

22.5X26X7.5X16.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W15H25">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, Standard, THT

22.5X26X15X25(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W9H18">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, Standard, THT

22.5X26X9X18(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W6H15">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, Standard, THT

22.5X26X6X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W10H21">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, Standard, THT

22.5X26X10X21(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W7H14.5">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, Standard, THT

22.5X26X7X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P7.5L10W6H12_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 7.5mm, CS, THT

7.5X10X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P7.5L11W6H10_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 7.5mm, CS, THT

7.5X11X6X10(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W10H21_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, CS, THT

22.5X26X10X21(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W11H20_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, CS, THT

22.5X26X11X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W15H25_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, CS, THT

22.5X26X15X25(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W7.5H15_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, CS, THT

22.5X26X7.5X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W7H14.5_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, CS, THT

22.5X26X7X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W6H12_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, CS, THT

22.5X26X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W7.5H16.5_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, CS, THT

22.5X26X7.5X16.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W9H18_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, CS, THT

22.5X26X9X18(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTX2_P22.5L26W6H15_CS">
<description>WCAP-FTX2 Film Capacitors

Pitch 22.5mm, CS, THT

22.5X26X6X15(PitchXLXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-FTX2_P37.5_CS" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2023-10-30
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L41.5W22.5H35.5" package="WCAP-FTX2_P37.5L41.5W22.5H35.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324028008CS">
<attribute name="C" value="6.8 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="35.5mm"/>
<attribute name="LENGTH" value="41.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324028008CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="110V/us"/>
<attribute name="RISO" value="1.47 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="22.5mm"/>
<attribute name="VALUE" value="6.8 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324028008CS?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P27.5" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2023-10-30
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L31W10.5H20" package="WCAP-FTX2_P27.5L31W10.5H20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027006">
<attribute name="C" value="680 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324027006"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="10.5mm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324027006?ae"/>
</technology>
</technologies>
</device>
<device name="_L31W13H22" package="WCAP-FTX2_P27.5L31W13H22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027012">
<attribute name="C" value="1.2 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="22mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324027012"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="8.33 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="13mm"/>
<attribute name="VALUE" value="1.2 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324027012?ae"/>
</technology>
</technologies>
</device>
<device name="_L31W15.5H29" package="WCAP-FTX2_P27.5L31W15.5H29">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027025">
<attribute name="C" value="3.3 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="29mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324027025"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="3.03 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="15.5mm"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324027025?ae"/>
</technology>
</technologies>
</device>
<device name="_L31W8H17" package="WCAP-FTX2_P27.5L31W8H17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027009">
<attribute name="C" value="1 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324027009"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="100V/us"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="8mm"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324027009?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P15" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2023-10-30
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L18W10H16" package="WCAP-FTX2_P15L18W10H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025045">
<attribute name="C" value="680 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025045"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025045?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W5H11" package="WCAP-FTX2_P15L18W5H11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025004">
<attribute name="C" value="27 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025004"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="27 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025004?ae"/>
</technology>
<technology name="_890324025006">
<attribute name="C" value="33 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025006"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="33 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025006?ae"/>
</technology>
<technology name="_890324025007">
<attribute name="C" value="39 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025007"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="39 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025007?ae"/>
</technology>
<technology name="_890324025009">
<attribute name="C" value="47 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025009"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025009?ae"/>
</technology>
<technology name="_890324025011">
<attribute name="C" value="56 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025011"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="250V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="56 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025011?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W6H11.5" package="WCAP-FTX2_P15L18W6H11.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025027">
<attribute name="C" value="220 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025027"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="180V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025027?ae"/>
</technology>
<technology name="_890324025027AP">
<attribute name="C" value="220 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Ammopack"/>
<attribute name="PART-NUMBER" value="890324025027AP"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="180V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025027AP?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W6H12" package="WCAP-FTX2_P15L18W6H12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025013">
<attribute name="C" value="68 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025013"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="270V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025013?ae"/>
</technology>
<technology name="_890324025015">
<attribute name="C" value="82 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025015"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="290V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="82 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025015?ae"/>
</technology>
<technology name="_890324025017">
<attribute name="C" value="100 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025017"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025017?ae"/>
</technology>
<technology name="_890324025022">
<attribute name="C" value="150 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025022"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="210V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025022?ae"/>
</technology>
<technology name="_890324025025">
<attribute name="C" value="180 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025025"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="180 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025025?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W7.5H13.5" package="WCAP-FTX2_P15L18W7.5H13.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025020">
<attribute name="C" value="120 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025020"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7.5mm"/>
<attribute name="VALUE" value="120 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025020?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W7.5H14.5" package="WCAP-FTX2_P15L18W7.5H14.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025031">
<attribute name="C" value="270 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025031"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="250V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7.5mm"/>
<attribute name="VALUE" value="270 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025031?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W8.5H14.5" package="WCAP-FTX2_P15L18W8.5H14.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025034">
<attribute name="C" value="330 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025034"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="260V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="8.5mm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025034?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W8H14" package="WCAP-FTX2_P15L18W8H14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025039">
<attribute name="C" value="470 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025039"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="8mm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025039?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W9H15" package="WCAP-FTX2_P15L18W9H15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025043">
<attribute name="C" value="560 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025043"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="17.86 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="9mm"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025043?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P10_CS" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2023-10-30
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L13W4.5H9.5" package="WCAP-FTX2_P10L13W4.5H9.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023008CS">
<attribute name="C" value="15 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324023008CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023008CS?ae"/>
</technology>
<technology name="_890324023011CS">
<attribute name="C" value="22 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324023011CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023011CS?ae"/>
</technology>
<technology name="_890324023015CS">
<attribute name="C" value="47 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324023015CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023015CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L13W5H10" package="WCAP-FTX2_P10L13W5H10_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023002CS">
<attribute name="C" value="5.6 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324023002CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="600V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="5.6 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023002CS?ae"/>
</technology>
<technology name="_890324023003CS">
<attribute name="C" value="6.8 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324023003CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="6.8 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023003CS?ae"/>
</technology>
<technology name="_890324023004CS">
<attribute name="C" value="8.2 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324023004CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="8.2 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023004CS?ae"/>
</technology>
<technology name="_890324023017CS">
<attribute name="C" value="56 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023017CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="56 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023017CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L13W5H11" package="WCAP-FTX2_P10L13W5H11_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023006CS">
<attribute name="C" value="10 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324023006CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023006CS?ae"/>
</technology>
<technology name="_890324023007CS">
<attribute name="C" value="12 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324023007CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="12 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023007CS?ae"/>
</technology>
<technology name="_890324023010CS">
<attribute name="C" value="18 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023010CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="18 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023010CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L13W7H12" package="WCAP-FTX2_P10L13W7H12_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023025CS">
<attribute name="C" value="150 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324023025CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023025CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L13W7H13" package="WCAP-FTX2_P10L13W7H13_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023019CS">
<attribute name="C" value="68 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324023019CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023019CS?ae"/>
</technology>
<technology name="_890324023021CS">
<attribute name="C" value="82 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023021CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="82 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023021CS?ae"/>
</technology>
<technology name="_890324023023CS">
<attribute name="C" value="100 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324023023CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023023CS?ae"/>
</technology>
<technology name="_890324023024CS">
<attribute name="C" value="120 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023024CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="120 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023024CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L13W8H14" package="WCAP-FTX2_P10L13W8H14_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023028CS">
<attribute name="C" value="220 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324023028CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="8mm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023028CS?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P27.5_CS" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2026-07-20
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L31W10.5H20" package="WCAP-FTX2_P27.5L31W10.5H20_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027006CS">
<attribute name="C" value="680 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324027006CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="10.5mm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324027006CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L31W13H22" package="WCAP-FTX2_P27.5L31W13H22_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027012CS">
<attribute name="C" value="1.2 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="22mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324027012CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="8.33 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="13mm"/>
<attribute name="VALUE" value="1.2 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324027012CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L31W15.5H29" package="WCAP-FTX2_P27.5L31W15.5H29_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027025CS">
<attribute name="C" value="3.3 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="29mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324027025CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="3.03 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="15.5mm"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324027025CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L31W19H32.5" package="WCAP-FTX2_P27.5L31W19H32.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324027030CS">
<attribute name="C" value="4.7 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="32.5mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324027030CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="2.13 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="19mm"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324027030CS?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P15_CS" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2023-10-30
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L18W10H16" package="WCAP-FTX2_P15L18W10H16_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025045CS">
<attribute name="C" value="680 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025045CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025045CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W5H11" package="WCAP-FTX2_P15L18W5H11_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025004CS">
<attribute name="C" value="27 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025004CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="27 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025004CS?ae"/>
</technology>
<technology name="_890324025006CS">
<attribute name="C" value="33 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025006CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="33 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025006CS?ae"/>
</technology>
<technology name="_890324025007CS">
<attribute name="C" value="39 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025007CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="39 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025007CS?ae"/>
</technology>
<technology name="_890324025009CS">
<attribute name="C" value="47 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025009CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025009CS?ae"/>
</technology>
<technology name="_890324025011CS">
<attribute name="C" value="56 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025011CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="250V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="56 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025011CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W6H11.5" package="WCAP-FTX2_P15L18W6H11.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025027CS">
<attribute name="C" value="220 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025027CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="180V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025027CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W6H12" package="WCAP-FTX2_P15L18W6H12_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025013CS">
<attribute name="C" value="68 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025013CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="270V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025013CS?ae"/>
</technology>
<technology name="_890324025015CS">
<attribute name="C" value="82 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025015CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="290V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="82 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025015CS?ae"/>
</technology>
<technology name="_890324025017CS">
<attribute name="C" value="100 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025017CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025017CS?ae"/>
</technology>
<technology name="_890324025022CS">
<attribute name="C" value="150 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025022CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="210V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025022CS?ae"/>
</technology>
<technology name="_890324025025CS">
<attribute name="C" value="180 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025025CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="180 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025025CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W7.5H13.5" package="WCAP-FTX2_P15L18W7.5H13.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025020CS">
<attribute name="C" value="120 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025020CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7.5mm"/>
<attribute name="VALUE" value="120 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025020CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W7.5H14.5" package="WCAP-FTX2_P15L18W7.5H14.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025031CS">
<attribute name="C" value="270 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324025031CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="250V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7.5mm"/>
<attribute name="VALUE" value="270 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025031CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W8.5H14.5" package="WCAP-FTX2_P15L18W8.5H14.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025034CS">
<attribute name="C" value="330 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025034CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="260V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="8.5mm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025034CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W8H14" package="WCAP-FTX2_P15L18W8H14_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025039CS">
<attribute name="C" value="470 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025039CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="8mm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025039CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W9H15" package="WCAP-FTX2_P15L18W9H15_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025043CS">
<attribute name="C" value="560 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025043CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="17.86 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="9mm"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025043CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L18W10H17.5" package="WCAP-FTX2_P15L18W10H17.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324025047CS">
<attribute name="C" value="820 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="17.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324025047CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="12.2 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="VALUE" value="820 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324025047CS?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P10" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2023-10-30
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L13W4.5H9.5" package="WCAP-FTX2_P10L13W4.5H9.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023008">
<attribute name="C" value="15 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023008"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023008?ae"/>
</technology>
<technology name="_890324023011">
<attribute name="C" value="22 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023011"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023011?ae"/>
</technology>
<technology name="_890324023015">
<attribute name="C" value="47 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023015"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="4.5mm"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023015?ae"/>
</technology>
</technologies>
</device>
<device name="_L13W5H10" package="WCAP-FTX2_P10L13W5H10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023002">
<attribute name="C" value="5.6 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023002"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="600V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="5.6 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023002?ae"/>
</technology>
<technology name="_890324023003">
<attribute name="C" value="6.8 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023003"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="6.8 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023003?ae"/>
</technology>
<technology name="_890324023004">
<attribute name="C" value="8.2 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023004"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="8.2 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023004?ae"/>
</technology>
<technology name="_890324023017">
<attribute name="C" value="56 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023017"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="56 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023017?ae"/>
</technology>
</technologies>
</device>
<device name="_L13W5H11" package="WCAP-FTX2_P10L13W5H11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023006">
<attribute name="C" value="10 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023006"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023006?ae"/>
</technology>
<technology name="_890324023007">
<attribute name="C" value="12 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023007"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="12 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023007?ae"/>
</technology>
<technology name="_890324023010">
<attribute name="C" value="18 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023010"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="5mm"/>
<attribute name="VALUE" value="18 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023010?ae"/>
</technology>
</technologies>
</device>
<device name="_L13W7H12" package="WCAP-FTX2_P10L13W7H12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023025">
<attribute name="C" value="150 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023025"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023025?ae"/>
</technology>
</technologies>
</device>
<device name="_L13W7H13" package="WCAP-FTX2_P10L13W7H13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023019">
<attribute name="C" value="68 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023019"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023019?ae"/>
</technology>
<technology name="_890324023021">
<attribute name="C" value="82 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023021"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="82 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023021?ae"/>
</technology>
<technology name="_890324023023">
<attribute name="C" value="100 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023023"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023023?ae"/>
</technology>
<technology name="_890324023024">
<attribute name="C" value="120 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023024"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="120 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023024?ae"/>
</technology>
</technologies>
</device>
<device name="_L13W8H14" package="WCAP-FTX2_P10L13W8H14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324023028">
<attribute name="C" value="220 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324023028"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="8mm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324023028?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P12.5" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2023-10-30
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L15W10H16" package="WCAP-FTX2_P12.5L15W10H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024005">
<attribute name="C" value="470 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324024005"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="280V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324024005?ae"/>
</technology>
</technologies>
</device>
<device name="_L15W6H11.5" package="WCAP-FTX2_P12.5L15W6H11.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024001">
<attribute name="C" value="150 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324024001"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="210V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324024001?ae"/>
</technology>
</technologies>
</device>
<device name="_L15W7H12.5" package="WCAP-FTX2_P12.5L15W7H12.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024002">
<attribute name="C" value="220 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12.5mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324024002"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="240V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324024002?ae"/>
</technology>
</technologies>
</device>
<device name="_L15W8.5H14" package="WCAP-FTX2_P12.5L15W8.5H14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024003">
<attribute name="C" value="330 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324024003"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="260V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="8.5mm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324024003?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P7.5" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2023-10-30
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L10W6H12" package="WCAP-FTX2_P7.5L10W6H12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324022017">
<attribute name="C" value="68 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324022017"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324022017?ae"/>
</technology>
</technologies>
</device>
<device name="_L11W6H10" package="WCAP-FTX2_P7.5L11W6H10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324022007">
<attribute name="C" value="15 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324022007"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324022007?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P12.5_CS" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2023-10-30
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L15W10H16" package="WCAP-FTX2_P12.5L15W10H16_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024005CS">
<attribute name="C" value="470 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324024005CS"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="280V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324024005CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L15W6H11.5" package="WCAP-FTX2_P12.5L15W6H11.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024001CS">
<attribute name="C" value="150 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324024001CS"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="210V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324024001CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L15W7H12.5" package="WCAP-FTX2_P12.5L15W7H12.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024002CS">
<attribute name="C" value="220 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12.5mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324024002CS"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="240V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324024002CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L15W8.5H14" package="WCAP-FTX2_P12.5L15W8.5H14_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324024003CS">
<attribute name="C" value="330 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324024003CS"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="260V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="8.5mm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324024003CS?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P37.5" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2023-10-30
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L41.5W22.5H35.5" package="WCAP-FTX2_P37.5L41.5W22.5H35.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324028008">
<attribute name="C" value="6.8 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="35.5mm"/>
<attribute name="LENGTH" value="41.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324028008"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="110V/us"/>
<attribute name="RISO" value="1.47 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="22.5mm"/>
<attribute name="VALUE" value="6.8 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324028008?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P22.5" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2025-04-24
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L26W10H21" package="WCAP-FTX2_P22.5L26W10H21">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026030">
<attribute name="C" value="1.5 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="21mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324026030"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="6.67 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="VALUE" value="1.5 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026030?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W11H20" package="WCAP-FTX2_P22.5L26W11H20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026027">
<attribute name="C" value="1 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324026027"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="11mm"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026027?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W15H25" package="WCAP-FTX2_P22.5L26W15H25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026034">
<attribute name="C" value="2.2 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="25mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324026034"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="4.55 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="15mm"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026034?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W6H15" package="WCAP-FTX2_P22.5L26W6H15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026003">
<attribute name="C" value="220 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324026003"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026003?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W7.5H15" package="WCAP-FTX2_P22.5L26W7.5H15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026020">
<attribute name="C" value="680 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324026020"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7.5mm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026020?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W7.5H16.5" package="WCAP-FTX2_P22.5L26W7.5H16.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026018">
<attribute name="C" value="560 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="16.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324026018"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="17.86 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7.5mm"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026018?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W9H18" package="WCAP-FTX2_P22.5L26W9H18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026024">
<attribute name="C" value="820 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="18mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324026024"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="12.2 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="9mm"/>
<attribute name="VALUE" value="820 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026024?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W7H14.5" package="WCAP-FTX2_P22.5L26W7H14.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026014">
<attribute name="C" value="470 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324026014"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026014?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P7.5_CS" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2023-10-30
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L10W6H12" package="WCAP-FTX2_P7.5L10W6H12_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324022017CS">
<attribute name="C" value="68 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324022017CS"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324022017CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L11W6H10" package="WCAP-FTX2_P7.5L11W6H10_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324022007CS">
<attribute name="C" value="15 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324022007CS"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324022007CS?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTX2_P22.5_CS" prefix="C">
<description>WCAP-FTX2 Film Capacitors

X2-Capacitors   

Characteristics
Product series for interference suppression
Self-healing properties
Certificates: ENEC 10 by VDE, cULus, CQC
Safety class: X2
Mounting style: Boxed THT
Dielectric: Polypropylene
Capacitance range: 5.6 nF ‒ 6.8 µF
Capacitance tolerance: ±10 %
Voltage range (UR): 275 V(AC)
Operating temperature: -40 °C up to + 105 °C
Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm
Recommended soldering: Wave soldering

Applications
Safety applications
Filter
Interference suppression
e.g. EMI filter for power supplies

Details see: www.we-online.com/en/components/products/WCAP-FTX2

Updated by Ella Wu 2023-10-30
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L26W10H21" package="WCAP-FTX2_P22.5L26W10H21_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026030CS">
<attribute name="C" value="1.5 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="21mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324026030CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="6.67 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="10mm"/>
<attribute name="VALUE" value="1.5 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026030CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W11H20" package="WCAP-FTX2_P22.5L26W11H20_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026027CS">
<attribute name="C" value="1 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324026027CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="10 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="11mm"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026027CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W15H25" package="WCAP-FTX2_P22.5L26W15H25_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026034CS">
<attribute name="C" value="2.2 µF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="25mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324026034CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="4.55 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="15mm"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026034CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W6H15" package="WCAP-FTX2_P22.5L26W6H15_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026003CS">
<attribute name="C" value="220 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324026003CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026003CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W7.5H15" package="WCAP-FTX2_P22.5L26W7.5H15_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026020CS">
<attribute name="C" value="680 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324026020CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7.5mm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026020CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W7.5H16.5" package="WCAP-FTX2_P22.5L26W7.5H16.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026018CS">
<attribute name="C" value="560 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="16.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324026018CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="17.86 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7.5mm"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026018CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W9H18" package="WCAP-FTX2_P22.5L26W9H18_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026024CS">
<attribute name="C" value="820 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="18mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Bulk"/>
<attribute name="PART-NUMBER" value="890324026024CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="12.2 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="9mm"/>
<attribute name="VALUE" value="820 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026024CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W6H12" package="WCAP-FTX2_P22.5L26W6H12_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026007CS">
<attribute name="C" value="330 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324026007CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="6mm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026007CS?ae"/>
</technology>
</technologies>
</device>
<device name="_L26W7H14.5" package="WCAP-FTX2_P22.5L26W7H14.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890324026014CS">
<attribute name="C" value="470 nF"/>
<attribute name="DF" value="0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGING" value="Carton"/>
<attribute name="PART-NUMBER" value="890324026014CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VR" value="275VAC"/>
<attribute name="WIDTH" value="7mm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/890324026014CS?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
