<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Film Capacitors - Interference Suppression - WCAP-FTXH&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-09-03&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-FTXH_P22.5L26.5W12.5H22">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=22.5X26.5X12.5X22mm</description>
</package>
<package name="WCAP-FTXH_P15L18W9.5H15.5">
<description>&lt;B&gt;WCAP-FTXH Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=15X18X9.5X15.5mm</description>
</package>
<package name="WCAP-FTXH_P37.5L41W26H37">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=37.5X41X26X37mm</description>
</package>
<package name="WCAP-FTXH_P10L13W8H16">
<description>&lt;B&gt;WCAP-FTXH Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=10X13X8X16mm</description>
</package>
<package name="WCAP-FTXH_P37.5L41W26H41">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=37.5X41X26X41mm</description>
</package>
<package name="WCAP-FTXH_P37.5L41W17H31">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=37.5X41X17X31mm</description>
</package>
<package name="WCAP-FTXH_P22.5L26.5W10H19">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=22.5X26.5X10X19mm</description>
</package>
<package name="WCAP-FTXH_P37.5L41W30H45">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=37.5X42X30X45mm</description>
</package>
<package name="WCAP-FTXH_P37.5L41W20H35">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=37.5X41X20X35mm</description>
</package>
<package name="WCAP-FTXH_P37.5L41W15H29">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=37.5X41X15X29mm</description>
</package>
<package name="WCAP-FTXH_P22.5L26.5W15.5H24.5">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=22.5X26.5X15.5X24.5mm</description>
</package>
<package name="WCAP-FTXH_P22.5L26.5W14.5H24.5">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=22.5X26.5X14.5X24.5mm</description>
</package>
<package name="WCAP-FTXH_P27.5L32W13H22">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=27.5X32X13X22mm</description>
</package>
<package name="WCAP-FTXH_P27.5L31W14H25">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=27.5X31X14X25mm</description>
</package>
<package name="WCAP-FTXH_P27.5L32W9H18">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=27.5X32X9X18mm</description>
</package>
<package name="WCAP-FTXH_P27.5L31W11H20">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=27.5X31X11X20mm</description>
</package>
<package name="WCAP-FTXH_P27.5L32W14H28">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=27.5X32X12X21mm</description>
</package>
<package name="WCAP-FTXH_P27.5L32W20H34">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=27.5X32X20X34mm</description>
</package>
<package name="WCAP-FTXH_P27.5L32W16H30">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=27.5X32X16X30mm</description>
</package>
<package name="WCAP-FTXH_P27.5L32W12H21">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=27.5X32X12X21mm</description>
</package>
<package name="WCAP-FTXH_P22.5L26W11H20">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=22.5X26X11X20mm</description>
</package>
<package name="WCAP-FTXH_P22.5L26.5W15H29.5">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=22.5X26.5X15X29.5mm</description>
</package>
<package name="WCAP-FTXH_P22.5L26.5W12H22">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=22.5X26.5X12X22mm</description>
</package>
<package name="WCAP-FTXH_P22.5L26.5W8.5H17">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=22.5X26.5X8.5X17mm</description>
</package>
<package name="WCAP-FTXH_P22.5L26W12.5H22">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=22.5X26X12.5X22mm</description>
</package>
<package name="WCAP-FTXH_P15L18W11.2H19.2">
<description>&lt;B&gt;WCAP-FTXH Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=15X18X11.2X19.2mm</description>
</package>
<package name="WCAP-FTXH_P15L18W10H18">
<description>&lt;B&gt;WCAP-FTXH Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=15X18X10X18mm</description>
</package>
<package name="WCAP-FTXH_P15L18W8.5H14.5">
<description>&lt;B&gt;WCAP-FTXH Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=15X18X8.5X14.5mm</description>
</package>
<package name="WCAP-FTXH_P15L18W7.5H13.5">
<description>&lt;B&gt;WCAP-FTXH Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=15X18X7.5X13.5mm</description>
</package>
<package name="WCAP-FTXH_P15L18W10H15.8">
<description>&lt;B&gt;WCAP-FTXH Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=15X18X10X15.8mm</description>
</package>
<package name="WCAP-FTXH_P15L18W11H18.5">
<description>&lt;B&gt;WCAP-FTXH Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=15X18X11X18.5mm</description>
</package>
<package name="WCAP-FTXH_P15L18W7H12.5">
<description>&lt;B&gt;WCAP-FTXH Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=15X18X7X12.5mm</description>
</package>
<package name="WCAP-FTXH_P15L18W12H20">
<description>&lt;B&gt;WCAP-FTXH Film Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;PitchXLXWXH=15X18X12X20mm</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-FTXH_P10" prefix="C">
<description>&lt;b&gt;WCAP-FTXH THB X2-Capacitors&lt;BR&gt;
THB X2-Capacitors (Temperature Humidity Bias)&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;For harsh enviromental conditions (THB: Temperature Humidity Bias)
&lt;BR&gt;THB Test: 1000 h @ 85°C @ 85% RH with rated voltage applied
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Dielectric: Polypropylene

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt; Mains Voltage Filter
&lt;BR&gt; Interference suppression

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o693349v209%20family-wcap-ftxh-27.5x31x20x34.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o693349v209%20family-wcap-ftxh-27.5x31x20x34.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
        
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-09-03
&lt;br&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L13W8H16" package="WCAP-FTXH_P10L13W8H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414023001CS">
<attribute name="C" value="100 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414023001CS?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890414023001CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXH_P37.5" prefix="C">
<description>&lt;b&gt;WCAP-FTXH THB X2-Capacitors&lt;BR&gt;
THB X2-Capacitors (Temperature Humidity Bias)&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;For harsh enviromental conditions (THB: Temperature Humidity Bias)
&lt;BR&gt;THB Test: 1000 h @ 85°C @ 85% RH with rated voltage applied
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Dielectric: Polypropylene

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt; Mains Voltage Filter
&lt;BR&gt; Interference suppression

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o693349v209%20family-wcap-ftxh-27.5x31x20x34.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o693349v209%20family-wcap-ftxh-27.5x31x20x34.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
        
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXH&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2024-05-17
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L41W17H31" package="WCAP-FTXH_P37.5L41W17H31">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414028001CS">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414028001CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="31mm"/>
<attribute name="LENGTH" value="41mm"/>
<attribute name="PART-NUMBER" value="890414028001CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="100V/us"/>
<attribute name="RISO" value="1.59 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="17mm"/>
</technology>
</technologies>
</device>
<device name="_L41W20H35" package="WCAP-FTXH_P37.5L41W20H35">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414028003CS">
<attribute name="C" value="6.8 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414028003CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="35mm"/>
<attribute name="LENGTH" value="41mm"/>
<attribute name="PART-NUMBER" value="890414028003CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="100V/us"/>
<attribute name="RISO" value="1.1 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="6.8 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="20mm"/>
</technology>
<technology name="_890414028006CS">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414028006CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="35mm"/>
<attribute name="LENGTH" value="41mm"/>
<attribute name="PART-NUMBER" value="890414028006CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="100V/us"/>
<attribute name="RISO" value="1.59 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="20mm"/>
</technology>
</technologies>
</device>
<device name="_L41W26H41" package="WCAP-FTXH_P37.5L41W26H41">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414028002CS">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414028002CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="41mm"/>
<attribute name="LENGTH" value="41mm"/>
<attribute name="PART-NUMBER" value="890414028002CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="100V/us"/>
<attribute name="RISO" value="750 Mohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="26mm"/>
</technology>
</technologies>
</device>
<device name="_L41W15H29" package="WCAP-FTXH_P37.5L41W15H29">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414028005CS">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414028005CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="29mm"/>
<attribute name="LENGTH" value="41mm"/>
<attribute name="PART-NUMBER" value="890414028005CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="100V/us"/>
<attribute name="RISO" value="2.27 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_L42W30H45" package="WCAP-FTXH_P37.5L41W30H45">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414028007CS">
<attribute name="C" value="10 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414028007CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="45mm"/>
<attribute name="LENGTH" value="42mm"/>
<attribute name="PART-NUMBER" value="890414028007CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="100V/us"/>
<attribute name="RISO" value="750 Mohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="30mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXH_P27.5" prefix="C">
<description>&lt;b&gt;WCAP-FTXH THB X2-Capacitors&lt;BR&gt;
THB X2-Capacitors (Temperature Humidity Bias)&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;For harsh enviromental conditions (THB: Temperature Humidity Bias)
&lt;BR&gt;THB Test: 1000 h @ 85°C @ 85% RH with rated voltage applied
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Dielectric: Polypropylene

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt; Mains Voltage Filter
&lt;BR&gt; Interference suppression

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o693349v209%20family-wcap-ftxh-27.5x31x20x34.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o693349v209%20family-wcap-ftxh-27.5x31x20x34.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
        
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-05-17
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L31W11H20" package="WCAP-FTXH_P27.5L31W11H20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414027005CS">
<attribute name="C" value="680 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027005CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890414027005CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="11.02 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
<technology name="_890414027006CS">
<attribute name="C" value="820 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027006CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890414027006CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="9.14 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="820 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
<technology name="_890414027007CS">
<attribute name="C" value="1 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027007CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890414027007CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="7.5 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
<technology name="_890414027008CS">
<attribute name="C" value="1.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027008CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890414027008CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="6.25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="1.2 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
</technologies>
</device>
<device name="_L31W14H25" package="WCAP-FTXH_P27.5L31W14H25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414027001CS">
<attribute name="C" value="2.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027001CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="25mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890414027001CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="3.4 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="14mm"/>
</technology>
</technologies>
</device>
<device name="_L32W13H22" package="WCAP-FTXH_P27.5L32W13H22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414027009CS">
<attribute name="C" value="1.5 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027009CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="22mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="PART-NUMBER" value="890414027009CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="5 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="1.5 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="13mm"/>
</technology>
<technology name="_890414027010CS">
<attribute name="C" value="1.8 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027010CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="22mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="PART-NUMBER" value="890414027010CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="4.16 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="1.8 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="13mm"/>
</technology>
<technology name="_890414027012CS">
<attribute name="C" value="1 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027012CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="22mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="PART-NUMBER" value="890414027012CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="7.5 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="13mm"/>
</technology>
</technologies>
</device>
<device name="_L32W16H30" package="WCAP-FTXH_P27.5L32W16H30">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414027002CS">
<attribute name="C" value="3.3 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027002CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="30mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="PART-NUMBER" value="890414027002CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="2.27 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
<technology name="_890414027011CS">
<attribute name="C" value="2.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027011CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="30mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="PART-NUMBER" value="890414027011CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="3.4 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
</technologies>
</device>
<device name="_L32W20H34" package="WCAP-FTXH_P27.5L32W20H34">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414027003CS">
<attribute name="C" value="4.7 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027003CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="34mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="PART-NUMBER" value="890414027003CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="1.59 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="20mm"/>
</technology>
</technologies>
</device>
<device name="_L32W9H18" package="WCAP-FTXH_P27.5L32W9H18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414027004CS">
<attribute name="C" value="560 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027004CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="18mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="PART-NUMBER" value="890414027004CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="13.39 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
<device name="_L32W12H21" package="WCAP-FTXH_P27.5L32W12H21">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414027013CS">
<attribute name="C" value="1.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027013CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="21mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="PART-NUMBER" value="890414027013CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="6.25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="1.2 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
</technologies>
</device>
<device name="_L32W14H28" package="WCAP-FTXH_P27.5L32W14H28">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414027014CS">
<attribute name="C" value="1.8 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414027014CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="28mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="PART-NUMBER" value="890414027014CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="4.16 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="1.8 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="14mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXH_P22.5" prefix="C">
<description>&lt;b&gt;WCAP-FTXH THB X2-Capacitors&lt;BR&gt;
THB X2-Capacitors (Temperature Humidity Bias)&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;For harsh enviromental conditions (THB: Temperature Humidity Bias)
&lt;BR&gt;THB Test: 1000 h @ 85°C @ 85% RH with rated voltage applied
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Dielectric: Polypropylene

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt; Mains Voltage Filter
&lt;BR&gt; Interference suppression

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o693349v209%20family-wcap-ftxh-27.5x31x20x34.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o693349v209%20family-wcap-ftxh-27.5x31x20x34.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
        
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXH&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2024-05-17
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L26.5W10H19" package="WCAP-FTXH_P22.5L26.5W10H19">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414026004CS">
<attribute name="C" value="560 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414026004CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="19mm"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="PART-NUMBER" value="890414026004CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="13.39 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_890414026005CS">
<attribute name="C" value="680 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414026005CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="19mm"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="PART-NUMBER" value="890414026005CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="11.02 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L26.5W15.5H24.5" package="WCAP-FTXH_P22.5L26.5W15.5H24.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414026010CS">
<attribute name="C" value="1.8 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414026010CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="24.5mm"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="PART-NUMBER" value="890414026010CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="4.16 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="1.8 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="15.5mm"/>
</technology>
</technologies>
</device>
<device name="_L26.5W14.5H24.5" package="WCAP-FTXH_P22.5L26.5W14.5H24.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414026009CS">
<attribute name="C" value="1.5 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414026009CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="24.5mm"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="PART-NUMBER" value="890414026009CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="5 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="1.5 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="14.5mm"/>
</technology>
</technologies>
</device>
<device name="_L26.5W15H29.5" package="WCAP-FTXH_P22.5L26.5W15H29.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414026011CS">
<attribute name="C" value="2.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414026011CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="29.5mm"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="PART-NUMBER" value="890414026011CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="3.4 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="15mm"/>
</technology>
<technology name="_890414026013CS">
<attribute name="C" value="1.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414026013CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="29.5mm"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="PART-NUMBER" value="890414026013CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="6.25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="1.2 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_L26.5W8.5H17" package="WCAP-FTXH_P22.5L26.5W8.5H17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414026001CS">
<attribute name="C" value="330 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414026001CS?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="PART-NUMBER" value="890414026001CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
<technology name="_890414026002CS">
<attribute name="C" value="390 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414026002CS?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="PART-NUMBER" value="890414026002CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="19.23 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="390 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
<technology name="_890414026003CS">
<attribute name="C" value="470 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414026003CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="PART-NUMBER" value="890414026003CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="15.95 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
<device name="_L26W11H20" package="WCAP-FTXH_P22.5L26W11H20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414026006CS">
<attribute name="C" value="820 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414026006CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890414026006CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="9.14 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="820 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
<technology name="_890414026007CS">
<attribute name="C" value="1 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414026007CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890414026007CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="7.5 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
</technologies>
</device>
<device name="_L26.5W12H22" package="WCAP-FTXH_P22.5L26.5W12H22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414026008CS">
<attribute name="C" value="1.2 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414026008CS?ae"/>
<attribute name="DF" value="0.3%"/>
<attribute name="HEIGHT" value="22mm"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="PART-NUMBER" value="890414026008CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="6.25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="1.2 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
</technologies>
</device>
<device name="_L26W12.5H22" package="WCAP-FTXH_P22.5L26W12.5H22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414026014CS">
<attribute name="C" value="1 µF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414026014CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="22mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890414026014CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="7.5 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="12.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXH_P15" prefix="C">
<description>&lt;b&gt;WCAP-FTXH THB X2-Capacitors&lt;BR&gt;
THB X2-Capacitors (Temperature Humidity Bias)&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression
&lt;BR&gt;For harsh enviromental conditions (THB: Temperature Humidity Bias)
&lt;BR&gt;THB Test: 1000 h @ 85°C @ 85% RH with rated voltage applied
&lt;BR&gt;Self-healing properties
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;BR&gt;Safety class: X2
&lt;BR&gt;Dielectric: Polypropylene

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications
&lt;BR&gt; Mains Voltage Filter
&lt;BR&gt; Interference suppression

&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o693349v209%20family-wcap-ftxh-27.5x31x20x34.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o693349v209%20family-wcap-ftxh-27.5x31x20x34.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
        
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-05-17
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L18W10H15.8" package="WCAP-FTXH_P15L18W10H15.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414025005CS">
<attribute name="C" value="390 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414025005CS?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="HEIGHT" value="15.8mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890414025005CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="19.23 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="390 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L18W11.2H19.2" package="WCAP-FTXH_P15L18W11.2H19.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414025010CS">
<attribute name="C" value="560 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414025010CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="19.2mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890414025010CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="13.39 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="11.2mm"/>
</technology>
</technologies>
</device>
<device name="_L18W7.5H13.5" package="WCAP-FTXH_P15L18W7.5H13.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414025001CS">
<attribute name="C" value="100 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414025001CS?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890414025001CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
<technology name="_890414025002CS">
<attribute name="C" value="150 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414025002CS?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890414025002CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
<technology name="_890414025008CS">
<attribute name="C" value="120 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414025008CS?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890414025008CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="120 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W7H12.5" package="WCAP-FTXH_P15L18W7H12.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414025007CS">
<attribute name="C" value="33 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414025007CS?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="HEIGHT" value="12.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890414025007CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="33 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L18W8.5H14.5" package="WCAP-FTXH_P15L18W8.5H14.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414025003CS">
<attribute name="C" value="220 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414025003CS?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890414025003CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
<technology name="_890414025009CS">
<attribute name="C" value="270 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414025009CS?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890414025009CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="270 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W10H18" package="WCAP-FTXH_P15L18W10H18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414025011CS">
<attribute name="C" value="330 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414025011CS?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="HEIGHT" value="18mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890414025011CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L18W11H18.5" package="WCAP-FTXH_P15L18W11H18.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414025013CS">
<attribute name="C" value="270 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414025013CS?ae"/>
<attribute name="DF" value="0.1%"/>
<attribute name="HEIGHT" value="18.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890414025013CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="25 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="270 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
</technologies>
</device>
<device name="_L18W12H20" package="WCAP-FTXH_P15L18W12H20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890414025012CS">
<attribute name="C" value="470 nF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890414025012CS?ae"/>
<attribute name="DF" value="0.2%"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890414025012CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="15.95 Gohm"/>
<attribute name="SAFETY-CLASS" value="X2"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="310VAC"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
