<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Film Capacitors - Interference Suppression - WCAP-FTXX&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-10-31&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-FTXX_P37.5L41.5W22.5H35.5_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 37.5mm, CS, THT
&lt;BR&gt;37.5X41.5X22.5X35.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P7.5L11W6H10_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 7.5mm, CS, THT
&lt;BR&gt;7.5X11X6X10(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P7.5L10W6H12_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 7.5mm, CS, THT
&lt;BR&gt;7.5X10X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P12.5L15W10H16_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, CS, THT
&lt;BR&gt;12.5X15X10X16(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P12.5L15W6H11.5_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, CS, THT
&lt;BR&gt;12.5X15X6X11.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P12.5L15W8.5H14_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, CS, THT
&lt;BR&gt;12.5X15X8.5X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P12.5L15W7H12.5_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, CS, THT
&lt;BR&gt;12.5X15X7X12.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W6H11.5">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X6X11.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W10H16">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X10X16(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W5H11">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W6H12">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W7.5H13.5">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X7.5X13.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P10L13W5H11">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W8H14">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X8X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W8.5H14.5">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X8.5X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W7.5H14.5">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X7.5X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W9H15">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X9X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P10L13W7H12">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X7X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P10L13W5H10">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X5X10(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W10H21_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X10X21(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P10L13W4.5H9.5">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X4.5X9.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P10L13W8H14">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X8X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W7.5H15_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X7.5X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P10L13W7H13">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X7X13(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W15H25_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X15X25(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W11H20_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X11X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W9H18_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X9X18(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W7.5H16.5_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X7.5X16.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W6H12_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W6H15_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X6X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W7H14.5_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, CS, THT
&lt;BR&gt;22.5X26X7X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P27.5L31W10.5H20">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, Standard, THT
&lt;BR&gt;27.5X31X10.5X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P37.5L41.5W22.5H35.5">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 37.5mm, Standard, THT
&lt;BR&gt;37.5X41.5X22.5X35.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W11H20">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X11X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P27.5L31W13H22">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, Standard, THT
&lt;BR&gt;27.5X31X13X22(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W10H21">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X10X21(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W6H15">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X6X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P27.5L31W15.5H29">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, Standard, THT
&lt;BR&gt;27.5X31X15.5X29(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P27.5L31W8H17">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, Standard, THT
&lt;BR&gt;27.5X31X8X17(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W15H25">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X15X25(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W7.5H16.5">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X7.5X16.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W9H18">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X9X18(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W7.5H15">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X7.5X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W6H12">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P22.5L26W7H14.5">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26X7X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P7.5L10W6H12">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 7.5mm, Standard, THT
&lt;BR&gt;7.5X10X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P27.5L31W10.5H20_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, CS, THT
&lt;BR&gt;27.5X31X10.5X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P7.5L11W6H10">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 7.5mm, Standard, THT
&lt;BR&gt;7.5X11X6X10(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P27.5L31W13H22_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, CS, THT
&lt;BR&gt;27.5X31X13X22(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P27.5L31W8H17_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, Standard, THT
&lt;BR&gt;27.5X31X8X17(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P12.5L15W6H11.5">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, Standard, THT
&lt;BR&gt;12.5X15X6X11.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P27.5L31W12.5W21_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, CS, THT
&lt;BR&gt;27.5X31X12.5X21(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P27.5L31W15.5H29_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, CS, THT
&lt;BR&gt;27.5X31X15.5X29(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P27.5L31W19H32.5_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, CS, THT
&lt;BR&gt;27.5X31X19X32.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P12.5L15W10H16">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, Standard, THT
&lt;BR&gt;12.5X15X10X16(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W7.5H13.5_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X7.5X13.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W10H16_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X10X16(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P12.5L15W8.5H14">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, Standard, THT
&lt;BR&gt;12.5X15X8.5X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P12.5L15W7H12.5">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 12.5mm, Standard, THT
&lt;BR&gt;12.5X15X7X12.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W6H12_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W5H11_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W8.5H14.5_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X8.5X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P10L13W4.5H9.5_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, CS, THT
&lt;BR&gt;10X13X4.5X9.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W7.5H14.5_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X7.5X14.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W9H15_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X9X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W8H14_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X8X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P10L13W5H10_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, CS, THT
&lt;BR&gt;10X13X5X10(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P10L13W5H11_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, CS, THT
&lt;BR&gt;10X13X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P15L18W6H11.5_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, CS, THT
&lt;BR&gt;15X18X6X11.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P10L13W7H12_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, CS, THT
&lt;BR&gt;10X13X7X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P10L13W7H13_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, CS, THT
&lt;BR&gt;10X13X7X13(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTXX_P10L13W8H14_CS">
<description>&lt;B&gt;WCAP-FTXX Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, CS, THT
&lt;BR&gt;10X13X8X14(PitchXLXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-FTXX_P37.5_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L41.5W22.5H35.5" package="WCAP-FTXX_P37.5L41.5W22.5H35.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334028008CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334028008CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="35.5mm"/>
<attribute name="LENGTH" value="41.5mm"/>
<attribute name="PART-NUMBER" value="890334028008CS"/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="110V/us"/>
<attribute name="RISO" value="1.47 GOhm"/>
<attribute name="VALUE" value="6.8 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="22.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX_P7.5_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L10W6H12" package="WCAP-FTXX_P7.5L10W6H12_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334022017CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334022017CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="PART-NUMBER" value="890334022017CS"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L11W6H10" package="WCAP-FTXX_P7.5L11W6H10_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334022007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334022007CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value="890334022007CS"/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX_P12.5_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L15W10H16" package="WCAP-FTXX_P12.5L15W10H16_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334024005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334024005CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value="890334024005CS"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="280V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L15W6H11.5" package="WCAP-FTXX_P12.5L15W6H11.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334024001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334024001CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value="890334024001CS"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="210V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L15W7H12.5" package="WCAP-FTXX_P12.5L15W7H12.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334024002CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334024002CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12.5mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value="890334024002CS"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="240V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L15W8.5H14" package="WCAP-FTXX_P12.5L15W8.5H14_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334024003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334024003CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value="890334024003CS"/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="260V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX_P15" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L18W10H16" package="WCAP-FTXX_P15L18W10H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025045">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025045?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025045 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L18W5H11" package="WCAP-FTXX_P15L18W5H11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025004?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025004 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="27 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334025006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025006?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025006 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="33 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334025007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025007?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025007 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="39 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334025009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025009?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025009 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334025011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025011?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025011 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="250V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="56 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W6H11.5" package="WCAP-FTXX_P15L18W6H11.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025027?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025027 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="180V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890334025027RP">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025027RP?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025027RP"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="180V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L18W6H12" package="WCAP-FTXX_P15L18W6H12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025013?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025013 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="270V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890334025015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025015?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025015 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="290V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="82 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890334025017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025017?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025017 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890334025022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025022?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025022 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="210V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890334025025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025025?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025025 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="180 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L18W7.5H13.5" package="WCAP-FTXX_P15L18W7.5H13.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025020?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025020 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="120 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W7.5H14.5" package="WCAP-FTXX_P15L18W7.5H14.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025031?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025031 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="250V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="270 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W8.5H14.5" package="WCAP-FTXX_P15L18W8.5H14.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025034">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025034?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025034 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="260V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W8H14" package="WCAP-FTXX_P15L18W8H14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025039?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025039 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
</technologies>
</device>
<device name="_L18W9H15" package="WCAP-FTXX_P15L18W9H15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025043">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025043?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value=" 890334025043 "/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="17.86 GOhm"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX_P10" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L13W4.5H9.5" package="WCAP-FTXX_P10L13W4.5H9.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334023008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023008?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023008 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
<technology name="_890334023011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023011?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023011 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
<technology name="_890334023015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023015?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023015 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
</technologies>
</device>
<device name="_L13W5H10" package="WCAP-FTXX_P10L13W5H10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334023002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023002?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023002 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="600V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="5.6 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334023003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023003?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023003 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="6.8 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334023004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023004?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023004 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="8.2 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334023017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023017?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023017 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="56 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L13W5H11" package="WCAP-FTXX_P10L13W5H11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334023006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023006?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023006 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334023007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023007?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023007 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="12 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334023010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023010?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023010 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="18 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L13W7H12" package="WCAP-FTXX_P10L13W7H12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334023025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023025?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023025 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L13W7H13" package="WCAP-FTXX_P10L13W7H13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334023019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023019?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023019 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_890334023021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023021?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023021 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="82 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_890334023023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023023?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023023 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_890334023024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023024?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023024 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="120 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L13W8H14" package="WCAP-FTXX_P10L13W8H14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334023028">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023028?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value=" 890334023028 "/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX_P22.5_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L26W10H21" package="WCAP-FTXX_P22.5L26W10H21_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026030CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026030CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="21mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890334026030CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="6.67 GOhm"/>
<attribute name="VALUE" value="1.5 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L26W11H20" package="WCAP-FTXX_P22.5L26W11H20_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026027CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026027CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890334026027CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="10.00 GOhm"/>
<attribute name="VALUE" value="1 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
</technologies>
</device>
<device name="_L26W15H25" package="WCAP-FTXX_P22.5L26W15H25_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026034CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026034CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="25mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890334026034CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="4.55 GOhm"/>
<attribute name="VALUE" value="2.2 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_L26W6H15" package="WCAP-FTXX_P22.5L26W6H15_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026003CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890334026003CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L26W7.5H15" package="WCAP-FTXX_P22.5L26W7.5H15_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026020CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026020CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890334026020CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L26W7.5H16.5" package="WCAP-FTXX_P22.5L26W7.5H16.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026018CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026018CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="16.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890334026018CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="17.86 GOhm"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L26W9H18" package="WCAP-FTXX_P22.5L26W9H18_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026024CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026024CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="18mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890334026024CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="12.20 GOhm"/>
<attribute name="VALUE" value="820 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
<device name="_L26W6H12" package="WCAP-FTXX_P22.5L26W6H12_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026007CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890334026007CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L26W7H14.5" package="WCAP-FTXX_P22.5L26W7H14.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026014CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026014CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value="890334026014CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX_P37.5" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L41.5W22.5H35.5" package="WCAP-FTXX_P37.5L41.5W22.5H35.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334028008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334028008?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="35.5mm"/>
<attribute name="LENGTH" value="41.5mm"/>
<attribute name="PART-NUMBER" value=" 890334028008 "/>
<attribute name="PITCH" value="37.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="110V/us"/>
<attribute name="RISO" value="1.47 GOhm"/>
<attribute name="VALUE" value="6.8 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="22.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX_P27.5" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L31W10.5H20" package="WCAP-FTXX_P27.5L31W10.5H20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334027006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334027006?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value=" 890334027006 "/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
</technologies>
</device>
<device name="_L31W13H22" package="WCAP-FTXX_P27.5L31W13H22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334027012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334027012?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="22mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value=" 890334027012 "/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="8.33 GOhm"/>
<attribute name="VALUE" value="1.2 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="13mm"/>
</technology>
</technologies>
</device>
<device name="_L31W15.5H29" package="WCAP-FTXX_P27.5L31W15.5H29">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334027025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334027025?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="29mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value=" 890334027025 "/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="3.03 GOhm"/>
<attribute name="VALUE" value="3.3 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="15.5mm"/>
</technology>
</technologies>
</device>
<device name="_L31W8H17" package="WCAP-FTXX_P27.5L31W8H17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334027009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334027009?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value=" 890334027009 "/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="100V/us"/>
<attribute name="RISO" value="10.00 GOhm"/>
<attribute name="VALUE" value="1 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX_P22.5" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L26W10H21" package="WCAP-FTXX_P22.5L26W10H21">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026030?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="21mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890334026030 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="6.67 GOhm"/>
<attribute name="VALUE" value="1.5 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L26W11H20" package="WCAP-FTXX_P22.5L26W11H20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026027?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890334026027 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="10.00 GOhm"/>
<attribute name="VALUE" value="1 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
</technologies>
</device>
<device name="_L26W15H25" package="WCAP-FTXX_P22.5L26W15H25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026034">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026034?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="25mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890334026034 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="4.55 GOhm"/>
<attribute name="VALUE" value="2.2 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_L26W6H15" package="WCAP-FTXX_P22.5L26W6H15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026003?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890334026003 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L26W7.5H15" package="WCAP-FTXX_P22.5L26W7.5H15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026020?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890334026020 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L26W7.5H16.5" package="WCAP-FTXX_P22.5L26W7.5H16.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026018?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="16.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890334026018 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="17.86 GOhm"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L26W9H18" package="WCAP-FTXX_P22.5L26W9H18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026024?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="18mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890334026024 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="160V/us"/>
<attribute name="RISO" value="12.20 GOhm"/>
<attribute name="VALUE" value="820 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
<device name="_L26W6H12" package="WCAP-FTXX_P22.5L26W6H12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026007?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890334026007 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="0.33 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L26W7H14.5" package="WCAP-FTXX_P22.5L26W7H14.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334026014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334026014?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="26mm"/>
<attribute name="PART-NUMBER" value=" 890334026014 "/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="150V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX_P7.5" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L10W6H12" package="WCAP-FTXX_P7.5L10W6H12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334022017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334022017?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="PART-NUMBER" value=" 890334022017 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L11W6H10" package="WCAP-FTXX_P7.5L11W6H10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334022007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334022007?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="PART-NUMBER" value=" 890334022007 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX_P27.5_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L31W10.5H20" package="WCAP-FTXX_P27.5L31W10.5H20_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334027006CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334027006CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890334027006CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="170V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
</technologies>
</device>
<device name="_L31W13H22" package="WCAP-FTXX_P27.5L31W13H22_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334027012CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334027012CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="22mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890334027012CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="8.33 GOhm"/>
<attribute name="VALUE" value="1.2 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="13mm"/>
</technology>
</technologies>
</device>
<device name="_L31W15.5H29" package="WCAP-FTXX_P27.5L31W15.5H29_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334027025CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334027025CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="29mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890334027025CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="3.03 GOhm"/>
<attribute name="VALUE" value="3.3 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="15.5mm"/>
</technology>
</technologies>
</device>
<device name="_L31W8H17" package="WCAP-FTXX_P27.5L31W8H17_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334027009CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334027009CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890334027009CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="100V/us"/>
<attribute name="RISO" value="10.00 GOhm"/>
<attribute name="VALUE" value="1 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
</technologies>
</device>
<device name="_L31W19H32.5" package="WCAP-FTXX_P27.5L31W19H32.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334027030CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334027030CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="32.5mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890334027030CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="2.13 GOhm"/>
<attribute name="VALUE" value="4.7 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="19mm"/>
</technology>
</technologies>
</device>
<device name="_L31W12.5H21" package="WCAP-FTXX_P27.5L31W12.5W21_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334027021CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334027021CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="21mm"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="PART-NUMBER" value="890334027021CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="110V/us"/>
<attribute name="RISO" value="4.55 GOhm"/>
<attribute name="VALUE" value="2.2 uF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="12.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX_P12.5" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L15W10H16" package="WCAP-FTXX_P12.5L15W10H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334024005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334024005?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value=" 890334024005 "/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="280V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L15W6H11.5" package="WCAP-FTXX_P12.5L15W6H11.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334024001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334024001?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value=" 890334024001 "/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="210V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L15W7H12.5" package="WCAP-FTXX_P12.5L15W7H12.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334024002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334024002?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12.5mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value=" 890334024002 "/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="240V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L15W8.5H14" package="WCAP-FTXX_P12.5L15W8.5H14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334024003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334024003?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="PART-NUMBER" value=" 890334024003 "/>
<attribute name="PITCH" value="12.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="260V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX_P15_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L18W10H16" package="WCAP-FTXX_P15L18W10H16_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025045CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025045CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025045CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="14.71 GOhm"/>
<attribute name="VALUE" value="680 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L18W5H11" package="WCAP-FTXX_P15L18W5H11_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025004CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025004CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="27 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334025006CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025006CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025006CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="33 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334025007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025007CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025007CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="39 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334025009CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025009CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025009CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334025011CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025011CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025011CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="250V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="56 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W6H11.5" package="WCAP-FTXX_P15L18W6H11.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025027CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025027CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025027CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="180V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L18W6H12" package="WCAP-FTXX_P15L18W6H12_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025013CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025013CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025013CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="270V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890334025015CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025015CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025015CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="290V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="82 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890334025017CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025017CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025017CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890334025022CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025022CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025022CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="210V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_890334025025CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025025CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025025CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="230V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="180 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L18W7.5H13.5" package="WCAP-FTXX_P15L18W7.5H13.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025020CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025020CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025020CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="120 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W7.5H14.5" package="WCAP-FTXX_P15L18W7.5H14.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025031CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025031CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025031CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="250V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="270 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W8.5H14.5" package="WCAP-FTXX_P15L18W8.5H14.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025034CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025034CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025034CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="260V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W8H14" package="WCAP-FTXX_P15L18W8H14_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025039CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025039CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025039CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="21.28 GOhm"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
</technologies>
</device>
<device name="_L18W9H15" package="WCAP-FTXX_P15L18W9H15_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334025043CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334025043CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="15mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890334025043CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="17.86 GOhm"/>
<attribute name="VALUE" value="560 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTXX_P10_CS" prefix="C">
<description>&lt;b&gt;WCAP-FTXX Film Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;X2-Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series for interference suppression 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Certificates: ENEC 10 by VDE, cULus, CQC 
&lt;BR&gt;Safety class: X2 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 5.6 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±10 % 
&lt;BR&gt;Voltage range (UR): 310 V(AC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 12.5 / 15.0 / 22.5 / 27.5 / 37.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Safety applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Interference suppression 
&lt;BR&gt;e.g. EMI filter for power supplies 
&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14734v209%20family-WCAP-FTXX-10x13x5x11.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;           
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTXX/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-FTXX&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-31&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L13W4.5H9.5" package="WCAP-FTXX_P10L13W4.5H9.5_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334023008CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023008CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023008CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
<technology name="_890334023011CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023011CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023011CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
<technology name="_890334023015CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023015CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="9.5mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023015CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="4.5mm"/>
</technology>
</technologies>
</device>
<device name="_L13W5H10" package="WCAP-FTXX_P10L13W5H10_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334023002CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023002CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023002CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="600V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="5.6 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334023003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023003CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023003CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="6.8 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334023004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023004CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023004CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="8.2 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334023017CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023017CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023017CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="56 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L13W5H11" package="WCAP-FTXX_P10L13W5H11_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334023006CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023006CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023006CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334023007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023007CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023007CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="12 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890334023010CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023010CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023010CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="18 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L13W7H12" package="WCAP-FTXX_P10L13W7H12_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334023025CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023025CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023025CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="150 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L13W7H13" package="WCAP-FTXX_P10L13W7H13_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334023019CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023019CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023019CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_890334023021CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023021CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023021CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="82 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_890334023023CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023023CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023023CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_890334023024CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023024CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023024CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="120 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L13W8H14" package="WCAP-FTXX_P10L13W8H14_CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890334023028CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890334023028CS?ae"/>
<attribute name="DF1" value=" 0.1%@1kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890334023028CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30 GOhm"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="310V(AC)"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
