<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Film Capacitors - Interference Suppression - WCAP-FTY2&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025b, 2025-10-16&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-FTY2_P27.5L32W17H28">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, Standard, THT
&lt;BR&gt;27.5X32X11X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTY2_P15L18W10H18">
<description>&lt;B&gt;WCAP-FTY2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X10X18(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTY2_P15L18W5H11">
<description>&lt;B&gt;WCAP-FTY2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTY2_P15L18W7H12.5">
<description>&lt;B&gt;WCAP-FTY2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X7X12.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTY2_P15L18W9.5H15.5">
<description>&lt;B&gt;WCAP-FTY2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 15mm, Standard, THT
&lt;BR&gt;15X18X9.5X15.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTY2_P22.5L26.5W8.5H17">
<description>&lt;B&gt;WCAP-FTY2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 22.5mm, Standard, THT
&lt;BR&gt;22.5X26.5X8.5X17(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTY2_P10L13W5H11">
<description>&lt;B&gt;WCAP-FTY2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTY2_P27.5L32W11H20">
<description>&lt;B&gt;WCAP-FTX2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 27.5mm, Standard, THT
&lt;BR&gt;27.5X32X11X20(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTY2_P10L13W4H9">
<description>&lt;B&gt;WCAP-FTY2 Film Capacitors

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Pitch 10mm, Standard, THT
&lt;BR&gt;10X13X4X9(PitchXLXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-FTY2_P15" prefix="C">
<description>&lt;b&gt;WCAP-FTY2 Film Capacitors&lt;br&gt;
&lt;/b&gt;Y2-/X1-Capacitors
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Product series for interference suppression
&lt;br&gt;Self-healing properties
&lt;br&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;br&gt;Safety class: Y2/X1
&lt;br&gt;Dielectric: Polypropylene
&lt;br&gt;Pitch: 10.0 / 15.0 / 22.5 / 27.5 mm

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Safety applications
&lt;br&gt;Main filter
&lt;br&gt;Interference suppression
&lt;br&gt;&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o843246v209%20multi-WCAP-FTY2-27.5x32x17x28-Iso.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o843246v209%20multi-WCAP-FTY2-27.5x32x17x28-Iso.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTY2_Y2_X1/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-FTY2_Y2_X1&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-04-24 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L18W10H18" package="WCAP-FTY2_P15L18W10H18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890404125011CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890404125011CS?ae"/>
<attribute name="DF" value="0.15%@1kHz"/>
<attribute name="HEIGHT" value="18mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890404125011CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="600V/us"/>
<attribute name="RISO" value="25 GO"/>
<attribute name="SAFETY-CLASS" value="Y2/X1"/>
<attribute name="VALUE" value="68 nF"/>
<attribute name="VR" value="300V(DC)"/>
<attribute name="VR2" value="330V(DC)"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_L18W5H11" package="WCAP-FTY2_P15L18W5H11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890404125004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890404125004CS?ae"/>
<attribute name="DF" value="0.15%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890404125004CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="600V/us"/>
<attribute name="RISO" value="25 GO"/>
<attribute name="SAFETY-CLASS" value="Y2/X1"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="300V(DC)"/>
<attribute name="VR2" value="330V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890404125005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890404125005CS?ae"/>
<attribute name="DF" value="0.15%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890404125005CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="600V/us"/>
<attribute name="RISO" value="25 GO"/>
<attribute name="SAFETY-CLASS" value="Y2/X1"/>
<attribute name="VALUE" value="15 nF"/>
<attribute name="VR" value="300V(DC)"/>
<attribute name="VR2" value="330V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_L18W7H12.5" package="WCAP-FTY2_P15L18W7H12.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890404125007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890404125007CS?ae"/>
<attribute name="DF" value="0.15%@1kHz"/>
<attribute name="HEIGHT" value="12.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890404125007CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="600V/us"/>
<attribute name="RISO" value="25 GO"/>
<attribute name="SAFETY-CLASS" value="Y2/X1"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="300V(DC)"/>
<attribute name="VR2" value="330V(DC)"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_L18W9.5H15.5" package="WCAP-FTY2_P15L18W9.5H15.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890404125010CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890404125010CS?ae"/>
<attribute name="DF" value="0.15%@1kHz"/>
<attribute name="HEIGHT" value="15.5mm"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="PART-NUMBER" value="890404125010CS"/>
<attribute name="PITCH" value="15mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="600V/us"/>
<attribute name="RISO" value="25 GO"/>
<attribute name="SAFETY-CLASS" value="Y2/X1"/>
<attribute name="VALUE" value="47 nF"/>
<attribute name="VR" value="300V(DC)"/>
<attribute name="VR2" value="330V(DC)"/>
<attribute name="WIDTH" value="9.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTY2_P22.5" prefix="C">
<description>&lt;b&gt;WCAP-FTY2 Film Capacitors&lt;br&gt;
&lt;/b&gt;Y2-/X1-Capacitors
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Product series for interference suppression
&lt;br&gt;Self-healing properties
&lt;br&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;br&gt;Safety class: Y2/X1
&lt;br&gt;Dielectric: Polypropylene
&lt;br&gt;Pitch: 10.0 / 15.0 / 22.5 / 27.5 mm

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Safety applications
&lt;br&gt;Main filter
&lt;br&gt;Interference suppression
&lt;br&gt;&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o843246v209%20multi-WCAP-FTY2-27.5x32x17x28-Iso.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o843246v209%20multi-WCAP-FTY2-27.5x32x17x28-Iso.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTY2_Y2_X1/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-FTY2_Y2_X1&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-04-24 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L26.5W8.5H17" package="WCAP-FTY2_P22.5L26.5W8.5H17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890404126003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890404126003CS?ae"/>
<attribute name="DF" value="0.15%@1kHz"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="PART-NUMBER" value="890404126003CS"/>
<attribute name="PITCH" value="22.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="500V/us"/>
<attribute name="RISO" value="25 GO"/>
<attribute name="SAFETY-CLASS" value="Y2/X1"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="300V(DC)"/>
<attribute name="VR2" value="330V(DC)"/>
<attribute name="WIDTH" value="8.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTY2_P27.5" prefix="C">
<description>&lt;b&gt;WCAP-FTY2 Film Capacitors&lt;br&gt;
&lt;/b&gt;Y2-/X1-Capacitors
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Product series for interference suppression
&lt;br&gt;Self-healing properties
&lt;br&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;br&gt;Safety class: Y2/X1
&lt;br&gt;Dielectric: Polypropylene
&lt;br&gt;Pitch: 10.0 / 15.0 / 22.5 / 27.5 mm

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Safety applications
&lt;br&gt;Main filter
&lt;br&gt;Interference suppression
&lt;br&gt;&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o843246v209%20multi-WCAP-FTY2-27.5x32x17x28-Iso.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o843246v209%20multi-WCAP-FTY2-27.5x32x17x28-Iso.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTY2_Y2_X1/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-FTY2_Y2_X1&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-04-24 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L32W11H20" package="WCAP-FTY2_P27.5L32W11H20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890404127002CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890404127002CS?ae"/>
<attribute name="DF" value="0.15%@1kHz"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="PART-NUMBER" value="890404127002CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="25 GO"/>
<attribute name="SAFETY-CLASS" value="Y2/X1"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="300V(DC)"/>
<attribute name="VR2" value="330V(DC)"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
</technologies>
</device>
<device name="_L32W17H28" package="WCAP-FTY2_P27.5L32W17H28">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890404127006CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890404127006CS?ae"/>
<attribute name="DF" value="0.15%@1kHz"/>
<attribute name="HEIGHT" value="28mm"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="PART-NUMBER" value="890404127006CS"/>
<attribute name="PITCH" value="27.5mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="400V/us"/>
<attribute name="RISO" value="15.95 GO"/>
<attribute name="SAFETY-CLASS" value="Y2/X1"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="300V(DC)"/>
<attribute name="VR2" value="330V(DC)"/>
<attribute name="WIDTH" value="17mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTY2_P10" prefix="C">
<description>&lt;b&gt;WCAP-FTY2 Film Capacitors&lt;br&gt;
&lt;/b&gt;Y2-/X1-Capacitors
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Product series for interference suppression
&lt;br&gt;Self-healing properties
&lt;br&gt;Certificates: ENEC 10 by VDE, cULus, CQC
&lt;br&gt;Safety class: Y2/X1
&lt;br&gt;Dielectric: Polypropylene
&lt;br&gt;Pitch: 10.0 / 15.0 / 22.5 / 27.5 mm

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Safety applications
&lt;br&gt;Main filter
&lt;br&gt;Interference suppression
&lt;br&gt;&lt;br&gt;

&lt;a href="https://www.we-online.com/components/media/o843246v209%20multi-WCAP-FTY2-27.5x32x17x28-Iso.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o843246v209%20multi-WCAP-FTY2-27.5x32x17x28-Iso.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WCAP-FTY2_Y2_X1/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-FTY2_Y2_X1&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-10-16 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_L13W4H9" package="WCAP-FTY2_P10L13W4H9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890404123001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890404123001CS?ae"/>
<attribute name="DF" value="0.15%@1kHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890404123001CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="800V/us"/>
<attribute name="RISO" value="25 GO"/>
<attribute name="SAFETY-CLASS" value="Y2/X1"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="300V(DC)"/>
<attribute name="VR2" value="330V(DC)"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_890404123003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890404123003CS?ae"/>
<attribute name="DF" value="0.15%@1kHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890404123003CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="800V/us"/>
<attribute name="RISO" value="25 GO"/>
<attribute name="SAFETY-CLASS" value="Y2/X1"/>
<attribute name="VALUE" value="2 nF"/>
<attribute name="VR" value="300V(DC)"/>
<attribute name="VR2" value="330V(DC)"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
</technologies>
</device>
<device name="_L13W5H11" package="WCAP-FTY2_P10L13W5H11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890404123005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890404123005CS?ae"/>
<attribute name="DF" value="0.15%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890404123005CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="800V/us"/>
<attribute name="RISO" value="25 GO"/>
<attribute name="SAFETY-CLASS" value="Y2/X1"/>
<attribute name="VALUE" value="3.3 nF"/>
<attribute name="VR" value="300V(DC)"/>
<attribute name="VR2" value="330V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_890404123007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/890404123007CS?ae"/>
<attribute name="DF" value="0.15%@1kHz"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="PART-NUMBER" value="890404123007CS"/>
<attribute name="PITCH" value="10mm"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="800V/us"/>
<attribute name="RISO" value="25 GO"/>
<attribute name="SAFETY-CLASS" value=""/>
<attribute name="VALUE" value="4.7 nF"/>
<attribute name="VR" value="300V(DC)"/>
<attribute name="VR2" value="330V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
