<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Aluminium Hybrid Polymer Capacitors - WCAP-HTG5&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-04-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-HTG5_D10H12.5">
<description>&lt;b&gt;WCAP-HTG5 Polymer Electrolytic Capacitor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Diameter X Length X Pitch X Pin Diameter = 10mmX12.5mmX5mmX0.8mm
&lt;br&gt;THT, 2pins</description>
</package>
<package name="WCAP-HTG5_D10H10">
<description>&lt;b&gt;WCAP-HTG5 Polymer Electrolytic Capacitor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Diameter X Length X Pitch X Pin Diameter = 10mmX10mmX5mmX0.6mm
&lt;br&gt;THT, 2pins</description>
</package>
<package name="WCAP-HTG5_D6.3H8">
<description>&lt;b&gt;WCAP-HTG5 Polymer Electrolytic Capacitor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Diameter X Length X Pitch X Pin Diameter = 6.3mmX8mmX2.5mmX0.6mm
&lt;br&gt;THT, 2pins</description>
</package>
<package name="WCAP-HTG5_D8H11.5">
<description>&lt;b&gt;WCAP-HTG5 Polymer Electrolytic Capacitor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Diameter X Length X Pitch X Pin Diameter = 8mmX11.5mmX3.5mmX0.6mm
&lt;br&gt;THT, 2pins</description>
</package>
<package name="WCAP-HTG5_D8H9">
<description>&lt;b&gt;WCAP-HTG5 Polymer Electrolytic Capacitor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Diameter X Length X Pitch X Pin Diameter = 8mmX9mmX3.5mmX0.6mm
&lt;br&gt;THT, 2pins</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-HTG5_D10H12.5" prefix="C">
<description>&lt;b&gt;WCAP-HTG5 General Purpose 105°C&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series
&lt;BR&gt;Low ESR
&lt;BR&gt;High ripple current characteristics
&lt;BR&gt;High stability over the temperature range
&lt;BR&gt;Low leakage current
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Industry and telecommunication
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. Servo inverter, air conditioner, industrial power supply, security camera, base station
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o696155v209%20multi-WCAP-HTG5-870575373001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o696155v209%20multi-WCAP-HTG5-870575373001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-HTG5"&gt;www.we-online.com/en/components/products/WCAP-HTG5&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-26&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-HTG5_D10H12.5">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_870575575005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575575005?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="2900mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value=" 870575575005 "/>
<attribute name="RESR" value="16mohm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_870575875006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575875006?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="35.3uA"/>
<attribute name="I-RIPPLE" value="2400mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value=" 870575875006 "/>
<attribute name="RESR" value="22mohm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_870575975005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575975005?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="15uA"/>
<attribute name="I-RIPPLE" value="1660mA"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="PART-NUMBER" value=" 870575975005 "/>
<attribute name="RESR" value="60mohm"/>
<attribute name="VALUE" value="15 µF"/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-HTG5_D8H9" prefix="C">
<description>&lt;b&gt;WCAP-HTG5 General Purpose 105°C&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series
&lt;BR&gt;Low ESR
&lt;BR&gt;High ripple current characteristics
&lt;BR&gt;High stability over the temperature range
&lt;BR&gt;Low leakage current
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Industry and telecommunication
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. Servo inverter, air conditioner, industrial power supply, security camera, base station
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o696155v209%20multi-WCAP-HTG5-870575373001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o696155v209%20multi-WCAP-HTG5-870575373001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-HTG5"&gt;www.we-online.com/en/components/products/WCAP-HTG5&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-05-05&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-HTG5_D8H9">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_870575374002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575374002?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="43.2uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="PART-NUMBER" value=" 870575374002 "/>
<attribute name="RESR" value="26mohm"/>
<attribute name="VALUE" value="270 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870575574002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575574002?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="37.5uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="PART-NUMBER" value=" 870575574002 "/>
<attribute name="RESR" value="27mohm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_870575774002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575774002?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="1670mA"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="PART-NUMBER" value=" 870575774002 "/>
<attribute name="RESR" value="35mohm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_870575874002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575874002?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="13.9uA"/>
<attribute name="I-RIPPLE" value="1560mA"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="PART-NUMBER" value=" 870575874002 "/>
<attribute name="RESR" value="40mohm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-HTG5_D8H11.5" prefix="C">
<description>&lt;b&gt;WCAP-HTG5 General Purpose 105°C&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series
&lt;BR&gt;Low ESR
&lt;BR&gt;High ripple current characteristics
&lt;BR&gt;High stability over the temperature range
&lt;BR&gt;Low leakage current
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Industry and telecommunication
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. Servo inverter, air conditioner, industrial power supply, security camera, base station
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o696155v209%20multi-WCAP-HTG5-870575373001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o696155v209%20multi-WCAP-HTG5-870575373001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-HTG5"&gt;www.we-online.com/en/components/products/WCAP-HTG5&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-26&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-HTG5_D8H11.5">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_870575374003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575374003?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="2350mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 870575374003 "/>
<attribute name="RESR" value="23mohm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870575574003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575574003?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="2250mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 870575574003 "/>
<attribute name="RESR" value="24mohm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_870575774003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575774003?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="PART-NUMBER" value=" 870575774003 "/>
<attribute name="RESR" value="30mohm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-HTG5_D10H10" prefix="C">
<description>&lt;b&gt;WCAP-HTG5 General Purpose 105°C&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series
&lt;BR&gt;Low ESR
&lt;BR&gt;High ripple current characteristics
&lt;BR&gt;High stability over the temperature range
&lt;BR&gt;Low leakage current
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Industry and telecommunication
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. Servo inverter, air conditioner, industrial power supply, security camera, base station
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o696155v209%20multi-WCAP-HTG5-870575373001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o696155v209%20multi-WCAP-HTG5-870575373001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-HTG5"&gt;www.we-online.com/en/components/products/WCAP-HTG5&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-26&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-HTG5_D10H10">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_870575375004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575375004?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="2600mA"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="PART-NUMBER" value=" 870575375004 "/>
<attribute name="RESR" value="21mohm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870575875004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575875004?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="20.8uA"/>
<attribute name="I-RIPPLE" value="2100mA"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="PART-NUMBER" value=" 870575875004 "/>
<attribute name="RESR" value="30mohm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_870575875005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575875005?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="10000h"/>
<attribute name="I-LEAK" value="29.6uA"/>
<attribute name="I-RIPPLE" value="2100mA"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="PART-NUMBER" value=" 870575875005 "/>
<attribute name="RESR" value="30mohm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-HTG5_D6.3H8" prefix="C">
<description>&lt;b&gt;WCAP-HTG5 General Purpose 105°C&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series
&lt;BR&gt;Low ESR
&lt;BR&gt;High ripple current characteristics
&lt;BR&gt;High stability over the temperature range
&lt;BR&gt;Low leakage current
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Industry and telecommunication
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. Servo inverter, air conditioner, industrial power supply, security camera, base station
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o696155v209%20multi-WCAP-HTG5-870575373001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o696155v209%20multi-WCAP-HTG5-870575373001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-HTG5"&gt;www.we-online.com/en/components/products/WCAP-HTG5&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-26&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-HTG5_D6.3H8">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_870575373001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575373001?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="19.2uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="LENGTH" value="8mm"/>
<attribute name="PART-NUMBER" value=" 870575373001 "/>
<attribute name="RESR" value="40mohm"/>
<attribute name="VALUE" value="120 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870575573001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575573001?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="17uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="LENGTH" value="8mm"/>
<attribute name="PART-NUMBER" value=" 870575573001 "/>
<attribute name="RESR" value="45mohm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_870575773001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575773001?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="7.5uA"/>
<attribute name="I-RIPPLE" value="1200mA"/>
<attribute name="LENGTH" value="8mm"/>
<attribute name="PART-NUMBER" value=" 870575773001 "/>
<attribute name="RESR" value="80mohm"/>
<attribute name="VALUE" value="15 µF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_870575873001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/870575873001?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="6.3uA"/>
<attribute name="I-RIPPLE" value="1060mA"/>
<attribute name="LENGTH" value="8mm"/>
<attribute name="PART-NUMBER" value=" 870575873001 "/>
<attribute name="RESR" value="100mohm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
