<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminium Polymer Capacitors - WCAP-PHSE&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-05-25&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-PHSE_7.3X4.3X1.9(LXWXH)">
<description>&lt;B&gt;WCAP-PHSE Aluminum Polymer Capacitors
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;7.3X4.3X1.9(LXWXH), SMT, 2pins</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-PHSE_7.3X4.3X1.9" prefix="C">
<description>&lt;b&gt;WCAP-PHSE Aluminum Polymer Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Super low ESR &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Super low ESR product series 
&lt;BR&gt;High ripple current capability 
&lt;BR&gt;Low profile 
&lt;BR&gt;Mounting style: H-Chip SMT 
&lt;BR&gt;Capacitance range: 330 µF ‒ 560 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 2 ‒ 2.5 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (LxWxH) in mm: 7.3 x 4.3 x 1.9 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Noise suppression 
&lt;BR&gt;Input and output capacitor for DC/DC converter 
&lt;BR&gt;USB Charger, Smart Meter, Power 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135450v209%20Family_WCAP-PH_xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135450v209%20Family_WCAP-PH_xx.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PHSE/"&gt;https://www.we-online.com/catalog/en/WCAP-PHSE/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu, 2021-05-25
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PHSE_7.3X4.3X1.9(LXWXH)">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_875046219001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875046219001.pdf"/>
<attribute name="DF" value="6%"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="HEIGHT" value="1.9mm"/>
<attribute name="I-LEAK" value="66uA"/>
<attribute name="I-RIPPLE" value="10200mA"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875046219001 "/>
<attribute name="RESR" value="3mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSE2917331M002DH3T2HT19"/>
<attribute name="VALUE" value="330uF"/>
<attribute name="VR" value="2V(DC)"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_875046219002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875046219002.pdf"/>
<attribute name="DF" value="6%"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="HEIGHT" value="1.9mm"/>
<attribute name="I-LEAK" value="94uA"/>
<attribute name="I-RIPPLE" value="10200mA"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875046219002 "/>
<attribute name="RESR" value="3mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSE2917471M002DH3T2HT19"/>
<attribute name="VALUE" value="470uF"/>
<attribute name="VR" value="2V(DC)"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_875046219003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875046219003.pdf"/>
<attribute name="DF" value="6%"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="HEIGHT" value="1.9mm"/>
<attribute name="I-LEAK" value="112uA"/>
<attribute name="I-RIPPLE" value="10200mA"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875046219003 "/>
<attribute name="RESR" value="3mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSE2917561M002DH3T2HT19"/>
<attribute name="VALUE" value="560uF"/>
<attribute name="VR" value="2V(DC)"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_875046319001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875046319001.pdf"/>
<attribute name="DF" value="6%"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="HEIGHT" value="1.9mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="10200mA"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875046319001 "/>
<attribute name="RESR" value="3mohm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSE2917471M2R5DH3T2HT19"/>
<attribute name="VALUE" value="470uF"/>
<attribute name="VR" value="2.5V(DC)"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
