<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminium Polymer Capacitors - WCAP-PSHP&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-06&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-PSHP_8X8.7(DXL)">
<description>&lt;B&gt;WCAP-PSHP&lt;/B&gt;&lt;BR&gt; Aluminum Polymer Capacitors ,8x8.7x3.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-PSHP_10X10.5(DXL)">
<description>&lt;B&gt;WCAP-PSHP&lt;/B&gt;&lt;BR&gt; Aluminum Polymer Capacitors ,10x10.5x4.5(DiameterXLengthXP)</description>
</package>
<package name="WCAP-PSHP_6.3X5.8(DXL)">
<description>&lt;B&gt;WCAP-PSHP&lt;/B&gt;&lt;BR&gt;Aluminum Polymer Capacitors ,6.3x5.8x2.2(DiameterXLengthXP)</description>
</package>
<package name="WCAP-PSHP_8X11.7(DXL)">
<description>&lt;B&gt;WCAP-PSHP&lt;/B&gt;&lt;BR&gt; Aluminum Polymer Capacitors ,8x11.7x3.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-PSHP_6.3X7.7(DXL)">
<description>&lt;B&gt;WCAP-PSHP&lt;/B&gt;&lt;BR&gt;Aluminum Polymer Capacitors ,6.3X7.7X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-PSHP_8X7.7(DXL)">
<description>&lt;B&gt;WCAP-PSHP&lt;/B&gt;&lt;BR&gt; Aluminum Polymer Capacitors ,8x7.7x3.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-PSHP_10X8.7(DXL)">
<description>&lt;B&gt;WCAP-PSHP&lt;/B&gt;&lt;BR&gt; Aluminum Polymer Capacitors ,10x8.7x4.5(DiameterXLengthXP)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-PSHP_8X8.7" prefix="C">
<description>&lt;b&gt;WCAP-PSHP Aluminum Polymer Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Ripple Current&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with ultra high permissible ripple current 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 1200 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 5.8 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;LLow ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PSHP/"&gt;https://www.we-online.com/catalog/en/WCAP-PSHP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-06
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSHP_8X8.7(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875115152006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115152006.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="705.6uA"/>
<attribute name="I-RIPPLE" value="4800mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115152006 "/>
<attribute name="RESR" value="11mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087561M6R3DVCTEB000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875115152007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115152007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="856uA"/>
<attribute name="I-RIPPLE" value="4800mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115152007 "/>
<attribute name="RESR" value="11mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087681M6R3DVCTEB000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875115252003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115252003.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="940uA"/>
<attribute name="I-RIPPLE" value="4800mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115252003 "/>
<attribute name="RESR" value="11mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087471M010DVCTEB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875115352003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115352003.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="432uA"/>
<attribute name="I-RIPPLE" value="4800mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115352003 "/>
<attribute name="RESR" value="11mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087271M016DVCTEB000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875115452001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115452001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="272uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115452001 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087680M020DVCTEB000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875115452002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115452002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="328uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115452002 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087820M020DVCTEB000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875115452003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115452003.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="400uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115452003 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087101M020DVCTEB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875115452004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115452004.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115452004 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087151M020DVCTEB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875115552001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115552001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="340uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115552001 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087680M025DVCTEB000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875115552002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115552002.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="410uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115552002 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087820M025DVCTEB000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875115652006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115652006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="574uA"/>
<attribute name="I-RIPPLE" value="2600mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115652006 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087820M035DVCTEB000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875115652007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115652007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="700uA"/>
<attribute name="I-RIPPLE" value="3000mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115652007 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087101M035DVCTEB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875115652014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115652014.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115652014 "/>
<attribute name="RESR" value="40mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087390M035DVCTEE000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875115752001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115752001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115752001 "/>
<attribute name="RESR" value="45mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087100M050DVCTEB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875115852001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115852001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="126uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115852001 "/>
<attribute name="RESR" value="45mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087100M063DVCTEB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_875115952001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115952001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="136uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115952001 "/>
<attribute name="RESR" value="48mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE0876R8M100DVCTEB000"/>
<attribute name="VALUE" value="6.8  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_875116152001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875116152001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875116152001 "/>
<attribute name="RESR" value="45mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE087100M080DVCTEB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSHP_10X10.5" prefix="C">
<description>&lt;b&gt;WCAP-PSHP Aluminum Polymer Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Ripple Current&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with ultra high permissible ripple current 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 1200 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 5.8 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;LLow ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PSHP/"&gt;https://www.we-online.com/catalog/en/WCAP-PSHP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-06
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSHP_10X10.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875115157010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115157010.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1260uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115157010 "/>
<attribute name="RESR" value="11mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF105122M6R3DVCTEB000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875115257007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115257007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1640uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115257007 "/>
<attribute name="RESR" value="11mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF105821M010DVCTEB000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875115357006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115357006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="752uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115357006 "/>
<attribute name="RESR" value="11mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF105471M016DVCTEB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875115457008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115457008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1080uA"/>
<attribute name="I-RIPPLE" value="3700mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115457008 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF105271M020DVCTEB000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875115557005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115557005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="750uA"/>
<attribute name="I-RIPPLE" value="3700mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115557005 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF105151M025DVCTEB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875115657008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115657008.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="840uA"/>
<attribute name="I-RIPPLE" value="3200mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115657008 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF105121M035DVCTEB000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875115657016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115657016.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2500mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115657016 "/>
<attribute name="RESR" value="32mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF105680M035DVCTEE000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875115957002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115957002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="240uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115957002 "/>
<attribute name="RESR" value="45mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF105120M100DVCTEB000"/>
<attribute name="VALUE" value="12  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_875116157002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875116157002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="240uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875116157002 "/>
<attribute name="RESR" value="40mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF105150M080DVCTEB000"/>
<attribute name="VALUE" value="15  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSHP_6.3X5.8" prefix="C">
<description>&lt;b&gt;WCAP-PSHP Aluminum Polymer Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Ripple Current&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with ultra high permissible ripple current 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 1200 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 5.8 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;LLow ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PSHP/"&gt;https://www.we-online.com/catalog/en/WCAP-PSHP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-06
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSHP_6.3X5.8(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875115644009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115644009.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="980mA"/>
<attribute name="L" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115644009 "/>
<attribute name="RESR" value="75mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSED058100M035DVCTBE000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSHP_8X11.7" prefix="C">
<description>&lt;b&gt;WCAP-PSHP Aluminum Polymer Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Ripple Current&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with ultra high permissible ripple current 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 1200 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 5.8 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;LLow ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PSHP/"&gt;https://www.we-online.com/catalog/en/WCAP-PSHP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-06
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSHP_8X11.7(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875115655003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115655003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="700uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115655003 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117101M035DVCTFE000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875115655011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115655011.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2300mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115655011 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117220M035DVCTFE000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875115655013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115655013.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2300mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115655013 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117330M035DVCTFE000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875115655015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115655015.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2300mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115655015 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117560M035DVCTFE000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSHP_6.3X7.7" prefix="C">
<description>&lt;b&gt;WCAP-PSHP Aluminum Polymer Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Ripple Current&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with ultra high permissible ripple current 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 1200 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 5.8 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;LLow ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PSHP/"&gt;https://www.we-online.com/catalog/en/WCAP-PSHP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-06
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSHP_6.3X7.7(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875115645010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115645010.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115645010 "/>
<attribute name="RESR" value="60mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSED077180M035DVCTCE000"/>
<attribute name="VALUE" value="18  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875115645012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115645012.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115645012 "/>
<attribute name="RESR" value="60mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSED077270M035DVCTCE000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSHP_8X7.7" prefix="C">
<description>&lt;b&gt;WCAP-PSHP Aluminum Polymer Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Ripple Current&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with ultra high permissible ripple current 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 1200 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 5.8 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;LLow ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PSHP/"&gt;https://www.we-online.com/catalog/en/WCAP-PSHP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-06
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSHP_8X7.7(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875115150001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115150001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="277.2uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115150001 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE077221M6R3DVCTDB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875115150002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115150002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="340.2uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115150002 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE077271M6R3DVCTDB000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875115150003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115150003.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="415.8uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115150003 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE077331M6R3DVCTDB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875115150004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115150004.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="491uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115150004 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE077391M6R3DVCTDB000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875115150005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115150005.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="592uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115150005 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE077471M6R3DVCTDB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875115250001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115250001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="660uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115250001 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE077331M010DVCTDB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875115250002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115250002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="780uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115250002 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE077391M010DVCTDB000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875115350001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115350001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="288uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115350001 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE077181M016DVCTDB000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875115350002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115350002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="352uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115350002 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE077221M016DVCTDB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875115650005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115650005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="392uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115650005 "/>
<attribute name="RESR" value="40mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE077560M035DVCTDB000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSHP_10X8.7" prefix="C">
<description>&lt;b&gt;WCAP-PSHP Aluminum Polymer Capacitors   &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;High Ripple Current&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with ultra high permissible ripple current 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 6.8 µF ‒ 1200 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 5.8 up to 10.0 x 10.5 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;LLow ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14735v209%20Family_WCAP-PSHP.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PSHP/"&gt;https://www.we-online.com/catalog/en/WCAP-PSHP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-06
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSHP_10X8.7(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875115160008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115160008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1033.2uA"/>
<attribute name="I-RIPPLE" value="3700mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115160008 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF087821M6R3DVCTEB000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875115160009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115160009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1260uA"/>
<attribute name="I-RIPPLE" value="3700mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115160009 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF087102M6R3DVCTEB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875115260004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115260004.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="940uA"/>
<attribute name="I-RIPPLE" value="3700mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115260004 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF087471M010DVCTEB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875115260005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115260005.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1120uA"/>
<attribute name="I-RIPPLE" value="3700mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115260005 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF087561M010DVCTEB000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875115260006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115260006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1360uA"/>
<attribute name="I-RIPPLE" value="3700mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115260006 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF087681M010DVCTEB000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875115360004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115360004.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="3700mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115360004 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF087331M016DVCTEB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875115360005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115360005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="624uA"/>
<attribute name="I-RIPPLE" value="3700mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115360005 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF087391M016DVCTEB000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875115460005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115460005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="3100mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115460005 "/>
<attribute name="RESR" value="25mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF087151M020DVCTEB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875115460006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115460006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="720uA"/>
<attribute name="I-RIPPLE" value="3100mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115460006 "/>
<attribute name="RESR" value="25mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF087181M020DVCTEB000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875115460007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115460007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="880uA"/>
<attribute name="I-RIPPLE" value="3100mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115460007 "/>
<attribute name="RESR" value="25mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF087221M020DVCTEB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875115560003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115560003.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="410uA"/>
<attribute name="I-RIPPLE" value="3100mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115560003 "/>
<attribute name="RESR" value="25mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF087820M025DVCTEB000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875115560004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875115560004.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="500uA"/>
<attribute name="I-RIPPLE" value="3100mA"/>
<attribute name="L" value="8.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875115560004 "/>
<attribute name="RESR" value="25mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF087101M025DVCTEB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
