<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminium Polymer Capacitors - WCAP-PSLC&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020b, 2020-08-14&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-PSLC_10X12.4(DXL)">
<description>&lt;B&gt;WCAP-PSLC&lt;/B&gt;&lt;BR&gt; Aluminum Polymer Capacitors ,10x12.4x4.5(DiameterXLengthXP)</description>
</package>
<package name="WCAP-PSLC_8X11.7(DXL)">
<description>&lt;B&gt;WCAP-PSLC&lt;/B&gt;&lt;BR&gt; Aluminum Polymer Capacitors ,8x11.7x3.1(DiameterXLengthXP)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-PSLC_10X12.4" prefix="C">
<description>&lt;b&gt;WCAP-PSLC Aluminum Polymer Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Large Capacitance  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Large capacitance product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 10 µF ‒ 2000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 8.0 x 11.7 up to 10.0 x 12.4 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14736v209%20Family_WCAP-PSLC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14736v209%20Family_WCAP-PSLC.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PSLC/"&gt;https://www.we-online.com/catalog/en/WCAP-PSLC/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu;2020-08-14
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSLC_10X12.4(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875075161011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075161011.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1512uA"/>
<attribute name="I-RIPPLE" value="5500mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075161011 "/>
<attribute name="RESR" value="8mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124122M6R3DVCTFB000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875075161012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075161012.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1890uA"/>
<attribute name="I-RIPPLE" value="5500mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075161012 "/>
<attribute name="RESR" value="8mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124152M6R3DVCTFB000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875075161013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075161013.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="2520uA"/>
<attribute name="I-RIPPLE" value="5500mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075161013 "/>
<attribute name="RESR" value="8mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124202M6R3DVCTFB000"/>
<attribute name="VALUE" value="2000  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875075361005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075361005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1504uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075361005 "/>
<attribute name="RESR" value="10mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124471M016DVCTFB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875075361006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075361006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="2176uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075361006 "/>
<attribute name="RESR" value="10mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124681M016DVCTFB000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875075361007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075361007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="2624uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075361007 "/>
<attribute name="RESR" value="10mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124821M016DVCTFB000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875075561005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075561005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="500uA"/>
<attribute name="I-RIPPLE" value="4800mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075561005 "/>
<attribute name="RESR" value="15mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124101M025DVCTFB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875075561006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075561006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="750uA"/>
<attribute name="I-RIPPLE" value="4800mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075561006 "/>
<attribute name="RESR" value="15mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124151M025DVCTFB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875075561007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075561007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="900uA"/>
<attribute name="I-RIPPLE" value="4800mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075561007 "/>
<attribute name="RESR" value="15mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124181M025DVCTFB000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875075561008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075561008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1100uA"/>
<attribute name="I-RIPPLE" value="4800mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075561008 "/>
<attribute name="RESR" value="15mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124221M025DVCTFB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875075561009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075561009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="4800mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075561009 "/>
<attribute name="RESR" value="15mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124271M025DVCTFB000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875075661004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075661004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="700uA"/>
<attribute name="I-RIPPLE" value="3800mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075661004 "/>
<attribute name="RESR" value="25mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124101M035DVCTFB000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875075661007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075661007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1260uA"/>
<attribute name="I-RIPPLE" value="4100mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075661007 "/>
<attribute name="RESR" value="22mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124181M035DVCTFB000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875075661008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075661008.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1540uA"/>
<attribute name="I-RIPPLE" value="4100mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075661008 "/>
<attribute name="RESR" value="22mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124221M035DVCTFB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875075661009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075661009.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1890uA"/>
<attribute name="I-RIPPLE" value="4400mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075661009 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124271M035DVCTFB000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875075661010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075661010.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="2310uA"/>
<attribute name="I-RIPPLE" value="4400mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075661010 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124331M035DVCTFB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875075761003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075761003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="330uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075761003 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124330M050DVCTFB000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875075761004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075761004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="390uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075761004 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124390M050DVCTFB000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875075761005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075761005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075761005 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124470M050DVCTFB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875075761006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075761006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="560uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075761006 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124560M050DVCTFB000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875075761007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075761007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="680uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075761007 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124680M050DVCTFB000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875075861003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075861003.pdf"/>
<attribute name="DF" value=" 0.12 "/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="227.2uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075861003 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124220M063DVCTFB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_875075861004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075861004.pdf"/>
<attribute name="DF" value=" 0.12 "/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="415.8uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075861004 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124330M063DVCTFB000"/>
<attribute name="VALUE" value="33 µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_875075861006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075861006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="592.2uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075861006 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124470M063DVCTFB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_875075961002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075961002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="440uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075961002 "/>
<attribute name="RESR" value="50mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124220M100DVCTFB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_875076161003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875076161003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="352uA"/>
<attribute name="I-RIPPLE" value="2300mA"/>
<attribute name="L" value="12.4mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875076161003 "/>
<attribute name="RESR" value="38mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEF124220M080DVCTFB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSLC_8X11.7" prefix="C">
<description>&lt;b&gt;WCAP-PSLC Aluminum Polymer Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Large Capacitance  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Large capacitance product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 10 µF ‒ 2000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 8.0 x 11.7 up to 10.0 x 12.4 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14736v209%20Family_WCAP-PSLC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14736v209%20Family_WCAP-PSLC.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PSLC/"&gt;https://www.we-online.com/catalog/en/WCAP-PSLC/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSLC_8X11.7(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875075155001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075155001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="226.8uA"/>
<attribute name="I-RIPPLE" value="5200mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075155001 "/>
<attribute name="RESR" value="8mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117181M6R3DVCTFB000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875075155002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075155002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="277.2uA"/>
<attribute name="I-RIPPLE" value="5200mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075155002 "/>
<attribute name="RESR" value="8mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117221M6R3DVCTFB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875075155003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075155003.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="340.2uA"/>
<attribute name="I-RIPPLE" value="5200mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075155003 "/>
<attribute name="RESR" value="8mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117271M6R3DVCTFB000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875075155004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075155004.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="416uA"/>
<attribute name="I-RIPPLE" value="5200mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075155004 "/>
<attribute name="RESR" value="8mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117331M6R3DVCTFB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875075155005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075155005.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="491uA"/>
<attribute name="I-RIPPLE" value="5200mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075155005 "/>
<attribute name="RESR" value="8mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117391M6R3DVCTFB000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875075155006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075155006.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="592uA"/>
<attribute name="I-RIPPLE" value="5200mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075155006 "/>
<attribute name="RESR" value="8mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117471M6R3DVCTFB000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875075155007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075155007.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="705.6uA"/>
<attribute name="I-RIPPLE" value="5200mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075155007 "/>
<attribute name="RESR" value="8mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117561M6R3DVCTFB000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875075155008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075155008.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="856uA"/>
<attribute name="I-RIPPLE" value="5200mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075155008 "/>
<attribute name="RESR" value="8mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117681M6R3DVCTFB000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875075155009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075155009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="1033.2uA"/>
<attribute name="I-RIPPLE" value="5200mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075155009 "/>
<attribute name="RESR" value="8mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117821M6R3DVCTFB000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875075155010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075155010.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="1260uA"/>
<attribute name="I-RIPPLE" value="5200mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075155010 "/>
<attribute name="RESR" value="8mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117102M6R3DVCTFB000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875075355001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075355001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="576uA"/>
<attribute name="I-RIPPLE" value="4700mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075355001 "/>
<attribute name="RESR" value="10mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117181M016DVCTFB000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875075355002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075355002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="704uA"/>
<attribute name="I-RIPPLE" value="4700mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075355002 "/>
<attribute name="RESR" value="10mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117221M016DVCTFB000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875075355003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075355003.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="864uA"/>
<attribute name="I-RIPPLE" value="4700mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075355003 "/>
<attribute name="RESR" value="10mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117271M016DVCTFB000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875075355004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075355004.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="1056uA"/>
<attribute name="I-RIPPLE" value="4700mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075355004 "/>
<attribute name="RESR" value="10mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117331M016DVCTFB000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875075555001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075555001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="195uA"/>
<attribute name="I-RIPPLE" value="4210mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075555001 "/>
<attribute name="RESR" value="15mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117390M025DVCTFB000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875075555002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075555002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="4210mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075555002 "/>
<attribute name="RESR" value="15mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117470M025DVCTFB000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875075555003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075555003.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="340uA"/>
<attribute name="I-RIPPLE" value="4210mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075555003 "/>
<attribute name="RESR" value="15mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117680M025DVCTFB000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875075555004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075555004.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="410uA"/>
<attribute name="I-RIPPLE" value="4210mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075555004 "/>
<attribute name="RESR" value="15mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117820M025DVCTFB000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875075655001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075655001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="273uA"/>
<attribute name="I-RIPPLE" value="2700mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075655001 "/>
<attribute name="RESR" value="32mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117390M035DVCTFB000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875075655002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075655002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="476uA"/>
<attribute name="I-RIPPLE" value="3300mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075655002 "/>
<attribute name="RESR" value="28mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117680M035DVCTFB000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875075655003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075655003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="574uA"/>
<attribute name="I-RIPPLE" value="3300mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075655003 "/>
<attribute name="RESR" value="28mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117820M035DVCTFB000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875075655005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075655005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="840uA"/>
<attribute name="I-RIPPLE" value="3800mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075655005 "/>
<attribute name="RESR" value="25mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117121M035DVCTFB000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875075655006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075655006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="840uA"/>
<attribute name="I-RIPPLE" value="3800mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075655006 "/>
<attribute name="RESR" value="25mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117151M035DVCTFB000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875075755001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075755001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075755001 "/>
<attribute name="RESR" value="40mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117100M050DVCTFB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875075755002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075755002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075755002 "/>
<attribute name="RESR" value="40mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117220M050DVCTFB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875075855001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075855001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="126uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075855001 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117100M063DVCTFB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_875075855002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075855002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="277.2uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075855002 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117220M063DVCTFB000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_875075855005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075855005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="491.4uA"/>
<attribute name="I-RIPPLE" value="3500mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075855005 "/>
<attribute name="RESR" value="27mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117390M063DVCTFB000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_875075955001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875075955001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="200uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875075955001 "/>
<attribute name="RESR" value="55mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value=""/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_875076155002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/875076155002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="192uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="11.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875076155002 "/>
<attribute name="RESR" value="40mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PSEE117120M080DVCTFB000"/>
<attribute name="VALUE" value="12  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
