<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Aluminium Polymer Capacitors - WCAP-PSLP&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-08-24&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-PSLP_6.3X7.7(DXL)">
<description>&lt;B&gt;WCAP-PSLP&lt;/B&gt;&lt;BR&gt;Aluminum Polymer Capacitors ,6.3X7.7X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-PSLP_4X5.5(DXL)">
<description>&lt;B&gt;WCAP-PSLP&lt;/B&gt;&lt;BR&gt;Aluminum Polymer Capacitors ,4X5.5X1(DiameterXLengthXPitch)</description>
</package>
<package name="WCAP-PSLP_5X5.5(DXL)">
<description>&lt;B&gt;WCAP-PSLP&lt;/B&gt;&lt;BR&gt;Aluminum Polymer Capacitors,5X5.5X1.4(DiameterXLengthXP)</description>
</package>
<package name="WCAP-PSLP_6.3X5.8(DXL)">
<description>&lt;B&gt;WCAP-PSLP&lt;/B&gt;&lt;BR&gt;Aluminum Polymer Capacitors ,6.3x5.8x2.2(DiameterXLengthXP)</description>
</package>
<package name="WCAP-PSLP_5X5.8(DXL)">
<description>&lt;B&gt;WCAP-PSLP&lt;/B&gt;&lt;BR&gt;Aluminum Polymer Capacitors,5x5.8x1.4(DiameterXLengthXP)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-PSLP_6.3X7.7" prefix="C">
<description>&lt;b&gt;WCAP-PSLP Aluminum Polymer Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Profile  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low profile product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 4.7 µF ‒ 390 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 6.3 x 7.7 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14737v209%20family-WCAP-PSLP-6.3x5.8x2.2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14737v209%20family-WCAP-PSLP-6.3x5.8x2.2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;Details see: &lt;a href="www.we-online.com/catalog/WCAP-PSLP/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-PSLP&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella Wu 2023-08-24
&lt;br&gt;2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSLP_6.3X7.7(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875105145011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105145011?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="3400mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105145011 "/>
<attribute name="RESR" value="15mOhm"/>
<attribute name="VALUE" value="390 µF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875105245014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105245014?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="2690mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105245014 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="VALUE" value="270 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875105245015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105245015?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="2690mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105245015 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875105345011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105345011?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="400uA"/>
<attribute name="I-RIPPLE" value="2690mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105345011 "/>
<attribute name="RESR" value="25mOhm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875105445005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105445005?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2670mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105445005 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="39 µF"/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875105445006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105445006?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2670mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105445006 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875105445007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105445007?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2670mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105445007 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875105545004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105545004?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2670mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105545004 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875105545005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105545005?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2670mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105545005 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="39 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875105645005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105645005?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105645005 "/>
<attribute name="RESR" value="50mOhm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875105945001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105945001?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="1060mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105945001 "/>
<attribute name="RESR" value="100mOhm"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSLP_6.3X5.8" prefix="C">
<description>&lt;b&gt;WCAP-PSLP Aluminum Polymer Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Profile  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low profile product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 4.7 µF ‒ 390 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 6.3 x 7.7 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14737v209%20family-WCAP-PSLP-6.3x5.8x2.2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14737v209%20family-WCAP-PSLP-6.3x5.8x2.2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;Details see: &lt;a href="www.we-online.com/catalog/WCAP-PSLP/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-PSLP&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella Wu 2023-08-24
&lt;br&gt;2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSLP_6.3X5.8(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875105144007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105144007?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="2390mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105144007 "/>
<attribute name="RESR" value="22mOhm"/>
<attribute name="VALUE" value="180 µF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875105144008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105144008?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="3000mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105144008 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875105144009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105144009?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="3000mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105144009 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="VALUE" value="270 µF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875105144010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105144010?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="3100mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105144010 "/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875105244011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105244011?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105244011 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875105244012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105244012?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105244012 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="180 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875105244013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105244013?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105244013 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875105344006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105344006?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="400uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105344006 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875105344007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105344007?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="400uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105344007 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875105344008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105344008?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="400uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105344008 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875105344009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105344009?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="400uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105344009 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="VALUE" value="82 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875105344010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105344010?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="400uA"/>
<attribute name="I-RIPPLE" value="2690mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105344010 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875105444001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105444001?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105444001 "/>
<attribute name="RESR" value="40mOhm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875105444002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105444002?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105444002 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="VALUE" value="15 µF"/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875105444003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105444003?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105444003 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875105444004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105444004?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105444004 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="20V(DC)"/>
</technology>
<technology name="_875105544001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105544001?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105544001 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875105544002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105544002?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105544002 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="VALUE" value="15 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875105544003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105544003?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105544003 "/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875105644004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105644004?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="900mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105644004 "/>
<attribute name="RESR" value="64mOhm"/>
<attribute name="VALUE" value="18 µF"/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_875105744001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105744001?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105744001 "/>
<attribute name="RESR" value="80mOhm"/>
<attribute name="VALUE" value="8.2 µF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875105744002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105744002?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105744002 "/>
<attribute name="RESR" value="80mOhm"/>
<attribute name="VALUE" value="12 µF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875105744003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105744003?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105744003 "/>
<attribute name="RESR" value="80mOhm"/>
<attribute name="VALUE" value="15 µF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875105844001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105844001?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="700mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105844001 "/>
<attribute name="RESR" value="100mOhm"/>
<attribute name="VALUE" value="5.6 µF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_875105844002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105844002?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="600uA"/>
<attribute name="I-RIPPLE" value="700mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105844002 "/>
<attribute name="RESR" value="100mOhm"/>
<attribute name="VALUE" value="8.2 µF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSLP_4X5.5" prefix="C">
<description>&lt;b&gt;WCAP-PSLP Aluminum Polymer Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Profile  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low profile product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 4.7 µF ‒ 390 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 6.3 x 7.7 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14737v209%20family-WCAP-PSLP-6.3x5.8x2.2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14737v209%20family-WCAP-PSLP-6.3x5.8x2.2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;Details see: &lt;a href="www.we-online.com/catalog/WCAP-PSLP/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-PSLP&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella Wu 2023-08-24
&lt;br&gt;2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSLP_4X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875105240001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105240001?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1200mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105240001 "/>
<attribute name="RESR" value="80mOhm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875105240002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105240002?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1200mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105240002 "/>
<attribute name="RESR" value="80mOhm"/>
<attribute name="VALUE" value="15 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875105240003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105240003?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1200mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105240003 "/>
<attribute name="RESR" value="80mOhm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSLP_5X5.8" prefix="C">
<description>&lt;b&gt;WCAP-PSLP Aluminum Polymer Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Profile  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low profile product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 4.7 µF ‒ 390 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 6.3 x 7.7 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14737v209%20family-WCAP-PSLP-6.3x5.8x2.2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14737v209%20family-WCAP-PSLP-6.3x5.8x2.2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;Details see: &lt;a href="www.we-online.com/catalog/WCAP-PSLP/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-PSLP&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella Wu 2023-08-24
&lt;br&gt;2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSLP_5X5.8(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875105359001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105359001?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="400uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105359001 "/>
<attribute name="RESR" value="40mOhm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875105359002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105359002?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="400uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105359002 "/>
<attribute name="RESR" value="40mOhm"/>
<attribute name="VALUE" value="15 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875105359003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105359003?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="400uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105359003 "/>
<attribute name="RESR" value="40mOhm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875105359004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105359004?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="400uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105359004 "/>
<attribute name="RESR" value="40mOhm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875105359005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105359005?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="400uA"/>
<attribute name="I-RIPPLE" value="2200mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105359005 "/>
<attribute name="RESR" value="40mOhm"/>
<attribute name="VALUE" value="39 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PSLP_5X5.5" prefix="C">
<description>&lt;b&gt;WCAP-PSLP Aluminum Polymer Capacitors &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Profile  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low profile product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 4.7 µF ‒ 390 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 6.3 x 7.7 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14737v209%20family-WCAP-PSLP-6.3x5.8x2.2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14737v209%20family-WCAP-PSLP-6.3x5.8x2.2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;&lt;br&gt;Details see: &lt;a href="www.we-online.com/catalog/WCAP-PSLP/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-PSLP&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by Ella Wu 2023-08-24
&lt;br&gt;2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PSLP_5X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_875105142001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105142001?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105142001 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875105142002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105142002?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105142002 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875105142003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105142003?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105142003 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875105142004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105142004?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105142004 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="82 µF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875105142005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105142005?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105142005 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875105142006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105142006?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105142006 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_875105242004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105242004?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105242004 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875105242005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105242005?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105242005 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="39 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875105242006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105242006?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105242006 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875105242007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105242007?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105242007 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875105242008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105242008?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105242008 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875105242009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105242009?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105242009 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="82 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
<technology name="_875105242010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875105242010?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="1970mA"/>
<attribute name="LENGTH" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 875105242010 "/>
<attribute name="RESR" value="30mOhm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="10V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
