<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminium Polymer Capacitors - WCAP-PT5H&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-05&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-PT5H_6.3X5.2(DXL)">
<description>&lt;B&gt;WCAP-PT5H&lt;/B&gt;&lt;BR&gt; Aluminium Polymer Capacitors ,6.3x5.2x2.5x0.6(DiameterXLengthXPinXØ Pin)</description>
</package>
<package name="WCAP-PT5H_8X7(DXL)">
<description>&lt;B&gt;WCAP-PT5H&lt;/B&gt;&lt;BR&gt;  Aluminium Polymer Capacitors ,8x7x3.5x0.6(DiameterXLengthXPinXØ Pin)</description>
</package>
<package name="WCAP-PT5H_8X11.5(DXL)">
<description>&lt;B&gt;WCAP-PT5H&lt;/B&gt;&lt;BR&gt;  Aluminium Polymer Capacitors ,8x11.5x3.5x0.6(DiameterXLengthXPinXØ Pin)</description>
</package>
<package name="WCAP-PT5H_10X12.5(DXL)">
<description>&lt;B&gt;WCAP-PT5H&lt;/B&gt;&lt;BR&gt;  Aluminium Polymer Capacitors ,10x12.5x5x0.6(DiameterXLengthXPinXØ Pin)</description>
</package>
<package name="WCAP-PT5H_8X8(DXL)">
<description>&lt;B&gt;WCAP-PT5H&lt;/B&gt;&lt;BR&gt;  Aluminium Polymer Capacitors ,8x8x3.5x0.6(DiameterXLengthXPinXØ Pin)</description>
</package>
<package name="WCAP-PT5H_6.3X11(DXL)">
<description>&lt;B&gt;WCAP-PT5H&lt;/B&gt;&lt;BR&gt; Aluminium Polymer Capacitors ,6.3x11x2.5x0.6(DiameterXLengthXPinXØ Pin)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-PT5H_8X7" prefix="C">
<description>&lt;b&gt;WCAP-PT5H Aluminum Polymer Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long Life product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 2000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 35 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C bis +105 °C 
&lt;BR&gt;Endurance: 5000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 5.2 up to 10.0 x 12.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14738v209%20Family_WCAP-PT5H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14738v209%20Family_WCAP-PT5H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PT5H/"&gt;https://www.we-online.com/catalog/en/WCAP-PT5H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PT5H_8X7(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_870235674003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235674003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="273uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="L" value="7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235674003 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="RESR" value="32mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE070390M035DSPA7E000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PT5H_6.3X5.2" prefix="C">
<description>&lt;b&gt;WCAP-PT5H Aluminum Polymer Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long Life product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 2000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 35 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C bis +105 °C 
&lt;BR&gt;Endurance: 5000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 5.2 up to 10.0 x 12.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14738v209%20Family_WCAP-PT5H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14738v209%20Family_WCAP-PT5H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PT5H/"&gt;https://www.we-online.com/catalog/en/WCAP-PT5H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PT5H_6.3X5.2(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_870235673001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235673001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="300uA"/>
<attribute name="I-RIPPLE" value="2600mA"/>
<attribute name="L" value="5.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235673001 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="RESR" value="35mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTED052220M035DSPA4E000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PT5H_8X11.5" prefix="C">
<description>&lt;b&gt;WCAP-PT5H Aluminum Polymer Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long Life product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 2000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 35 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C bis +105 °C 
&lt;BR&gt;Endurance: 5000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 5.2 up to 10.0 x 12.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14738v209%20Family_WCAP-PT5H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14738v209%20Family_WCAP-PT5H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PT5H/"&gt;https://www.we-online.com/catalog/en/WCAP-PT5H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PT5H_8X11.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_870235174004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235174004.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="428uA"/>
<attribute name="I-RIPPLE" value="6100mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235174004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="RESR" value="7mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115681M6R3DSPA7E000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870235174005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235174005.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="516.6uA"/>
<attribute name="I-RIPPLE" value="6100mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235174005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="RESR" value="7mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115821M6R3DSPA7E000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870235374006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235374006.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="5600mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235374006 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="RESR" value="9mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115331M016DSPA7E000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870235674004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235674004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="476uA"/>
<attribute name="I-RIPPLE" value="3600mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235674004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115680M035DSPA7E000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_870235674005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235674005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="574uA"/>
<attribute name="I-RIPPLE" value="3600mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235674005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="RESR" value="20mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115820M035DSPA7E000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PT5H_10X12.5" prefix="C">
<description>&lt;b&gt;WCAP-PT5H Aluminum Polymer Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long Life product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 2000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 35 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C bis +105 °C 
&lt;BR&gt;Endurance: 5000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 5.2 up to 10.0 x 12.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14738v209%20Family_WCAP-PT5H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14738v209%20Family_WCAP-PT5H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PT5H/"&gt;https://www.we-online.com/catalog/en/WCAP-PT5H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PT5H_10X12.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_870235175006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235175006.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="6640mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235175006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="RESR" value="7mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125102M6R3DSPA9E000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870235175007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235175007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="756uA"/>
<attribute name="I-RIPPLE" value="6640mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235175007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="RESR" value="7mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125122M6R3DSPA9E000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870235175008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235175008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="6640mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235175008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="RESR" value="7mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125152M6R3DSPA9E000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870235175009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235175009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1260uA"/>
<attribute name="I-RIPPLE" value="6640mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235175009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="RESR" value="7mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125202M6R3DSPA9E000"/>
<attribute name="VALUE" value="2000  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870235375007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235375007.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="624uA"/>
<attribute name="I-RIPPLE" value="6100mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235375007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="RESR" value="9mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125391M016DSPA9E000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870235375008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235375008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="752uA"/>
<attribute name="I-RIPPLE" value="6100mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235375008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="RESR" value="9mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125471M016DSPA9E000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870235375009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235375009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="896uA"/>
<attribute name="I-RIPPLE" value="6100mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235375009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="RESR" value="9mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125561M016DSPA9E000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870235675002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235675002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="231uA"/>
<attribute name="I-RIPPLE" value="3100mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235675002 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="RESR" value="25mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125330M035DSPA9E000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_870235675006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235675006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="840uA"/>
<attribute name="I-RIPPLE" value="4000mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235675006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="RESR" value="18mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125121M035DSPA9E000"/>
<attribute name="VALUE" value="120  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_870235675007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235675007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1050uA"/>
<attribute name="I-RIPPLE" value="4000mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235675007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="RESR" value="18mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125151M035DSPA9E000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PT5H_8X8" prefix="C">
<description>&lt;b&gt;WCAP-PT5H Aluminum Polymer Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long Life product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 2000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 35 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C bis +105 °C 
&lt;BR&gt;Endurance: 5000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 5.2 up to 10.0 x 12.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14738v209%20Family_WCAP-PT5H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14738v209%20Family_WCAP-PT5H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PT5H/"&gt;https://www.we-online.com/catalog/en/WCAP-PT5H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PT5H_8X8(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_870235174001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235174001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="491.4uA"/>
<attribute name="I-RIPPLE" value="6100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235174001 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="RESR" value="7mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080391M6R3DSPA7E000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870235174002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235174002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="592uA"/>
<attribute name="I-RIPPLE" value="6100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235174002 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="RESR" value="7mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080471M6R3DSPA7E000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870235174003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235174003.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="705.6uA"/>
<attribute name="I-RIPPLE" value="6100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235174003 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="RESR" value="7mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080561M6R3DSPA7E000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870235374003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235374003.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="288uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235374003 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="RESR" value="10mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080181M016DSPA7E000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870235374004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235374004.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="352uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235374004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="RESR" value="10mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080221M016DSPA7E000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870235374005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235374005.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="432uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235374005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="RESR" value="10mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080271M016DSPA7E000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PT5H_6.3X11" prefix="C">
<description>&lt;b&gt;WCAP-PT5H Aluminum Polymer Capacitors  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Long Life  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long Life product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 22 µF ‒ 2000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 35 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C bis +105 °C 
&lt;BR&gt;Endurance: 5000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 5.2 up to 10.0 x 12.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life applications (industry, medical) 
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14738v209%20Family_WCAP-PT5H.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14738v209%20Family_WCAP-PT5H.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PT5H/"&gt;https://www.we-online.com/catalog/en/WCAP-PT5H/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PT5H_6.3X11(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_870235373001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235373001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="4800mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235373001 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="RESR" value="12mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTED110101M016DSPA4E000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870235373002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870235373002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="288uA"/>
<attribute name="I-RIPPLE" value="5600mA"/>
<attribute name="L" value="11mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870235373002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="RESR" value="9mOhm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTED110181M016DSPA4E000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
