<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminium Polymer Capacitors - WCAP-PTG5&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-05&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-PTG5_8X11.5(DXL)">
<description>&lt;B&gt;WCAP-PTG5&lt;/B&gt;&lt;BR&gt; Aluminium Polymer Capacitors ,8x11.5x3.5x0.6(DiameterXLengthXPinXØ Pin)</description>
</package>
<package name="WCAP-PTG5_8X8(DXL)">
<description>&lt;B&gt;WCAP-PTG5&lt;/B&gt;&lt;BR&gt; Aluminium Polymer Capacitors ,8x8x3.5x0.6(DiameterXLengthXPinXØ Pin)</description>
</package>
<package name="WCAP-PTG5_10X12.5(DXL)">
<description>&lt;B&gt;WCAP-PTG5&lt;/B&gt;&lt;BR&gt; Aluminium Polymer Capacitors ,10x12.5x5x0.6(DiameterXLengthXPinXØ Pin)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-PTG5_8X11.5" prefix="C">
<description>&lt;b&gt;WCAP-PTG5 Aluminium Polymer Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 39 µF ‒ 2000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 25 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 8.0 x 8.0 up to 10.0 x 12.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14739v209%20Family_WCAP-PTG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14739v209%20Family_WCAP-PTG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PTG5/"&gt;https://www.we-online.com/catalog/en/WCAP-PTG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PTG5_8X11.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_870025174011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025174011.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="756uA"/>
<attribute name="I-RIPPLE" value="5500mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025174011 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115122M6R3DSPA7B000"/>
<attribute name="VALUE" value="1200  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870025374001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025374001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="4800mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025374001 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115101M016DSPA7B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870025374006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025374006.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="624uA"/>
<attribute name="I-RIPPLE" value="5000mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025374006 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115391M016DSPA7B000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870025374007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025374007.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="752uA"/>
<attribute name="I-RIPPLE" value="5000mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025374007 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115471M016DSPA7B000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PTG5_8X8" prefix="C">
<description>&lt;b&gt;WCAP-PTG5 Aluminium Polymer Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 39 µF ‒ 2000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 25 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 8.0 x 8.0 up to 10.0 x 12.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14739v209%20Family_WCAP-PTG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14739v209%20Family_WCAP-PTG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PTG5/"&gt;https://www.we-online.com/catalog/en/WCAP-PTG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PTG5_8X8(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_870025174001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025174001.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="226.8uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025174001 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080181M6R3DSPA7B000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870025174002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025174002.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="277uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025174002 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080221M6R3DSPA7B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870025174003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025174003.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="340.2uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025174003 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080271M6R3DSPA7B000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870025174004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025174004.pdf"/>
<attribute name="DF" value="7%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="416uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025174004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080331M6R3DSPA7B000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870025174005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025174005.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="491uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025174005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080391M6R3DSPA7B000"/>
<attribute name="VALUE" value="390  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870025174006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025174006.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="592uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025174006 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080471M6R3DSPA7B000"/>
<attribute name="VALUE" value="470  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870025174007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025174007.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="705.6uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025174007 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080561M6R3DSPA7B000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870025174008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025174008.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="428uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025174008 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080681M6R3DSPA7B000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870025174009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025174009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="516.6uA"/>
<attribute name="I-RIPPLE" value="5100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025174009 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080821M6R3DSPA7B000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870025374002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025374002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="288uA"/>
<attribute name="I-RIPPLE" value="4500mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025374002 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080181M016DSPA7B000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870025374003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025374003.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="352uA"/>
<attribute name="I-RIPPLE" value="4500mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025374003 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080221M016DSPA7B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870025374004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025374004.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="432uA"/>
<attribute name="I-RIPPLE" value="4500mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025374004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080271M016DSPA7B000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870025374005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025374005.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="4500mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025374005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080331M016DSPA7B000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870025574001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025574001.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="195uA"/>
<attribute name="I-RIPPLE" value="4500mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025574001 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080390M025DSPA7B000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_870025574002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025574002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="4500mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025574002 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080470M025DSPA7B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_870025574003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025574003.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="340uA"/>
<attribute name="I-RIPPLE" value="4500mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025574003 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080680M025DSPA7B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_870025574004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025574004.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="410uA"/>
<attribute name="I-RIPPLE" value="4500mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025574004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080820M025DSPA7B000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_870025574005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025574005.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="500uA"/>
<attribute name="I-RIPPLE" value="4500mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025574005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080101M025DSPA7B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PTG5_10X12.5" prefix="C">
<description>&lt;b&gt;WCAP-PTG5 Aluminium Polymer Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;General Purpose +105 °C  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 39 µF ‒ 2000 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 25 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 8.0 x 8.0 up to 10.0 x 12.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14739v209%20Family_WCAP-PTG5.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14739v209%20Family_WCAP-PTG5.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PTG5/"&gt;https://www.we-online.com/catalog/en/WCAP-PTG5/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PTG5_10X12.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_870025175010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025175010.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="630uA"/>
<attribute name="I-RIPPLE" value="5900mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025175010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125102M6R3DSPA9B000"/>
<attribute name="VALUE" value="1000  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870025175012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025175012.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="945uA"/>
<attribute name="I-RIPPLE" value="5900mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025175012 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125152M6R3DSPA9B000"/>
<attribute name="VALUE" value="1500  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870025175013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025175013.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1260uA"/>
<attribute name="I-RIPPLE" value="5900mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025175013 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125202M6R3DSPA9B000"/>
<attribute name="VALUE" value="2000  µF "/>
<attribute name="VR" value="6.3V(DC)"/>
</technology>
<technology name="_870025375008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025375008.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="896uA"/>
<attribute name="I-RIPPLE" value="5500mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025375008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125561M016DSPA9B000"/>
<attribute name="VALUE" value="560  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870025375009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025375009.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1000uA"/>
<attribute name="I-RIPPLE" value="5500mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025375009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125681M016DSPA9B000"/>
<attribute name="VALUE" value="680  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870025375010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025375010.pdf"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1000uA"/>
<attribute name="I-RIPPLE" value="5500mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025375010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125821M016DSPA9B000"/>
<attribute name="VALUE" value="820  µF "/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_870025575006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025575006.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="900uA"/>
<attribute name="I-RIPPLE" value="4900mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025575006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125181M025DSPA9B000"/>
<attribute name="VALUE" value="180  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_870025575007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025575007.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1100uA"/>
<attribute name="I-RIPPLE" value="4900mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025575007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125221M025DSPA9B000"/>
<attribute name="VALUE" value="220  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_870025575008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025575008.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1350uA"/>
<attribute name="I-RIPPLE" value="4900mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025575008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125271M025DSPA9B000"/>
<attribute name="VALUE" value="270  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_870025575009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870025575009.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1650uA"/>
<attribute name="I-RIPPLE" value="4900mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870025575009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125331M025DSPA9B000"/>
<attribute name="VALUE" value="330  µF "/>
<attribute name="VR" value="25V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
