<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminium Polymer Capacitors - WCAP-PTHR&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-05&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-PTHR_6.3X8(DXL)">
<description>&lt;B&gt;WCAP-PTHR&lt;/B&gt;&lt;BR&gt; Aluminium Polymer Capacitors ,6.3x8x2.5x0.6(DiameterXLengthXPinXØ Pin)</description>
</package>
<package name="WCAP-PTHR_10X12.5(DXL)">
<description>&lt;B&gt;WCAP-PTHR&lt;/B&gt;&lt;BR&gt; Aluminium Polymer Capacitors ,10x12.5x5x0.6(DiameterXLengthXPinXØ Pin)</description>
</package>
<package name="WCAP-PTHR_8X11.5(DXL)">
<description>&lt;B&gt;WCAP-PTHR&lt;/B&gt;&lt;BR&gt; Aluminium Polymer Capacitors ,8x11.5x3.5x0.6(DiameterXLengthXPinXØ Pin)</description>
</package>
<package name="WCAP-PTHR_8X8(DXL)">
<description>&lt;B&gt;WCAP-PTHR&lt;/B&gt;&lt;BR&gt; Aluminium Polymer Capacitors ,8x8x3.5x0.6(DiameterXLengthXPinXØ Pin)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-PTHR_6.3X8" prefix="C">
<description>&lt;b&gt;WCAP-PTHR Aluminium Polymer Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low ESR &amp; High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High voltage product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 150 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 35 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 8.0 up to 10.0 x 12.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14740v209%20Family_WCAP-PTHR.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14740v209%20Family_WCAP-PTHR.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PTHR/"&gt;https://www.we-online.com/catalog/en/WCAP-PTHR/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PTHR_6.3X8(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_870055673001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055673001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="2100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055673001 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTED080100M035DSPA4B000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_870055673002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055673002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="154uA"/>
<attribute name="I-RIPPLE" value="2100mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055673002 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTED080220M035DSPA4B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PTHR_10X12.5" prefix="C">
<description>&lt;b&gt;WCAP-PTHR Aluminium Polymer Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low ESR &amp; High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High voltage product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 150 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 35 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 8.0 up to 10.0 x 12.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14740v209%20Family_WCAP-PTHR.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14740v209%20Family_WCAP-PTHR.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PTHR/"&gt;https://www.we-online.com/catalog/en/WCAP-PTHR/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PTHR_10X12.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_870055675008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055675008.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="574uA"/>
<attribute name="I-RIPPLE" value="3700mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055675008 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125820M035DSPA9B000"/>
<attribute name="VALUE" value="82  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_870055675009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055675009.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="700uA"/>
<attribute name="I-RIPPLE" value="3700mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055675009 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125101M035DSPA9B000"/>
<attribute name="VALUE" value="100  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_870055675010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055675010.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="1050uA"/>
<attribute name="I-RIPPLE" value="3700mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055675010 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125151M035DSPA9B000"/>
<attribute name="VALUE" value="150  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_870055775003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055775003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="330uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055775003 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125330M050DSPA9B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_870055775004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055775004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="390uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055775004 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125390M050DSPA9B000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_870055775005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055775005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055775005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125470M050DSPA9B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_870055775006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055775006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="560uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055775006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125560M050DSPA9B000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_870055775007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055775007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="680uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055775007 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125680M050DSPA9B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_870055875003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055875003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="415.8uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055875003 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125330M063DSPA9B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_870055875004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055875004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="491.4uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055875004 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125390M063DSPA9B000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_870055875005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055875005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="592.2uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055875005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125470M063DSPA9B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_870055875006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055875006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="705.6uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055875006 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125560M063DSPA9B000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_870055975002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055975002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="440uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055975002 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125220M100DSPA9B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_870055975003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055975003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="660uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055975003 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125330M100DSPA9B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_870055975004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055975004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="940uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055975004 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125470M100DSPA9B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_870056175003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870056175003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="352uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870056175003 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125220M080DSPA9B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
<technology name="_870056175004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870056175004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="432uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870056175004 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125270M080DSPA9B000"/>
<attribute name="VALUE" value="27  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
<technology name="_870056175005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870056175005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="L" value="12.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870056175005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEF125330M080DSPA9B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PTHR_8X11.5" prefix="C">
<description>&lt;b&gt;WCAP-PTHR Aluminium Polymer Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low ESR &amp; High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High voltage product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 150 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 35 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 8.0 up to 10.0 x 12.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14740v209%20Family_WCAP-PTHR.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14740v209%20Family_WCAP-PTHR.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PTHR/"&gt;https://www.we-online.com/catalog/en/WCAP-PTHR/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PTHR_8X11.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_870055674005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055674005.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="329uA"/>
<attribute name="I-RIPPLE" value="2890mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055674005 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115470M035DSPA7B000"/>
<attribute name="VALUE" value="47  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_870055674006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055674006.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="392uA"/>
<attribute name="I-RIPPLE" value="2890mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055674006 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115560M035DSPA7B000"/>
<attribute name="VALUE" value="56  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_870055674007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055674007.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="476uA"/>
<attribute name="I-RIPPLE" value="2890mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055674007 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115680M035DSPA7B000"/>
<attribute name="VALUE" value="68  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_870055774002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055774002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055774002 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115220M050DSPA7B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_870055874001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055874001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="126uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055874001 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115100M063DSPA7B000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_870055874002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055874002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="277.2uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055874002 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115220M063DSPA7B000"/>
<attribute name="VALUE" value="22  µF "/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_870055974001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055974001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="200uA"/>
<attribute name="I-RIPPLE" value="1400mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055974001 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115100M100DSPA7B000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="100V(DC)"/>
</technology>
<technology name="_870056174002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870056174002.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="192uA"/>
<attribute name="I-RIPPLE" value="2100mA"/>
<attribute name="L" value="11.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870056174002 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE115120M080DSPA7B000"/>
<attribute name="VALUE" value="12  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-PTHR_8X8" prefix="C">
<description>&lt;b&gt;WCAP-PTHR Aluminium Polymer Capacitors&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Low ESR &amp; High Voltage  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;High voltage product series 
&lt;BR&gt;Low ESR over high frequency range 
&lt;BR&gt;High permissible ripple current 
&lt;BR&gt;Mounting style: THT Radial 
&lt;BR&gt;Capacitance range: 10 µF ‒ 150 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 35 ‒ 100 V(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C 
&lt;BR&gt;Endurance: 2000h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 6.3 x 8.0 up to 10.0 x 12.5 
&lt;BR&gt;Recommended soldering: Wave soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low ripple voltage at the switching converter 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;Coupling 
&lt;BR&gt;e.g. High-end power supply, industrial computer, VGA card, charger, digital set-top box 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14740v209%20Family_WCAP-PTHR.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14740v209%20Family_WCAP-PTHR.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-PTHR/"&gt;https://www.we-online.com/catalog/en/WCAP-PTHR/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-05
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-PTHR_8X8(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_870055674003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055674003.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="231uA"/>
<attribute name="I-RIPPLE" value="2500mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055674003 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080330M035DSPA7B000"/>
<attribute name="VALUE" value="33  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_870055674004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055674004.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="273uA"/>
<attribute name="I-RIPPLE" value="2500mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055674004 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080390M035DSPA7B000"/>
<attribute name="VALUE" value="39  µF "/>
<attribute name="VR" value="35V(DC)"/>
</technology>
<technology name="_870055774001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870055774001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870055774001 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080100M050DSPA7B000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_870056174001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/870056174001.pdf"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="160uA"/>
<attribute name="I-RIPPLE" value="1900mA"/>
<attribute name="L" value="8mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 870056174001 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="TECHNICAL-REFERENCE" value="PTEE080100M080DSPA7B000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="80V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
