<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Super Capacitors (EDLCs) - WCAP-STSC&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-08-11&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-STSC_D10L20">
<description>&lt;b&gt;WCAP-STSC Super Capacitors (EDLCs)
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
10X20X5X0.6(Diameter X Length X Pitch X Pin Diameter)</description>
</package>
<package name="WCAP-STSC_D8L20">
<description>&lt;b&gt;WCAP-STSC Super Capacitors (EDLCs)
&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;8X20X3.5X0.6(Diameter X Length X Pitch X Pin Diameter)</description>
</package>
<package name="WCAP-STSC_D10L25">
<description>&lt;b&gt;WCAP-STSC Super Capacitors (EDLCs)
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
10X25X5X0.6(Diameter X Length X Pitch X Pin Diameter)</description>
</package>
<package name="WCAP-STSC_D18L40">
<description>&lt;b&gt;WCAP-STSC Super Capacitors (EDLCs)
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
18X40X7.5X0.8(Diameter X Length X Pitch X Pin Diameter)</description>
</package>
<package name="WCAP-STSC_D16L25">
<description>&lt;b&gt;WCAP-STSC Super Capacitors (EDLCs)
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
16X25X7.5X0.8(Diameter X Length X Pitch X Pin Diameter)</description>
</package>
<package name="WCAP-STSC_D13L25">
<description>&lt;b&gt;WCAP-STSC Super Capacitors (EDLCs)
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
13X25X5X0.6(Diameter X Length X Pitch X Pin Diameter)</description>
</package>
</packages>
<symbols>
<symbol name="C-POLAR">
<description>C-POLAR</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-STSC_10X20" prefix="C">
<description>&lt;b&gt; WCAP-STSC Supercapacitors (EDLC‘s)
&lt;br&gt;Standard Cylindrical – THT
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt;Product series with standard cylindrical size
&lt;br&gt; Electric Double Layer Capacitors
&lt;br&gt; Higher energy density than usual capacitors
&lt;br&gt; Mounting style: Radial THT
&lt;br&gt; Capacitance range: 3 F ‒ 50 F
&lt;br&gt; Capacitance tolerance: -10 % / +30 %
&lt;br&gt; Rated Voltage: 2.7 V(DC)
&lt;br&gt; Operating temperature: -40 °C up to +65 °C
&lt;br&gt; Life Cycles: 500000 Cycles
&lt;br&gt; Dimensions (DxL) in mm: 8.0 x 20.0 up to 18.0 x 40.0
&lt;br&gt; Recommended soldering: Wave soldering

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Memory backup
&lt;br&gt;Smart meter
&lt;br&gt;Network equipment
&lt;br&gt;UPS systems
&lt;br&gt;Power assist
&lt;br&gt;Energy harvesting

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o129765v209%20WCAP-STSC_group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o129765v209%20WCAP-STSC_group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WCAP-STSC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-STSC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-08-11
&lt;br&gt;2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C-POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-STSC_D10L20">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_850617021001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/850617021001?ae"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENERGY-DENSITY" value="2.41 Wh/kg"/>
<attribute name="I-LEAK" value="0.012mA"/>
<attribute name="I-MAX" value="5.4A"/>
<attribute name="I-RATED" value="1.29A"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value=" 850617021001 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POWER-DENSITY" value="17.35 KW/kg"/>
<attribute name="RESR-AC" value="40mohm"/>
<attribute name="RESR-DC" value="50mohm"/>
<attribute name="VALUE" value="5F"/>
<attribute name="VR" value="2.7V(DC)"/>
</technology>
<technology name="_850617021002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/850617021002?ae"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENERGY-DENSITY" value="3.3 Wh/kg"/>
<attribute name="I-LEAK" value="0.02mA"/>
<attribute name="I-MAX" value="7.1A"/>
<attribute name="I-RATED" value="1.7A"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value=" 850617021002 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POWER-DENSITY" value="18.92 KW/kg"/>
<attribute name="RESR-AC" value="35mohm"/>
<attribute name="RESR-DC" value="45mohm"/>
<attribute name="VALUE" value="7F"/>
<attribute name="VR" value="2.7V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-STSC_8X20" prefix="C">
<description>&lt;b&gt; WCAP-STSC Supercapacitors (EDLC‘s)
&lt;br&gt;Standard Cylindrical – THT
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt;Product series with standard cylindrical size
&lt;br&gt; Electric Double Layer Capacitors
&lt;br&gt; Higher energy density than usual capacitors
&lt;br&gt; Mounting style: Radial THT
&lt;br&gt; Capacitance range: 3 F ‒ 50 F
&lt;br&gt; Capacitance tolerance: -10 % / +30 %
&lt;br&gt; Rated Voltage: 2.7 V(DC)
&lt;br&gt; Operating temperature: -40 °C up to +65 °C
&lt;br&gt; Life Cycles: 500000 Cycles
&lt;br&gt; Dimensions (DxL) in mm: 8.0 x 20.0 up to 18.0 x 40.0
&lt;br&gt; Recommended soldering: Wave soldering

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Memory backup
&lt;br&gt;Smart meter
&lt;br&gt;Network equipment
&lt;br&gt;UPS systems
&lt;br&gt;Power assist
&lt;br&gt;Energy harvesting

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o129765v209%20WCAP-STSC_group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o129765v209%20WCAP-STSC_group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WCAP-STSC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-STSC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-08-11
&lt;br&gt;2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C-POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-STSC_D8L20">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_850617030001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/850617030001?ae"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENERGY-DENSITY" value="2.1 Wh/kg"/>
<attribute name="I-LEAK" value="0.008mA"/>
<attribute name="I-MAX" value="3.3A"/>
<attribute name="I-RATED" value="0.7A"/>
<attribute name="LENGTH" value="20mm"/>
<attribute name="PART-NUMBER" value=" 850617030001 "/>
<attribute name="PITCH" value="3.5mm"/>
<attribute name="POWER-DENSITY" value="18.08 KW/kg"/>
<attribute name="RESR-AC" value="60mohm"/>
<attribute name="RESR-DC" value="70mohm"/>
<attribute name="VALUE" value="3F"/>
<attribute name="VR" value="2.7V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-STSC_10X25" prefix="C">
<description>&lt;b&gt; WCAP-STSC Supercapacitors (EDLC‘s)
&lt;br&gt;Standard Cylindrical – THT
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt;Product series with standard cylindrical size
&lt;br&gt; Electric Double Layer Capacitors
&lt;br&gt; Higher energy density than usual capacitors
&lt;br&gt; Mounting style: Radial THT
&lt;br&gt; Capacitance range: 3 F ‒ 50 F
&lt;br&gt; Capacitance tolerance: -10 % / +30 %
&lt;br&gt; Rated Voltage: 2.7 V(DC)
&lt;br&gt; Operating temperature: -40 °C up to +65 °C
&lt;br&gt; Life Cycles: 500000 Cycles
&lt;br&gt; Dimensions (DxL) in mm: 8.0 x 20.0 up to 18.0 x 40.0
&lt;br&gt; Recommended soldering: Wave soldering

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Memory backup
&lt;br&gt;Smart meter
&lt;br&gt;Network equipment
&lt;br&gt;UPS systems
&lt;br&gt;Power assist
&lt;br&gt;Energy harvesting

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o129765v209%20WCAP-STSC_group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o129765v209%20WCAP-STSC_group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WCAP-STSC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-STSC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-08-11
&lt;br&gt;2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C-POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-STSC_D10L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_850617021004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/850617021004?ae"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENERGY-DENSITY" value="3.7 Wh/kg"/>
<attribute name="I-LEAK" value="0.03mA"/>
<attribute name="I-MAX" value="10A"/>
<attribute name="I-RATED" value="2.5A"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value=" 850617021004 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POWER-DENSITY" value="19.1 KW/kg"/>
<attribute name="RESR-AC" value="30mohm"/>
<attribute name="RESR-DC" value="35mohm"/>
<attribute name="VALUE" value="10F"/>
<attribute name="VR" value="2.7V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-STSC_16X25" prefix="C">
<description>&lt;b&gt; WCAP-STSC Supercapacitors (EDLC‘s)
&lt;br&gt;Standard Cylindrical – THT
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt;Product series with standard cylindrical size
&lt;br&gt; Electric Double Layer Capacitors
&lt;br&gt; Higher energy density than usual capacitors
&lt;br&gt; Mounting style: Radial THT
&lt;br&gt; Capacitance range: 3 F ‒ 50 F
&lt;br&gt; Capacitance tolerance: -10 % / +30 %
&lt;br&gt; Rated Voltage: 2.7 V(DC)
&lt;br&gt; Operating temperature: -40 °C up to +65 °C
&lt;br&gt; Life Cycles: 500000 Cycles
&lt;br&gt; Dimensions (DxL) in mm: 8.0 x 20.0 up to 18.0 x 40.0
&lt;br&gt; Recommended soldering: Wave soldering

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Memory backup
&lt;br&gt;Smart meter
&lt;br&gt;Network equipment
&lt;br&gt;UPS systems
&lt;br&gt;Power assist
&lt;br&gt;Energy harvesting

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o129765v209%20WCAP-STSC_group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o129765v209%20WCAP-STSC_group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WCAP-STSC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-STSC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-08-11
&lt;br&gt;2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C-POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-STSC_D16L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_850617022001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/850617022001?ae"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENERGY-DENSITY" value="3.7 Wh/kg"/>
<attribute name="I-LEAK" value="0.068mA"/>
<attribute name="I-MAX" value="20.7A"/>
<attribute name="I-RATED" value="6A"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value=" 850617022001 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="POWER-DENSITY" value="10.72 KW/kg"/>
<attribute name="RESR-AC" value="20mohm"/>
<attribute name="RESR-DC" value="25mohm"/>
<attribute name="VALUE" value="25F"/>
<attribute name="VR" value="2.7V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-STSC_13X25" prefix="C">
<description>&lt;b&gt; WCAP-STSC Supercapacitors (EDLC‘s)
&lt;br&gt;Standard Cylindrical – THT
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt;Product series with standard cylindrical size
&lt;br&gt; Electric Double Layer Capacitors
&lt;br&gt; Higher energy density than usual capacitors
&lt;br&gt; Mounting style: Radial THT
&lt;br&gt; Capacitance range: 3 F ‒ 50 F
&lt;br&gt; Capacitance tolerance: -10 % / +30 %
&lt;br&gt; Rated Voltage: 2.7 V(DC)
&lt;br&gt; Operating temperature: -40 °C up to +65 °C
&lt;br&gt; Life Cycles: 500000 Cycles
&lt;br&gt; Dimensions (DxL) in mm: 8.0 x 20.0 up to 18.0 x 40.0
&lt;br&gt; Recommended soldering: Wave soldering

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Memory backup
&lt;br&gt;Smart meter
&lt;br&gt;Network equipment
&lt;br&gt;UPS systems
&lt;br&gt;Power assist
&lt;br&gt;Energy harvesting

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o129765v209%20WCAP-STSC_group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o129765v209%20WCAP-STSC_group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WCAP-STSC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-STSC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-08-11
&lt;br&gt;2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C-POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-STSC_D13L25">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_850617021005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/850617021005?ae"/>
<attribute name="DIAMETER" value="13mm"/>
<attribute name="ENERGY-DENSITY" value="3.3 Wh/kg"/>
<attribute name="I-LEAK" value="0.06mA"/>
<attribute name="I-MAX" value="13.5A"/>
<attribute name="I-RATED" value="3.6A"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="PART-NUMBER" value=" 850617021005 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POWER-DENSITY" value="12.27 KW/kg"/>
<attribute name="RESR-AC" value="30mohm"/>
<attribute name="RESR-DC" value="33mohm"/>
<attribute name="VALUE" value="15F"/>
<attribute name="VR" value="2.7V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-STSC_18X40" prefix="C">
<description>&lt;b&gt; WCAP-STSC Supercapacitors (EDLC‘s)
&lt;br&gt;Standard Cylindrical – THT
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;&lt;/b&gt;Product series with standard cylindrical size
&lt;br&gt; Electric Double Layer Capacitors
&lt;br&gt; Higher energy density than usual capacitors
&lt;br&gt; Mounting style: Radial THT
&lt;br&gt; Capacitance range: 3 F ‒ 50 F
&lt;br&gt; Capacitance tolerance: -10 % / +30 %
&lt;br&gt; Rated Voltage: 2.7 V(DC)
&lt;br&gt; Operating temperature: -40 °C up to +65 °C
&lt;br&gt; Life Cycles: 500000 Cycles
&lt;br&gt; Dimensions (DxL) in mm: 8.0 x 20.0 up to 18.0 x 40.0
&lt;br&gt; Recommended soldering: Wave soldering

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Memory backup
&lt;br&gt;Smart meter
&lt;br&gt;Network equipment
&lt;br&gt;UPS systems
&lt;br&gt;Power assist
&lt;br&gt;Energy harvesting

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o129765v209%20WCAP-STSC_group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o129765v209%20WCAP-STSC_group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WCAP-STSC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WCAP-STSC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-08-11
&lt;br&gt;2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="C-POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-STSC_D18L40">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_850617022002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/850617022002?ae"/>
<attribute name="DIAMETER" value="18mm"/>
<attribute name="ENERGY-DENSITY" value="4.5 Wh/kg"/>
<attribute name="I-LEAK" value="0.105mA"/>
<attribute name="I-MAX" value="33.7A"/>
<attribute name="I-RATED" value="11.2A"/>
<attribute name="LENGTH" value="40mm"/>
<attribute name="PART-NUMBER" value=" 850617022002 "/>
<attribute name="PITCH" value="7.5mm"/>
<attribute name="POWER-DENSITY" value="8.13 KW/kg"/>
<attribute name="RESR-AC" value="15mohm"/>
<attribute name="RESR-DC" value="20mohm"/>
<attribute name="VALUE" value="50F"/>
<attribute name="VR" value="2.7V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
