<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Signal &amp; Communications - Balun - WE-BAL&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-11-12&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="7484252450">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0805, SMT, 6pins
&lt;br&gt;LXWXH=2X1.25X0.95mm</description>
</package>
<package name="7484112450">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0603, SMT, 6pins
&lt;br&gt;LXWXH=1.6X0.8X0.7mm</description>
</package>
<package name="7484212300">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0805, SMT, 6pins
&lt;br&gt;LXWXH=2X1.25X0.9mm</description>
</package>
<package name="748411245">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0603, SMT, 6pins
&lt;br&gt;LXWXH=1.6X0.8X0.6mm</description>
</package>
<package name="7484152450">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0603, SMT, 6pins
&lt;br&gt;LXWXH=1.6X0.8X0.5mm</description>
</package>
<package name="748422245">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0805, SMT, 6pins
&lt;br&gt;LXWXH=2X1.25X0.95mm</description>
</package>
<package name="7484111680">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0603, SMT, 6pins
&lt;br&gt;LXWXH=1.6X0.8X0.7mm</description>
</package>
<package name="7484212450">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0805, SMT, 6pins
&lt;br&gt;LXWXH=2X1.25X0.95mm</description>
</package>
<package name="748421245">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0805, SMT, 6pins
&lt;br&gt;LXWXH=2X1.25X0.95mm</description>
</package>
<package name="7484215510">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0805, SMT, 6pins
&lt;br&gt;LXWXH=2X1.25X0.95mm</description>
</package>
<package name="748421551">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0805, SMT, 6pins
&lt;br&gt;LXWXH=2X1.25X0.95mm</description>
</package>
<package name="748412245">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0603, SMT, 6pins
&lt;br&gt;LXWXH=1.6X0.8X0.6mm</description>
</package>
<package name="7484112500">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0603, SMT, 6pins
&lt;br&gt;LXWXH=1.6X0.8X0.4mm</description>
</package>
<package name="748425245">
<description>&lt;B&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;&lt;/b&gt;Size: 0805, SMT, 6pins
&lt;br&gt;LXWXH=2X1.25X0.95mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-BAL_DCBIAS">
<pin name="OUT2" direction="pas"/>
<pin name="OUT1" direction="pas"/>
<pin name="IN" direction="pas"/>
<pin name="GND/DC" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="WE-BAL_GENERIC">
<pin name="OUT2" direction="pas"/>
<pin name="OUT1" direction="pas"/>
<pin name="IN" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
</symbol>
<symbol name="WE-BAL_0603_748411245">
<pin name="OUT1" direction="pas"/>
<pin name="OUT2" direction="pas"/>
<pin name="IN" direction="pas"/>
<pin name="GND/DC" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="7484252450" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_DCBIAS"/>
</gates>
<devices>
<device name="" package="7484252450">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND/DC" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7484252450?ae"/>
<attribute name="IL" value="1.2dB"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7484252450 "/>
<attribute name="SIZE" value="0805"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value=" 1.7 "/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7484112450" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_DCBIAS"/>
</gates>
<devices>
<device name="" package="7484112450">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND/DC" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="100Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7484112450?ae"/>
<attribute name="IL" value="1.2dB"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7484112450 "/>
<attribute name="SIZE" value="0603"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value=" 2 "/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7484212300" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_GENERIC"/>
</gates>
<devices>
<device name="" package="7484212300">
<connects>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="100Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7484212300?ae"/>
<attribute name="IL" value="1dB"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7484212300 "/>
<attribute name="SIZE" value="0805"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="1500-3100 MHz"/>
<attribute name="VSWR" value=" 2 "/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="748411245" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_0603_748411245"/>
</gates>
<devices>
<device name="" package="748411245">
<connects>
<connect gate="G$1" pin="GND/DC" pad="3"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="100Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/748411245?ae"/>
<attribute name="IL" value="1dB"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 748411245 "/>
<attribute name="SIZE" value="0603"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value=" 2 "/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7484152450" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_DCBIAS"/>
</gates>
<devices>
<device name="" package="7484152450">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND/DC" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7484152450?ae"/>
<attribute name="IL" value="1.2dB"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7484152450 "/>
<attribute name="SIZE" value="0603"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value=" 2 "/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="748422245" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_DCBIAS"/>
</gates>
<devices>
<device name="" package="748422245">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND/DC" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="200Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/748422245?ae"/>
<attribute name="IL" value="0.76dB"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 748422245 "/>
<attribute name="SIZE" value="0805"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value=" 2 "/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7484111680" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_GENERIC"/>
</gates>
<devices>
<device name="" package="7484111680">
<connects>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="100Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7484111680?ae"/>
<attribute name="IL" value="1.7dB"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7484111680 "/>
<attribute name="SIZE" value="0603"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="673-2700 MHz"/>
<attribute name="VSWR" value=" 2.45 "/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7484212450" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_DCBIAS"/>
</gates>
<devices>
<device name="" package="7484212450">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND/DC" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="100Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7484212450?ae"/>
<attribute name="IL" value="1dB"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7484212450 "/>
<attribute name="SIZE" value="0805"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value=" 2 "/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="748421245" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_DCBIAS"/>
</gates>
<devices>
<device name="" package="748421245">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND/DC" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="100Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/748421245?ae"/>
<attribute name="IL" value="0.54dB"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 748421245 "/>
<attribute name="SIZE" value="0805"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value=" 2 "/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7484215510" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_GENERIC"/>
</gates>
<devices>
<device name="" package="7484215510">
<connects>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="100Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7484215510?ae"/>
<attribute name="IL" value="1.2dB"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7484215510 "/>
<attribute name="SIZE" value="0805"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="4900-5900 MHz"/>
<attribute name="VSWR" value=" 1.7 "/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="748421551" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_DCBIAS"/>
</gates>
<devices>
<device name="" package="748421551">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND/DC" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="100Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/748421551?ae"/>
<attribute name="IL" value="0.68dB"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 748421551 "/>
<attribute name="SIZE" value="0805"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="5150-5875 MHz"/>
<attribute name="VSWR" value=" 2 "/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="748412245" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_DCBIAS"/>
</gates>
<devices>
<device name="" package="748412245">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND/DC" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/748412245?ae"/>
<attribute name="IL" value="1.2dB"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 748412245 "/>
<attribute name="SIZE" value="0603"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value=" 2 "/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="748425245" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_DCBIAS"/>
</gates>
<devices>
<device name="" package="748425245">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND/DC" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/748425245?ae"/>
<attribute name="IL" value="0.53dB"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 748425245 "/>
<attribute name="SIZE" value="0805"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value=" 2 "/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7484112500" prefix="Z">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;Power Capacity: 2 W max.
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14748v209%20Multi-WE-BAL-7484215510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BAL&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2024-11-08&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL_GENERIC"/>
</gates>
<devices>
<device name="" package="7484112500">
<connects>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="BALANCED-IMPEDANCE" value="100Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7484112500?ae"/>
<attribute name="IL" value="0.55dB"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7484112500 "/>
<attribute name="SIZE" value="0603"/>
<attribute name="UNBALANCED-IMPEDANCE" value="50Ohm"/>
<attribute name="VALUE" value="2300-2700 MHz"/>
<attribute name="VSWR" value=" 1.7 "/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
