<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Signal &amp; Communications - Signal Transformers - WE-BMS&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-04-08&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-BMS_74942402">
</package>
<package name="WE-BMS_74941300">
</package>
<package name="WE-BMS_74942401">
</package>
<package name="WE-BMS_74941301">
</package>
<package name="WE-BMS_74942300">
</package>
<package name="WE-BMS_74942400">
</package>
<package name="WE-BMS_74942301">
</package>
<package name="WE-BMS_74942302">
</package>
<package name="WE-BMS_74941302">
</package>
</packages>
<symbols>
<symbol name="WE-BMS_74942402">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-BMS_74942401">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="WE-BMS_74941300">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-BMS_74942302">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="WE-BMS_74942300">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="WE-BMS_74942301">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-BMS_74941301">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-BMS_74941302">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-BMS_74942400">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-BMS_74942402" prefix="T">
<description>&lt;b&gt;WE-BMS Transformer for Battery Management Systems
&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Supports BMS isolation
&lt;BR&gt;Supports serial daisy chain isoSPI and SPI
&lt;BR&gt;800 VDC and 1000 VDC working voltage
&lt;BR&gt;AEC-Q200 qualification
&lt;BR&gt;Operating temperature: -40°C up to +125°C
&lt;BR&gt;
&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Solar energy storage
&lt;BR&gt;Energy Storage systems
&lt;BR&gt;Uninterrupted Power Supply (UPS)
&lt;BR&gt;E-bikes, E-scooters
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BMS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BMS&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-04-08&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BMS_74942402"/>
</gates>
<devices>
<device name="" package="WE-BMS_74942402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CREEPAGE-DISTANCE" value="15mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74942402?ae"/>
<attribute name="HEIGHT" value="7.3mm"/>
<attribute name="INSULATION-TEST-VOLTAGE" value="6400V(DC)"/>
<attribute name="LENGTH" value="12.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="NUMBER-OF-PORTS" value=" 1 "/>
<attribute name="PART-NUMBER" value=" 74942402 "/>
<attribute name="VALUE" value=" 74942402 "/>
<attribute name="WIDTH" value="28mm"/>
<attribute name="WORKING-VOLTAGE" value="1500V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-BMS_74941300" prefix="T">
<description>&lt;b&gt;WE-BMS Transformer for Battery Management Systems
&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Supports BMS isolation
&lt;BR&gt;Supports serial daisy chain isoSPI and SPI
&lt;BR&gt;800 VDC and 1000 VDC working voltage
&lt;BR&gt;AEC-Q200 qualification
&lt;BR&gt;Operating temperature: -40°C up to +125°C
&lt;BR&gt;
&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Solar energy storage
&lt;BR&gt;Energy Storage systems
&lt;BR&gt;Uninterrupted Power Supply (UPS)
&lt;BR&gt;E-bikes, E-scooters
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BMS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BMS&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-04-13
&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BMS_74941300"/>
</gates>
<devices>
<device name="" package="WE-BMS_74941300">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CREEPAGE-DISTANCE" value="6mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74941300?ae"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="INSULATION-TEST-VOLTAGE" value="4300V(DC)"/>
<attribute name="LENGTH" value="7.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="NUMBER-OF-PORTS" value=" 1 "/>
<attribute name="PART-NUMBER" value=" 74941300 "/>
<attribute name="VALUE" value=" 74941300 "/>
<attribute name="WIDTH" value="9.5mm"/>
<attribute name="WORKING-VOLTAGE" value="1000V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-BMS_74942401" prefix="T">
<description>&lt;b&gt;WE-BMS Transformer for Battery Management Systems
&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Supports BMS isolation
&lt;BR&gt;Supports serial daisy chain isoSPI and SPI
&lt;BR&gt;800 VDC and 1000 VDC working voltage
&lt;BR&gt;AEC-Q200 qualification
&lt;BR&gt;Operating temperature: -40°C up to +125°C
&lt;BR&gt;
&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Solar energy storage
&lt;BR&gt;Energy Storage systems
&lt;BR&gt;Uninterrupted Power Supply (UPS)
&lt;BR&gt;E-bikes, E-scooters
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BMS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BMS&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-04-08&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BMS_74942401"/>
</gates>
<devices>
<device name="" package="WE-BMS_74942401">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CREEPAGE-DISTANCE" value="15mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74942401?ae"/>
<attribute name="HEIGHT" value="4.85mm"/>
<attribute name="INSULATION-TEST-VOLTAGE" value="6400V(DC)"/>
<attribute name="LENGTH" value="15.45mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="NUMBER-OF-PORTS" value=" 2 "/>
<attribute name="PART-NUMBER" value=" 74942401 "/>
<attribute name="VALUE" value=" 74942401 "/>
<attribute name="WIDTH" value="27.85mm"/>
<attribute name="WORKING-VOLTAGE" value="1500V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-BMS_74941301" prefix="T">
<description>&lt;b&gt;WE-BMS Transformer for Battery Management Systems
&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Supports BMS isolation
&lt;BR&gt;Supports serial daisy chain isoSPI and SPI
&lt;BR&gt;800 VDC and 1000 VDC working voltage
&lt;BR&gt;AEC-Q200 qualification
&lt;BR&gt;Operating temperature: -40°C up to +125°C
&lt;BR&gt;
&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Solar energy storage
&lt;BR&gt;Energy Storage systems
&lt;BR&gt;Uninterrupted Power Supply (UPS)
&lt;BR&gt;E-bikes, E-scooters
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BMS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BMS&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-04-13
&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BMS_74941301"/>
</gates>
<devices>
<device name="" package="WE-BMS_74941301">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CREEPAGE-DISTANCE" value="5mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74941301?ae"/>
<attribute name="HEIGHT" value="5.5mm"/>
<attribute name="INSULATION-TEST-VOLTAGE" value="4300V(DC)"/>
<attribute name="LENGTH" value="7.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="NUMBER-OF-PORTS" value=" 1 "/>
<attribute name="PART-NUMBER" value=" 74941301 "/>
<attribute name="VALUE" value=" 74941301 "/>
<attribute name="WIDTH" value="9.5mm"/>
<attribute name="WORKING-VOLTAGE" value="1000V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-BMS_74942300" prefix="T">
<description>&lt;b&gt;WE-BMS Transformer for Battery Management Systems
&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Supports BMS isolation
&lt;BR&gt;Supports serial daisy chain isoSPI and SPI
&lt;BR&gt;800 VDC and 1000 VDC working voltage
&lt;BR&gt;AEC-Q200 qualification
&lt;BR&gt;Operating temperature: -40°C up to +125°C
&lt;BR&gt;
&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Solar energy storage
&lt;BR&gt;Energy Storage systems
&lt;BR&gt;Uninterrupted Power Supply (UPS)
&lt;BR&gt;E-bikes, E-scooters
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BMS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BMS&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-04-13
&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BMS_74942300"/>
</gates>
<devices>
<device name="" package="WE-BMS_74942300">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CREEPAGE-DISTANCE" value="10mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74942300?ae"/>
<attribute name="HEIGHT" value="4.75mm"/>
<attribute name="INSULATION-TEST-VOLTAGE" value="4300V(DC)"/>
<attribute name="LENGTH" value="15.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="NUMBER-OF-PORTS" value=" 2 "/>
<attribute name="PART-NUMBER" value=" 74942300 "/>
<attribute name="VALUE" value=" 74942300 "/>
<attribute name="WIDTH" value="14.7mm"/>
<attribute name="WORKING-VOLTAGE" value="1000V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-BMS_74942400" prefix="T">
<description>&lt;b&gt;WE-BMS Transformer for Battery Management Systems
&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Supports BMS isolation
&lt;BR&gt;Supports serial daisy chain isoSPI and SPI
&lt;BR&gt;800 VDC and 1000 VDC working voltage
&lt;BR&gt;AEC-Q200 qualification
&lt;BR&gt;Operating temperature: -40°C up to +125°C
&lt;BR&gt;
&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Solar energy storage
&lt;BR&gt;Energy Storage systems
&lt;BR&gt;Uninterrupted Power Supply (UPS)
&lt;BR&gt;E-bikes, E-scooters
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BMS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BMS&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-04-08&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BMS_74942400"/>
</gates>
<devices>
<device name="" package="WE-BMS_74942400">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CREEPAGE-DISTANCE" value="15mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74942400?ae"/>
<attribute name="HEIGHT" value="4.85mm"/>
<attribute name="INSULATION-TEST-VOLTAGE" value="6400V(DC)"/>
<attribute name="LENGTH" value="15.45mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="NUMBER-OF-PORTS" value=" 2 "/>
<attribute name="PART-NUMBER" value=" 74942400 "/>
<attribute name="VALUE" value=" 74942400 "/>
<attribute name="WIDTH" value="27.85mm"/>
<attribute name="WORKING-VOLTAGE" value="1500V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-BMS_74942301" prefix="T">
<description>&lt;b&gt;WE-BMS Transformer for Battery Management Systems
&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Supports BMS isolation
&lt;BR&gt;Supports serial daisy chain isoSPI and SPI
&lt;BR&gt;800 VDC and 1000 VDC working voltage
&lt;BR&gt;AEC-Q200 qualification
&lt;BR&gt;Operating temperature: -40°C up to +125°C
&lt;BR&gt;
&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Solar energy storage
&lt;BR&gt;Energy Storage systems
&lt;BR&gt;Uninterrupted Power Supply (UPS)
&lt;BR&gt;E-bikes, E-scooters
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BMS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BMS&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-04-13
&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BMS_74942301"/>
</gates>
<devices>
<device name="" package="WE-BMS_74942301">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CREEPAGE-DISTANCE" value="10mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74942301?ae"/>
<attribute name="HEIGHT" value="3.45mm"/>
<attribute name="INSULATION-TEST-VOLTAGE" value="4300V(DC)"/>
<attribute name="LENGTH" value="15.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="NUMBER-OF-PORTS" value=" 2 "/>
<attribute name="PART-NUMBER" value=" 74942301 "/>
<attribute name="VALUE" value=" 74942301 "/>
<attribute name="WIDTH" value="14.9mm"/>
<attribute name="WORKING-VOLTAGE" value="1000V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-BMS_74942302" prefix="T">
<description>&lt;b&gt;WE-BMS Transformer for Battery Management Systems
&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Supports BMS isolation
&lt;BR&gt;Supports serial daisy chain isoSPI and SPI
&lt;BR&gt;800 VDC and 1000 VDC working voltage
&lt;BR&gt;AEC-Q200 qualification
&lt;BR&gt;Operating temperature: -40°C up to +125°C
&lt;BR&gt;
&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Solar energy storage
&lt;BR&gt;Energy Storage systems
&lt;BR&gt;Uninterrupted Power Supply (UPS)
&lt;BR&gt;E-bikes, E-scooters
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BMS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BMS&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-04-13
&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BMS_74942302"/>
</gates>
<devices>
<device name="" package="WE-BMS_74942302">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CREEPAGE-DISTANCE" value="10mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74942302?ae"/>
<attribute name="HEIGHT" value="3.45mm"/>
<attribute name="INSULATION-TEST-VOLTAGE" value="4300V(DC)"/>
<attribute name="LENGTH" value="15.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="NUMBER-OF-PORTS" value=" 2 "/>
<attribute name="PART-NUMBER" value=" 74942302 "/>
<attribute name="VALUE" value=" 74942302 "/>
<attribute name="WIDTH" value="15.4mm"/>
<attribute name="WORKING-VOLTAGE" value="1000V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-BMS_74941302" prefix="T">
<description>&lt;b&gt;WE-BMS Transformer for Battery Management Systems
&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Supports BMS isolation
&lt;BR&gt;Supports serial daisy chain isoSPI and SPI
&lt;BR&gt;800 VDC and 1000 VDC working voltage
&lt;BR&gt;AEC-Q200 qualification
&lt;BR&gt;Operating temperature: -40°C up to +125°C
&lt;BR&gt;
&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Solar energy storage
&lt;BR&gt;Energy Storage systems
&lt;BR&gt;Uninterrupted Power Supply (UPS)
&lt;BR&gt;E-bikes, E-scooters
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o489329v209%20UtBMS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-BMS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-BMS&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-04-13
&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BMS_74941302"/>
</gates>
<devices>
<device name="" package="WE-BMS_74941302">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CREEPAGE-DISTANCE" value="10mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74941302?ae"/>
<attribute name="HEIGHT" value="3.45mm"/>
<attribute name="INSULATION-TEST-VOLTAGE" value="4300V(DC)"/>
<attribute name="LENGTH" value="9.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="NUMBER-OF-PORTS" value=" 1 "/>
<attribute name="PART-NUMBER" value=" 74941302 "/>
<attribute name="VALUE" value=" 74941302 "/>
<attribute name="WIDTH" value="15.4mm"/>
<attribute name="WORKING-VOLTAGE" value="1000V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
