<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Ferrites For PCB Assembly - WE-CBFHF&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CBF_HF_0402(W=2.2)">
<description>&lt;b&gt;WE-CBF HF SMT EMI Suppression Ferrite Bead (High Frequency)&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;0402</description>
</package>
<package name="WE-CBF_HF_0402(W=1.5)">
<description>&lt;b&gt;WE-CBF HF SMT EMI Suppression Ferrite Bead (High Frequency)&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;0402</description>
</package>
<package name="WE-CBF_HF_0603(W=2.2)">
<description>&lt;b&gt;WE-CBF HF SMT EMI Suppression Ferrite Bead (High Frequency)&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;0603</description>
</package>
<package name="WE-CBF_HF_0603(W=2.6)">
<description>&lt;b&gt;WE-CBF HF SMT EMI Suppression Ferrite Bead (High Frequency)&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;0603</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CBF_HF_0603" prefix="L">
<description>&lt;b&gt; WE-CBF HF SMD EMI Suppression Ferrite Bead (High Frequency)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Available in 3 types 
&lt;br&gt; Modified internal layout increases the effective suppression range 
&lt;br&gt; The impedance at 1 GHz are at least 3 times higher compared to the WE-CBF product family 
&lt;br&gt; Operating temperature: –55 °C to +125 °C 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Especially for the suppression of signal lines in the high frequency range 
&lt;br&gt; For fast data lines: CPU, highspeed bus systems, HDD 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Package name and Variant abbreviation:&lt;br&gt;&lt;br&gt;
Package: 
&lt;/b&gt;&lt;br&gt;Wide Band /High Speed: W=Width= 2.2
&lt;br&gt;High Current: W=Width= 2.6
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation:
&lt;/b&gt;&lt;br&gt;WB = Wide Band 
&lt;br&gt;HS=High Speed
&lt;br&gt;HC=High Current 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14752v209%20WE-TMSB_74269200x_0201.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14752v209%20WE-TMSB_74269200x_0201.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBF_HF?"&gt;http://katalog.we-online.de/en/pbs/WE-CBF_HF?&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-01-02&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_WB_HS" package="WE-CBF_HF_0603(W=2.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742861118">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/742861118.pdf"/>
<attribute name="IR1" value="200mA"/>
<attribute name="IR2" value="700mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 742861118 "/>
<attribute name="RDC-MAX" value="0.55Ohm"/>
<attribute name="RDC-TYP" value="0.25Ohm"/>
<attribute name="TYPE" value="Wide Band"/>
<attribute name="VALUE" value="180Ohm@100MHz"/>
<attribute name="Z" value="180Ohm@1GMHz"/>
<attribute name="ZMAX" value="270Ohm"/>
</technology>
<technology name="_742861160">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/742861160.pdf"/>
<attribute name="IR1" value="200mA"/>
<attribute name="IR2" value="500mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 742861160 "/>
<attribute name="RDC-MAX" value="0.9Ohm"/>
<attribute name="RDC-TYP" value="0.27Ohm"/>
<attribute name="TYPE" value="Wide Band"/>
<attribute name="VALUE" value="600Ohm@100MHz"/>
<attribute name="Z" value="450Ohm@1GMHz"/>
<attribute name="ZMAX" value="1000Ohm"/>
</technology>
<technology name="_742861210">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/742861210.pdf"/>
<attribute name="IR1" value="50mA"/>
<attribute name="IR2" value="300mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 742861210 "/>
<attribute name="RDC-MAX" value="1.8Ohm"/>
<attribute name="RDC-TYP" value="1.2Ohm"/>
<attribute name="TYPE" value="Wide Band"/>
<attribute name="VALUE" value="1000Ohm@100MHz"/>
<attribute name="Z" value="1100Ohm@1GMHz"/>
<attribute name="ZMAX" value="2200Ohm"/>
</technology>
<technology name="_742862160">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/742862160.pdf"/>
<attribute name="IR1" value="100mA"/>
<attribute name="IR2" value="350mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 742862160 "/>
<attribute name="RDC-MAX" value="1.5Ohm"/>
<attribute name="RDC-TYP" value="0.8Ohm"/>
<attribute name="TYPE" value="High Speed"/>
<attribute name="VALUE" value="600Ohm@100MHz"/>
<attribute name="Z" value="850Ohm@1GMHz"/>
<attribute name="ZMAX" value="1700Ohm"/>
</technology>
</technologies>
</device>
<device name="_HC" package="WE-CBF_HF_0603(W=2.6)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742863122">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/742863122.pdf"/>
<attribute name="IR1" value="600mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 742863122 "/>
<attribute name="RDC-MAX" value="0.25Ohm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="220Ohm@100MHz"/>
<attribute name="Z" value="250Ohm@1GMHz"/>
<attribute name="ZMAX" value="500Ohm"/>
</technology>
<technology name="_742863147">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/742863147.pdf"/>
<attribute name="IR1" value="500mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 742863147 "/>
<attribute name="RDC-MAX" value="0.32Ohm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="470Ohm@100MHz"/>
<attribute name="Z" value="600Ohm@1GMHz"/>
<attribute name="ZMAX" value="1000Ohm"/>
</technology>
<technology name="_742863160">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/742863160.pdf"/>
<attribute name="IR1" value="500mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 742863160 "/>
<attribute name="RDC-MAX" value="0.35Ohm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="600Ohm@100MHz"/>
<attribute name="Z" value="800Ohm@1GMHz"/>
<attribute name="ZMAX" value="1250Omh"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBF_HF_0402" prefix="L">
<description>&lt;b&gt; WE-CBF HF SMD EMI Suppression Ferrite Bead (High Frequency)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Available in 3 types 
&lt;br&gt; Modified internal layout increases the effective suppression range 
&lt;br&gt; The impedance at 1 GHz are at least 3 times higher compared to the WE-CBF product family 
&lt;br&gt; Operating temperature: –55 °C to +125 °C 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Especially for the suppression of signal lines in the high frequency range 
&lt;br&gt; For fast data lines: CPU, highspeed bus systems, HDD 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Package name and Variant abbreviation:&lt;br&gt;&lt;br&gt;
Package: 
&lt;/b&gt;&lt;br&gt;Wide Band /High Speed: W=Width= 1.5
&lt;br&gt;High Current: W=Width= 2.2
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation:
&lt;/b&gt;&lt;br&gt;WB = Wide Band 
&lt;br&gt;HS=High Speed
&lt;br&gt;HC=High Current 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14752v209%20WE-TMSB_74269200x_0201.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14752v209%20WE-TMSB_74269200x_0201.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBF_HF?"&gt;http://katalog.we-online.de/en/pbs/WE-CBF_HF?&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-01-02&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_WB_HS" package="WE-CBF_HF_0402(W=1.5)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742841160">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/742841160.pdf"/>
<attribute name="IR1" value="100mA"/>
<attribute name="IR2" value="250mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 742841160 "/>
<attribute name="RDC-MAX" value="1.6Ohm"/>
<attribute name="RDC-TYP" value="0.82Ohm"/>
<attribute name="TYPE" value="Wide Band"/>
<attribute name="VALUE" value="600Ohm@100MHz"/>
<attribute name="Z" value="1100Ohm@1GMHz"/>
<attribute name="ZMAX" value="1300Ohm"/>
</technology>
<technology name="_742841210">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/742841210.pdf"/>
<attribute name="IR1" value="50mA"/>
<attribute name="IR2" value="250mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 742841210 "/>
<attribute name="RDC-MAX" value="1.8Ohm"/>
<attribute name="RDC-TYP" value="0.9Ohm"/>
<attribute name="TYPE" value="Wide Band"/>
<attribute name="VALUE" value="1000Ohm@100MHz"/>
<attribute name="Z" value="900Ohm@1GMHz"/>
<attribute name="ZMAX" value="1700Ohm"/>
</technology>
</technologies>
</device>
<device name="_HC" package="WE-CBF_HF_0402(W=2.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742843122">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/742843122.pdf"/>
<attribute name="IR1" value="500mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 742843122 "/>
<attribute name="RDC-MAX" value="0.38Ohm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="220Ohm@100MHz"/>
<attribute name="Z" value="300Ohm@1GMHz"/>
<attribute name="ZMAX" value="550Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
