<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Common Mode Chokes for Low Voltage and Data Lines - WE-CCMF&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020b, 2020-10-29&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CCMF_0504">
<description>&lt;B&gt;WE-CCMF Ceramic Common Mode Filter
&lt;br&gt;Size : 0504
&lt;BR&gt;&lt;/B&gt;Length X Width X Height = 1.25mm X 1mm X 0.8mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-CCMF_0504">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="GND5" direction="pas"/>
<pin name="GND6" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CCMF_0504" prefix="L">
<description>&lt;b&gt;WE-CCMF Ceramic Common Mode Filter
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Compact multilayer common mode choke/filter
&lt;br&gt;High common mode attenuation on WiFi frequencies (&gt; 30 dB @ bandwidth)
&lt;br&gt;Ultra-high-speed differential signal transmission
&lt;br&gt;Differential mode cut-off frequency up to 8 GHz
&lt;br&gt;LTCC based low-loss and highly reliable structure
&lt;br&gt;High thermal stability
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -40 °C up to +85 °C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;High speed data lines
&lt;br&gt;Wireless LAN/WiFi, bluetooth enabled devices (notebooks, laptops, routers with USB interface, IoT devices with WiFi and USB functionalities)
&lt;br&gt;HDMI 1.4 &amp; 2.0, USB 3.1 Gen 1 &amp; 2, USB 3.2, Sata 3.0 &amp; 3.2, Thunderbolt 2 &amp; 3

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161697v209%20test2_Family_WE-CCMF_7480200xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161697v209%20test2_Family_WE-CCMF_7480200xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-CCMF"&gt;https://www.we-online.com/catalog/en/WE-CCMF&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-10-29&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-CCMF_0504"/>
</gates>
<devices>
<device name="" package="WE-CCMF_0504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="GND5" pad="5"/>
<connect gate="G$1" pin="GND6" pad="6"/>
</connects>
<technologies>
<technology name="_748020024">
<attribute name="CUT-OFF-FREQUENCY" value="8GHz"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/748020024.pdf"/>
<attribute name="IL" value="30dB"/>
<attribute name="IR" value="300mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 748020024 "/>
<attribute name="RDC" value="2.5Ohm"/>
<attribute name="RISO" value="100MOhm"/>
<attribute name="VALUE" value="2Ohm@100MHz"/>
<attribute name="VR" value="5Vdc"/>
</technology>
<technology name="_748030024">
<attribute name="CUT-OFF-FREQUENCY" value="12GHz"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/748030024.pdf"/>
<attribute name="IL" value="30dB"/>
<attribute name="IR" value="300mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 748030024 "/>
<attribute name="RDC" value="2.5Ohm"/>
<attribute name="RISO" value="100MOhm"/>
<attribute name="VALUE" value="2Ohm@100MHz"/>
<attribute name="VR" value="5Vdc"/>
</technology>
<technology name="_748032455">
<attribute name="CUT-OFF-FREQUENCY" value="12GHz"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/748032455.pdf"/>
<attribute name="IL" value="20dB"/>
<attribute name="IR" value="300mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 748032455 "/>
<attribute name="RDC" value="2.5Ohm"/>
<attribute name="RISO" value="100MOhm"/>
<attribute name="VALUE" value="1.6Ohm@100MHz"/>
<attribute name="VR" value="5Vdc"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
