<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - EMC Components - Common Mode Chokes for Extra-low Voltage and Data Lines - WE-CNSW&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025b, 2025-06-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CNSW_0805">
<description>&lt;b&gt;WE-CNSW SMT Common Mode Line Filter
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size: 0805, SMT, 4pins
&lt;br&gt;LXWXH=2X1.2X1.2mm</description>
</package>
<package name="WE-CNSW_1210">
<description>&lt;b&gt;WE-CNSW SMT Common Mode Line Filter
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size: 1210, SMT, 4pins
&lt;br&gt;LXWXH=3.2X2.5X2.4mm</description>
</package>
<package name="WE-CNSW_1206">
<description>&lt;b&gt;WE-CNSW SMT Common Mode Line Filter
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size: 1206, SMT, 4pins
&lt;br&gt;LXWXH=3.2X1.6X1.8mm</description>
</package>
<package name="WE-CNSW_0603">
<description>&lt;b&gt;WE-CNSW SMT Common Mode Line Filter
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size: 0603, SMT, 4pins
&lt;br&gt;LXWXH=1.6X0.85X1.1mm</description>
</package>
<package name="WE-CNSW_1812">
<description>&lt;b&gt;WE-CNSW SMT Common Mode Line Filter
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size: 1812, SMT, 4pins
&lt;br&gt;LXWXH=4.5X3.2X2.8mm</description>
</package>
</packages>
<symbols>
<symbol name="CM2W-H">
<description>&lt;b&gt;Common Mode Choke&lt;br&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CNSW_0805" prefix="L">
<description>&lt;b&gt; WE-CNSW SMT Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Current compensated data line filter
&lt;br&gt;High common mode noise suppression at high frequencies
&lt;br&gt;Small influence on high speed signals through winding symmetry
&lt;br&gt;Climatic category 40/105/21 (Size 0603)
&lt;br&gt;Climatic category 40/125/21 (Size 0805/1206/1812)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;USB 2.0
&lt;br&gt;IEEE 1394 (Firewire)
&lt;br&gt;LVDS
&lt;br&gt;High Speed Data Lines
&lt;br&gt;LAN
&lt;br&gt;Size 1812: recommended for CAN bus and CAN FD
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg"&gt;
&lt;img src="https://www.we-online.com/components/media/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CNSW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-CNSW&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu 2019-01-09&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CNSW_0805">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744231061">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744231061?ae"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="400mA"/>
<attribute name="L" value="0.088uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744231061"/>
<attribute name="RDC-MAX" value="0.25Ohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="0.088uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="1.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="67Ohm@100MHz"/>
</technology>
<technology name="_744231091">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744231091?ae"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="370mA"/>
<attribute name="L" value="0.131uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744231091"/>
<attribute name="RDC-MAX" value="0.3Ohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="0.131uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="1.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="90Ohm@100MHz"/>
</technology>
<technology name="_744231121">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744231121?ae"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="370mA"/>
<attribute name="L" value="0.166uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744231121"/>
<attribute name="RDC-MAX" value="0.3Ohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="0.166uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="1.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="120Ohm@100MHz"/>
</technology>
<technology name="_744231181">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744231181?ae"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="330mA"/>
<attribute name="L" value="0.252uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744231181"/>
<attribute name="RDC-MAX" value="0.35Ohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="0.252uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="1.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="180Ohm@100MHz"/>
</technology>
<technology name="_744231261">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744231261?ae"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="300mA"/>
<attribute name="L" value="0.367uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744231261"/>
<attribute name="RDC-MAX" value="0.4Ohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="0.367uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="1.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="260Ohm@100MHz"/>
</technology>
<technology name="_744231371">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744231371?ae"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="280mA"/>
<attribute name="L" value="0.478uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744231371"/>
<attribute name="RDC-MAX" value="0.45Ohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="0.478uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="1.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="370Ohm@100MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CNSW_1210" prefix="L">
<description>&lt;b&gt; WE-CNSW SMT Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Current compensated data line filter
&lt;br&gt;High common mode noise suppression at high frequencies
&lt;br&gt;Small influence on high speed signals through winding symmetry
&lt;br&gt;Climatic category 40/105/21 (Size 0603)
&lt;br&gt;Climatic category 40/125/21 (Size 0805/1206/1812)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;USB 2.0
&lt;br&gt;IEEE 1394 (Firewire)
&lt;br&gt;LVDS
&lt;br&gt;High Speed Data Lines
&lt;br&gt;LAN
&lt;br&gt;Size 1812: recommended for CAN bus and CAN FD
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg"&gt;
&lt;img src="https://www.we-online.com/components/media/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CNSW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-CNSW&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-23&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CNSW_1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="3"/>
</connects>
<technologies>
<technology name="_744234101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744234101?ae"/>
<attribute name="HEIGHT" value="2.4mm"/>
<attribute name="IR" value="200mA"/>
<attribute name="L" value="100uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744234101"/>
<attribute name="RDC-MAX" value="3Ohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="2.5mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="5500Ohm@10MHz"/>
</technology>
<technology name="_744234510">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744234510?ae"/>
<attribute name="HEIGHT" value="2.4mm"/>
<attribute name="IR" value="400mA"/>
<attribute name="L" value="51uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744234510"/>
<attribute name="RDC-MAX" value="1.1Ohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="51uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="2.5mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="2800Ohm@10MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CNSW_1206" prefix="L">
<description>&lt;b&gt; WE-CNSW SMT Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Current compensated data line filter
&lt;br&gt;High common mode noise suppression at high frequencies
&lt;br&gt;Small influence on high speed signals through winding symmetry
&lt;br&gt;Climatic category 40/105/21 (Size 0603)
&lt;br&gt;Climatic category 40/125/21 (Size 0805/1206/1812)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;USB 2.0
&lt;br&gt;IEEE 1394 (Firewire)
&lt;br&gt;LVDS
&lt;br&gt;High Speed Data Lines
&lt;br&gt;LAN
&lt;br&gt;Size 1812: recommended for CAN bus and CAN FD
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg"&gt;
&lt;img src="https://www.we-online.com/components/media/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CNSW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-CNSW&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu 2019-01-09&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CNSW_1206">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744232090">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744232090?ae"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="IR" value="370mA"/>
<attribute name="L" value="0.111uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744232090"/>
<attribute name="RDC-MAX" value="0.3Ohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="0.111uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="90Ohm@100MHz"/>
</technology>
<technology name="_744232101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744232101?ae"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="IR" value="90mA"/>
<attribute name="L" value="105.3uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744232101"/>
<attribute name="RDC-MAX" value="5.5Ohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="105.3uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="6000Ohm@10MHz"/>
</technology>
<technology name="_744232102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744232102?ae"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="IR" value="230mA"/>
<attribute name="L" value="1.263uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744232102"/>
<attribute name="RDC-MAX" value="1Ohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1.263uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="1000Ohm@100MHz"/>
</technology>
<technology name="_744232161">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744232161?ae"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="IR" value="340mA"/>
<attribute name="L" value="0.196uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744232161"/>
<attribute name="RDC-MAX" value="0.4Ohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="0.196uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="160Ohm@100MHz"/>
</technology>
<technology name="_744232222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744232222?ae"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="IR" value="200mA"/>
<attribute name="L" value="2.578uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744232222"/>
<attribute name="RDC-MAX" value="1.2Ohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.578uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="2200Ohm@100MHz"/>
</technology>
<technology name="_744232261">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744232261?ae"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="IR" value="310mA"/>
<attribute name="L" value="0.304uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744232261"/>
<attribute name="RDC-MAX" value="0.5Ohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="0.304uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="260Ohm@100MHz"/>
</technology>
<technology name="_744232601">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744232601?ae"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="IR" value="260mA"/>
<attribute name="L" value="0.3621uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744232601"/>
<attribute name="RDC-MAX" value="0.8Ohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="0.3621uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="600Ohm@100MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CNSW_1812" prefix="L">
<description>&lt;b&gt; WE-CNSW SMT Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Current compensated data line filter
&lt;br&gt;High common mode noise suppression at high frequencies
&lt;br&gt;Small influence on high speed signals through winding symmetry
&lt;br&gt;Climatic category 40/105/21 (Size 0603)
&lt;br&gt;Climatic category 40/125/21 (Size 0805/1206/1812)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;USB 2.0
&lt;br&gt;IEEE 1394 (Firewire)
&lt;br&gt;LVDS
&lt;br&gt;High Speed Data Lines
&lt;br&gt;LAN
&lt;br&gt;Size 1812: recommended for CAN bus and CAN FD
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg"&gt;
&lt;img src="https://www.we-online.com/components/media/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CNSW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-CNSW&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu 2019-01-09&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CNSW_1812">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744235101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744235101?ae"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IR" value="150mA"/>
<attribute name="L" value="100uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744235101"/>
<attribute name="RDC-MAX" value="2Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VR" value="60V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="5000Ohm@10MHz"/>
</technology>
<technology name="_744235110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744235110?ae"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IR" value="450mA"/>
<attribute name="L" value="11uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744235110"/>
<attribute name="RDC-MAX" value="0.8Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="11uH"/>
<attribute name="VR" value="60V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="5000Ohm@100MHz"/>
</technology>
<technology name="_744235220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744235220?ae"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IR" value="250mA"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744235220"/>
<attribute name="RDC-MAX" value="2.65Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VR" value="60V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="8000Ohm@100MHz"/>
</technology>
<technology name="_744235251">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744235251?ae"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IR" value="200mA"/>
<attribute name="L" value="250uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744235251"/>
<attribute name="RDC-MAX" value="1.6Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="250uH"/>
<attribute name="VR" value="60V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="10000Ohm@10MHz"/>
</technology>
<technology name="_744235510">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744235510?ae"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IR" value="200mA"/>
<attribute name="L" value="51uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744235510"/>
<attribute name="RDC-MAX" value="1Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="51uH"/>
<attribute name="VR" value="60V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="3000Ohm@10MHz"/>
</technology>
<technology name="_744235601">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744235601?ae"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IR" value="1200mA"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744235601"/>
<attribute name="RDC-MAX" value="0.1Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VR" value="60V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="600Ohm@100MHz"/>
</technology>
<technology name="_744235801">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744235801?ae"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IR" value="1000mA"/>
<attribute name="L" value="1.3uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744235801"/>
<attribute name="RDC-MAX" value="0.12Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1.3uH"/>
<attribute name="VR" value="60V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="800Ohm@100MHz"/>
</technology>
<technology name="_744235900">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744235900?ae"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="IR" value="2000mA"/>
<attribute name="L" value="0.3uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744235900"/>
<attribute name="RDC-MAX" value="0.05Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="0.3uH"/>
<attribute name="VR" value="60V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="90Ohm@100MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CNSW_0603" prefix="L">
<description>&lt;b&gt; WE-CNSW SMT Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Current compensated data line filter
&lt;br&gt;High common mode noise suppression at high frequencies
&lt;br&gt;Small influence on high speed signals through winding symmetry
&lt;br&gt;Climatic category 40/105/21 (Size 0603)
&lt;br&gt;Climatic category 40/125/21 (Size 0805/1206/1812)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;USB 2.0
&lt;br&gt;IEEE 1394 (Firewire)
&lt;br&gt;LVDS
&lt;br&gt;High Speed Data Lines
&lt;br&gt;LAN
&lt;br&gt;Size 1812: recommended for CAN bus and CAN FD
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg"&gt;
&lt;img src="https://www.we-online.com/components/media/o14771v209%20we-cnsw_stroko_smd_gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CNSW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-CNSW&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu 2019-01-09&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CNSW_0603">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744230121">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744230121?ae"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="IR" value="450mA"/>
<attribute name="L" value="0.146uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744230121"/>
<attribute name="RDC-MAX" value="0.175Ohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="0.146uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="0.85mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="120Ohm@100MHz"/>
</technology>
<technology name="_744230181">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744230181?ae"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="IR" value="400mA"/>
<attribute name="L" value="0.22uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744230181"/>
<attribute name="RDC-MAX" value="0.21Ohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="0.85mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="180Ohm@100MHz"/>
</technology>
<technology name="_744230220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744230220?ae"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="IR" value="800mA"/>
<attribute name="L" value="0.027uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744230220"/>
<attribute name="RDC-MAX" value="0.08Ohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="0.027uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="0.85mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="22Ohm@100MHz"/>
</technology>
<technology name="_744230251">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744230251?ae"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="IR" value="350mA"/>
<attribute name="L" value="0.279uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744230251"/>
<attribute name="RDC-MAX" value="0.28Ohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="0.279uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="0.85mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="250Ohm@100MHz"/>
</technology>
<technology name="_744230450">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744230450?ae"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="IR" value="650mA"/>
<attribute name="L" value="0.056uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744230450"/>
<attribute name="RDC-MAX" value="0.11Ohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="0.056uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="0.85mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="45Ohm@100MHz"/>
</technology>
<technology name="_744230900">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744230900?ae"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="IR" value="550mA"/>
<attribute name="L" value="0.134uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744230900"/>
<attribute name="RDC-MAX" value="0.145Ohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="0.134uH"/>
<attribute name="VR" value="50V"/>
<attribute name="VT" value="125VAC"/>
<attribute name="WIDTH" value="0.85mm"/>
<attribute name="WINDING-STYLE" value="bifiliar"/>
<attribute name="Z" value="90Ohm@100MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
