<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Signal &amp; Communications - Filtered Connectors - WE-D-SUB&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-D-SUB_SMD90_240617113">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;&lt;/b&gt;9 Poles , Female</description>
</package>
<package name="WE-D-SUB_SMD90_244617113">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;&lt;/b&gt;25 Poles , Female</description>
</package>
<package name="WE-D-SUB_THT_TH_210611003">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;9 Poles , Female
&lt;BR&gt;TH means Size Through Hole</description>
</package>
<package name="WE-D-SUB_SMD90_242617113">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;&lt;/b&gt;15 Poles , Female</description>
</package>
<package name="WE-D-SUB_THT90_EC_214612013">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;25 Poles , Female&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_THT_TH_216111003">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;37 Poles , Male
&lt;BR&gt;TH means Size Through Hole</description>
</package>
<package name="WE-D-SUB_SMD90_246617113">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;&lt;/b&gt;37 Poles , Female</description>
</package>
<package name="WE-D-SUB_THT90_EC_210112013">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;9 Poles , Male&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_THT_UNC4/40_210611023">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;9 Poles , Female
&lt;BR&gt;UNC 4/40  means Size UNC 4/40</description>
</package>
<package name="WE-D-SUB_THT_TH_214111003">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;25 Poles , Male
&lt;BR&gt;TH means Size Through Hole</description>
</package>
<package name="WE-D-SUB_THT90_EC_210612013">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;9 Poles , Female&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_THT_TH_214611003">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;25 Poles , Female
&lt;BR&gt;TH means Size Through Hole</description>
</package>
<package name="WE-D-SUB_THT_UNC4/40_214111023">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;25 Poles , Male
&lt;BR&gt;UNC 4/40  means Size UNC 4/40</description>
</package>
<package name="WE-D-SUB_THT_TH_216611003">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;37 Poles , Female
&lt;BR&gt;TH means Size Through Hole</description>
</package>
<package name="WE-D-SUB_THT90_EC_214112013">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;25 Poles , Male&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_THT_UNC4/40_212111023">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;15 Poles , Male
&lt;BR&gt;UNC 4/40  means Size UNC 4/40</description>
</package>
<package name="WE-D-SUB_THT_UNC4/40_214611023">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;25 Poles , Female
&lt;BR&gt;UNC 4/40  means Size UNC 4/40</description>
</package>
<package name="WE-D-SUB_THT_TH_212111003">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;15 Poles , Male
&lt;BR&gt;TH means Size Through Hole</description>
</package>
<package name="WE-D-SUB_THT90_EC_212112013">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;15 Poles , Male&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_THT_TH_212611003">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;15 Poles , Female
&lt;BR&gt;TH means Size Through Hole</description>
</package>
<package name="WE-D-SUB_THT90_MS_216112043">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;37 Poles , Male&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_THT_UNC4/40_216111023">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;37 Poles , Male
&lt;BR&gt;UNC 4/40  means Size UNC 4/40</description>
</package>
<package name="WE-D-SUB_THT90_MS_216612043">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;37 Poles , Female&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_THT90_MS_214112043">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;25 Poles , Male&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_THT_UNC4/40_216611023">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;37 Poles , Female
&lt;BR&gt;UNC 4/40  means Size UNC 4/40</description>
</package>
<package name="WE-D-SUB_THT90_MS_210112043">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;9 Poles , Male&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_THT90_MS_214612043">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;25 Poles , Female&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_THT90_MS_212112043">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;15 Poles , Male&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_SMD90_246117113">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;&lt;/b&gt;37 Poles , Male</description>
</package>
<package name="WE-D-SUB_THT90_EC_216612013">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;37 Poles , Female&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_SMD90_244117113">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;&lt;/b&gt;25 Poles , Male</description>
</package>
<package name="WE-D-SUB_THT90_MS_210612043">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;9 Poles , Female&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_SMD90_240117113">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;&lt;/b&gt;9 Poles , Male</description>
</package>
<package name="WE-D-SUB_THT_TH_210111003">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;9 Poles , Male
&lt;BR&gt;TH means Size Through Hole</description>
</package>
<package name="WE-D-SUB_THT90_MS_212612043">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;15 Poles , Female&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_THT_UNC4/40_212611023">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;15 Poles , Female
&lt;BR&gt;UNC 4/40  means Size UNC 4/40</description>
</package>
<package name="WE-D-SUB_THT90_EC_212612013">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;15 Poles , Female&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_THT_UNC4/40_210111023">
<description>&lt;b&gt;WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;&lt;/b&gt;9 Poles , Male
&lt;BR&gt;UNC 4/40  means Size UNC 4/40</description>
</package>
<package name="WE-D-SUB_THT90_EC_216112013">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° THT
&lt;br&gt;&lt;/b&gt;37 Poles , Male&lt;br&gt;
&lt;BR&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip</description>
</package>
<package name="WE-D-SUB_SMD90_242117113">
<description>&lt;b&gt;WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;&lt;/b&gt;15 Poles , Male</description>
</package>
</packages>
<symbols>
<symbol name="SMD_9PIN_FEMALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="THT_9PIN_FEMALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="THT_25PIN_FEMALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="SMD_37PIN_FAMALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="THT_37PIN_MALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="THT_25PIN_MALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="SMD_15PIN_FEMALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="THT_37PIN_FEMALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="THT_15PIN_MALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="SMD_25PIN_MALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="THT_9PIN_MALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="SMD_25PIN_FEMALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="THT_15PIN_FEMALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="SMD_15PIN_MALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="SMD_9PIN_MALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="SMD_37PIN_MALE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-D-SUB_SMD90_240617113" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;Low size: 6.3 mm
&lt;br&gt;Rated voltage: 125 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="SMD_9PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_SMD90_240617113">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="8"/>
<connect gate="G$1" pin="8" pad="7"/>
<connect gate="G$1" pin="9" pad="6"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2 Z3 Z4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/240617113.pdf"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 240617113 "/>
<attribute name="POLES" value=" 9 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_SMD90_244617113" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;Low size: 6.3 mm
&lt;br&gt;Rated voltage: 125 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="SMD_25PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_SMD90_244617113">
<connects>
<connect gate="G$1" pin="1" pad="13"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="11" pad="3"/>
<connect gate="G$1" pin="12" pad="2"/>
<connect gate="G$1" pin="13" pad="1"/>
<connect gate="G$1" pin="14" pad="25"/>
<connect gate="G$1" pin="15" pad="24"/>
<connect gate="G$1" pin="16" pad="23"/>
<connect gate="G$1" pin="17" pad="22"/>
<connect gate="G$1" pin="18" pad="21"/>
<connect gate="G$1" pin="19" pad="20"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="20" pad="19"/>
<connect gate="G$1" pin="21" pad="18"/>
<connect gate="G$1" pin="22" pad="17"/>
<connect gate="G$1" pin="23" pad="16"/>
<connect gate="G$1" pin="24" pad="15"/>
<connect gate="G$1" pin="25" pad="14"/>
<connect gate="G$1" pin="3" pad="11"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="5"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2 Z3 Z4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/244617113.pdf"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 244617113 "/>
<attribute name="POLES" value=" 25 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_TH_210611003" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;TH means Size Through Hole
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_9PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_TH_210611003">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="8"/>
<connect gate="G$1" pin="8" pad="7"/>
<connect gate="G$1" pin="9" pad="6"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/210611003.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 210611003 "/>
<attribute name="POLES" value=" 9 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_EC_214612013" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_25PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_EC_214612013">
<connects>
<connect gate="G$1" pin="1" pad="13"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="11" pad="3"/>
<connect gate="G$1" pin="12" pad="2"/>
<connect gate="G$1" pin="13" pad="1"/>
<connect gate="G$1" pin="14" pad="25"/>
<connect gate="G$1" pin="15" pad="24"/>
<connect gate="G$1" pin="16" pad="23"/>
<connect gate="G$1" pin="17" pad="22"/>
<connect gate="G$1" pin="18" pad="21"/>
<connect gate="G$1" pin="19" pad="20"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="20" pad="19"/>
<connect gate="G$1" pin="21" pad="18"/>
<connect gate="G$1" pin="22" pad="17"/>
<connect gate="G$1" pin="23" pad="16"/>
<connect gate="G$1" pin="24" pad="15"/>
<connect gate="G$1" pin="25" pad="14"/>
<connect gate="G$1" pin="3" pad="11"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="5"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/214612013.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 214612013 "/>
<attribute name="POLES" value=" 25 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_TH_216111003" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;TH means Size Through Hole
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_37PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_TH_216111003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/216111003.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 216111003 "/>
<attribute name="POLES" value=" 37 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_SMD90_246617113" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;Low size: 6.3 mm
&lt;br&gt;Rated voltage: 125 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="SMD_37PIN_FAMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_SMD90_246617113">
<connects>
<connect gate="G$1" pin="1" pad="19"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="9"/>
<connect gate="G$1" pin="12" pad="8"/>
<connect gate="G$1" pin="13" pad="7"/>
<connect gate="G$1" pin="14" pad="6"/>
<connect gate="G$1" pin="15" pad="5"/>
<connect gate="G$1" pin="16" pad="4"/>
<connect gate="G$1" pin="17" pad="3"/>
<connect gate="G$1" pin="18" pad="2"/>
<connect gate="G$1" pin="19" pad="1"/>
<connect gate="G$1" pin="2" pad="18"/>
<connect gate="G$1" pin="20" pad="37"/>
<connect gate="G$1" pin="21" pad="36"/>
<connect gate="G$1" pin="22" pad="35"/>
<connect gate="G$1" pin="23" pad="34"/>
<connect gate="G$1" pin="24" pad="33"/>
<connect gate="G$1" pin="25" pad="32"/>
<connect gate="G$1" pin="26" pad="31"/>
<connect gate="G$1" pin="27" pad="30"/>
<connect gate="G$1" pin="28" pad="29"/>
<connect gate="G$1" pin="29" pad="28"/>
<connect gate="G$1" pin="3" pad="17"/>
<connect gate="G$1" pin="30" pad="27"/>
<connect gate="G$1" pin="31" pad="26"/>
<connect gate="G$1" pin="32" pad="25"/>
<connect gate="G$1" pin="33" pad="24"/>
<connect gate="G$1" pin="34" pad="23"/>
<connect gate="G$1" pin="35" pad="22"/>
<connect gate="G$1" pin="36" pad="21"/>
<connect gate="G$1" pin="37" pad="20"/>
<connect gate="G$1" pin="4" pad="16"/>
<connect gate="G$1" pin="5" pad="15"/>
<connect gate="G$1" pin="6" pad="14"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="12"/>
<connect gate="G$1" pin="9" pad="11"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2 Z3 Z4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/246617113.pdf"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 246617113 "/>
<attribute name="POLES" value=" 37 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_EC_210612013" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_9PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_EC_210612013">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="8"/>
<connect gate="G$1" pin="8" pad="7"/>
<connect gate="G$1" pin="9" pad="6"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/210612013.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 210612013 "/>
<attribute name="POLES" value=" 9 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_UNC4/40_210611023" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;UNC 4/40  means Size UNC 4/40 
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_9PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_UNC4/40_210611023">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="8"/>
<connect gate="G$1" pin="8" pad="7"/>
<connect gate="G$1" pin="9" pad="6"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/210611023.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 210611023 "/>
<attribute name="POLES" value=" 9 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_EC_210112013" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_9PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_EC_210112013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/210112013.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 210112013 "/>
<attribute name="POLES" value=" 9 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_TH_214111003" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;TH means Size Through Hole
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_25PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_TH_214111003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/214111003.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 214111003 "/>
<attribute name="POLES" value=" 25 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_TH_214611003" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;TH means Size Through Hole
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_25PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_TH_214611003">
<connects>
<connect gate="G$1" pin="1" pad="13"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="11" pad="3"/>
<connect gate="G$1" pin="12" pad="2"/>
<connect gate="G$1" pin="13" pad="1"/>
<connect gate="G$1" pin="14" pad="25"/>
<connect gate="G$1" pin="15" pad="24"/>
<connect gate="G$1" pin="16" pad="23"/>
<connect gate="G$1" pin="17" pad="22"/>
<connect gate="G$1" pin="18" pad="21"/>
<connect gate="G$1" pin="19" pad="20"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="20" pad="19"/>
<connect gate="G$1" pin="21" pad="18"/>
<connect gate="G$1" pin="22" pad="17"/>
<connect gate="G$1" pin="23" pad="16"/>
<connect gate="G$1" pin="24" pad="15"/>
<connect gate="G$1" pin="25" pad="14"/>
<connect gate="G$1" pin="3" pad="11"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="5"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/214611003.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 214611003 "/>
<attribute name="POLES" value=" 25 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_TH_216611003" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;TH means Size Through Hole
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_37PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_TH_216611003">
<connects>
<connect gate="G$1" pin="1" pad="19"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="9"/>
<connect gate="G$1" pin="12" pad="8"/>
<connect gate="G$1" pin="13" pad="7"/>
<connect gate="G$1" pin="14" pad="6"/>
<connect gate="G$1" pin="15" pad="5"/>
<connect gate="G$1" pin="16" pad="4"/>
<connect gate="G$1" pin="17" pad="3"/>
<connect gate="G$1" pin="18" pad="2"/>
<connect gate="G$1" pin="19" pad="1"/>
<connect gate="G$1" pin="2" pad="18"/>
<connect gate="G$1" pin="20" pad="37"/>
<connect gate="G$1" pin="21" pad="36"/>
<connect gate="G$1" pin="22" pad="35"/>
<connect gate="G$1" pin="23" pad="34"/>
<connect gate="G$1" pin="24" pad="33"/>
<connect gate="G$1" pin="25" pad="32"/>
<connect gate="G$1" pin="26" pad="31"/>
<connect gate="G$1" pin="27" pad="30"/>
<connect gate="G$1" pin="28" pad="29"/>
<connect gate="G$1" pin="29" pad="28"/>
<connect gate="G$1" pin="3" pad="17"/>
<connect gate="G$1" pin="30" pad="27"/>
<connect gate="G$1" pin="31" pad="26"/>
<connect gate="G$1" pin="32" pad="25"/>
<connect gate="G$1" pin="33" pad="24"/>
<connect gate="G$1" pin="34" pad="23"/>
<connect gate="G$1" pin="35" pad="22"/>
<connect gate="G$1" pin="36" pad="21"/>
<connect gate="G$1" pin="37" pad="20"/>
<connect gate="G$1" pin="4" pad="16"/>
<connect gate="G$1" pin="5" pad="15"/>
<connect gate="G$1" pin="6" pad="14"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="12"/>
<connect gate="G$1" pin="9" pad="11"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/216611003.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 216611003 "/>
<attribute name="POLES" value=" 37 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_SMD90_242617113" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;Low size: 6.3 mm
&lt;br&gt;Rated voltage: 125 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="SMD_15PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_SMD90_242617113">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="10" pad="14"/>
<connect gate="G$1" pin="11" pad="13"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="11"/>
<connect gate="G$1" pin="14" pad="10"/>
<connect gate="G$1" pin="15" pad="9"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="9" pad="15"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2 Z3 Z4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/242617113.pdf"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 242617113 "/>
<attribute name="POLES" value=" 15 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_EC_214112013" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_25PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_EC_214112013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/214112013.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 214112013 "/>
<attribute name="POLES" value=" 25 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_UNC4/40_214611023" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;UNC 4/40  means Size UNC 4/40 
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_25PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_UNC4/40_214611023">
<connects>
<connect gate="G$1" pin="1" pad="13"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="11" pad="3"/>
<connect gate="G$1" pin="12" pad="2"/>
<connect gate="G$1" pin="13" pad="1"/>
<connect gate="G$1" pin="14" pad="25"/>
<connect gate="G$1" pin="15" pad="24"/>
<connect gate="G$1" pin="16" pad="23"/>
<connect gate="G$1" pin="17" pad="22"/>
<connect gate="G$1" pin="18" pad="21"/>
<connect gate="G$1" pin="19" pad="20"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="20" pad="19"/>
<connect gate="G$1" pin="21" pad="18"/>
<connect gate="G$1" pin="22" pad="17"/>
<connect gate="G$1" pin="23" pad="16"/>
<connect gate="G$1" pin="24" pad="15"/>
<connect gate="G$1" pin="25" pad="14"/>
<connect gate="G$1" pin="3" pad="11"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="5"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/214611023.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 214611023 "/>
<attribute name="POLES" value=" 25 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_TH_212111003" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;TH means Size Through Hole
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_15PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_TH_212111003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/212111003.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 212111003 "/>
<attribute name="POLES" value=" 15 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_EC_212112013" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_15PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_EC_212112013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/212112013.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 212112013 "/>
<attribute name="POLES" value=" 15 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_UNC4/40_212111023" prefix="J">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;UNC 4/40  means Size UNC 4/40 
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_15PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_UNC4/40_212111023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/212111023.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 212111023 "/>
<attribute name="POLES" value=" 15 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_UNC4/40_216111023" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;UNC 4/40  means Size UNC 4/40 
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_37PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_UNC4/40_216111023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/216111023.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 216111023 "/>
<attribute name="POLES" value=" 37 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_UNC4/40_214111023" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;UNC 4/40  means Size UNC 4/40 
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_25PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_UNC4/40_214111023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/214111023.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 214111023 "/>
<attribute name="POLES" value=" 25 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_MS_216112043" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_37PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_MS_216112043">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/216112043.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 216112043 "/>
<attribute name="POLES" value=" 37 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_MS_216612043" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_37PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_MS_216612043">
<connects>
<connect gate="G$1" pin="1" pad="19"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="9"/>
<connect gate="G$1" pin="12" pad="8"/>
<connect gate="G$1" pin="13" pad="7"/>
<connect gate="G$1" pin="14" pad="6"/>
<connect gate="G$1" pin="15" pad="5"/>
<connect gate="G$1" pin="16" pad="4"/>
<connect gate="G$1" pin="17" pad="3"/>
<connect gate="G$1" pin="18" pad="2"/>
<connect gate="G$1" pin="19" pad="1"/>
<connect gate="G$1" pin="2" pad="18"/>
<connect gate="G$1" pin="20" pad="37"/>
<connect gate="G$1" pin="21" pad="36"/>
<connect gate="G$1" pin="22" pad="35"/>
<connect gate="G$1" pin="23" pad="34"/>
<connect gate="G$1" pin="24" pad="33"/>
<connect gate="G$1" pin="25" pad="32"/>
<connect gate="G$1" pin="26" pad="31"/>
<connect gate="G$1" pin="27" pad="30"/>
<connect gate="G$1" pin="28" pad="29"/>
<connect gate="G$1" pin="29" pad="28"/>
<connect gate="G$1" pin="3" pad="17"/>
<connect gate="G$1" pin="30" pad="27"/>
<connect gate="G$1" pin="31" pad="26"/>
<connect gate="G$1" pin="32" pad="25"/>
<connect gate="G$1" pin="33" pad="24"/>
<connect gate="G$1" pin="34" pad="23"/>
<connect gate="G$1" pin="35" pad="22"/>
<connect gate="G$1" pin="36" pad="21"/>
<connect gate="G$1" pin="37" pad="20"/>
<connect gate="G$1" pin="4" pad="16"/>
<connect gate="G$1" pin="5" pad="15"/>
<connect gate="G$1" pin="6" pad="14"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="12"/>
<connect gate="G$1" pin="9" pad="11"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/216612043.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 216612043 "/>
<attribute name="POLES" value=" 37 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_TH_212611003" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;TH means Size Through Hole
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_15PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_TH_212611003">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="10" pad="14"/>
<connect gate="G$1" pin="11" pad="13"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="11"/>
<connect gate="G$1" pin="14" pad="10"/>
<connect gate="G$1" pin="15" pad="9"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="9" pad="15"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/212611003.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 212611003 "/>
<attribute name="POLES" value=" 15 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_MS_214112043" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ��C: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_25PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_MS_214112043">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/214112043.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 214112043 "/>
<attribute name="POLES" value=" 25 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_MS_210112043" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_9PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_MS_210112043">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/210112043.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 210112043 "/>
<attribute name="POLES" value=" 9 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_UNC4/40_216611023" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;UNC 4/40  means Size UNC 4/40 
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_37PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_UNC4/40_216611023">
<connects>
<connect gate="G$1" pin="1" pad="19"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="9"/>
<connect gate="G$1" pin="12" pad="8"/>
<connect gate="G$1" pin="13" pad="7"/>
<connect gate="G$1" pin="14" pad="6"/>
<connect gate="G$1" pin="15" pad="5"/>
<connect gate="G$1" pin="16" pad="4"/>
<connect gate="G$1" pin="17" pad="3"/>
<connect gate="G$1" pin="18" pad="2"/>
<connect gate="G$1" pin="19" pad="1"/>
<connect gate="G$1" pin="2" pad="18"/>
<connect gate="G$1" pin="20" pad="37"/>
<connect gate="G$1" pin="21" pad="36"/>
<connect gate="G$1" pin="22" pad="35"/>
<connect gate="G$1" pin="23" pad="34"/>
<connect gate="G$1" pin="24" pad="33"/>
<connect gate="G$1" pin="25" pad="32"/>
<connect gate="G$1" pin="26" pad="31"/>
<connect gate="G$1" pin="27" pad="30"/>
<connect gate="G$1" pin="28" pad="29"/>
<connect gate="G$1" pin="29" pad="28"/>
<connect gate="G$1" pin="3" pad="17"/>
<connect gate="G$1" pin="30" pad="27"/>
<connect gate="G$1" pin="31" pad="26"/>
<connect gate="G$1" pin="32" pad="25"/>
<connect gate="G$1" pin="33" pad="24"/>
<connect gate="G$1" pin="34" pad="23"/>
<connect gate="G$1" pin="35" pad="22"/>
<connect gate="G$1" pin="36" pad="21"/>
<connect gate="G$1" pin="37" pad="20"/>
<connect gate="G$1" pin="4" pad="16"/>
<connect gate="G$1" pin="5" pad="15"/>
<connect gate="G$1" pin="6" pad="14"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="12"/>
<connect gate="G$1" pin="9" pad="11"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/216611023.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 216611023 "/>
<attribute name="POLES" value=" 37 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_MS_212112043" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_15PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_MS_212112043">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/212112043.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 212112043 "/>
<attribute name="POLES" value=" 15 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_SMD90_246117113" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;Low size: 6.3 mm
&lt;br&gt;Rated voltage: 125 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="SMD_37PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_SMD90_246117113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2 Z3 Z4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/246117113.pdf"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 246117113 "/>
<attribute name="POLES" value=" 37 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_MS_214612043" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_25PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_MS_214612043">
<connects>
<connect gate="G$1" pin="1" pad="13"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="11" pad="3"/>
<connect gate="G$1" pin="12" pad="2"/>
<connect gate="G$1" pin="13" pad="1"/>
<connect gate="G$1" pin="14" pad="25"/>
<connect gate="G$1" pin="15" pad="24"/>
<connect gate="G$1" pin="16" pad="23"/>
<connect gate="G$1" pin="17" pad="22"/>
<connect gate="G$1" pin="18" pad="21"/>
<connect gate="G$1" pin="19" pad="20"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="20" pad="19"/>
<connect gate="G$1" pin="21" pad="18"/>
<connect gate="G$1" pin="22" pad="17"/>
<connect gate="G$1" pin="23" pad="16"/>
<connect gate="G$1" pin="24" pad="15"/>
<connect gate="G$1" pin="25" pad="14"/>
<connect gate="G$1" pin="3" pad="11"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="5"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/214612043.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 214612043 "/>
<attribute name="POLES" value=" 25 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_EC_216612013" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_37PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_EC_216612013">
<connects>
<connect gate="G$1" pin="1" pad="19"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="9"/>
<connect gate="G$1" pin="12" pad="8"/>
<connect gate="G$1" pin="13" pad="7"/>
<connect gate="G$1" pin="14" pad="6"/>
<connect gate="G$1" pin="15" pad="5"/>
<connect gate="G$1" pin="16" pad="4"/>
<connect gate="G$1" pin="17" pad="3"/>
<connect gate="G$1" pin="18" pad="2"/>
<connect gate="G$1" pin="19" pad="1"/>
<connect gate="G$1" pin="2" pad="18"/>
<connect gate="G$1" pin="20" pad="37"/>
<connect gate="G$1" pin="21" pad="36"/>
<connect gate="G$1" pin="22" pad="35"/>
<connect gate="G$1" pin="23" pad="34"/>
<connect gate="G$1" pin="24" pad="33"/>
<connect gate="G$1" pin="25" pad="32"/>
<connect gate="G$1" pin="26" pad="31"/>
<connect gate="G$1" pin="27" pad="30"/>
<connect gate="G$1" pin="28" pad="29"/>
<connect gate="G$1" pin="29" pad="28"/>
<connect gate="G$1" pin="3" pad="17"/>
<connect gate="G$1" pin="30" pad="27"/>
<connect gate="G$1" pin="31" pad="26"/>
<connect gate="G$1" pin="32" pad="25"/>
<connect gate="G$1" pin="33" pad="24"/>
<connect gate="G$1" pin="34" pad="23"/>
<connect gate="G$1" pin="35" pad="22"/>
<connect gate="G$1" pin="36" pad="21"/>
<connect gate="G$1" pin="37" pad="20"/>
<connect gate="G$1" pin="4" pad="16"/>
<connect gate="G$1" pin="5" pad="15"/>
<connect gate="G$1" pin="6" pad="14"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="12"/>
<connect gate="G$1" pin="9" pad="11"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/216612013.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 216612013 "/>
<attribute name="POLES" value=" 37 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_SMD90_244117113" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;Low size: 6.3 mm
&lt;br&gt;Rated voltage: 125 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="SMD_25PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_SMD90_244117113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2 Z3 Z4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/244117113.pdf"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 244117113 "/>
<attribute name="POLES" value=" 25 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_SMD90_240117113" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;Low size: 6.3 mm
&lt;br&gt;Rated voltage: 125 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="SMD_9PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_SMD90_240117113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2 Z3 Z4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/240117113.pdf"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 240117113 "/>
<attribute name="POLES" value=" 9 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_MS_210612043" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_9PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_MS_210612043">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="8"/>
<connect gate="G$1" pin="8" pad="7"/>
<connect gate="G$1" pin="9" pad="6"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/210612043.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 210612043 "/>
<attribute name="POLES" value=" 9 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_MS_212612043" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_15PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_MS_212612043">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="10" pad="14"/>
<connect gate="G$1" pin="11" pad="13"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="11"/>
<connect gate="G$1" pin="14" pad="10"/>
<connect gate="G$1" pin="15" pad="9"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="9" pad="15"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/212612043.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 212612043 "/>
<attribute name="POLES" value=" 15 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_TH_210111003" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;TH means Size Through Hole
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_9PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_TH_210111003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/210111003.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 210111003 "/>
<attribute name="POLES" value=" 9 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_UNC4/40_212611023" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;UNC 4/40  means Size UNC 4/40 
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_15PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_UNC4/40_212611023">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="10" pad="14"/>
<connect gate="G$1" pin="11" pad="13"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="11"/>
<connect gate="G$1" pin="14" pad="10"/>
<connect gate="G$1" pin="15" pad="9"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="9" pad="15"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/212611023.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 212611023 "/>
<attribute name="POLES" value=" 15 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_EC_212612013" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_15PIN_FEMALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_EC_212612013">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="10" pad="14"/>
<connect gate="G$1" pin="11" pad="13"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="11"/>
<connect gate="G$1" pin="14" pad="10"/>
<connect gate="G$1" pin="15" pad="9"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="9" pad="15"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/212612013.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 212612013 "/>
<attribute name="POLES" value=" 15 "/>
<attribute name="TYPE" value="Female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT_UNC4/40_210111023" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Solder Pin Straight
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of UNC 4/40 or through hole
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;UNC 4/40  means Size UNC 4/40 
&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14707v209%20Family_D-SUB-Filter_mit_geradem_Loetstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_9PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT_UNC4/40_210111023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/210111023.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 210111023 "/>
<attribute name="POLES" value=" 9 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_SMD90_242117113" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° SMT
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;Low size: 6.3 mm
&lt;br&gt;Rated voltage: 125 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14706v209%20Family_240117113_240617113.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD"&gt;https://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90-SMD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-10&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="SMD_15PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_SMD90_242117113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2 Z3 Z4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/242117113.pdf"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 242117113 "/>
<attribute name="POLES" value=" 15 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-D-SUB_THT90_EC_216112013" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-D-SUB Filter Bent 90° THT
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard type filtered with 1000 pF
&lt;br&gt;High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;Choice of earthing metal sheet or high speed earthing clip
&lt;br&gt;Rated voltage: 100 VDC
&lt;br&gt;Rated current @ 20 ºC: 5 A
&lt;br&gt;Withstand voltage: 250 VRMS
&lt;br&gt;Insulation resistance: min. 1000 MΩ
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Device and Package Name Note:
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;MS means Size Metal Sheet
&lt;BR&gt;EC means Size Earthing Clip

&lt;br&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14704v209%20Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90"&gt;https://katalog.we-online.com/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-11&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="THT_37PIN_MALE"/>
</gates>
<devices>
<device name="" package="WE-D-SUB_THT90_EC_216112013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/216112013.pdf"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 216112013 "/>
<attribute name="POLES" value=" 37 "/>
<attribute name="TYPE" value="Male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
